**3GPP TSG-CT WG4 Meeting #123C4-242547**

**Hyderabad, India; 27th – 31st May 2024**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **29.673** | **CR** | **0062** | **rev** | **-** | **Current version:** | **16.7.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | 29.673 Rel16 API version and External doc update |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | TEI16 |  | ***Date:*** | 2024-06-05 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The following CRs modifying the Nucmf\_UECapabilityManagement API have been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in TS 29.501, subclause 4.3.1.- CR 29.673 - 0054 (C4-241528) backwards correctionexternalDocs needs also to be updated to refer to the new version of the specification. |
|  |  |
| ***Summary of change:*** | The Nucmf\_UECapabilityManagement API version number is incremented from 1.0.6 to 1.0.7externalDocs is updated to 3GPP TS 29.673 V16.8.0 |
|  |  |
| ***Consequences if not approved:*** | Incorrect API version number and externalDocs field |
|  |  |
| ***Clauses affected:*** | A2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | The CR introduced a backwards compatible correction in Nucmf\_UECapabilityManagement API. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

## A.2 Nucmf\_UECapabilityManagement API

openapi: 3.0.0

info:

 title: Nucmf\_UECapabilityManagement

 version: 1.0.7

 description: |

 Nucmf\_UECapabilityManagement Service.

 © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.673 V16.8.0; 5G System; UE Radio Capability Management Services

 url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.673/

servers:

 - url: '{apiRoot}/nucmf-uecm/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

\* \* \* End of Changes \* \* \* \*