**3GPP TSG-****RAN2 Meeting#110e R2-20XXXX**

**April, 2020**

**Agenda Item:** XXX

**Source:** Ericsson

**Title:** NR Rel-16 ASN.1 Review, Class 0 and Class 1 issues

**Document for:** Discussion and decision

# Guidelines

* This file is used to log NR 38331 ASN:1 Review Class 0 and Class 1 issues.
1. **Trivial** e.g. editorials, commas, colon, misspelling, missing/ double spaces, italics etc.
2. **Minor** e.g. quite straightforward changes e.g. correction/ addition of specification references or sub-clauses
* Fill in the columns, see example.
	+ Make sure the inserted specification text is unique, such that the location of the issue is simple to find.
	+ Avoid indicating duplicated issues by checking if the concerned specification text is already reported in the table.
	+ Step the file name v(x) -> v(x+1) and upload to ftp server.
* The “status” column will be filled in by the ASN.1 review moderator.

# Class 0 and Class 1 issues

| **Issue number** | **Copied existing specification text.****Text should be unique, so that it can be easily found in the specification.****If needed, add also the new text.** | **Comment/description/****correction** | **Email address**  | **Status** |
| --- | --- | --- | --- | --- |
| Ex 1 | 2> derive the KUPint key associated with the *integrityProtAlgorithm* indicated in the SecurityModeCommand message, as specified in TS 33.501 [11]; | Missing italics. | hakan.l.palm@ericsson.com |  |
| Ex 2 | PUSCH scheduled by RAR UL grant (see 38.213 clause 8.3 and 38.214 clause 6.1.2.2) and uses interlaced PUCCH Format 0, 1, 2, and 3 for cell-specific PUCCH (see TS 38.213 [13], clause 9.2.1). | Incorrect reference, should be 9.2.101. | hakan.l.palm@ericsson.com |  |
| 1 | **Original text:**Performs logging of available measurements together with location and time for logged measurement configured UEs.**Proposal text:**Performs logging of available measurements together with location and time ~~for~~ if logged measurements is configured ~~UEs~~. | There are two places in section 4.2.1 with the said text and both needs to be reworded as proposed. The reason for changing is to phrase the sentence from a specific UE point of view rather than a group of UEs point of view.  | pradeepa.ramachandra@ericsson.com |  |
| 2 | The UE may discard the connection establishment failure information, i.e. release the UE variable VarConnEsFailReport, 48 hours after the last connection establishment failure is detected. | Missing Italics | pradeepa.ramachandra@ericsson.com |  |
| 3 | **Generic comment:**In some places the term SSB is used and in some other SS/PBCH Block is used. It is better to align the text with a single terminology | Alignment between SSB and SS/PBCH Block | pradeepa.ramachandra@ericsson.com |  |
| 4 | 5> set the *measResultListNR* in *measResultNeighCells* to include all the available measurement quantities of the best measured cells associated to the *measObjectNR*, other than the source PCell, ordered such that the cell with highest SS/PBCH block RSRP is listed first if SS/PBCH block RSRP measurement results are available, otherwise the cell with highest SS/PBCH block RSRQ is listed first if SS/PBCH block RSRQ measurement results are available, otherwise the cell with highest SS/PBCH block SINR is listed first, based on the available SS/PBCH block based measurements collected up to the moment the UE detected handover failure; | ‘:’ instead of ‘;’ | pradeepa.ramachandra@ericsson.com |  |
| 5 | 4> if the SS/PBCH block-based measurement quantities are available;5> set the *measResultListNR* in *measResultNeighCells* to include all the available measurement quantities of the best measured cells associated to the *measObjectNR*, other than the source PCell, ordered such that the cell with highest SS/PBCH block RSRP is listed first if SS/PBCH block RSRP measurement results are available, otherwise the cell with highest SS/PBCH block RSRQ is listed first if SS/PBCH block RSRQ measurement results are available, otherwise the cell with highest SS/PBCH block SINR is listed first, based on the available SS/PBCH block based measurements collected up to the moment the UE detected handover failure;6> for each neighbour cell included, include the optional fields that are available; | ‘:’ instead of ‘;’ | pradeepa.ramachandra@ericsson.com |  |
| 6 | 4> if the CSI-RS based measurement quantities are available;5> set the *measResultListNR* in *measResultNeighCells* to include all the available measurement quantities of the best measured cells, other than the source PCell, ordered such that the cell with highest CSI-RS RSRP is listed first if CSI-RS RSRP measurement results are available, otherwise the cell with highest CSI-RS RSRQ is listed first if CSI-RS RSRQ measurement results are available, otherwise the cell with highest CSI-RS SINR is listed first, based on the available CSI-RS based measurements collected up to the moment the UE detected handover failure;6> for each neighbour cell included, include the optional fields that are available; | ‘:’ instead of ‘;’ | pradeepa.ramachandra@ericsson.com |  |
| 7 | 3> for each of the configured EUTRA frequencies in which measurements are available;4> set the *measResultListEUTRA* in *measResultNeighCells* to include the best measured cells ordered such that the cell with highest RSRP is listed first if RSRP measurement results are available, otherwise the cell with highest RSRQ is listed first, and based on measurements collected up to the moment the UE detected radio link failure; | ‘:’ instead of ‘;’ | pradeepa.ramachandra@ericsson.com |  |
| 8 | 3> set the *timeConnFailure* to the elapsed time since reception of the last *RRCReconfiguration* message including the *reconfigurationWithSync*; | This field name, timeConnFailure is not very self-explanatory and could be improved. Instead we can change the field name to ‘timeBetweenHOCommandAndFailure’. The changes are applicable in all places including ASN.1 | pradeepa.ramachandra@ericsson.com |  |
| 9 | 7> set the measResultListNR in measResultNeighCells to include all the available measurement quantities of the best measured cells, other than the source PCell, ordered such that the cell with highest SS/PBCH block RSRP is listed first if SS/PBCH block RSRP measurement results are available, otherwise the cell with highest SS/PBCH block RSRQ is listed first if SS/PBCH block RSRQ measurement results are available, otherwise the cell with highest SS/PBCH block SINR is listed first, based on the available SS/PBCH block based measurements collected up to the moment the UE detected radio link failure;8> for each neighbour cell included, include the optional fields that are available; | Missing italics‘:’ instead of ‘;’ | pradeepa.ramachandra@ericsson.com |  |
| 10 | 7> set the *measResultListNR* in *measResultNeighCells* to include all the available measurement quantities of the best measured cells, other than the source PCell, ordered such that the cell with highest CSI-RS RSRP is listed first if CSI-RS RSRP measurement results are available, otherwise the cell with highest CSI-RS RSRQ is listed first if CSI-RS RSRQ measurement results are available, otherwise the cell with highest CSI-RS SINR is listed first, based on the available CSI-RS based measurements collected up to the moment the UE detected radio link failure;8> for each neighbour cell included, include the optional fields that are available; | ‘:’ instead of ‘;’ | pradeepa.ramachandra@ericsson.com |  |
| 11 | 5> set the connectionFailureType to rlf;5> set the *c-RNTI* to the C-RNTI used in the PCell;5> set the *rlf-Cause* to the trigger for detecting radio link failure;5> if the rlf-Cause is set to randomAccessProblem or beamFailureRecoveryFailure: | Missing italics | pradeepa.ramachandra@ericsson.com |  |
| 12 | 8> set the *numberOfPreamblesSentOnSSB* to indicate the number of successive random access attempts associated to the SS/PBCH block;  | Missing hyphen (-) between random access i.e., random-access. | pradeepa.ramachandra@ericsson.com |  |
| 13 | 2> if the UE has connection resume failure informaton available in *VarConnEstFailReport* and if the RPLMN is not equal to plmn-identity stored in *VarConnEstFailReport*: | Missing italics | pradeepa.ramachandra@ericsson.com |  |
| 14 | 2> if the *ul-DelayValueConfig* is configured for the associated *reportConfig*:3> ignore the *measObject;*3> for each of the configured DRBs*,* configure the PDCP layer to perform corresponding average UL PDCP packet delay measurement per DRB [x5]; | Missing reference | pradeepa.ramachandra@ericsson.com |  |
| 15 | 1> if the *includeCommonLocationInfo* is configured in the corresponding *reportConfig* for this *measId* and detailed location information that has not been reported is available, set the content of *commonLocationInfo* of the *locationInfo* as follows:2> include the locationTimestamp;2> include the *locationCoordinate*, if available;2> include the *velocityEstimate*, if available;2> include the *locationError*, if available;2> include the *locationSource*, if available;2> if available, include the *gnss-TOD-msec*, | In section 5.5.5.1Missing italics‘;’ instead of ‘,’ | pradeepa.ramachandra@ericsson.com |  |
| 16 | 1> if *reportType* is set to *periodical*:2> if a single reporting quantity is set to *true* in *reportQuantityRS-Indexes*;3> consider the configured single quantity as the sorting quantity;2> else:3> if *rsrp* is set to *true*;4> consider RSRP as the sorting quantity;3> else:4> consider RSRQ as the sorting quantity; | In section 5.5.5.2 ‘:’ instead of ‘;’ | pradeepa.ramachandra@ericsson.com |  |
| 17 | I1> if available, set the *locationInfo* as follows:2> if available, set the *commonLocationInfo* to include the detailed location information;2> if available, set the *bt-LocationInfo* to include the Bluetooth measurement results, in order of decreasing RSSI for Bluetooth beacons;2> if available, set the *wlan-LocationInfo* to include the WLAN measurement results, in order of decreasing RSSI for WLAN APs.2> if available, set the *sensor-LocationInfo* to include the sensor measurement results.  | n section 5.7.3.5 and 5.7.3a.3 ‘;’ instead of ‘.’ | pradeepa.ramachandra@ericsson.com |  |
| 18 | 1> if the number of RA-Report stored in the RA-ReportList-r16 is less than 8, then append the following contents associated to the successfully completed random-access procedure as a new entry in the *VarRA-Report*: | Missing italics | pradeepa.ramachandra@ericsson.com |  |
| 19 | 2> else:3> set the plmn-Identity to the PLMN selected by upper layers from the PLMN(s) included in the plmn-IdentityList in SIB1; | Missing italics | pradeepa.ramachandra@ericsson.com |  |
| 20 | 2> set the parameters associated to individual random-access attempt in the chronological order of attmepts in the *perRAInfoList* as specified in 5.3.10.3: | ‘;’ instead of ‘:’ | pradeepa.ramachandra@ericsson.com |  |
| 21 | NG-RAN initiates the logged measurement configuration procedure to UE in RRC\_CONNECTED by sending the *LoggedMeasurementConfiguration* message. | ‘towards’ instead of ‘to’NG-RAN initiates the logged measurement configuration procedure towards UE in RRC\_CONNECTED by sending the *LoggedMeasurementConfiguration* message. | pradeepa.ramachandra@ericsson.com |  |
| 22 | This procedure specifies the logging of available measurements by a UE in RRC\_IDLE and RRC\_INACTIVE that has a logged measurement configuration. The actual process of logging within the UE, takes place in RRC IDLE state could continue in RRC INACTIVE state or vice versa. | Missing ‘and’This procedure specifies the logging of available measurements by a UE in RRC\_IDLE and RRC\_INACTIVE that has a logged measurement configuration. The actual process of logging within the UE, takes place in RRC IDLE state and could continue in RRC INACTIVE state or vice versa. | pradeepa.ramachandra@ericsson.com |  |
| 23 | **Generic comment:**The terminology reportType used in loggedMeasurementConfiguration and the associated UE variable VarLogMeasConfig.  | The purpose of this field is to inform the UE ‘when’ to log, not ‘what’ to log. Therefore, the field name is misleading.It is proposed to change it to loggingType instead of reportType. | pradeepa.ramachandra@ericsson.com |  |
| 24 | 3> if the UE is camping normally on an NR cell and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport* and, if the cell is part of the area indicated by *areaConfiguration* if configured in *VarLogMeasConfig*: | Remove the ‘,’ | pradeepa.ramachandra@ericsson.com |  |
| 25 | 4> set the *measResultServCell* to include the quantities of the last logged cell the UE was camping on; 3> else:4> set the *servCellIdentity* to indicate global cell identity of the cell the UE is camping on;4> set the *measResultServCell* to include the quantities of the cell the UE is camping on; | There is no IE by the name ‘measResultServCell’.Missing part of the correct field name (‘ing’). It should have been measResultServingCell’ | pradeepa.ramachandra@ericsson.com |  |
| 26 | 4> if available, set the *measResultNeighCells*, in order of decreasing ranking-criterion as used for cell re-selection, to include neighbouring cell measurements ~~(excluding the~~ *~~resultsSSB-Indexes~~* ~~IE)~~ that became available during the last logging interval for at most the following number of neighbouring cells: 6 intra-frequency and 3 inter-frequency neighbours per frequency as well as 3 inter-RAT neighbours, per frequency/ set of frequencies per RAT and according to the following: | No need for the text in the brackets as the field *measResultNeighCells* does not contain *resultsSSB-Indexes* | pradeepa.ramachandra@ericsson.com |  |
| 27 | LoggedMeasurementConfiguration-r16-IEs ::= SEQUENCE { traceReference-r16 TraceReference-r16, traceRecordingSessionRef-r16 OCTET STRING (SIZE (2)), tce-Id-r16 OCTET STRING (SIZE (1)), absoluteTimeInfo-r16 AbsoluteTimeInfo-r16, areaConfiguration-r16 AreaConfiguration-r16 OPTIONAL, --Need R plmn-IdentityList-r16 PLMN-IdentityList3-r16 OPTIONAL, --Need R bt-NameList-r16 BT-NameListConfig-r16 OPTIONAL, --Need R wlan-NameList-r16 WLAN-NameListConfig-r16 OPTIONAL, --Need R sensor-NameList-r16  Sensor-NameListConfig-r16 OPTIONAL, --Need R loggingDuration-r16 LoggingDuration-r16, reportType CHOICE { periodical LoggedPeriodicalReportConfig-r16, eventTriggered LoggedEventTriggerConfig-r16 }} | Missing ‘-r16’ | pradeepa.ramachandra@ericsson.com |  |
| 28 | ***eventType***The value outOfCoverage indicates the UE to perform logging of measurements when the UE enters any cell selection state, and the value eventL1 indicates the UE to perform logging of measurements when the triggering condition (similar as event A2 as specified in 5.5.4.3) as configured in the event is met for the camping cell in camped normally state.  | Missing italics | pradeepa.ramachandra@ericsson.com |  |
| 29 | LogMeasInfo-r16 ::= SEQUENCE { locationInfo-r16 LocationInfo-r16 OPTIONAL, relativeTimeStamp-r16 INTEGER (0..7200), servCellIdentity-r16 CGI-InfoNR-Logging-r16, measResultServingCell-r16 MeasResultServingCell-r16 OPTIONAL, measResultNeighCells-r16 SEQUENCE { measResultNeighCellListNR MeasResultListLogging2NR-r16 OPTIONAL, measResultNeighCellListEUTRA MeasResultList2EUTRA-r16 OPTIONAL }, anyCellSelectionDetected-r16 ENUMERATED {true} OPTIONAL} | Missing -r16 | pradeepa.ramachandra@ericsson.com |  |
| 30 | ***timeStamp***Includes time stamps for the waypoints that describe planned locations for the UE.  | No such field. Remove the field description completely. | pradeepa.ramachandra@ericsson.com |  |
| 31 | ***numberOfConnFail***This field is used to indicate the number of failed connection setup attempts after radio link failure. | There is no relation to RLF. Remove ‘after radio link failure’ | pradeepa.ramachandra@ericsson.com |  |
| 32 | ***numberOfPreamblesSent***This field is used to indicate the number of random access preambles that were transmitted. | No such field. Remove the field description completely. | pradeepa.ramachandra@ericsson.com |  |
| 33 | ***maxTxPowerReached***This field is used to indicate whether or not the maximum power level was used for the last transmitted preamble.  | No such field. Remove the field description completely. | pradeepa.ramachandra@ericsson.com |  |
| 34 | ***cellIdentity-eutra-epc, cellIdentity-eutra-5GC***Unambiguously identify a cell within a PLMN and it belongs the first *PLMN-IdentityInfo* IE of *PLMN-IdentityInfoList* in *SIB1*. | Missing ‘to’***cellIdentity-eutra-epc, cellIdentity-eutra-5GC***Unambiguously identify a cell within a PLMN and it belongs to the first *PLMN-IdentityInfo* IE of *PLMN-IdentityInfoList* in *SIB1*. | pradeepa.ramachandra@ericsson.com |  |
| 35 | ***excessDelay***Indicates excess queueing delay ratio in UL, according to excess delay ratio measurement report mapping table, as defined in TS 38.314 [x5], Table 4.2.1.1.1-1.  | No such field. Remove the field description completely. | pradeepa.ramachandra@ericsson.com |  |
| 36 | -- ASN1START-- TAG-ULDELAYVALUECONFIG-STARTUL-DelayValueConfig-r16 ::= SEQUENCE { delay-DRBlist SEQUENCE (SIZE(1..maxDRB)) OF DRB-Identity}-- TAG-ULDELAYVALUECONFIG-STOP-- ASN1STOP | Missing ‘-r16’ | pradeepa.ramachandra@ericsson.com |  |
| 37 | Sensor-NameList-r16 ::= SEQUENCE {  measUncomBarPre-r16 BOOLEAN OPTIONAL, -- Need R measUeSpeed BOOLEAN OPTIONAL, -- Need R measUeOrientation BOOLEAN OPTIONAL -- Need R}-- TAG-SENSORNAMELISTCONFIG-STOP-- ASN1STOP | Missing ‘-r16’ | pradeepa.ramachandra@ericsson.com |  |
| 38 | ***measUncomBarPre***If configured, the UE reports the uncompensated Barometeric pressure measurement as defined in uncompensatedBarometricPressure-r16. | There is no IE called ‘uncompensatedBarometricPressure-r16’. But it is defined in 37.355. Therefore, propose to change the field description as;***measUncomBarPre***If configured, the UE reports the uncompensated Barometeric pressure measurement as defined by *uncompensatedBarometricPressure* is TS 37.355 [YY]. | pradeepa.ramachandra@ericsson.com |  |
| 39 | reportType CHOICE { periodical LoggedPeriodicalReportConfig-r16, eventTriggered LoggedEventTriggerConfig-r16 } | Missing ‘-r16’ | pradeepa.ramachandra@ericsson.com |  |
| 40 | -- ASN1START-- TAG-VARLOGMEAREPORT-STARTVarLogMeasReport-r16 ::= SEQUENCE { absoluteTimeStamp-r16 AbsoluteTimeInfo-r16, traceReference-r16 TraceReference-r16, traceRecordingSessionRef-r16 OCTET STRING (SIZE (2)), tce-Id-r16 OCTET STRING (SIZE (1)), logMeasInfoList-r16 LogMeasInfoList-r16, plmn-IdentityList-r16 PLMN-IdentityList3-r16}-- TAG-VARLOGMEAREPORT-STOP-- ASN1STOP | Missing ‘S’VARLOGMEASREPORT | pradeepa.ramachandra@ericsson.com |  |
| 41 | MeasResultServingCell-r16 ::= SEQUENCE { physCellId PhysCellId OPTIONAL, resultsSSB-Cell MeasQuantityResults OPTIONAL, resultsSSB SEQUENCE{ best-ssb-Index SSB-Index, best-ssb-Results MeasQuantityResults OPTIONAL, numberOfGoodSSB INTEGER (1..maxNrofSSBs) OPTIONAL } OPTIONAL, ...} | Missing ‘-r16’ | pradeepa.ramachandra@ericsson.com |  |
| 42 | [[    simultaneousTCI-UpdateList-r16                   SEQUENCE (SIZE (1..maxNrofServingCells)) OF ServCellIndex           OPTIONAL,   -- Need R    simultaneousTCI-UpdateListSecond-r16             SEQUENCE (SIZE (1..maxNrofServingCells)) OF ServCellIndex           OPTIONAL,   -- Need R    simultaneousSpatial-UpdatedList-r16               SEQUENCE (SIZE (1..maxNrofServingCells)) OF ServCellIndex           OPTIONAL,   -- Need R    simultaneousSpatial-UpdatedListSecond-r16        SEQUENCE (SIZE (1..maxNrofServingCells)) OF ServCellIndex           OPTIONAL    -- Need R    ]]In CellGroupConfig IE |     [[    tci-RelationCellList1-r16                    SEQUENCE (SIZE (1..maxNrofServingCells)) OF ServCellIndex           OPTIONAL,   -- Need R    tci-RelationCellList2-r16                    SEQUENCE (SIZE (1..maxNrofServingCells)) OF ServCellIndex           OPTIONAL,   -- Need R    spatialRelationCellList1-r16                 SEQUENCE (SIZE (1..maxNrofServingCells)) OF ServCellIndex           OPTIONAL,   -- Need R    spatialRelationCellList2-r16                  SEQUENCE (SIZE (1..maxNrofServingCells)) OF ServCellIndex           OPTIONAL    -- Need R    ]] | Helka-liina.maattanen@ericsson.com |  |
| 43 |  lte-CRS-PatternList-r16 SetupRelease { LTE-CRS-PatternList-r16 } OPTIONAL, -- Cond LTE-CRS lte-CRS-PatternListSecond-r16 SetupRelease { LTE-CRS-PatternList-r16 } OPTIONAL, -- Cond CORESETPoolIN servingCellConfig IE |     lte-CRS-PatternList1-r16             SetupRelease { LTE-CRS-PatternList-r16 }                          OPTIONAL,   -- Cond LTE-CRS    lte-CRS-PatternList2-r16             SetupRelease { LTE-CRS-PatternList-r16 }                          OPTIONAL,   -- Cond CORESETPool | Helka-liina.maattanen@ericsson.com |  |
| 44 | The field description of ***sps-ConfigList*** in IE BWP-DownlinkDedicated“UE specific **multiple** SPS (Semi-Persistent Scheduling) configurations for one BWP.” should be “UE specific **one or multiple** SPS (Semi-Persistent Scheduling) configurations for one BWP.” | The list can have one element and the wording “multiple” is not precise | zhenhua.zou@ericsson.com |  |
| 45 | The field description of ***configuredGrantConfigList*** in IE BWP-UplinkDedicated“A list of **multiple** configured grant configurations for one BWP.” should be “A list of **one or multiple** configured grant configurations for one BWP.” | The list can have one element and the wording “multiple” is not precise | zhenhua.zou@ericsson.com |  |
| 46 | The definition of the IE *ConfiguredGrantConfigList*: “The IE *ConfiguredGrantConfigList* is used to configure **multiple** uplink Configured Grant configurations in one BWP.”should be “The IE *ConfiguredGrantConfigList* is used to configure **one or multiple** uplink Configured Grant configurations in one BWP.” | The list can have one element and the wording “multiple” is not precise | zhenhua.zou@ericsson.com |  |
| 47 | In the field description of IE *ConfiguredGrantConfigList:*“Indicates a list of **multiple** UL Configured Grant configurations to be added or modified.”should be “Indicates a list of **one or multiple** UL Configured Grant configurations to be added or modified.” | The list can have one element and the wording “multiple” is not precise | zhenhua.zou@ericsson.com |  |
| 48 | In the field description of IE *ConfiguredGrantConfigList:*“Indicates a list of **multiple** UL Configured Grant configurations to be released.”should be “Indicates a list of **one or** **multiple** UL Configured Grant configurations to be released.” | The list can have one element and the wording “multiple” is not precise | zhenhua.zou@ericsson.com |  |
| 49 | In the definition of IE SPS-ConfigList“The IE *SPS-ConfigList* is used to configure **multiple** downlink SPS configurations in one BWP.”should be “The IE *SPS-ConfigList* is used to configure **one or multiple** downlink SPS configurations in one BWP.” | The list can have one element and the wording “multiple” is not precise | zhenhua.zou@ericsson.com |  |
| 50 | In the field description of IE SPS-ConfigList“Indicates a list of **multiple** DL SPS configurations to be added or modified“should be“Indicates a list of **one or multiple** DL SPS configurations to be added or modified” | The list can have one element and the wording “multiple” is not precise | zhenhua.zou@ericsson.com |  |
| 51 | In the field description of IE SPS-ConfigList“Indicates a list of **multiple** DL SPS configurations to be released.”should be “Indicates a list of **one or multiple** DL SPS configurations to be released.” | The list can have one element and the wording “multiple” is not precise | zhenhua.zou@ericsson.com |  |
| 52 | In the BeamFailureRecoveryConfig field descriptions, for the field description of ra-prioritization and ra-PrioritizationTwoStep, the reference to 38.321 should point to clause 5.1.1a instead of 5.1.1***ra-prioritization***Parameters which apply for prioritized random access procedure for BFR (see TS 38.321 [3], clause 5.1.1).***ra-PrioritizationTwoStep***Parameters which apply for prioritized 2-step random access procedure for BFR (see TS 38.321 [3], clause 5.1.1). | ***ra-prioritization***Parameters which apply for prioritized random access procedure for BFR (see TS 38.321 [3], clause 5.1.1a).***ra-PrioritizationTwoStep***Parameters which apply for prioritized 2-step random access procedure for BFR (see TS 38.321 [3], clause 5.1.1a). | eswar.vutukuri@zte.com.cn |  |
| 53 | *RACH-ConfigCommonTwoStepRA* information elementrach-ConfigGenericTwoStepRA-r16 RACH-ConfigCommonTwoStepRA-r16,The highlighted text should have been RACH-ConfigGenericTwoStepRA-r16 | Change as follows: rach-ConfigGenericTwoStepRA-r16 ~~RACH-ConfigCommonTwoStepRA-r16~~ Rach-ConfigGenericTwoStepRA-r16, | eswar.vutukuri@zte.com.cn |  |
| 54 | 5.7.10.33> set the *rlf-Report* in the *UEInformationResponse* message to the value of *rlf-Report* in *VarRLF-Report*;3> discard the *rlf-Report* from *VarRLF-Report* upon successful delivery of the *UEInformationResponse* message confirmed by lower layers;3> discard the *rlf-Report* from *VarRLF-Report* of TS 36.331 [10] upon successful delivery of the *UEInformationResponse* message confirmed by lower layers; | 3> set the *rlf-Report* in the *UEInformationResponse* message to the value of *rlf-Report* in *VarRLF-Report* of TS 36.331 [10];3> discard the *rlf-Report* from *VarRLF-Report* of TS 36.331 [10] upon successful delivery of the *UEInformationResponse* message confirmed by lower layers; | fanjiangsheng@catt.cn |  |
| 55 | 5.5a.3.23> if the UE is camping normally on an NR cell and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport* and, if the cell is part of the area indicated by *areaConfiguration* if configured in *VarLogMeasConfig*:4> perform the logging at regular time intervals, as defined by the *loggingInterval* in the *LoggedEventTriggerConfig*; | 3> if the UE is camping normally on an NR cell and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport* and, if the cell is part of the area indicated by *areaConfiguration* if configured in *VarLogMeasConfig*:4> perform the logging at regular time intervals, as defined by the *loggingInterval* in the *periodical*; | fanjiangsheng@catt.cn |  |
| 56 | 5.5a.3.22> else if the *reportType* is set to *eventTriggered*, which indicates *outOfCoverage*:3> perform the logging at regular time intervals as defined by the *loggingInterval* in *VarLogMeasConfig* only when the UE is in any cell selection state;2> else if the *reportType* is set to *eventType* and *eventL1* is indicated:3> perform the logging at regular time intervals as defined by the *loggingInterval* in *VarLogMeasConfig* only when the conditions indicated by the *eventL1* are met; | 2> else if the *reportType* is set to *eventTriggered*, which indicates *outOfCoverage*:3> perform the logging at regular time intervals as defined by the *loggingInterval* in *eventTriggered* only when the UE is in any cell selection state;2> else if the *reportType* is set to *eventType* and *eventL1* is indicated:3> perform the logging at regular time intervals as defined by the *loggingInterval* in *eventTriggered* only when the conditions indicated by the *eventL1* are met; | fanjiangsheng@catt.cn |  |
| 57 | *RadioLinkMonitoringConfig*The IE *RadioLinkMonitoringConfig* is used to configure radio link monitoring for detection of beam- and/or cell radio link failure. See also TS 38.321 [3], clause 5.1.1. | *RadioLinkMonitoringConfig*The IE *RadioLinkMonitoringConfig* is used to configure radio link monitoring for detection of beam- and/or cell radio link failure. See also TS 38.321 [3], clause 5.17. | fanjiangsheng@catt.cn |  |
| 58 | 5.3.5.91> if the received *otherConfig* includes the *BT-NameListConfig*:2> if *BT-NameListConfig* is set to *setup*, attempt to have Bluetooth measurement results available for subsequent measurement report;1> if the received *otherConfig* includes the *WLAN-NameListConfg*:2> if *WLAN-NameListConfg* is set to *setup*, attempt to have WLAN measurement results available for subsequent measurement report;NOTE 2: The UE is requested to attempt to have valid Bluetooth measurements and WLAN measurements whenever sending a measurement report for which it is configured to include these measurements. The UE may not succeed e.g. because the user manually disabled the WLAN or Bluetooth hardware. Further details, e.g. regarding when to activate WLAN or Bluetooth, are up to UE implementation.1> if the received *otherConfig* includes the *Sensor-NameListConfig*:2> if *Sensor-NameListConfig* is set to *setup*, attempt to have Sensor measurement results available for subsequent measurement report; | 1> if the received *otherConfig* includes the *bt-NameList*:2> if *bt-NameList* is set to *setup*, attempt to have Bluetooth measurement results available for subsequent measurement report;1> if the received *otherConfig* includes the *wlan-NameList*:2> if *wlan-NameList* is set to *setup*, attempt to have WLAN measurement results available for subsequent measurement report;NOTE 2: The UE is requested to attempt to have valid Bluetooth measurements and WLAN measurements whenever sending a measurement report for which it is configured to include these measurements. The UE may not succeed e.g. because the user manually disabled the WLAN or Bluetooth hardware. Further details, e.g. regarding when to activate WLAN or Bluetooth, are up to UE implementation.1> if the received *otherConfig* includes the *sensor-NameList*:2> if *sensor-NameList* is set to *setup*, attempt to have Sensor measurement results available for subsequent measurement report; | fanjiangsheng@catt.cn |  |
| 59 | 5.3.5.8.33> if detailed location information is available, set the content of the *LocationInfo* as follows:4> if available, set the *commonLocationInfo* to include the detailed location information;4> if available, set the *bt-LocationInfo* to include the Bluetooth measurement results, in order of decreasing RSSI for Bluetooth beacons;4> if available, set the *wlan-LocationInfo* to include the WLAN measurement results, in order of decreasing RSSI for WLAN APs;4> if available, set the *sensor-LocationInfo* to include the sensor measurement results; | 3> if available, set the content of the *locationInfo* as follows:4> if available, set the *commonLocationInfo* to include the detailed location information;4> if available, set the *bt-LocationInfo* to include the Bluetooth measurement results, in order of decreasing RSSI for Bluetooth beacons;4> if available, set the *wlan-LocationInfo* to include the WLAN measurement results, in order of decreasing RSSI for WLAN APs;4> if available, set the *sensor-LocationInfo* to include the sensor measurement results; | fanjiangsheng@catt.cn |  |
| 60 | 5.3.10.35> if detailed location information is available, set the content of *locationInfo* as follows:6> if available, set the *commonLocationInfo* to include the detailed location information;6> if available, set the *bt-LocationInfo* in *locationInfo* to include the Bluetooth measurement results, in order of decreasing RSSI for Bluetooth beacons;6> if available, set the *wlan-LocationInfo* in *locationInfo* to include the WLAN measurement results, in order of decreasing RSSI for WLAN APs;6> if available, set the *sensor-LocationInfo* in *locationInfo* to include the sensor measurement results; | 5> if available, set the content of *locationInfo* as follows:6> if available, set the *commonLocationInfo* to include the detailed location information;6> if available, set the *bt-LocationInfo* in *locationInfo* to include the Bluetooth measurement results, in order of decreasing RSSI for Bluetooth beacons;6> if available, set the *wlan-LocationInfo* in *locationInfo* to include the WLAN measurement results, in order of decreasing RSSI for WLAN APs;6> if available, set the *sensor-LocationInfo* in *locationInfo* to include the sensor measurement results; | fanjiangsheng@catt.cn |  |
| 61 | 5.5.5.1 General1> if the *includeCommonLocationInfo* is configured in the corresponding *reportConfig* for this *measId* and detailed location information that has not been reported is available, set the content of *commonLocationInfo* of the *locationInfo* as follows:2> include the locationTimestamp;2> include the *locationCoordinate*, if available;2> include the *velocityEstimate*, if available;2> include the *locationError*, if available;2> include the *locationSource*, if available;2> if available, include the *gnss-TOD-msec*,1> if the *includeWLAN-Meas* is configured in the corresponding *reportConfig* for this *measId*, set the *wlan-LocationInfo* of the *locationInfo* in the *measResults* as follows:2> if available, include the *LogMeasResultWLAN*, in order of decreasing RSSI for WLAN APs;1> if the *includeBT-Meas* is configured in the corresponding *reportConfig* for this *measId*, set the *BT-LocationInfo* of the *locationInfo* in the *measResults* as follows:2> if available, include the *LogMeasResultBT*, in order of decreasing RSSI for Bluetooth beacons;1> if the *includeSensor-Meas* is configured in the corresponding reportConfig for this *measId*, set the *sensor-LocationInfo* of the *locationInfo* in the *measResults* as follows:2> if available, include the sensor-MeasurementInformation;2> if available, include the *sensor-MotionInformation*; | 1> if the *includeCommonLocationInfo* is configured in the corresponding *reportConfigNR* for this *measId* and detailed location information that has not been reported is available, set the content of *commonLocationInfo* of the *locationInfo* as follows:2> include the locationTimeStamp;2> include the *locationCoordinate*, if available;2> include the *velocityEstimate*, if available;2> include the *locationError*, if available;2> include the *locationSource*, if available;2> include the *gnss-TOD-msec*, if available;1> if the *includeWLAN-Meas* is configured in the corresponding *reportConfigNR* for this *measId*, set the *wlan-LocationInfo* of the *locationInfo* in the *measResults* as follows:2> if available, include the *wlan-LocationInfo*, in order of decreasing RSSI for WLAN APs;1> if the *includeBT-Meas* is configured in the corresponding *reportConfigNR* for this *measId*, set the *bt-LocationInfo* of the *locationInfo* in the *measResults* as follows:2> if available, include the *bt-LocationInfo*, in order of decreasing RSSI for Bluetooth beacons;1> if the *includeSensor-Meas* is configured in the corresponding *reportConfigNR* for this *measId*, set the *sensor-LocationInfo* of the *locationInfo* in the *measResults* as follows:2> if available, include the sensor-MeasurementInformation;2> if available, include the *sensor-MotionInformation*; | fanjiangsheng@catt.cn |  |
| 62 | 5.5a.3.24> include the *locationCoordinates*;3> if *WLAN-NameList* is included in *VarLogMeasConfig*:4> if detailed WLAN measurements are available:5> include *logMeasResultListWLAN*, in order of decreasing RSSI for WLAN APs;3> if *BT-NameList* is included in *VarLogMeasConfig*:4> if detailed Bluetooth measurements are available:5> include *logMeasResultListBT*, in order of decreasing RSSI for Bluetooth beacons;3> if *Sensor-NameList* is included in *VarLogMeasConfig*:4> if detailed Sensor measurements are available:5> include *Sensor-LocationInfo-r16* for sensors; | 4> include the *locationCoordinate*;3> if *wlan-NameList* is included in *VarLogMeasConfig*:4> if detailed WLAN measurements are available:5> include *wlan-LocationInfo*, in order of decreasing RSSI for WLAN APs;3> if *bt-NameList* is included in *VarLogMeasConfig*:4> if detailed Bluetooth measurements are available:5> include *bt-LocationInfo*, in order of decreasing RSSI for Bluetooth beacons;3> if *sensor-NameList* is included in *VarLogMeasConfig*:4> if detailed Sensor measurements are available:5> include *sensor-LocationInfo*for sensors; | fanjiangsheng@catt.cn |  |
| 63 | *LogMeasReport* field descriptions***logMeasResultListBT***and ***logMeasResultListWLAN*** | Remove field description for ***logMeasResultListBT***and ***logMeasResultListWLAN*** as no related IE | fanjiangsheng@catt.cn |  |
| 64 | ***CommonLocationInfo* information element**locationTimestamp-r16 OCTET STRING OPTIONAL,Field ***LocationTimeStamp*** | locationTimeStamp-r16 OCTET STRING OPTIONAL,Field ***locationTimeStamp*** | fanjiangsheng@catt.cn |  |
| 65 | Definition of *BT-NameList* | Change *BT-NameList* to *BT-NameListConfig* for the whole definition | fanjiangsheng@catt.cn |  |
| 66 | Definition of *LogMeasResultListWLAN*Field description name | Use lowercase letters for the whole Field description name. | fanjiangsheng@catt.cn |  |
| 67 | Definition of *Sensor-NameListConfig* ***measUncomBarPre***If configured, the UE reports the uncompensated Barometeric pressure measurement as defined in uncompensatedBarometricPressure-r16 | ***measUncomBarPre***If configured, the UE reports the uncompensated Barometeric pressure measurement as defined in TS 37.355 [x1]; | fanjiangsheng@catt.cn |  |
| 68 | Definition of *WLAN-NameList* | Change *WLAN-NameList* to *WLAN-NameListConfig* for the whole definition | fanjiangsheng@catt.cn |  |
| 69 | *RACH-ConfigDedicated* information elementCFRA-TwoStep-r16 ::= SEQUENCE { occasionsTwoStepRA-r16 SEQUENCE { rach-ConfigGenericTwoStepRA-r16 RACH-ConfigGeneric, … -- Cond SSB-CFRA }  | The IE rach-ConfigGenericTwoStepRA-r16 definition should change to rach-ConfigGenericTwoStepRA-r16 ~~RACH-ConfigGeneric~~ RACH-ConfigGenericTwoStepRA, | erlin.zeng@catt.cn |  |
| 70 | In the definition of PNI-NPN identity,**PNI-NPN identity:** an identifier of a PNI-NPN compromising of a PLMN ID and a CAG -ID combination. | “compromising” should be “comprising” here | zhourui@catt.cn |  |
| 71 | SIB-TypeInfo ::= SEQUENCE { type ENUMERATED {sibType2, sibType3, sibType4, sibType5, sibType6, sibType7, sibType8, sibType9, spare8, spare7, spare6, spare5, spare4, spare3, spare2, spare1,... }, | “sibType10~ sibType14” should be defined as SIB10~SIB14 has been newly added | zhourui@catt.cn |  |
| 72 | In the *“NPN-Identity* field descriptions*”****CAG-Identity***A CAG-ID as specified in TS 23.003 [21]. The PLMN ID and a CAG ID in the *NPN-Identity* identifies a PNI-NPN.***NID***A NID as specified in TS 23.003 [21]. The PLMN ID and a NID in the *NPN-Identity* identifies a SNPN. | Field identifiers shall start with a lowercase letter*~~CAG-Identity~~**cag-Identity****~~NID~~***nid | zhourui@catt.cn |  |
| 73 | In the *“NPN-IdentityInfoList* field descriptions”***NPN-IdentityInfo***The *NPN-IdentityInfo* contains one or more NPN identities and additional information associated with those NPNs. | Suggest to remove the description for ***NPN-IdentityInfo*** as “NPN-IdentityInfo” is a information element,it is not a field | zhourui@catt.cn |  |
| 74 | **Existing text:** SIBs other than *SIB1* and posSIBs are carried in *SystemInformation* (SI) messages**New text:**SIBs (other than *SIB1)* and posSIBs are carried in *SystemInformation* (SI) messages | Ambiguous text. It could be misread that posSIBs are not carried in SI messages. Placing the SIB1 inside parenthesis removes ambiguity. | mani.thyagarajan@nokia.com |  |
| 75 |  sl-OffsetDFN-r16 INTEGER (0..1000) OPTIONAL, -- Need R t400 ENUMERATED {ms100, ms200, ms300, ms400, ms600, ms1000, ms1500, ms2000} OPTIONAL, -- Need Rin SL-ConfigCommonNR-r16 | Suffix of T400 is missing, i.e., “-r16” | qianxi.lu@oppo.com |  |
| 76 | ***sl-TimeResourcePSCCH***Indicates the number of sumbols of PSCCH in a resource pool. | Typo of “sumbols” should be corrected as “symbols” | qianxi.lu@oppo.com |  |
| 77 | – *SL-CBR-TxConfigList*The IE *SL-CBR-CommonTxConfigList* indicates | The name of the IE is not aligned with the description, should be corrected as – *SL-CBR-CommonTxConfigList*The IE *SL-CBR-CommonTxConfigList* indicates | qianxi.lu@oppo.com |  |
| 78 | **3. NR sidelink measurement identities:** A list of NR sidelink measurement identities where each NR sidelink measurement identity links one NR sidelink measurement object with one NR sidelink reporting configuration. By configuring multiple NR sidelink measurement identities, it is possible to link more than one NR sidelink measurement object to the same NR sidelink reporting configuration, as well as to link more than one NR sidelink reporting configuration to the same NR sidelink measurement object. The NR sidelink measurement identity is also included in the NR sidelink measurement report that triggered the reporting, serving as a reference to the network. | This section is for measurement and report via PC5-RRC, so the report is not to network, but the associated peer UE, so it should be corrected to **3. NR sidelink measurement identities:** A list of NR sidelink measurement identities where each NR sidelink measurement identity links one NR sidelink measurement object with one NR sidelink reporting configuration. By configuring multiple NR sidelink measurement identities, it is possible to link more than one NR sidelink measurement object to the same NR sidelink reporting configuration, as well as to link more than one NR sidelink reporting configuration to the same NR sidelink measurement object. The NR sidelink measurement identity is also included in the NR sidelink measurement report that triggered the reporting, serving as a reference to the associated peer UE. | qianxi.lu@oppo.com |  |
| 79 | In 5.5.4.11,***Thresh*** is the threshold parameter for this event (i.e. *s1-Threshold* as defined within *reportConfigNR-SL* for this event).apparently this should be c1-threshold instead of s1-threshold | Correct it to c1-threshold | qianxi.lu@oppo.com |  |
| 80 | In 5.5.4.12,***Thresh*** is the threshold parameter for this event (i.e. *v2-Threshold* as defined within *reportConfigNR-SL* for this event).apparently this should be c2-threshold instead of v2-threshold | Correct it to c2-threshold | qianxi.lu@oppo.com |  |
| 81 | In field description of “*SL-PSSCH* field descriptions”*sl-BetaOffsets* *Configure beta-offset values for the second stage SCI mapping.*There is no such IE of sl-BetaOffsets, so no need for this field description | Remove this field description | qianxi.lu@oppo.com |  |
| 82 | upon indication of consistent uplink LBT failures from SCG MAC: | "; or" is missing before "1> upon indication of consistent uplink LBT failures from SCG MAC:" | jack.jang@samsung.com |  |
| 83 | cg-minDFIDelay | It should be corrected to 'cg-minDFI-Delay' ('-' is missing) | jack.jang@samsung.com |  |
| 84 | channellAccessPriority | It should be corrected to ' channelAccessPriority' (i.e. double l) | jack.jang@samsung.com |  |
| 85 | dl-DCI-triggered-UL-ChannelAccess-CPext | It should be corrected to ' dl-DCI-triggered-UL-ChannelAccess-CP-ext-r16' (i.e. to add '-' after acronym CP). | jack.jang@samsung.com |  |
| 86 | ul-dci-triggered-UL-ChannelAccess-CPext-CAPC | It should be corrected to ' ul-dci-triggered-UL-ChannelAccessCP-ext-CAPC-r16' (i.e. to remove '-' after Access and add '-' after acronym CP). | jack.jang@samsung.com |  |
| 87 | 3> if the UE is in any cell seletion state (as specificed in TS 38.304 [20]): | Spelling errorsSeletion 🡪 selectionSpecified 🡪 specified | pradeepa.ramachandra@ericsson.com |  |
| 88 | In section 5.3.3.7 and 5.3.13.53> set *perRAInfoList* to indicate random access failure information as specified in 5.3.10.3; | As the cause for connection establishment/resume failure might not be due to random access procedure, the term ‘random access failure’ here is nor appropriate. We propose to change it to ‘random access procedure related’ i.e.,3> set *perRAInfoList* to indicate random access ~~failure~~ procedure related information as specified in 5.3.10.3; | pradeepa.ramachandra@ericsson.com |  |
| 89 | **Existing text: 5.3.5.13**The network configures the UE with one or more candidate target SpCells in the conditional configuration. The UE evaluates the condition of each configured candidate target SpCell. The UE applies the conditional configuration associated with one of the target SpCells which fulfils associated execution condition. The network provides the configuration parameters for the target SpCell in the *ConditionalReconfiguration* IE.**New text:**The network configures the UE with one or more candidate target SpCells in the conditional configuration. The UE evaluates the condition of each configured candidate target SpCell. The UE applies the conditional configuration associated with one of the target SpCells which fulfils associated execution condition. The network provides the configuration parameters for the target SpCells in the *ConditionalReconfiguration* IE. | The field *conditionReconfiguration* can include more than one target SpCells configuration. | chandrika@catt.cn |  |
| 90 | Section 5.3.10.3:4> set the *ssbRLMConfigBitmap* and/or *csi-rsRLMConfigBitmap* in *measResultLastServCell* to include the radio link monitoring configuration of the source PCell; | The same text in context of HO failure (exists in section 5.3.5.8.3) – but over there it makes sense. Here “source PCell” does not exist, as the section specify RLF failure related actions.Change to:4> set the *ssbRLMConfigBitmap* and/or *csi-rsRLMConfigBitmap* in *measResultLastServCell* to include the radio link monitoring configuration of the PCell where radio link failure is detected;; | malgorzata.tomala@nokia.com |  |
| 91 | *UEInformationResponse-IEs* field descriptions***ra-Report***This field is used to provide the list of RA reports that is stored by the UE for the past upto *maxRAReport-r16* number of successful random access procedues. | Change the field name to:ra-ReportList | malgorzata.tomala@nokia.com |  |
| 92 | 5.7.10.3 Reception of the UEInformationRequest message1> if *ra-ReportReq* is set to *true* and the UE has random access related information available in *VarRA-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRA-Report*:2> set the *ra-Report* in the *UEInformationResponse* message to the value of *ra-Report* in *VarRA-Report*;2> discard the *ra-Report* from *VarRA-Report* upon successful delivery of the *UEInformationResponse* message confirmed by lower layers; | Change to:1> if *ra-ReportReq* is set to *true* and the UE has random access related information available in *VarRA-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRA-Report*:2> set the *ra-ReportList* in the *UEInformationResponse* message to the value of *ra-ReportList* in *VarRA-Report*;2> discard the *ra-ReportList* from *VarRA-Report* upon successful delivery of the *UEInformationResponse* message confirmed by lower layers; | malgorzata.tomala@nokia.com |  |
| 93 |     raPurpose-r16                          ENUMERATED {accessRelated, beamFailureRecovery, reconfigurationWithSync, ulUnSynchronized,                                                  schedulingRequestFailure, noPUCCHResourceAvailable, sCellAdditionTAAdjestment,                                                  requestForOtherSI, spare8, spare7, spare6, spare5, spare4, spare3, spare2, spare1}, | Change to:sCellAdditionTAAdjustment | malgorzata.tomala@nokia.com |  |
| 94 | 5.3.5.3 Reception of an RRCReconfiguration by the UE2> if the UE transmitted a *UEAssistanceInformation* message during the last 1 second, and the UE is still configured to provide UE assistance information: | Remove underline  | malgorzata.tomala@nokia.com |  |
| 95 | ***candidateBeamRSList, candidateBeamRSListExt-r16***A list of reference signals (CSI-RS and/or SSB) identifying the candidate beams for recovery and the associated RA parameters. The network configures these reference signals to be within the linked DL BWP (i.e., within the DL BWP with the same *bwp-Id*) of the UL BWP in which the *BeamFailureRecoveryConfig* is provided. | Remove "-r16" for the name of candidateBeamRSListExt-r16 in field description. | seungri.jin@samsung.com |  |
| 96 | maxNrofServingCells-r16 INTEGER ::= ffsValue -- Maximum number of serving cells in simultaneousTCI-UpdateList.maxNrofServingCellsTCI-r16 INTEGER ::= ffsValue -- | Remove maxNrofServingCells-r16 in 6.4 and add the comments (i.e. -- Maximum number of serving cells in simultaneousTCI-UpdateList) to the maxNrofServingCellsTCI-r16 | seungri.jin@samsung.com |  |
| 97 | PDSCH-TimeDomainResourceAllocationList-v16xy ::= SEQUENCE (SIZE(1..maxNrofDL-Allocations)) OF PDSCH-TimeDomainResourceAllocation-v16xyPDSCH-TimeDomainResourceAllocation-v16xy ::= SEQUENCE { repetitionNumber-r16 ENUMERATED {n2, n3, n4, n5, n6, n7, n8, n16} OPTIONAL -- Need R} | change IE name of PDSCH-TimeDomainResourceAllocation-v16xy to PDSCH-TimeDomainResourceAllocation-r16. | seungri.jin@samsung.com |  |
| 98 | maxNrofSRS-PathlossReferenceRS-r16-1 INTEGER ::= ffsValue --  | change the variable name for maxNrofSRS-PathlossReferenceRS-r16-1 to maxNrofSRS-PathlossReferenceRS-1-r16 | seungri.jin@samsung.com |  |
| 99 | ***bh-RLC-ChannelToAddModList***Configuration of the MAC Logical Channel, the corresponding backhaul RLC enitities to be added and modified. | Typo. Change ‘enitities’ to ‘entities’. | m.tesanovic@samsung.com |  |
| 100 | ***bap-Address***BAP address of node that is hosting this cell group. | Unusual choice of words. Change ‘hosting’ to ‘serving’. | m.tesanovic@samsung.com |  |
| 101 | ***Bap-Address***The ID of a destination IAB node or IAB donor-DU used in the BAP header. | The "Bap-Address" is defined here as "The ID of a destination IAB node or IAB donor-DU used in the BAP header". However, this Routing ID is only for default uplink routing. So, it should be "The ID of IAB donor-DU used in the BAP header" | m.tesanovic@samsung.com |  |
| 102 | ***iab-Support***This field combines both the support of IAB-node and the cell status for IAB-node. If the field is present, the cell supports IAB-nodes and the cell is also considered as a candidate for IAB-nodes; if the field is absent, the cell does not support IAB and/or the cell is barred for IAB-node. | Change to:'This field combines both the support of IAB-node and the cell status for IAB-node. If the field is present, the cell supports IAB-nodes and the cell is also considered as a candidate parent node for IAB-nodes; if the field is absent, the cell does not support IAB and/or the cell is barred for IAB-nodes.' | m.tesanovic@samsung.com |  |
| 103 | BAP-Config-r16 ::= SEQUENCE { bap-Address-r16 BIT STRING (SIZE (10)), defaultUL-BAProutingID-r16 BAP-Routing-ID-r16 OPTIONAL, -- Need FFS defaultUL-BH-RLC-Channel-r16 BH-LogicalChannelIdentity-r16 OPTIONAL, -- Need M ...} | The IE name 'defaultUL-BAProutingID-r16' can be updated to 'defaultUL-BAP-routingID-r16' to follow the convention (i.e. BAP (acronym) is followed by '-') | m.tesanovic@samsung.com |  |
| 104 | ***iab-NodeIndication-r16***This field is used to indicate that the connection is being established by an IAB-node [2]. | The suffix '-r16' from 'iab-NodeIndication-r16' should be removed from the field description title (not from ASN.1 code). | m.tesanovic@samsung.com |  |
| 105 | AvailabilityIndicator-r16 ::= SEQUENCE { ai-RNTI-r16 AI-RNTI-r16, dci-PayloadSize-AI-r16 INTEGER (1..maxAI-DCI-PayloadSize-r16), availableCombToAddModList-r16 SEQUENCE (SIZE(1..maxNrofAssociatedDUCellsPerMT-r16)) OF AvailabilityCombinationsPerCell-r16 OPTIONAL, -- Need FFS availableCombToReleaseList-r16 SEQUENCE (SIZE(1..maxNrofDUCells-r16)) OF CellIdentity OPTIONAL, -- Need FFS ...} | The field name 'dci-PayloadSize-AI-r16' can be updated to 'dci-PayloadSizeAI-r16' (i.e. no '-' after Size: '-' is placed only after acronym) | m.tesanovic@samsung.com |  |
| 106 | maxNrofDUCells-r16 INTEGER ::= 512 -- Max number of cells configured on the collocated IAB-DUmaxNrofAssociatedDUCellsPerMT-r16 INTEGER ::= 65535 -- FFSmaxNrofAvailabilityCombinationsPerSet-r16 INTEGER ::= 512 -- Max number of AvailabilityCombinationId used in the DCI format 2\_5… | The constant name 'maxNrofAssociatedDUCellsPerMT' can be updated to 'maxNrofAssociatedDU-CellsPerMT' | m.tesanovic@samsung.com |  |
| 107 | – *BAP-Routing-ID*The IE *BAP-Routing-ID* is used for IAB nodes to configure the default uplink Routing ID.***BAP-Routing-ID* information element**etc | The IE name 'BAP-Routing-ID' can be updated to 'BAP-RoutingID' | m.tesanovic@samsung.com |  |
| 108 | ***Bap-Address***The ID of a destination IAB node or IAB donor-DU used in the BAP header. | The field name should begin with lower case in the field description title (i.e. it should be bap-Address). | m.tesanovic@samsung.com |  |
| 109 | ***Bap-PathId***The ID of a path used in the BAP header. | The field name should begin with lower case in the field description title (i.e. it should be bap-PathId). | m.tesanovic@samsung.com |  |
| 110 | ***ssb-MTC-Periodity***SMTC window periodicity. | Generally, current SSB-MTC3 field descriptions are rather sparse. ssb-MTC-Periodity could be extended to "The periodicity of the measurement window in which to receive SS, in number of subframes."Also, typo: change ***ssb-MTC-Periodity*** to ***ssb-MTC-Periodicity*** | m.tesanovic@samsung.com |  |
| 111 | ***ssb-MTC-Timingoffset***SMTC window timing offset. | ssb-MTC-Timingoffset description could be enhanced to "The offset of the measurement window in which to receive SS, see 5.5.2.10. Periodicity and offset are given in number of subframes. | m.tesanovic@samsung.com |  |
| 112 | ***ssb-MTC-Duration***SMTC window duration. | ssb-MTC-Duration could become "Duration of the measurement window in which to receive SS. It is given in number of subframes (see TS 38.213 [13], clause 4.1)" | m.tesanovic@samsung.com |  |
| 113 | ***ssb-MTC-pci-List***List of physical cell IDs to be measured. | ssb-MTC-pci-List could become "PCIs that are known to follow this SMTC, used for IAB node discovery." | m.tesanovic@samsung.com |  |
| 114 | ***pdcp-Duplication***Indicates whether or not uplink duplication status at the time of receiving this IE is configured and activated as specified in TS 38.323 [5]. The presence of this field indicates that duplication is configured. PDCP duplication is not configured for CA packet duplication of LTE RLC bearer. The value of this field, when the field is present, indicates the initial state of the duplication. If set to *true*, duplication is activated. The value of this field is always *true*, when configured for a SRB. This field is absent, if the field *moreThanTwoRLC* is present. | “an SRB” instead of “a SRB” | sangkyu.baek@samsung.com |  |
| 115 | 2> add the SCell, corresponding to the *sCellIndex*, in accordance with the *sCellConfigCommon* and *sCellConfigDedicated*;2> if the *sCellState* is included and set to *activated*:3> configure lower layers to consider the SCell to be in activated state;2> else:3> configure lower layers to consider the SCell to be in deactivated state; | There statement regarding *sCellState* should be removed as covered by the general statement concerning sCellConfigDedicated (same for modification in this section) | Himke van der Velde at Samsung |  |
| 116 | Upon receiving the *DLInformationTransferMRDC*, the UE shall:1> if the *RRCReconfiguration* message is included in *dl-DCCH-MessageNR*:2> perform the RRC reconfiguration procedure according to 5.3.5.3;1> else if the *RRCRelease* message is included in *dl-DCCH-MessageNR*:2> perform the RRC release procedure according to 5.3.8;1> else if the E-UTRA *RRCConnectionReconfiguration* message is included in *dl-DCCH-MessageEUTRA*:2> perform the RRC connection reconfiguration procedure as specified in TS 36.331 [10], clause 5.3.5.3;1> else if the E-UTRA *RRCConnectionRelease* message is included in *dl-DCCH-MessageEUTRA*:2> perform the RRC connection release as specified in TS 36.331 [10], clause 5.3.8; | There is no need to list each message (we don’t do anything like this for DL-DCCH). Any constraints regarding which messages network may include should be specified in field description, as done in other cases. | Himke van der Velde at Samsung |  |
| 117 | Parameters for cross-carrier scheduling, i.e., a serving cell is scheduled by a PDCCH on another (scheduling) cell. The network configures this field only for SCells. When SCS of scheduling PDCCH is different from SCS of scheduled PDSCH, the time gap delta-values between the end of the PDCCH and start of the PDSCH is required to be not smaller than the minimal values specified in TS 38.214 [19]. | Seems not really appropriate to (also) include this also in RAN2 specs | Himke van der Velde at Samsung |  |
| 118 | 5.2.2.3.5 Request for on demand system information in RRC\_CONNECTED The UE shall:1> if the UE is in RRC\_CONNECTED with an active BWP not configured with common search and the UE has not stored a valid version of a SIB, in accordance with sub-clause 5.2.2.2.1, of one or several required SIB(s), in accordance with sub-clause 5.2.2.1: | The word “space” is missed here, should be added1> if the UE is in RRC\_CONNECTED with an active BWP not configured with common search space and the UE has not stored a valid version of a SIB | zhourui@catt.cn |  |
| 119 |  |  |  |  |
| 120 |  |  |  |  |
| 121 |  |  |  |  |
| 122 |  |  |  |  |
| 123 |  |  |  |  |
| 124 |  |  |  |  |
| 125 |  |  |  |  |
| 126 |  |  |  |  |
| 127 |  |  |  |  |
| 128 |  |  |  |  |