**3GPP TSG-****RAN2 Meeting#118e R2-22xxxxx**

**May, 2022**

**Agenda Item:** XXX

**Source:** Ericsson

**Title:** NR Rel-17 38331 ASN.1 Review, Class 0 issues

**Document for:** Discussion and decision

# Guidelines

* This file is used to log NR 38331 ASN:1 Review Class 0.
  + **- Typo, minor wording improvement etc.**
  + **- ASN.1 field not following naming rules (e.g. incorrect suffix, capitalization, “-“, etc).**
* Fill in the columns, see example.
  + Make sure the inserted specification text is unique, such that the location of the issue is simple to find.
  + Avoid indicating duplicated issues by checking if the concerned specification text is already reported in the table.
  + Step the file name v(x) -> v(x+1) and upload to ftp server.
* The “status” column will be filled in by the ASN.1 review moderator.

# Class 0 issues

| **Issue** | | **ASN1?**  **Y/N** | **Copied existing specification text.**  **Text should be unique, so that it can be easily found in the specification.**  **If needed, add also the new text.** | **Comment/description/**  **correction** | **Email address** | **Status** |
| --- | --- | --- | --- | --- | --- | --- |
| Ex 1 | | N  N | 2> derive the KUPint key associated with the *integrityProtAlgorithm* indicated in the SecurityModeCommand message, as specified in TS 33.501 [11]; | Missing italics. | hakan.l.palm@ericsson.com |  |
| Ex 2 | | N | PUSCH scheduled by RAR UL grant (see 38.213 clause 8.3 and 38.214 clause 6.1.2.2) and uses interlaced PUCCH Format 0, 1, 2, and 3 for cell-specific PUCCH (see TS 38.213 [13], clause 9.2.1). | Incorrect reference, should be 9.2.101. | hakan.l.palm@ericsson.com |  |
| Ex 3 | | Y | RbSetGroup, rbSetGroups | RB-SetGroup, rb-SetGroups | hakan.l.palm@ericsson.com |  |
| 4 | | Y | UEAssistanceInformation-v1700-IEs ::= SEQUENCE {  ul-GapFR2-Preference-r17 UL-GapFR2-Preference-r17 OPTIONAL,  musim-Assistance-r17 MUSIM-Assistance-r17 OPTIONAL,  overheatingAssistance-r17 OverheatingAssistance-r17 OPTIONAL,  maxBW-PreferenceFR2-2-r17 MaxBW-PreferenceFR2-2-r17 OPTIONAL,  maxMIMO-LayerPreferenceFR2-2-r17 MaxMIMO-LayerPreferenceFR2-2-r17 OPTIONAL,  minSchedulingOffsetPreferenceExt-r17 MinSchedulingOffsetPreferenceExt-r17 OPTIONAL,  rlm-MeasRelaxationState-r17 BOOLEAN OPTIONAL,  bfd-MeasRelaxationState-r17 BIT STRING (SIZE (32)) OPTIONAL,  nonSDT-DataIndication-r17 SEQUENCE {  resumeCause-r17 ResumeCause OPTIONAL  } OPTIONAL,  scg-DeactivationPreference ENUMERATED { scgDeactivationPreferred, noPreferrence } OPTIONAL,  uplinkData-r17 ENUMERATED { true } OPTIONAL,  rrm-MeasRelaxationFulfilment-r17 BOOLEAN OPTIONAL,  nonCriticalExtension SEQUENCE {} OPTIONAL  } | The yellow should be replaced with "(maxNrofServingCells)" | Mattias.a.bergstrom@ericsson.com |  |
| 5 | | Y | SIB12-IEs-r16 ::= SEQUENCE {  sl-ConfigCommonNR-r16 SL-ConfigCommonNR-r16,  lateNonCriticalExtension OCTET STRING OPTIONAL,  ...,  [[  sl-DRX-ConfigCommon-GC-BC-r17 SL-DRX-Config-GC-BC-r17 OPTIONAL, -- Need R  sl-DiscConfigCommon-r17 SL-DiscConfigCommon-r17 OPTIONAL, -- Need R  sl-L2U2N-Relay ENUMERATED {support} OPTIONAL, -- Need R  sl-NonRelayDiscovery ENUMERATED {support} OPTIONAL, -- Need R  sl-L3U2N-RelayDiscovery ENUMERATED {support} OPTIONAL -- Need R  ]]  } | "support" here should be "enabled". Usually we talk about what the gNB has enabled/disabled not what the gNB supports/doesn't support. For example, the gNB may support these features but the operator has not enabled the feature (e.g. at the moment). | Mattias.a.bergstrom@ericsson.com |  |
| 6 | | N | In 5.3.7.2  2> if the PC5-RRC connection with the U2N Relay UE is determined to be released:  3> perform the PC5-RRC connection release as specified in 5.8.9.5;  3>perform either cell selection in accordance with the cell selection process as specified in TS 38.304 [20], or relay selection as specified in clause 5.8.x3.3, or both;  2> else maintain the PC5 RRC connection and stop T311 if running; | The else branch should be split into two levels for condition and operation  2> else  3> maintain the PC5 RRC connection and stop T311 if running; | qianxi.lu@oppo.com |  |
| 7 | | N | In 5.3.13.6  1> else if cell selection or reselection occurs while T390 is running, or cell change due to relay selection or reselection occurs while T390 is running:  2> stop T390 for all access categories;  2> perform the actions as specified in 5.3.14.4. | It would be clearer if split the long else-if into two-level condition as follows  1> else  2> if cell selection or reselection occurs while T390 is running, or  2> if cell change due to relay selection or reselection occurs while T390 is running:  3> stop T390 for all access categories;  3> perform the actions as specified in 5.3.14.4. | qianxi.lu@oppo.com |  |
| 8 | | N | In 5.5.5.1  5> else:  6> include the applicable cells for which the new measurement results became available since the last periodical reporting or since the measurement was initiated or reset; | Indentation error  5> else:  6> include the applicable cells for which the new measurement results became available since the last periodical reporting or since the measurement was initiated or reset; | qianxi.lu@oppo.com |  |
| 9 | | N | In 5.8.15.3  NOTE 2: If multiple suitable candidate Relay UEs which meet all AS-layer & higher layer criteria are available, it is up to Remote UE implementation to choose one Relay UE. The details of the interaction with upper layers are up to UE implementation. | Suggest to change & to and  NOTE 2: If multiple suitable candidate Relay UEs which meet all AS-layer and higher layer criteria are available, it is up to Remote UE implementation to choose one Relay UE. The details of the interaction with upper layers are up to UE implementation. | qianxi.lu@oppo.com |  |
| 10 | | N | In 5.8.9.7.2,  Upon PC5-RRC connection is established between the L2 U2N Relay UE and L2 U2N Relay UE, the L2 U2N Relay UE shall: | One of the relay UE should be remote UE, i.e., to correct the typo  Upon PC5-RRC connection is established between the L2 U2N Remote UE and L2 U2N Relay UE, the L2 U2N Relay UE shall: | qianxi.lu@oppo.com |  |
| 11 | | Y | *– DRX-ConfigSL*  The IE *DRX-ConfigSL* is used to configure additional DRX parameters for the UE performing sidelink operation with resource allocation mode 1, as specified in TS 38.321 [3].  ***DRX-ConfigSL information element***  -- ASN1START  -- TAG-DRX-CONFIGSL-START  DRX-ConfigSL ::= SEQUENCE {  drx-HARQ-RTT-TimerSL INTEGER (0..56),  drx-RetransmissionTimerSL ENUMERATED {sl0, sl1, sl2, sl4, sl6, sl8, sl16, sl24, sl33, sl40, sl64, sl80, sl96, sl112, sl128, sl160,  sl320, spare15, spare14, spare13, spare12, spare11, spare10, spare9, spare8, spare7, spare6,  spare5, spare4, spare3, spare2, spare1}  }  -- TAG-DRX-CONFIGSL-STOP  -- ASN1STOP   |  | | --- | | ***DRX-ConfigSL field descriptions*** | | ***drx-HARQ-RTT-TimerSL***  Value in number of symbols of the BWP where the PDCCH was transmitted. | | ***drx-RetransmissionTimerSL***  Value in number of slot lengths of the BWP where the PDCCH was transmitted. *sl0* corresponds to 0 slots, *sl1* corresponds to 1 slot, *sl2* corresponds to 2 slots, and so on. | | Missing -r17 suffix for the following IEs  ***DRX-ConfigSL information element***  -- ASN1START  -- TAG-DRX-CONFIGSL-START  DRX-ConfigSL ::= SEQUENCE {  drx-HARQ-RTT-TimerSL INTEGER (0..56),  drx-RetransmissionTimerSL ENUMERATED {sl0, sl1, sl2, sl4, sl6, sl8, sl16, sl24, sl33, sl40, sl64, sl80, sl96, sl112, sl128, sl160,  sl320, spare15, spare14, spare13, spare12, spare11, spare10, spare9, spare8, spare7, spare6,  spare5, spare4, spare3, spare2, spare1}  }  -- TAG-DRX-CONFIGSL-STOP  -- ASN1STOP | qianxi.lu@oppo.com |  |
| 12 | | Y | RRCReconfiguration-v1700-IEs ::= SEQUENCE {  otherConfig-v1700 OtherConfig-v1700 OPTIONAL, -- Need M  ul-GapFR2-Config-r17 SetupRelease { UL-GapFR2-Config-r17 } OPTIONAL, -- Need M  sl-L2RelayUEConfig-r17 SetupRelease { SL-L2RelayUEConfig-r17 } OPTIONAL, -- Cond L2RelayUE  sl-L2RemoteUEConfig-r17 SetupRelease { SL-L2RemoteUEConfig-r17 } OPTIONAL, -- Cond L2RemoteUE  dedicatedPagingDelivery-r17 OCTET STRING (CONTAINING Paging) OPTIONAL, -- L2U2NRelay  needForNCSG-ConfigNR-r17 SetupRelease {NeedForNCSG-ConfigNR-r17} OPTIONAL, -- Need M  needForNCSG-ConfigEUTRA-r17 SetupRelease {NeedForNCSG-ConfigEUTRA-r17} OPTIONAL, -- Need M  musim-GapConfig-r17 SetupRelease {MUSIM-GapConfig-r17} OPTIONAL, -- Need M  scg-State-r17 ENUMERATED { deactivated } OPTIONAL, -- Need S  appLayerMeasConfig-r17 AppLayerMeasConfig-r17 OPTIONAL, -- Need M  nonCriticalExtension SEQUENCE {} OPTIONAL  } | Missing “-”  (this error is applicable to all places for the IE definition and usage) | qianxi.lu@oppo.com |  |
| 13 | | N | In 5.8.9.8.2  When entering RRC\_CONNECTED, if L2 U2N remote UE had send *sl-Requested-SI-List* and *sl-PagingInfo-RemoteUE,* the L2 U2N Remote UE shall: | send => sent | qianxi.lu@oppo.com |  |
| 14 | | N | In 5.3.5.16.2  The L2 U2N Relay UE shall:  1> if the release is triggered by reception of the *sl-RemoteUE-ToReleaseList*:  2> for each *sl-L2Identity-Remote* value included in the *sl-RemoteUE-ToReleaseList*:  3> if the current UE has a PC5 RRC connection to a L2 U2N Remote UE with *sl-L2Identity-Remote*:  4> perform the PC5-RRC connection release as specified in 5.8.9.5. | For the level-1 condition, since the only place that this sub-clause is called is as follows  1> if the *sl-L2RelayUEConfig* contains the *sl-RemoteUE-ToReleaseList*:  2> perform the L2 U2N Remote UE release as specified in 5.3.5.16.2;  There is no need to further check the condition of “if the release is triggered by reception of the *sl-RemoteUE-ToReleaseList*”, so can be removed. | qianxi.lu@oppo.com |  |
| 15 | | N | In 5.5.4.17  ***Thresh2*** is the threshold parameter for this event (i.e. *y1-Threshold2-Relay* as defined within *reportConfigInterRAT* for this even) | even=>event | xuhao@catt.cn |  |
| 16 | | N | In 5.5.5.1  1> if there is at least one applicable neighbouring cell to report:  2> if the *reportType* is set to *eventTriggered* or *periodical*:  3> if the measurement report concerns the candidate L2 U2N Relay UE:  4> set the *sl-MeasResultCandRelay* to include the best candidate L2 U2N Relay UEs up to *maxReportCells* in accordance with the following: | Missing “s”  *sl-MeasResultsCandRelay* | xuhao@catt.cn |  |
| 17 | | N | In 5.5.5.1  1> if there is at least one applicable neighbouring cell to report: | In agreed R2-2204226, candidate L2 U2N Relay UE was included:   1. if there is at least one applicable neighbouring cell/candidate L2 U2N Relay UEs to report.   But in TS 38.300, candidate L2 U2N Relay UE is missing.  Further, “/” should be clarify to or, and candidate L2 U2N Relay UEs should be candidate L2 U2N Relay UE.  Suggest to change to:  1> if there is at least one applicable neighbouring cell or candidate L2 U2N Relay UE to report: | xuhao@catt.cn |  |
| 18 | | N | In 5.5.5.1  3> for each L2 U2N Relay UE that is included in the *sl-MeasResultsCandRelay*, include the *sl-RelayUEIdentity*; | All NCGIs(in ASN.1 the IE is *cellIdentity*) should be included besides *sl-RelayUEIdentity.*  Suggest to change to:  3> for each L2 U2N Relay UE that is included in the *sl-MeasResultsCandRelay*, include the *sl-RelayUEIdentity and it’s cellIdentity*; | xuhao@catt.cn |  |
| 19 | | N | In 5.5.5.2  2> for a candidate L2 U2N Relay UE, consider the y*N-Threshold2-Relay* as the sorting quantity; | It should be clarify to “y*1-Threshold2-Relay”* | xuhao@catt.cn |  |
| 20 | | Y | ***y-Threshold1***  NR threshold to be used in measurement report triggering condition for event Y. | ***y1-Threshold1*** is only used for event Y1.  Suggest to change to:  ***y1-Threshold1***  NR threshold to be used in measurement report triggering condition for event Y1. | xuhao@catt.cn |  |
| 21 | | Y | ***y-Threshold2-Relay***  L2 U2N Relay threshold value associated with the selected trigger quantity (i.e. RSRP) to be used in measurement report triggering condition for event number Y. | ***y1-Threshold2-Relay*** is only used for event Y1.  Suggest to change to:  ***y1-Threshold2-Relay***  L2 U2N Relay threshold value associated with the selected trigger quantity (i.e. RSRP) to be used in measurement report triggering condition for event Y1. | xuhao@catt.cn |  |
| 22 | | Y | Absent field description of y2-Threshold-Relay | Suggest to add field description of y2-Threshold-Relay:  ***y2-Threshold-Relay***  L2 U2N Relay threshold value associated with the selected trigger quantity (i.e. RSRP) to be used in measurement report triggering condition for event Y2. | xuhao@catt.cn |  |
| 23 | | Y | ***xN-ThresholdM***  Threshold value associated to the selected trigger quantity (e.g. RSRP, RSRQ, SINR) per RS Type (e.g. SS/PBCH block, CSI-RS) to be used in NR measurement report triggering condition for event xN. If multiple thresholds are defined for event number xN, the thresholds are differentiated by M. x1-Threshold1 and x2-Threshold indicates the threshold value for the serving L2 U2N Relay UE, x1-Threshold2 indicates the threshold value for the NR Cells. | Suggest to use separate field descriptions for x1-Threshold1-Relay, x1-Threshold2 and x2-Threshold-Relay.  ***x1-Threshold1-Relay***  L2 U2N Relay threshold value associated with the selected trigger quantity (i.e. RSRP) to be used in measurement report triggering condition for event X1.  ***x1-Threshold2***  NR threshold to be used in measurement report triggering condition for event X1.  ***X2-Threshold-Relay***  L2 U2N Relay threshold value associated with the selected trigger quantity (i.e. RSRP) to be used in measurement report triggering condition for event X2. | xuhao@catt.cn |  |
| 24 | | N | In 5.8.1  For U2N Relay operation, one sidelink SRB (i.e. SL-SRB4) is used to transmit/receive the NR sidelink discovery messages. | Since for the other SL-SRB, only transmit is mentioned, hence it had better align the description for all SL-SRBs:  For U2N Relay operation, one sidelink SRB (i.e. SL-SRB4) is used to transmit~~/receive~~ the NR sidelink discovery messages. | xuhao@catt.cn |  |
| 25 | | N | In 5.8.9.7.2  For each *sl-RLC-ChannelID-PC5* received in the *sl-RLC-ChannelToAddModList-PC5* IE the UE shall:  1> if the current configuration contains a sidelink RLC bearer with the received *sl-RLC-ChannelID-PC5*:  2> reconfigure the sidelink RLC entity or entities in accordance with the received *sl-RLC-ConfigPC5*;  2> reconfigure the sidelink logical channel in accordance with the received *sl-MAC-LogicalChannelConfigPC5*;  1> else (a PC5 Relay RLC channel with the received *sl-RLC-ChannelID-PC5* was not configured before):  2> establish an sidelink RLC entity in accordance with the received *sl-RLC-ConfigPC5*;  2> configure the sidelink MAC entity with a logical channel in accordance with the received *sl-MAC-LogicalChannelConfigPC5*. | The descriptions marked with yellow are not aligned. In addition, in our understanding, the sidelink and Uu shares the same MAC entity, it is not proper to use “sidelink MAC entity”.  For each *sl-RLC-ChannelID-PC5* received in the *sl-RLC-ChannelToAddModList-PC5* IE the UE shall:  1> if the current configuration contains a sidelink RLC bearer with the received *sl-RLC-ChannelID-PC5*:  2> reconfigure the sidelink RLC entity or entities in accordance with the received *sl-RLC-ConfigPC5*;  2> reconfigure the sidelink MAC entity with a logical channel in accordance with the received *sl-MAC-LogicalChannelConfigPC5*;  1> else (a PC5 Relay RLC channel with the received *sl-RLC-ChannelID-PC5* was not configured before):  2> establish an sidelink RLC entity in accordance with the received *sl-RLC-ConfigPC5*;  2> configure the ~~sidelink~~ MAC entity with a logical channel in accordance with the received *sl-MAC-LogicalChannelConfigPC5*. | xuhao@catt.cn |  |
| 26 | | N | In 5.8.13.2  2> else if the cell chosen for NR sidelink discovery reception provides *SIB12*:  3> if *sl-DiscRxPool* for NR sidelink is included in *SIB12*:  4> configure lower layers to monitor sidelink control information and the corresponding data using the resource pool indicated by *sl-DiscRxPoo* for NR sidelink discovery reception *in SIB12*; | *sl-DiscRxPoo=> sl-DiscRxPool* | xuhao@catt.cn |  |
| 27 | | N | In 5.8.15.1  This procedure is used by a UE supporting NR sidelink U2N Remote UE operationconfigured by upper layers to receive/ transmit NR sidelink discovery message to evaluate AS layer conditions. | Lack of space  This procedure is used by a UE supporting NR sidelink U2N Remote UE operation configured by upper layers to receive/ transmit NR sidelink discovery message to evaluate AS layer conditions. | xuhao@catt.cn |  |
| 28 | | *Y* | In 6.2.2  RRCReconfiguration-v1700-IEs ::= SEQUENCE {  otherConfig-v1700 OtherConfig-v1700 OPTIONAL, -- Need M  ul-GapFR2-Config-r17 SetupRelease { UL-GapFR2-Config-r17 } OPTIONAL, -- Need M  sl-L2RelayUEConfig-r17 SetupRelease { SL-L2RelayUEConfig-r17 } OPTIONAL, -- Cond L2RelayUE  sl-L2RemoteUEConfig-r17 SetupRelease { SL-L2RemoteUEConfig-r17 } OPTIONAL, -- Cond L2RemoteUE  dedicatedPagingDelivery-r17 OCTET STRING (CONTAINING Paging) OPTIONAL, -- L2U2NRelay  needForNCSG-ConfigNR-r17 SetupRelease {NeedForNCSG-ConfigNR-r17} OPTIONAL, -- Need M  needForNCSG-ConfigEUTRA-r17 SetupRelease {NeedForNCSG-ConfigEUTRA-r17} OPTIONAL, -- Need M  musim-GapConfig-r17 SetupRelease {MUSIM-GapConfig-r17} OPTIONAL, -- Need M  scg-State-r17 ENUMERATED { deactivated } OPTIONAL, -- Need S  appLayerMeasConfig-r17 AppLayerMeasConfig-r17 OPTIONAL, -- Need M  nonCriticalExtension SEQUENCE {} OPTIONAL  }   |  |  | | --- | --- | | *L2RelayUE* | For L2 U2N Relay UE, the field is optionally present, Need M. Otherwise, it is absent. | | *L2RemoteUE* | The field is optional present for L2 U2N Remote UE, need M; otherwise it is absent. | | *L2U2NRelay* | For L2 U2N Relay UE, the field is optionally present, Need N. Otherwise, it is absent. | | For L2 U2N relay, there are two different descriptions ” L2RelayUE” and ” L2U2NRelay”, it had better align it.  RRCReconfiguration-v1700-IEs ::= SEQUENCE {  otherConfig-v1700 OtherConfig-v1700 OPTIONAL, -- Need M  ul-GapFR2-Config-r17 SetupRelease { UL-GapFR2-Config-r17 } OPTIONAL, -- Need M  sl-L2RelayUEConfig-r17 SetupRelease { SL-L2RelayUEConfig-r17 } OPTIONAL, -- Cond L2RelayUE  sl-L2RemoteUEConfig-r17 SetupRelease { SL-L2RemoteUEConfig-r17 } OPTIONAL, -- Cond L2RemoteUE  dedicatedPagingDelivery-r17 OCTET STRING (CONTAINING Paging) OPTIONAL, -- Cond L2~~U2N~~RelayUE  needForNCSG-ConfigNR-r17 SetupRelease {NeedForNCSG-ConfigNR-r17} OPTIONAL, -- Need M  needForNCSG-ConfigEUTRA-r17 SetupRelease {NeedForNCSG-ConfigEUTRA-r17} OPTIONAL, -- Need M  musim-GapConfig-r17 SetupRelease {MUSIM-GapConfig-r17} OPTIONAL, -- Need M  scg-State-r17 ENUMERATED { deactivated } OPTIONAL, -- Need S  appLayerMeasConfig-r17 AppLayerMeasConfig-r17 OPTIONAL, -- Need M  nonCriticalExtension SEQUENCE {} OPTIONAL  }   |  |  | | --- | --- | | *L2RelayUE* | For L2 U2N Relay UE, the field is optionally present, Need M. Otherwise, it is absent. | | *L2RemoteUE* | The field is optional present for L2 U2N Remote UE, need M; otherwise it is absent. | | *~~L2U2NRelay~~* | ~~For L2 U2N Relay UE, the field is optionally present, Need N. Otherwise, it is absent.~~ | | xuhao@catt.cn |  |
| 29 | | Y | In 6.2.2  ***dedicatedPagingDelivery***  This field is used to transfer *Paging* message to the L2 Relay UE in RRC\_CONNECTED. | It had better clarify that the paging message is belonging to remote UE.  ***dedicatedPagingDelivery***  This field is used to transfer *Paging* message of remote UE to the L2 Relay UE in RRC\_CONNECTED. | xuhao@catt.cn |  |
| 30 | | *N* | 1> if and only if upper layers indicate to stop performing location measurements towards E-UTRA or NR or stop subframe and slot timing detection towards E-UTRA and *preConfigGapID* is not activated:  2> initiate the procedure to indicate stop.  NOTE 2: The UE may initiate the procedure to indicate stop even if it did not previously initiate the procedure to indicate start.  1> if *preConfigGapID* is activated:  2> if a request from upper layers to transmit either a new *preConfigGapID* or to modify the current *measGapConfig* is received; or  2> if a request from upper layers indicate that the current gap is not needed:  3> trigger the lower layers to deactivate the current active measurement gap as specified in TS 38.321 [6]; | Incorrect punctuation.  The first highlighted one should be a semicolon and the second highlighted one should be a full stop. | panxiang@vivo.com |  |
| 31 | | *N* | Figure 5.7.14.1-1: UE Positioning Assistance Information procedure | The procedure of RRC reconfiguration should be bidirectional to align with that in Figure 5.7.4.1-1: UE Assistance Information | panxiang@vivo.com |  |
| 32 | | *Y* | SRS for positioning confifuration during RRC\_INACTIVE State. | Typo  Confifuration -> configuration | panxiang@vivo.com |  |
| 33 | | *Y* | The aperiodic SRS is not applicable for the UE in RRC\_INACTIVE | Missing full stop. | panxiang@vivo.com |  |
| 34 | | *N* | if transmission of the UEPositioningAssistanceInfo message is initiated to provide the association between UL SRS Resource for positioning and Tx TEG according to 5.X.2.2; | Incorrect reference, should be 5.7.14.2 | panxiang@vivo.com |  |
| 35 | | *N* | Figure 5.7.15.1-1: SRS For Positioning Configuration in RRC INACTIVE Mode | Missing “\_” | panxiang@vivo.com |  |
| 36 | | *Y* | Configures the periodicty of UE reporting for the association between Tx TEG and SRS Positioning resources. When configured with *oneShot* UE reports the association only one time. When configured with *periodicReporting* value ms120 means the UE reports every 120ms, ms240 means UE reports every 240ms and so on. | Missing italics. | panxiang@vivo.com |  |
| 37 | | *Y* | In 6.2.2  UEAssistanceInformation-v17xy-IEs ::= SEQUENCE {  scg-DeactivationPreference ENUMERATED { scgDeactivationPreferred, noPreferrence } OPTIONAL,  uplinkData-r17 ENUMERATED { true } OPTIONAL,  nonCriticalExtension SEQUENCE {} OPTIONAL  } | The codepoint marked in yellow is not aligned with the one used in the corresponding procedure, i.e., *scgDeactivationNotPreferred*. | wenjuan.pu@vivo.com |  |
| 38 | | *Y* | In 6.3.2  ***deactivated-SCG-Config***  Configuration applicable when the SCG is deactivated. The network always configures this field before or when indicating that the SCG is deactivated in an *RRCReconfiguration*, *RRCResume*, E-UTRA *RRCConnectionReconfiguration* or E-UTRA *RRCConnectionResume* message. | “***deactivated-SCG-Config***” should be “***deactivatedSCG-Config***” | wenjuan.pu@vivo.com |  |
| 39 | | *N* | In 5.7.4.2  A UE capable of providing its preference for SCG deactivation may initiated the procedure if it was configured to do so, upon determining that it prefers or does no more prefer the SCG to be deactivated. | “initiated” should be “initiate” | wenjuan.pu@vivo.com |  |
| 40 | | N | In 5.8.3.3  if the UE initiates the procedure to indicate it is (no more) interested to receive NR sidelink communication or to request (configuration/ release) of NR sidelink communication transmission resources or to report to the network that a sidelink radio link failure or sidelink RRC reconfiguration failure has been declared or to report to the network the sidelink DRX configuration for NR sidelink unicast communication or to report to the network the sidelink DRX assistance information for NR sidelink unicast communication or to report the Destination Layer-2 ID and QoS profile associated with its interested services that sidelink DRX is applied for NR sidelink groupcast or broadcast communication or to indicate it is (no more) interested to receive NR sidelink discovery announcements or to request (configuration/ release) of NR sidelink discovery announcements transmission resources or to request (configuration/ release) of NR sidelink U2N relay communication transmission resources (i.e. UE includes all concerned information, irrespective of what triggered the procedure): | To align the description of “report to the network” to other case in this sentence, the network needs to be added.  if the UE initiates the procedure to indicate it is (no more) interested to receive NR sidelink communication or to request (configuration/ release) of NR sidelink communication transmission resources or to report to the network that a sidelink radio link failure or sidelink RRC reconfiguration failure has been declared or to report to the network the sidelink DRX configuration for NR sidelink unicast communication or to report to the network the sidelink DRX assistance information for NR sidelink unicast communication or to report to the network the Destination Layer-2 ID and QoS profile associated with its interested services that sidelink DRX is applied for NR sidelink groupcast or broadcast communication or to indicate it is (no more) interested to receive NR sidelink discovery announcements or to request (configuration/ release) of NR sidelink discovery announcements transmission resources or to request (configuration/ release) of NR sidelink U2N relay communication transmission resources (i.e. UE includes all concerned information, irrespective of what triggered the procedure): | shijie@catt.cn |  |
| 41 | | N | In 5.8.8  NOTE 3: It is up to UE implementation to determines which one resource allocation scheme is used in the AS based on UE capability (for a UE in RRC\_IDLE/RRC\_INACTIVE) and the allowed resource schemes *sl-allowedResourceSelectionConfig* in the resource pool configuration. | Some wording is not right for “to determines which one resource allocation scheme”  to determine~~s~~ which ~~one~~ resource allocation scheme is used… | shijie@catt.cn |  |
| 42 | | N | In 5.8.9.6.3  NOTE: When UE determines the sidelink DRX configuration for its peer UE, it may take the sidelink DRX assistance information that is received from its peer UE into account. | Form the view of general wording, “that is” is better to be deleted.  it may take the sidelink DRX assistance information ~~that is~~ received from its peer UE into account. | shijie@catt.cn |  |
| 43 | | N | In 6.2.2  ***sl-LatencyBoundCSI-Report***  Indicate the latency bound of SL CSI report from the associated SL CSI triggering in terms of number of slots.  ***sl-LatencyBoundIUC-Report***  Indicates the latency bound of SL Inter-UE coordination report from the associated SL Inter-UE coordination explicit request triggering in terms of number of slots. | the field description of sl-LatencyBoundCSI-Report use the word “indicates”, but the field description of sl-LatencyBoundIUC-Report  Uses the word “indicate”, they should be aligned.  ***sl-LatencyBoundCSI-Report***  Indicates the latency bound of SL CSI report from the associated SL CSI triggering in terms of number of slots. | shijie@catt.cn |  |
| 44 | | N | In 6.3.1, SIB17:  SIB17-IEs-r17 ::= SEQUENCE {  trs-ResouceSetConfig-r17 SEQUENCE (SIZE (1..maxNrofTRS-ResourceSets-r17)) OF TRS-ResourceSet-r17 OPTIONAL, -- Need R  validityDuration-r17 ENUMERATED {t1, t2, t4, t8, t16, t32, t64, t128, t256, t512, spare6, spare5, spare4, spare3, spare2,  spare1} OPTIONAL, -- Need S  lateNonCriticalExtension OCTET STRING OPTIONAL,  ...  }  And in the field description table:  ***trs-ResouceSetConfig***  RS configuration of TRS occasion(s) for idle/inactive UE(s), … | Typo: “r” is missing to trs-ResouceSetConfig-r17:  SIB17-IEs-r17 ::= SEQUENCE {  trs-ResourceSetConfig-r17 SEQUENCE (SIZE (1..maxNrofTRS-ResourceSets-r17)) OF TRS-ResourceSet-r17 OPTIONAL, -- Need R  validityDuration-r17 ENUMERATED {t1, t2, t4, t8, t16, t32, t64, t128, t256, t512, spare6, spare5, spare4, spare3, spare2,  spare1} OPTIONAL, -- Need S  lateNonCriticalExtension OCTET STRING OPTIONAL,  ...  }  And in the field description table:  ***trs-ResourceSetConfig***  RS configuration of TRS occasion(s) for idle/inactive UE(s), | pierrebertrand@catt.cn |  |
| 45 | | N | In 6.3.1, field description of SIB17:  ***trs-ResouceSetConfig***  RS configuration of TRS occasion(s) for idle/inactive UE(s), in terms of a list of N>=1 NZP TRS resource set(s). The maximum number of TRS resource sets configured by higher layer is 64. If a TRS resource is configured, the L1 based availability indication is always enabled based on that configuration. A UE which acquired SIB-X with a TRS configuration but did not yet receive an associated L1-based availability indication considers the configured TRS as unavailable. | The font color of the last sentence needs to be updated. | pierrebertrand@catt.cn |  |
| 46 | | N | In 6.3.1, field descriptions of SIB17:  ***TRS-ResourceSet***  Common configuration parameters for the TRS resource set. | We don’t need to add the field description for *TRS-ResourceSet* as it is an IE, not a field. It should be removed. | pierrebertrand@catt.cn |  |
| 47 | | N | In 6.3.2, field descriptions of *SCellConfig*:  ***goodServingCellEvaluationBFD***  ***I***ndicates the criterion for a UE to detect the good serving cell quality for BFD relaxation in an SCell in RRC\_CONNECTED. | Typo. Change as follows:  ***goodServingCellEvaluationBFD***  Indicates the criterion for a UE to detect the good serving cell quality for BFD relaxation in an SCell in RRC\_CONNECTED. | pierrebertrand@catt.cn |  |
| 48 | | N | In 6.3.2, some typos in *PEI-Config* field descriptions.  ***firstPDCCH-MonitoringOccasionOfPEI-O***  Offset, in number of symbols, from the start of the reference frame for PEI-O to the start of the first PDCCH monitoring occasion of PEI-O, see TS 38.213 [13], clause 10.4A. For the case *po-NumPerPEI* is smaller than Ns, UE applies the (floor(i\_s/poNumPerPEI)+1)-th value out of (N\_s/po-NumPerPEI) configured values in *firstPDCCH-MonitoringOccasionOfPEI-O* for the symbol-level offset. When *po-NumPerPEI* is one or mutliple of Ns, UE applies the first configured value in *firstPDCCH-MonitoringOccasionOfPEI-O* for the symbol-level offset.  **pei-SearchSpace**  ID of dedicated search space for PEI. It can be configured to one of up to 4 common SS sets configured by *commonSearchSpaceList* with *SearchSpaceId* > 0. The CCE aggregation levels and maximum number of PDCCH candidates per CCE aggregation level follows Table 10.1-1 of TS38.213 [13]. SearchSpaceId = 0 can be configured for the case of SS/PBCH block and CORESET multiplexing pattern 2 or 3.  **po-NumPerPEI**  The number of PO(s) associated **with** one PEI monitoring occation. It is a factor of N x Ns (total PO number in a paging cycle). The Maximum number of PF associated with one PEI monitoring occation is up to 2. The number of PO mapping to one PEI should be multiple of Ns when po-NumPerPEI is larger than Ns. | Extra space character, italics fonts, etc. Change as follows:  ***firstPDCCH-MonitoringOccasionOfPEI-O***  Offset, in number of symbols, from the start of the reference frame for PEI-O to the start of the first PDCCH monitoring occasion of PEI-O, see TS 38.213 [13], clause 10.4A. For the case *po-NumPerPEI* is smaller than Ns, UE applies the (floor(i\_s/poNumPerPEI)+1)-th value out of (N\_s/po-NumPerPEI) configured values in *firstPDCCH-MonitoringOccasionOfPEI-O* for the symbol-level offset. When *po-NumPerPEI* is one or mutliple of Ns, UE applies the first configured value in *firstPDCCH-MonitoringOccasionOfPEI-O* for the symbol-level offset.  ***pei-SearchSpace***  ID of dedicated search space for PEI. It can be configured to one of up to 4 common SS sets configured by *commonSearchSpaceList* with *SearchSpaceId* > 0. The CCE aggregation levels and maximum number of PDCCH candidates per CCE aggregation level follows Table 10.1-1 of TS38.213 [13]. *SearchSpaceId* = 0 can be configured for the case of SS/PBCH block and CORESET multiplexing pattern 2 or 3.  ***po-NumPerPEI***  The number of PO(s) associated with one PEI monitoring occation. It is a factor of N x Ns (total PO number in a paging cycle). The Maximum number of PF associated with one PEI monitoring occation is up to 2. The number of PO mapping to one PEI should be multiple of Ns when *po-NumPerPEI* is larger than Ns. | pierrebertrand@catt.cn |  |
| 49 | | Y | In 6.3.2, typo in the IE SearchSpace  [[  dci-Format2-7-r17 SEQUENCE {  nrofCandidates-PEI-r17 SEQUENCE {  aggregationLevel4-r17 ENUMERATED {n0, n1, n2, n3, n4} OPTIONAL, -- Need R  aggregationLevel8-r17 ENUMERATED {n0,n1, n2} OPTIONAL, -- Need R  aggregationLevel16-r17 ENUMERATED {n0, n1} OPTIONAL -- Need R  },  ...  } OPTIONAL -- Need R  ]] | [[  dci-Format2-7-r17 SEQUENCE {  nrofCandidates-PEI-r17 SEQUENCE {  aggregationLevel4-r17 ENUMERATED {n0, n1, n2, n3, n4} OPTIONAL, -- Need R  aggregationLevel8-r17 ENUMERATED {n0, n1, n2} OPTIONAL, -- Need R  aggregationLevel16-r17 ENUMERATED {n0, n1} OPTIONAL -- Need R  },  ...  } OPTIONAL -- Need R  ]] | pierrebertrand@catt.cn |  |
| 50 | | Y | In 6.3.2, SI-SchedulingInfo IE:  SIB-TypeInfo-v1700 ::= SEQUENCE {  sibType-r17 CHOICE {  type1-r17 ENUMERATED {sibType15, sibType16, sibType17, sibType18, sibType19, sibType20, sibType21,...},  type2-r17 SEQUENCE {  posSibType-r17 ENUMERATED {posSibType1-9, posSibType1-10, posSibType2-24, posSibType2-25, posSibType6-4, posSibType6-5, posSibType6-6,...},  encrypted-r17 ENUMERATED { true } OPTIONAL, -- Need R  gnss-id-r17 GNSS-ID-r16 OPTIONAL, -- Need R  sbas-id-r17 SBAS-ID-r16 OPTIONAL -- Need R  }  },  valueTag-r17 INTEGER (0..31) OPTIONAL, -- Cond SIB-TYPE-POS  areaScope-r17 ENUMERATED {true} OPTIONAL -- Need S  } | Suffix is missing:  SIB-TypeInfo-v1700 ::= SEQUENCE {  sibType-r17 CHOICE {  type1-r17 ENUMERATED {sibType15-v1700, sibType16-v1700, sibType17-v1700, sibType18-v1700, sibType19-v1700, sibType20-v1700, sibType21,...},  type2-r17 SEQUENCE {  posSibType-r17 ENUMERATED {posSibType1-9, posSibType1-10, posSibType2-24, posSibType2-25, posSibType6-4, posSibType6-5, posSibType6-6,...},  encrypted-r17 ENUMERATED { true } OPTIONAL, -- Need R  gnss-id-r17 GNSS-ID-r16 OPTIONAL, -- Need R  sbas-id-r17 SBAS-ID-r16 OPTIONAL -- Need R  }  },  valueTag-r17 INTEGER (0..31) OPTIONAL, -- Cond SIB-TYPE-POS  areaScope-r17 ENUMERATED {true} OPTIONAL -- Need S  } | pierrebertrand@catt.cn |  |
| 51 | | N | In 6.3.4, *OtherConfig* field description:  ***bfd-RelaxationReportingConfig***  Configuration for the UE to report the relaxation state of BDF measurements. | Typo: BDF -> BFD  ***bfd-RelaxationReportingConfig***  Configuration for the UE to report the relaxation state of BFD measurements. | pierrebertrand@catt.cn |  |
| 52 | | Y | – *SIB19*  *SIB19* contains satellite assistance information.  ***SIB19* information element**  -- ASN1START  -- TAG-SIB19-START  SIB19-r17 ::= SEQUENCE {  ntn-Config NTN-Config-r17 OPTIONAL, -- Need R  t-Service-r17 INTEGER (0..549755813887) OPTIONAL, -- Need R  referenceLocation-r17 ReferenceLocation-r17 OPTIONAL, -- Need R  ta-Report-r17 ENUMERATED {enabled} OPTIONAL, -- Need R  lateNonCriticalExtension OCTET STRING OPTIONAL,  ...  } | Should have suffix -r17, i.e. ntn-Config-r17 | jiangxiaowei@xiaomi.com |  |
| 53 | | N | ***SIB19* field descriptions:**  ***ta-Report***  Indicates whether UE specific TA reporting is enabled during initial access (see TS 38.321 [3], clause x.x.x). | 1. “UE specific” should be removed to align with the naming in 38.321, i.e. Timing Advance Reporting   ‘,’ is missing before ‘is’ | jiangxiaowei@xiaomi.com |  |
| 54 | | Y | NTN-Config-r17 ::= SEQUENCE {  epochTime-r17 EpochTime-r17 OPTIONAL, -- Need R  ntn-UlSyncValidityDuration-r17 ENUMERATED{ s5, s10, s15, s20, s25, s30, s35,  s40, s45, s50, s55, s60, s120, s180, s240} OPTIONAL, -- Need R  cellSpecificKoffset-r17 INTEGER(0..1023) OPTIONAL, -- Need R  kmac-r17 INTEGER(0..512) OPTIONAL, -- Need R  ta-Info-r17 TAInfo-r17 OPTIONAL, -- Need R  ntn-PolarizationDL-r17 ENUMERATED {rhcp,lhcp,linear} OPTIONAL, -- Need R  ntn-PolarizationUL-r17 ENUMERATED {rhcp,lhcp,linear} OPTIONAL, -- Need R  ephemerisInfo-r17 EphemerisInfo-r17 OPTIONAL, -- Need R  ...  }  EpochTime-r17 ::= SEQUENCE {  sfn-r17 INTEGER(0..1023),  subFrameNR-r17 INTEGER(0..9)  }  TAInfo-r17 ::= SEQUENCE {  ta-Common-r17 INTEGER(0..66485757),  ta-CommonDrift-r17 INTEGER(-261935..261935) OPTIONAL, -- Need R  ta-CommonDriftVariant-r17 INTEGER(0..29470) OPTIONAL -- Need R  }  -- TAG-NTN-CONFIG-STOP  -- ASN1STOP | TAInfo-r17 => TA-Info-r17 | jiangxiaowei@xiaomi.com |  |
| 55 | | N | ***cellSpecificKoffset***  The CellSpecific\_K\_offset is a scheduling offset used for the timing relationships that need to be modified for NTN [see TS 38.2xy]. The unit of K\_offset is number of slots for a given subcarrier spacing of 15 kHz. FFS other SCS. | CellSpecific\_K\_offset => cellSpecificKoffset  K\_offset => cellSpecificKoffset | jiangxiaowei@xiaomi.com |  |
| 56 | | N | ***kmac***  K\_mac is a scheduling offset provided by network if downlink and uplink frame timing are not aligned at gNB. It is needed for UE action and assumption on downlink configuration indicated by a MAC-CE command in PDSCH [see TS 38.2xy]. When UE is not provided by network with a K\_mac value, UE assumes K\_mac = 0.  For the reference subcarrier spacing value for the unit of K\_mac in FR1, a value of 15 kHz is used. The unit of K\_mac is number of slots for a given subcarrier spacing. FFS other SCS. | K\_mac => kmac | jiangxiaowei@xiaomi.com |  |
| 57 | | N | ***ntn-PolarizationUL***  If present, this parameter indicates Polarization information for Uplink service link.  If not present and ntnPolarizationDL is present, UE assumes a same polarization for UL and DL. | ntnPolarizationDL => ntn-PolarizationDL | jiangxiaowei@xiaomi.com |  |
| 58 | | N | ***EphemerisInfo***  This field provides satellite ephemeris either in format of position and velocity state vector or in format of orbital parameters. This field is excluded when determining changes in system information, i.e. changes of XXX should neither result in system information change notifications nor in a modification of valueTag in SIB1. | ***EphemerisInfo => ephemerisInfo*** | jiangxiaowei@xiaomi.com |  |
| 59 | | N | ***ta-Common***  TACommon is a network-controlled common timing advanced value and it may include any timing offset considered necessary by the network. TACommon with value of 0 is supported. The granularity of TACommon is 4.07 × 10^(-3) μs. Values are given in unit of corresponding granularity. This field is excluded when determining changes in system information, i.e. changes of XXX should neither result in system information change notifications nor in a modification of valueTag in SIB1.” | TACommon => ta-Common  Remove the redundant “ | jiangxiaowei@xiaomi.com |  |
| 60 | | N | ***taCommonDrift***  Indicate drift rate of the common TA. The granularity of TACommonDrift is 0.2 × 10^(-3) μs⁄s Values are given in unit of corresponding granularity. *This field is excluded when determining changes in system information, i.e. changes of XXX should neither result in system information change notifications nor in a modification of valueTag in SIB1.* | ***taCommonDrift => ta-CommonDrift***  TACommonDrift => ***ta-CommonDrift***  Additional spaces before us/s should be removed.  ‘.’ Is missing before “Values” | jiangxiaowei@xiaomi.com |  |
| 61 | | N | ***taCommonDriftVariant***  Indicate drift rate variation of the common TA. The granularity of TACommonDriftVariation is 0.2×10^(-4) μs⁄s^2. Values are given in unit of corresponding granularity. *This field is excluded when determining changes in system information, i.e. changes of XXX should neither result in system information change notifications nor in a modification of valueTag in SIB1.* | ***taCommonDriftVariant => ta-CommonDriftVariant***  TACommonDriftVariation => ta-CommonDriftVariant | jiangxiaowei@xiaomi.com |  |
| 62 | | Y | – *ConfiguredGrantConfig*  [[  cg-betaOffsetsCrossPri0-r17 SetupRelease { BetaOffsetsCrossPriSelCG-r17 } OPTIONAL, -- Need M  cg-betaOffsetsCrossPri1-r17 SetupRelease { BetaOffsetsCrossPriSelCG-r17 } OPTIONAL, -- Need M  mappingPattern-r17 ENUMERATED {cyclicMapping, sequentialMapping} OPTIONAL, -- Need R  sequenceOffsetForRV-r17 INTEGER (0..3) OPTIONAL, -- Need R  p0-PUSCH-Alpha2-r17 P0-PUSCH-AlphaSetId OPTIONAL, -- Need R  powerControlLoopToUse2-r17 ENUMERATED {n0, n1} OPTIONAL, -- Need R  cg-COT-SharingList-r17 SEQUENCE (SIZE (1..1709)) OF CG-COT-Sharing-r17 OPTIONAL, -- Need R  periodicityExt-r17 INTEGER (1..40960) OPTIONAL, -- Need R  repK-r17 ENUMERATED {n12, n16, n24, n32} OPTIONAL, -- Need M  nrofHARQ-ProcessesExt-r17 INTEGER(17..32) OPTIONAL, -- Need M  harq-ProcID-Offset-v17 INTEGER (16..31) OPTIONAL, -- Need M  harq-ProcID-Offset2-v1700 INTEGER (16..31) OPTIONAL, -- Need M  configuredGrantTimer-v1700 INTEGER(66..576) OPTIONAL -- Need R  ]] | harq-ProcID-Offset-v17 =》 harq-ProcID-Offset-v1700 | jiangxiaowei@xiaomi.com |  |
| 63 | | N | ***uplinkHARQ-mode***  Used to set the HARQ mode per HARQ process ID, see TS 38.321 [3]. The first/leftmost bit corresponds to HARQ process ID 0, the next bit to HARQ process ID 1 and so on. Bits corresponding to HARQ process IDs that are not configured shall be ignored. A bit set to one identifies a HARQ process with *HARQmodeA* and a bit set to zero identifies a HARQ process with *HARQ modeB*. This field also applies for SRB1 to SRB3. | *HARQmodeA => harqModeA*  *HARQ modeB => harqModeB* | jiangxiaowei@xiaomi.com |  |
| 64 | | N | In 6.3.2  The execution condition that needs to be fulfilled in order to trigger the execution of a conditional reconfiguration for CHO, CPA, intra-SN CPC without MN involvement or MN initiated inter-SN CPC. When configuring 2 triggering events (Meas Ids) for a candidate cell, network ensures that both refer to the same *measObject.* If network configures *condEventD1* or *condEventT1* for a candidate cell network configures a second triggering event *condEventA3, condEventA4* or *condEventA5*. Network does not configure both *condEventD1* or *condEventT1* for the same candidate cell. For CPAC, the *RRCReconfiguration* message contained in *condRRCReconfig* cannot contain the field *scg-State*. | The comma is missing.  The execution condition that needs to be fulfilled in order to trigger the execution of a conditional reconfiguration for CHO, CPA, intra-SN CPC without MN involvement or MN initiated inter-SN CPC. When configuring 2 triggering events (Meas Ids) for a candidate cell, network ensures that both refer to the same *measObject.* If network configures *condEventD1* or *condEventT1* for a candidate cell, network configures a second triggering event *condEventA3, condEventA4* or *condEventA5*. Network does not configure both *condEventD1* or *condEventT1* for the same candidate cell. For CPAC, the *RRCReconfiguration* message contained in *condRRCReconfig* cannot contain the field *scg-State*. | lixiaolong1@xiaomi.com |  |
| 65 | | N | In 6.3.2 *EphemerisInfo* The IE *EphemerisInfo* provides satellite ephemeris. Ephemeris may be expressed either in format of position and velocity state vector or in format of orbital parameters. FFS more detailed description. | Suggest to remove the FFS part since the ephemeris is completed.  The IE *EphemerisInfo* provides satellite ephemeris. Ephemeris may be expressed either in format of position and velocity state vector or in format of orbital parameters. | Lixiaolong1@xiaomi.com |  |
| 66 | | N | In 6.3.2 *Hysteresis, HysteresisLocation* The IE *Hysteresis* is a parameter used within the entry and leave condition of an event triggered reporting condition. The actual value is field value \* 0.5 dB. The *HysteresisLocation* is a parameter used within entry and leave condition of a location based event triggered reporting condition. The actual value of field *HysteresisLocation* is field value \* 10 meters.  *Hysteresis* information element  -- ASN1START  -- TAG-HYSTERESIS-START  Hysteresis ::= INTEGER (0..30)  HysteresisLocation-r17 ::= INTEGER (0..32768)  -- TAG-HYSTERESIS-STOP  -- ASN1STOP | Suggest to describe the *Hysteresis* and *HysteresisLocation* separately since there are applied in different events and have different unit. *Hysteresis,* The IE *Hysteresis* is a parameter used within the entry and leave condition of an event triggered reporting condition. The actual value is field value \* 0.5 dB. *Hysteresis* information element  -- ASN1START  -- TAG-HYSTERESIS-START  Hysteresis ::= INTEGER (0..30)  -- TAG-HYSTERESIS-STOP  -- ASN1STOP *HysteresisLocation* The *HysteresisLocation* is a parameter used within entry and leave condition of a location based event triggered reporting condition. The actual value of field *HysteresisLocation* is field value \* 10 meters.  *HysteresisLocation* information element  -- ASN1START  -- TAG-HYSTERESIS-START  HysteresisLocation-r17 ::= INTEGER (0..32768)  -- TAG-HYSTERESIS-STOP  -- ASN1STOP | Lixiaolong1@xiaomi.com |  |
| 67 | | N | In 6.3.2  ***trackingAreaList***  List of Tracking Areas to which the cell indicated by *cellIdentity* field belongs. If this field is present, the UE shall ignore *trackingAreaCode*, if present.. Total number of TACs across different PLMNs of the cell cannot exceed *maxTAC*. | ***trackingAreaList***  List of Tracking Areas to which the cell indicated by *cellIdentity* field belongs. If this field is present, the UE shall ignore *trackingAreaCode*, if present, total number of TACs across different PLMNs of the cell cannot exceed *maxTAC*. | Lixiaolong1@xiaomi.com |  |
| 68 | | N | In 6.3.2  ReportConfigNR  Event D1:Distance between UE and a reference location referenceLocation1 becomes larger than configured threshold1 Thresh1 and distance between UE and a reference location referenceLocation2 becomes shorter than configured threshold Thresh2;  CondEvent T1: Time measured at UE becomes more than configured threshold Thresh1 but is less than Thresh2; | Event D1:Distance between UE and a reference location *referenceLocation1* becomes larger than configured threshold *Thresh1* and distance between UE and a reference location *referenceLocation2* becomes shorter than configured threshold *Thresh2*;  CondEvent T1: Time measured at UE becomes more than configured threshold *Thresh1* but is less than configured threshold *Thresh2*; | Lixiaolong1@xiaomi.com |  |
| 69 | | *N* | In 5.8.3  include *sl-TxResourceReqListDis* and set its fields (if needed) as follows for each destination for which it requests network to assign NR sidelink discovery announcements resource: | *sl-TxResourceReqListDis => sl-TxResourceReqListDisc* | gordonpetery@xiaomi.com |  |
| 70 | | No | In 6.3.1  ***periodicityAndOffset***  The periodicity and slot offset (slot) for periodicTRS. It is used to determine the location of the first slot of TRS resource set. The periodicity value *slots10* corresponds to 10 slots, value *slots20* corresponds to 20 slots, and so on. | Missing a space.  Change to: periodic TRS | Liyanhua1@xiaomi.com |  |
| 71 | | Y | In 6.3.2  *CellGroupConfig*  -- Serving cell specific MAC and PHY parameters for a SpCell:  SpCellConfig ::= SEQUENCE {  servCellIndex ServCellIndex OPTIONAL, -- Cond SCG  reconfigurationWithSync ReconfigurationWithSync OPTIONAL, -- Cond ReconfWithSync  rlf-TimersAndConstants SetupRelease { RLF-TimersAndConstants } OPTIONAL, -- Need M  rlmInSyncOutOfSyncThreshold ENUMERATED {n1} OPTIONAL, -- Need S  spCellConfigDedicated ServingCellConfig OPTIONAL, -- Need M  ...,  [[  lowMobilityEvaluationConnected-r17 SEQUENCE {  s-SearchDeltaP-Connected-r17 ENUMERATED {ffs},  t-SearchDeltaP-Connected-r17 ENUMERATED {ffs}  } OPTIONAL, -- Need R  goodServingCellEvaluationRLM-r17 GoodServingCellEvaluation-r17 OPTIONAL, -- Need R  goodServingCellEvaluationBFD-r17 GoodServingCellEvaluation-r17 OPTIONAL, -- Need R  deactivatedSCG-Config-r17 SetupRelease { DeactivatedSCG-Config-r17 } OPTIONAL -- Need M  ]]  } | Suggest to remove ‘,’ | Liyanhua1@xiaomi.com |  |
| 72 | | N | In 6.3.2  *SCellConfig* field descriptions  ***goodServingCellEvaluationBFD***  ***I***ndicates the criterion for a UE to detect the good serving cell quality for BFD relaxation in an SCell in RRC\_CONNECTED. | A typo  Change to “a” | Liyanhua1@xiaomi.com |  |
| 73 | | N | In 6.3.2  *SpCellConfig* field descriptions  ***lowMobilityEvaluationConnected***  Indicates the criterion for a UE to detect low mobility in RRC\_CONNECTED in an SpCell. The *s-SearchDeltaP-Connected* is the parameter "SSearchDeltaP-connected". And the *t-SearchDeltaP-Connected* is the parameter " TSearchDeltaP-Connected". Low mobility criterion is configured in NR Pcell for the case of NR SA/ NR CA/ NE-DC/NR-DC, and in the NR PSCell for the case of EN-DC. | A typo  Change to “a” | Liyanhua1@xiaomi.com |  |
| 74 | | N | In section 4.2.1  **- RRC\_INACTIVE**:  - A UE specific DRX may be configured by upper layers or by RRC layer;  - UE controlled mobility based on network configuration;  - The UE stores the UE Inactive AS context;  - A RAN-based notification area is configured by RRC layer;  - Transfer of unicast data and/or signalling to/from UE over radio bearers configured for SDT;  The UE:  - Monitors Short Messages transmitted with P-RNTI over DCI (see clause 6.5);  - During SDT procedure, monitors control channels associated with the shared data channel to determine if data is scheduled for it;  - While SDT procedure is not ongoing, monitors a Paging channel for CN paging using 5G-S-TMSI and RAN paging using fullI-RNTI;  - If configured by upper layers for MBS multicast reception, monitors Paging channel for paging using TMGI;  - Performs neighbouring cell measurements and cell (re-)selection;  - Performs RAN-based notification area updates periodically and when moving outside the configured RAN-based notification area;  - Acquires system information, while SDT procedure is not ongoing, and can send SI request (if configured);  - While SDT procedure is not ongoing, performs logging of available measurements together with location and time for logged measurement configured UEs;  - While SDT procedure is not ongoing, performs idle/inactive measurements for idle/inactive measurement configured UEs;  - If configured by upper layers for MBS broadcast reception, acquires MCCH change notification and MBS broadcast control information and data. | For inactive state, the SDT bullet (marked in yellow) can be put together, and the MBS related bullets (marked in green) can be put together.  Proposed change is as below:  **- RRC\_INACTIVE**:  - A UE specific DRX may be configured by upper layers or by RRC layer;  - UE controlled mobility based on network configuration;  - The UE stores the UE Inactive AS context;  - A RAN-based notification area is configured by RRC layer;  - Transfer of unicast data and/or signalling to/from UE over radio bearers configured for SDT;  The UE:  - Monitors Short Messages transmitted with P-RNTI over DCI (see clause 6.5);  - During SDT procedure, monitors control channels associated with the shared data channel to determine if data is scheduled for it;  - While SDT procedure is not ongoing,  - monitors a Paging channel for CN paging using 5G-S-TMSI and RAN paging using fullI-RNTI;  - acquires system information, and can send SI request (if configured);  - performs logging of available measurements together with location and time for logged measurement configured UEs;  - performs idle/inactive measurements for idle/inactive measurement configured UEs;  - Performs neighbouring cell measurements and cell (re-)selection;  - Performs RAN-based notification area updates periodically and when moving outside the configured RAN-based notification area;  - If configured by upper layers for MBS multicast reception,  - monitors Paging channel for paging using TMGI;  - acquires MCCH change notification and MBS broadcast control information and data.  . | Fangli\_xu@apple.com |  |
| 75 | | N | In 5.3.8.3  3> for SRB2, if it is resumed and for SRB1:  4> trigger the PDCP entity to perform SDU discard as specified in TS 38.323 [5]; | Comma (,) should be removed, and It should be updated as follow:  3> for SRB2 (if it is resumed) and for SRB1:  4> trigger the PDCP entity to perform SDU discard as specified in TS 38.323 [5]; | Fangli\_xu@apple.com |  |
| 76 | | N | In 5.3.8.3  3> if configured grant resources for SDT are configured:  4> configure the MAC entity with the configured grant resources for SDT and instruct MAC to start the *cg-SDT-TimeAlignmentTimer*; | “configured grant resources” should be replaced by the parameter name (sdt-MAC-PHY-CG-Config )in ASN.1  Following is the proposed change:  3> if configured grant resources for SDT are configured:  4> configure the MAC entity with the configured grant resources for SDT and instruct MAC to start the *cg-SDT-TimeAlignmentTimer*; | Fangli\_xu@apple.com |  |
| 77 | | N | Section 5.7.8.2a  While in RRC\_IDLE or RRC\_INACTIVE, and T331 is running and and T319a is not running, the UE shall: | Remove the duplicated “and”  While in RRC\_IDLE or RRC\_INACTIVE, and T331 is running and T319a is not running, the UE shall: | Fangli\_xu@apple.com |  |
| 78 | | Y | Field description part.  ***sdt-DataVolumeThreshold***  Data volume threshold used to determine whether SDT can be initiated, as specified in TS 38.321 [3]. Value *byte32* corresponds to 32 bytes, value *byte100* corresponds to 100 bytes, and so on. | Correct the color to black.  ***sdt-DataVolumeThreshold***  Data volume threshold used to determine whether SDT can be initiated, as specified in TS 38.321 [3]. Value *byte32* corresponds to 32 bytes, value *byte100* corresponds to 100 bytes, and so on. | Fangli\_xu@apple.com |  |
| 79 | | Y | Field description part.  ***sdt-LogicalChannelSR-DelayTimer***  The value of logicalChannelSR-DelayTimer applied during SDT for logical channels configured with SDT, as specified in TS 38.321 [3]. Value in number of subframes. Value *sf20* corresponds to 20 subframes, *sf40* corresponds to 40 subframes, and so on. If this field is not configured, then logicalChannelSR-DelayTimer is not applied for SDT logical channels. | “is” is missing in the first sentence.  ***sdt-LogicalChannelSR-DelayTimer***  The value of logicalChannelSR-DelayTimer **is** applied during SDT for logical channels configured with SDT, as specified in TS 38.321 [3]. Value in number of subframes. Value *sf20* corresponds to 20 subframes, *sf40* corresponds to 40 subframes, and so on. If this field is not configured, then logicalChannelSR-DelayTimer is not applied for SDT logical channels. | Fangli\_xu@apple.com |  |
| 80 | | Y | Field description part.  ***sdt-RSRP-Threshold***  RSRP threshold for UE to determine whether to perform SDT procedure, as specified in TS 38.321 [3]. | Improve the description and align the description as that for sdt-DataVolumeThreshold.  The proposed change:  ***sdt-RSRP-Threshold***  RSRP threshold used to determine whether SDT can be initiated, as specified in TS 38.321 [3]. | Fangli\_xu@apple.com |  |
| 81 | | N | Section 7.1.1.  T319, stop condition  Upon reception of *RRCResume,* *RRCSetup, RRCRelease, RRCRelease* with *suspendConfig* or *RRCReject* message, upon cell re-selection and upon relay (re)selection. | T319, stop condition, “and” should be “or”  The proposed change:  Upon reception of *RRCResume,* *RRCSetup, RRCRelease, RRCRelease* with *suspendConfig* or *RRCReject* message, upon cell re-selection or upon relay (re)selection. | Fangli\_xu@apple.com |  |
| 82 | | N | Section 5.3.1.1  In any case, the network will apply both ciphering and integrity protection for the RRC reconfiguration messages used to establish SRB2, DRBs and multicast MRBs. | “and” should be changed to “and/or”.  The proposed change:  In any case, the network will apply both ciphering and integrity protection for the RRC reconfiguration messages used to establish SRB2, DRBs and/or multicast MRBs. | Fangli\_xu@apple.com |  |
| 83 | | N | Section 5.3.1.1  For IAB-MT, a configuration with SRB2 without any DRB/MRB is supported. | “MRB” should be “multicast MRB”.  The proposed change:  For IAB-MT, a configuration with SRB2 without any DRB/multicast MRB is supported. | Fangli\_xu@apple.com |  |
| 84 | | N | Section 5.3.5.6.1  1> release all SDAP entities, if any, that have no associated DRB as specified in TS 37.324 [24] clause 5.1.2, and indicate the release of the user plane resources for PDU Sessions associated with the released SDAP entities to upper layers;  1> release all SDAP entities that have no associated multicast MRB, and indicate the release of user plane resources for these MBS multicast sessions to upper layers. | Align the description, and add the spec reference to the MRB SDAP handling as marked in red.  1> release all SDAP entities, if any, that have no associated DRB as specified in TS 37.324 [24] clause 5.1.2, and indicate the release of the user plane resources for PDU Sessions associated with the released SDAP entities to upper layers;  1> release all SDAP entities that have no associated multicast MRB as specified in TS 37.324 [24] clause 5.1.2, and indicate the release of user plane resources for these MBS multicast sessions to upper layers. | Fangli\_xu@apple.com |  |
| 85 | | N | Section 5.3.13.3  1> configure lower layers to apply integrity protection for all radio bearers except SRB0 and MRBs using the configured algorithm and the KRRCint key and KUPint key derived in this subclause immediately, i.e., integrity protection shall be applied to all subsequent messages received and sent by the UE;  NOTE 1: Only DRBs with previously configured UP integrity protection shall resume integrity protection.  1> configure lower layers to apply ciphering for all radio bearers except SRB0 and MRBs and to apply the configured ciphering algorithm, the KRRCenc key and the KUPenc key derived in this subclause, i.e. the ciphering configuration shall be applied to all subsequent messages received and sent by the UE; | “MRBs” should be “multicast MRBs”  The proposed change:  1> configure lower layers to apply integrity protection for all radio bearers except SRB0 and multicast MRBs using the configured algorithm and the KRRCint key and KUPint key derived in this subclause immediately, i.e., integrity protection shall be applied to all subsequent messages received and sent by the UE;  NOTE 1: Only DRBs with previously configured UP integrity protection shall resume integrity protection.  1> configure lower layers to apply ciphering for all radio bearers except SRB0 and multicast MRBs and to apply the configured ciphering algorithm, the KRRCenc key and the KUPenc key derived in this subclause, i.e. the ciphering configuration shall be applied to all subsequent messages received and sent by the UE; | Fangli\_xu@apple.com |  |
| 86 | | N | Section 5.9.2.3  1> if the UE enters a cell broadcasting *SIB20*:  2> acquire the *MBSBroadcastConfiguration* message on MCCH at the next repetition period; | “;” should be “.”  The proposed change:  1> if the UE enters a cell broadcasting *SIB20*:  2> acquire the *MBSBroadcastConfiguration* message on MCCH at the next repetition period. | Fangli\_xu@apple.com |  |
| 87 | | N | Section 5.9.3.2  The UE applies the broadcast MRB establishment procedure to start receiving an MBS session of a MBS broadcast service it is interested in. The procedure may be initiated e.g. upon start of the MBS session, upon entering a cell providing a MBS broadcast service UE is interested in, upon becoming interested in the MBS broadcast service, upon removal of UE capability limitations inhibiting reception of the MBS broadcast service UE is interested in.  The UE applies the broadcast MRB release procedure to stop receiving a session of a MBS broadcast service. The procedure may be initiated e.g. upon stop of the MBS session, upon leaving the cell broadcasting the MBS service UE is interested in, upon losing interest in the MBS service, when capability limitations start inhibiting reception of the concerned service. | “UE” should be “the UE”  The proposed change:  The UE applies the broadcast MRB establishment procedure to start receiving an MBS session of a MBS broadcast service it is interested in. The procedure may be initiated e.g. upon start of the MBS session, upon entering a cell providing a MBS broadcast service the UE is interested in, upon becoming interested in the MBS broadcast service, upon removal of the UE capability limitations inhibiting reception of the MBS broadcast service UE is interested in.  The UE applies the broadcast MRB release procedure to stop receiving a session of a MBS broadcast service. The procedure may be initiated e.g. upon stop of the MBS session, upon leaving the cell broadcasting the MBS service the UE is interested in, upon losing interest in the MBS service, when capability limitations start inhibiting reception of the concerned service. | Fangli\_xu@apple.com |  |
| 87 | | N | Section 5.9.4.3  2> for at least one of these MBS sessions *SIB21* acquired from the PCell includes for the concerned frequency one or more MBS FSAIs as indicated in the USD for this session; and | It should be “included in SIB21”  The proposed change:  2> for at least one of these MBS sessionsincluded in *SIB21* acquired from the PCell includes for the concerned frequency one or more MBS FSAIs as indicated in the USD for this session; and | Fangli\_xu@apple.com |  |
| 88 | | N | Section 5.9.4.5  2> if *SIB20* is scheduled by the PCell: | It should be updated as follow, which is aligned with the description in other place (e.g. 5.9.4.2)  2> if *SIB20* is provided by the PCell: | Fangli\_xu@apple.com |  |
| 89 | | Y | The field description  ***pdsch-ConfigMTCH***  Provides parameters for acquiring the PDSCH for MTCH. The UE shall use parameters in *pdsch-ConfigMCCH* also for PDSCH of MTCH when this field is absent. | The absent description can be reworded as below.  ***pdsch-ConfigMTCH***  Provides parameters for acquiring the PDSCH for MTCH. When this field is absent, the UE shall use parameters in *pdsch-ConfigMCCH* to acquire the PDSCH for MTCH. | Fangli\_xu@apple.com |  |
| 90 | | Y | allowCSI-SRS-Tx-MulticastDRX-Active-r17  MAC-CellGroupConfig ::= SEQUENCE {  …    allowCSI-SRS-Tx-MulticastDRX-Active-r17 BOOLEAN  ]]  } | The parameter should be optional.  MAC-CellGroupConfig ::= SEQUENCE {  …  allowCSI-SRS-Tx-MulticastDRX-Active-r17 BOOLEAN OPTIONAL, -- Need M  ]]  } | Fangli\_xu@apple.com |  |
| 91 | | Y | Field description  ***headerCompression***  If rohc is configured, the UE shall apply the configured ROHC profile(s) in both uplink and downlink. If *uplinkOnlyROHC* is configured, the UE shall apply the configured ROHC profile(s) in uplink (there is no header compression in downlink). ROHC can be configured for any bearer type. ROHC and EHC can be both configured simultaneously for a DRB or a multicast MRB. The network reconfigures *headerCompression* only upon reconfiguration involving PDCP re-establishment, and without any *drb-ContinueROHC*. Network configures *headerCompression* to *notUsed* when *outOfOrderDelivery* is configured. Network only configures this field when *uplinkDataCompression* is not configured | “Multicast MRB” should be " a bi-directional multicast MRB".  ***headerCompression***  If rohc is configured, the UE shall apply the configured ROHC profile(s) in both uplink and downlink. If *uplinkOnlyROHC* is configured, the UE shall apply the configured ROHC profile(s) in uplink (there is no header compression in downlink). ROHC can be configured for any bearer type. ROHC and EHC can be both configured simultaneously for a DRB or a bi-directional multicast MRB. The network reconfigures *headerCompression* only upon reconfiguration involving PDCP re-establishment, and without any *drb-ContinueROHC*. Network configures *headerCompression* to *notUsed* when *outOfOrderDelivery* is configured. Network only configures this field when *uplinkDataCompression* is not configured | Fangli\_xu@apple.com |  |
| 92 | | Y | Field description  ***tmgi***  Indicates which MBS session the bearer is associated with. | It should clarified as “multicast MBS session”.  ***tmgi***  Indicates which multicast MBS session the bearer is associated with. | Fangli\_xu@apple.com |  |
| 93 | | Y | section 6.3.6  *CarrierFreqListMBS*  The IE *CarrierFreqListMBS* is used to inform network of the frequencies on which the UE is receiving or interested to receive MBS broadcast service via a broadcast MRB | A full stop is missing.  *CarrierFreqListMBS*  The IE *CarrierFreqListMBS* is used to inform network of the frequencies on which the UE is receiving or interested to receive MBS broadcast service via a broadcast MRB. | Fangli\_xu@apple.com |  |
| 94 | | Y | section 6.3.6, TMGI  *– MBS-SessionInfoList*  The IE *MBS-SessionInfoList* provides the list of ongoing MBS broadcast sessions transmitted via broadcast MRB and, for each MBS broadcast session, the associated G-RNTI and scheduling information.  TMGI-r17 ::= SEQUENCE {  plmn-Id-r17 CHOICE {  plmn-Index-r17 INTEGER (1..maxPLMN),  explicitValue-r17 PLMN-Identity  },  serviceId-r17 OCTET STRING (SIZE (3))  } | TMGI is used in multiple places, so it should be specified as the separate information element, and should not under the MBS-SessionInfoList.  *– TMGI*  The IE *TMGI* is the identity which is associated with the MBS session  *TMGI*  information element  -- ASN1START  -- TAG-MBS-SESSIONINFOLIST-START  TMGI-r17 ::= SEQUENCE {  plmn-Id-r17 CHOICE {  plmn-Index-r17 INTEGER (1..maxPLMN),  explicitValue-r17 PLMN-Identity  },  serviceId-r17 OCTET STRING (SIZE (3))  }  -- TAG-MBS-SESSIONINFOLIST-STOP  -- ASN1STOP | Fangli\_xu@apple.com |  |
| 95 | | Y | Section 6.3.6, DRX-ConfigPTM  Condition of *HARQFeedback*  The field is mandatory present if HARQ feedback is enabled for a G-RNTI associated with this DRX configuration. It is absent otherwise. | For the condition, it is related to the HARQ feedback for G-RNTI and G-CS-RNTI.  Condition of *HARQFeedback*  The field is mandatory present if HARQ feedback is enabled for a G-RNTI/G-CS-RNTI associated with this DRX configuration. It is absent otherwise. | Fangli\_xu@apple.com |  |
| 96 | | N | 3> if *drb-ContinueUDC* is included in *pdcp-Config*:  4> indicate to lower layer that *drb-ContinueUDC* is configured;3> re-establish the PDCP entity of this DRB as specified in TS 38.323 [5], clause 5.1.2; | Incorrect formatting: “3>” needs to go on next line.  3> if drb-ContinueEHC-UL is included in pdcp-Config:  4> indicate to lower layer that drb-ContinueEHC-UL is configured;  3> if drb-ContinueUDC is included in pdcp-Config:  4> indicate to lower layer that drb-ContinueUDC is configured; | rrossbach@apple.com |  |
| 97 | | N | ***schedulingCellId***  If configured for a SpCell, this field indicates which SCell, in addition to the SpCell, signals the downlink allocations and uplink grants, if applicable, for the concerned SpCell. If configured for a Scell, this field indicates which cell signals the downlink allocations and uplink grants, if applicable, for the concerned SCell. | To align with other parts in the specification including the existing field descriptions of *CrossCarrierSchedulingConfig*, it is proposed to change “a SpCell” to “an SpCell”.  **schedulingCellId**  If configured for an SpCell, this field indicates which SCell, in addition to the SpCell, signals the downlink allocations and uplink grants, if applicable, for the concerned SpCell. If configured for an Scell, this field Iindicates which cell signals the downlink allocations and uplink grants, if applicable, for the concerned SCell. | rrossbach@apple.com |  |
| 98 | | N | The IE *PDCCH-Config* is used to configure UE specific or MBS multicast PDCCH parameters such as control resource sets (CORESET), search spaces and additional parameters for acquiring the PDCCH. | The IE *PDCCH-Config* is used to configure UE specific PDCCH parameters or MBS multicast PDCCH parameters such as control resource sets (CORESET), search spaces and additional parameters for acquiring the PDCCH. | rrossbach@apple.com |  |
| 99 | | N | ***searchSpaceId***  Identity of the search space. SearchSpaceId = 0 identifies the *searchSpaceZero* configured via PBCH (MIB) or *ServingCellConfigCommon* and may hence not be used in the *SearchSpace* IE. The *searchSpaceId* is unique among the BWPs of a Serving Cell. In case of cross carrier scheduling, search spaces with the same *searchSpaceId* in scheduled cell and scheduling cell are linked to each other. The UE applies the search space for the scheduled cell only if the DL BWPs in which the linked search spaces are configured in scheduling cell and scheduled cell are both active.  For an IAB-MT, the search space defines how/where to search for PDCCH candidates for an IAB-MT:each search space is associated with one ControlResearchSet; for a scheduled cell in the case of cross carrier scheduling, except for nrofCandidates, all the optional fields are absent. | As discussed in the DSS WI (R2-2203843), it was not initially clear that the original sentences (in version g70) are linked but IAB-specific.  ***searchSpaceId***  Identity of the search space. SearchSpaceId = 0 identifies the *searchSpaceZero* configured via PBCH (MIB) or *ServingCellConfigCommon* and may hence not be used in the *SearchSpace* IE. The *searchSpaceId* is unique among the BWPs of a Serving Cell. In case of cross carrier scheduling, search spaces with the same *searchSpaceId* in scheduled cell and scheduling cell are linked to each other. The UE applies the search space for the scheduled cell only if the DL BWPs in which the linked search spaces are configured in scheduling cell and scheduled cell are both active.  For an IAB-MT, the search space defines how/where to search for PDCCH candidates for an IAB-MT where each search space is associated with one ControlResearchSet; for a scheduled cell in the case of cross carrier scheduling, except for nrofCandidates, all the optional fields are absent. | rrossbach@apple.com |  |
| 100 | | N | The purpose of this procedure is to transfer NAS dedicated information from NG-RAN to a UE in RRC\_CONNECTED, or to transfer F1-C related information from IAB Donor-CU to IAB-DU via IAB-MT in RRC\_CONNECTED or to a UE in RRC\_INACTIVE during SDT. | The purpose of this procedure is to transfer NAS dedicated information from NG-RAN to a UE in RRC\_CONNECTED or to a UE in RRC\_INACTIVE during SDT, or to transfer F1-C related information from IAB Donor-CU to IAB-DU via IAB-MT in RRC\_CONNECTED. | rrossbach@apple.com |  |
| 101 | | N | CG-SDT-Configuration-r17 ::= SEQUENCE {  cg-SDT-RetransmissionTimer INTEGER (1..64) OPTIONAL, -- Need R  sdt-SSB-Subset-r17 CHOICE {  shortBitmap-r17 BIT STRING (SIZE (4)),  mediumBitmap-r17 BIT STRING (SIZE (8)),  longBitmap-r17 BIT STRING (SIZE (64))  } OPTIONAL, -- Need S  sdt-SSB-PerCG-PUSCH-r17 ENUMERATED {oneEighth, oneFourth, half, one, two, four, eight, sixteen} OPTIONAL, -- Need M  sdt-P0-PUSCH-r17 INTEGER (-16..15) OPTIONAL, -- Need M  sdt-Alpha-r17 ENUMERATED {alpha0, alpha04, alpha05, alpha06, alpha07, alpha08, alpha09, alpha1} OPTIONAL, -- Need M  sdt-DMRS-Ports-r17 CHOICE {  dmrsType1-r17 BIT STRING (SIZE (8)),  dmrsType2-r17 BIT STRING (SIZE (12))  } OPTIONAL, -- Need M  sdt-NrofDMRS-Sequences-r17 INTEGER (1..2) OPTIONAL -- Need M  } | The color coding of the sdt-DMRS-Ports-r17 struct needs to be corrected. | rrossbach@apple.com |  |
| 102 | | Y | In IE *LogicalChannelConfig:*  allowedHARQ-mode | allowedHARQ-mode-r17 | pnuggehalli@apple.com |  |
| 103 | | N | ***allowedHARQ-mode***  Indicates the allowed HARQ mode of a HARQ process mapped to this logical channel. If the parameter is not configured, there is no restriction for HARQ mode for the mapping. This field also applies to SRB1, SRB2 and SRB3. | ***allowedHARQ-mode***  Indicates the allowed HARQ mode of a HARQ process mapped to this logical channel. If the parameter is not configured, there is no restriction for HARQ mode for the mapping. This field also applies to SRB1, SRB2, SRB3, and SRB4. | pnuggehalli@apple.com |  |
| 104 | | Y | DL-AM-RLC-v1610 ::= SEQUENCE {  t-StatusProhibit-v1610 T-StatusProhibit-v1610 OPTIONAL, -- Need N  ...,  [[  t-ReassemblyExt-r17 T-ReassemblyExt-r17 OPTIONAL -- Need N  ]]  } | The highlighted part seems to be duplicated and should be removed | pnuggehalli@apple.com |  |
| 105 | | Y | In IE *MAC-CellGroupConfig:*  offsetThresholdTA | offsetThresholdTA-r17 | pnuggehalli@apple.com |  |
| 106 | | Y | UEAssistanceInformation-v1700-IEs ::= SEQUENCE {  ul-GapFR2-Preference-r17 UL-GapFR2-Preference-r17 OPTIONAL,  musim-Assistance-r17 MUSIM-Assistance-r17 OPTIONAL,  overheatingAssistance-r17 OverheatingAssistance-r17 OPTIONAL,  maxBW-PreferenceFR2-2-r17 MaxBW-PreferenceFR2-2-r17 OPTIONAL,  maxMIMO-LayerPreferenceFR2-2-r17 MaxMIMO-LayerPreferenceFR2-2-r17 OPTIONAL,  minSchedulingOffsetPreferenceExt-r17 MinSchedulingOffsetPreferenceExt-r17 OPTIONAL,  rlm-MeasRelaxationState-r17 BOOLEAN OPTIONAL,  bfd-MeasRelaxationState-r17 BIT STRING (SIZE (32)) OPTIONAL,  nonSDT-DataIndication-r17 SEQUENCE {  resumeCause-r17 ResumeCause OPTIONAL  } OPTIONAL,  scg-DeactivationPreference ENUMERATED { scgDeactivationPreferred, noPreferrence } OPTIONAL,  uplinkData-r17 ENUMERATED { true } OPTIONAL,  rrm-MeasRelaxationFulfilment-r17 BOOLEAN OPTIONAL,  nonCriticalExtension SEQUENCE {} OPTIONAL  } | noPreferrence to noPreference | naveen.palle@apple.com |  |
| 107 | | Y | DeactivatedSCG-Config-r17 ::= SEQUENCE {  bfd-and-RLM BOOLEAN,  ...  } | From BOOLEAN to ENUMERATED {perform}  [david.lecompte@huawei.com] This should be discussed in a session, this is not class 0. | naveen.palle@apple.com |  |
| 108 | | Y | CondReconfigToAddMod-r16 ::= SEQUENCE {  condReconfigId-r16 CondReconfigId-r16,  condExecutionCond-r16 SEQUENCE (SIZE (1..2)) OF MeasId OPTIONAL, -- Need M  condRRCReconfig-r16 OCTET STRING (CONTAINING RRCReconfiguration) OPTIONAL, -- Cond condReconfigAdd  ...,  [[  condExecutionCondSCG-r17 OCTET STRING (CONTAINING CondReconfigExecCondSCG-r17) OPTIONAL -- Need M  ]]  } | Define a seperate SEQUENCE for COndReconfigExecConfSCG-r17 instead of embedding an OCTECT STRING for condExecutionCondSCG-r17. We do not understand the advantage of OCTET STRING, better to have this as a SEQUENCE.  [david.lecompte@huawei.com] This should be discussed in a session, this is not class 0. | naveen.palle@apple.com |  |
| 109 | | Y | SIB12-IEs-r16 ::= SEQUENCE {  sl-ConfigCommonNR-r16 SL-ConfigCommonNR-r16,  lateNonCriticalExtension OCTET STRING OPTIONAL,  ...,  [[  sl-DRX-ConfigCommon-GC-BC-r17 SL-DRX-Config-GC-BC-r17 OPTIONAL, -- Need R  sl-DiscConfigCommon-r17 SL-DiscConfigCommon-r17 OPTIONAL, -- Need R  sl-L2U2N-Relay ENUMERATED {support} OPTIONAL, -- Need R  sl-NonRelayDiscovery ENUMERATED {support} OPTIONAL, -- Need R  sl-L3U2N-RelayDiscovery ENUMERATED {support} OPTIONAL -- Need R  ]]  } | Spurious hyphens, should be  sl-DRX-ConfigCommonGC-BC-r17 SL-DRX-ConfigGC-BC-r17 OPTIONAL, -- Need R | nathan.tenny@mediatek.com |  |
| 110 | | Y | SidelinkUEInformationNR-v1700-IEs ::= SEQUENCE {  sl-TxResourceReqList-v1700 SL-TxResourceReqList-v1700 OPTIONAL,  sl-RxDRX-ReportList-v1700 SL-RxDRX-ReportList-v1700 OPTIONAL,  sl-RxInterestedFreqListDisc-r17 SL-InterestedFreqList-r16 OPTIONAL,  sl-TxResourceReqListDisc-r17 SL-TxResourceReqListDisc-r17 OPTIONAL,  sl-TxResourceReqListCommRelay-r17 SL-TxResourceReqListCommRelay-r17 OPTIONAL,  ue-Type-r17 ENUMERATED {relayUE, remoteUE} OPTIONAL,  sl-SourceIdentity-RemoteUE-r17 SL-SourceIdentity-r17 OPTIONAL,  nonCriticalExtension SEQUENCE {} OPTIONAL  } | Spurious hyphen, should be  sl-SourceIdentityRemoteUE-r17 SL-SourceIdentity-r17 OPTIONAL, | nathan.tenny@mediatek.com |  |
| 111 | | Y | SL-TxResourceReqDisc-r17 ::= SEQUENCE {  sl-DestinationIdentityDisc-r17 SL-DestinationIdentity-r16,  sl-SourceIdentity-RelayUE-r17 SL-SourceIdentity-r17 OPTIONAL,  sl-CastTypeDisc-r17 ENUMERATED {broadcast, groupcast, unicast, spare1},  sl-TxInterestedFreqListDisc-r17 SL-TxInterestedFreqList-r16,  sl-TypeTxSyncListDis-r17 SEQUENCE (SIZE (1..maxNrofFreqSL-r16)) OF SL-TypeTxSync-r16,  sl-DiscoveryType-r17 ENUMERATED {relay, non-Relay},  ...  } | Spurious hyphen, should be  sl-SourceIdentityRelayUE-r17 SL-SourceIdentity-r17 OPTIONAL, | nathan.tenny@mediatek.com |  |
| 112 | | Y | RRCReconfigurationSidelink-v1700-IEs ::= SEQUENCE {  sl-DRX-ConfigUC-PC5-r17 SetupRelease { SL-DRX-ConfigUC-r17 } OPTIONAL, -- Need M  sl-LatencyBoundIUC-Report-r17 SetupRelease { SL-LatencyBoundIUC-Report-r17 } OPTIONAL, -- Need M  sl-RLC-ChannelToReleaseList-PC5-r17 SEQUENCE (SIZE (1..maxSL-LCID-r16)) OF SL-RLC-ChannelID-r17 OPTIONAL, -- Need N  sl-RLC-ChannelToAddModList-PC5-r17 SEQUENCE (SIZE (1..maxSL-LCID-r16)) OF SL-RLC-ChannelConfig-PC5-r17 OPTIONAL, -- Need N  nonCriticalExtension SEQUENCE {} OPTIONAL  } | Spurious hyphens, should be  sl-RLC-ChannelToReleaseListPC5-r17 SEQUENCE (SIZE (1..maxSL-LCID-r16)) OF SL-RLC-ChannelID-r17 OPTIONAL, -- Need N  sl-RLC-ChannelToAddModListPC5-r17 SEQUENCE (SIZE (1..maxSL-LCID-r16)) OF SL-RLC-ChannelConfigPC5-r17 OPTIONAL, -- Need N | nathan.tenny@mediatek.com |  |
| 113 | | Y | RemoteUEInformationSidelink-r17-IEs ::= SEQUENCE {  sl-Requested-SI-List-r17 SetupRelease { SL-Requested-SI-List-r17} OPTIONAL, -- Need M  sl-PagingInfo-RemoteUE-r17 SetupRelease { SL-PagingInfo-RemoteUE-r17} OPTIONAL, -- Need M  lateNonCriticalExtension OCTET STRING OPTIONAL,  nonCriticalExtension SEQUENCE {} OPTIONAL  }  SL-Requested-SI-List-r17 ::= BIT STRING (SIZE (maxSI-MessagePlus1-r17))  SL-PagingInfo-RemoteUE-r17 ::= SEQUENCE {  sl-PagingIdentity-RemoteUE-r17 SL-PagingIdentity-RemoteUE-r17 OPTIONAL, -- Need M  sl-PagingCycle-RemoteUE-r17 PagingCycle OPTIONAL -- Need M  } | Multiple spurious hyphens, should be  SEQUENCE {  sl-RequestedSI-List-r17 SetupRelease { SL-RequestedSI-List-r17} OPTIONAL, -- Need M  sl-PagingInfoRemoteUE-r17 SetupRelease { SL-PagingInfoRemoteUE-r17} OPTIONAL, -- Need M  lateNonCriticalExtension OCTET STRING OPTIONAL,  nonCriticalExtension SEQUENCE {} OPTIONAL  }  SL-RequestedSI-List-r17 ::= BIT STRING (SIZE (maxSI-MessagePlus1-r17))  SL-PagingInfoRemoteUE-r17 ::= SEQUENCE {  sl-PagingIdentityRemoteUE-r17 SL-PagingIdentityRemoteUE-r17 OPTIONAL, -- Need M  sl-PagingCycleRemoteUE-r17 PagingCycle OPTIONAL -- Need M  } | nathan.tenny@mediatek.com |  |
| 114 | | Y | freqPriorityListNRSlicing | Due to ASN.1 naming rules this is not correct: "-" is missing after "NR". Proposed to remove "NR" to shorten it. It will not cause any issues, as this only used in NR:  freqPriorityListSlicing  (Occurs several times) | [gyorgy.wolfner@nokia.com](mailto:gyorgy.wolfner@nokia.com) |  |
| 115 | | Y | FreqPriorityListNRSlicing | Due to ASN.1 naming rules this is not correct: "-" is missing after "NR". Proposed to remove "NR" to shorten it. It will not cause any issues, as this only used in NR:  FreqPriorityListSlicing  (Occurs several times) | [gyorgy.wolfner@nokia.com](mailto:gyorgy.wolfner@nokia.com) |  |
| 116 | | Y | sliceAllowCellListNR-r17 | Proposed to rename it to  "*sliceAllowedCellListNR-r17*" to align the name used in SIB3/SIB4 for similar type of list  (Occurs several times) | [gyorgy.wolfner@nokia.com](mailto:gyorgy.wolfner@nokia.com) |  |
| 117 | | Y | sliceExcludeCellListNR-r17 | Proposed to rename it to  "sliceExcludedCellListNR-r17" to align the name used in SIB3/SIB4 for similar type of list  (Occurs several times) | [gyorgy.wolfner@nokia.com](mailto:gyorgy.wolfner@nokia.com) |  |
| 118 | | N | Indicates the list of frequency priority information for frequencies. The 1st entry in the list corresponds to the current frequency (referring SIB2), the 2nd entry in the list corresponds to the first frequency indicated by the InterFreqCarrierFreqList in SIB4, and the 3rd entry in the list corresponds to the second frequency indicated by the InterFreqCarrierFreqList in SIB4, and so on. | Missing italics in the words highlighted by yellow | [gyorgy.wolfner@nokia.com](mailto:gyorgy.wolfner@nokia.com) |  |
| 119 | | N | Indicates the list of allow-list or exclude-listed neighbour cells for slicing. If *sliceInfo-r17* corresponds to the current frequency, this field should be absent. FFS if the field can be provided in *RRCRelease*. | Proposed editorial corrections:  Indicates the list of allow-listed or exclude-listed neighbour cells for slicing. If *SliceInfo* corresponds to the current frequency, this field should be absent. FFS if the field can be provided in *RRCRelease*. | [gyorgy.wolfner@nokia.com](mailto:gyorgy.wolfner@nokia.com) |  |
| 120 | | Y | ginsPerSNPN-List-r17 | Due to ASN. 1 name rules "-" should be added  gins-PerSNPN -List-r17  (Occurs several times) | [gyorgy.wolfner@nokia.com](mailto:gyorgy.wolfner@nokia.com) |  |
| 121 | | N | Indicates the supported GINs for each SNPN. The network includes the same number of entries as the number of SNPNs in *snpn-AccessInfoList* in provided in SIB1, and the n-th entry in this list corresponds to the n-th SNPN listed in *snpn-AccessInfoList* provided in SIB1. It is not present if there is only a single SNPN in *snpn-AccessInfoList* in SIB1, as in that case all GINs in this SIB is associated with that SNPN. | Editorial clarification proposal, as "It" may ambiguous in this context:  Indicates the supported GINs for each SNPN. The network includes the same number of entries as the number of SNPNs in *snpn-AccessInfoList* in provided in SIB1, and the n-th entry in this list corresponds to the n-th SNPN listed in *snpn-AccessInfoList* provided in SIB1. This field is not present if there is only a single SNPN in *snpn-AccessInfoList* in SIB1, as in that case all GINs in this SIB is associated with that SNPN. | [gyorgy.wolfner@nokia.com](mailto:gyorgy.wolfner@nokia.com) |  |
| 122 | | N | A bit set to 1 indicates that the GIN is supported by the SNPN. If the field is not present, then the corresponding SNPN does not support any GINs. | Editorial: "is" is duplicated  If the field is not present, then the corresponding SNPN does not support any GINs. | [gyorgy.wolfner@nokia.com](mailto:gyorgy.wolfner@nokia.com) |  |
| 123 | | N | The network signals a priority for all feature that map to at least one *FeatureCombinationPreambles*. | Change to plural:  The network signals a priority for all feature**s** that map to at least one *FeatureCombinationPreambles*. | malgorzata.tomala@nokia.com |  |
| 124 | | N | The IE *FeatureCombination* indicates a combination of features to be associated with a RA partition (i.e. an instance of *FeatureCombinationPreambles*). | Change the article to “an”:  The IE *FeatureCombination* indicates a combination of features to be associated with an RA partition (i.e. an instance of *FeatureCombinationPreambles*). | malgorzata.tomala@nokia.com |  |
| 125 | | N | if *measConfigAppLayerToAddReleaseList* is included in *appLayerMeasConfig* within *RRCReconfiguration* or *RRCResume*: | No *measConfigAppLayerToAddReleaseList* IE exists  Change to:  if *measConfigAppLayerTo~~Add~~ReleaseList* is included | malgorzata.tomala@nokia.com |  |
| 126 | | N | FeatureCombinatonPreambles field descriptions:   1. ”associated to the Feature Combination starting from the starting preamble(s) per SSB.” 2. ”It defines the first preamble associated with the Feature Combination” 3. It defines the first preamble associated with the Feature Combination | Some fields use upper case for the Feature Combination, some lower. Change all to lower:  1 to: associated to the Feature Combination starting from the starting preamble(s) per SSB.  2 to: It defines the first preamble associated with the feature combination”  3 to: It defines the first preamble associated with the feature combination | malgorzata.tomala@nokia.com |  |
| 127 | | N | If this feature combination preambles are associated to a *RACH-ConfigCommon-twostepRA*, this field correspond to *msgA-RSRP-ThresholdSSB*, otherwise it corresponds to *rsrp-ThresholdSSB*. | Change *RACH-ConfigCommon-****t****wo****s****tepRA* to upper case:  *RACH-ConfigCommon-TwoStepRA*, | malgorzata.tomala@nokia.com |  |
| 128 | | N | 3> indicate to lower layers that the SCG is activated.5.3.5.20 Application layer configuration | Split the procedure from previous section from the heading (formatting issue) | malgorzata.tomala@nokia.com |  |
| 130 | | N | in each PRACH occasion N blocks of preambles associated with the Feature Combination are define | Missing “d”. Change to:  in each PRACH occasion N blocks of preambles associated with the Feature Combination are defined | malgorzata.tomala@nokia.com |  |
| 131 | | N | In clause 5.3.3. note 2  NOTE 2: In case the L2 U2N Relay UE initiates RRC connection establishment according to conditions as specified in 5.3.3.1a, the L2 U2N Relay UE sets the *establishmentCause* by implementation. If the cause value in the message received from the L2 U2N Remote UE via SL-RLC0 is *emergency*, *mps-PriorityAccess*, or *mcs-PriorityAccess*, the L2 U2N Relay UE can set the same valuel Otherwise, the L2 U2N Relay UE does not set the value as *emergency*, *mps-PriorityAccess*, or *mcs-PriorityAccess*. | Typo, value1 should be updated as value | Min.w.wang@ericsson.com |  |
| 132 | | N | In clause 5.3.11  1> release all radio resources, including release of the RLC entity, the BAP entity, the MAC configuration and the associated PDCP entity and SDAP for all established RBs, BH RLC channels, Uu Relay RLC channels, PC5 Relay channels and SRAP entity; | “PC5 relay channel” is updated as “PC5 relay RLC channel” | Min.w.wang@ericsson.com |  |
| 133 | | N | In clause 5.3.14.1,  The purpose of this procedure is to perform access barring check for an access attempt associated with a given Access Category and one or more Access Identities upon request from upper layers according to TS 24.501 [23] or the RRC layer. This procedure does not apply to IAB-MT. This procedure does not apply to L2 U2N Relay UE initiating RRC connection establishment or RRC connection resume upon reception of any message from a L2 U2N remote UE via SL-RLC0 or SL-RLC1 in accordance to 5.3.3.1a and 5.3.13.1a. | Wording issue,  “and” is updated to “or” | [Min.w.wang@ericsson.com](mailto:Min.w.wang@ericsson.com) |  |
| 134 | | N | In clause 5.8.9.x2.2  When entering RRC\_CONNECTED, if L2 U2N remote UE had send *sl-Requested-SI-List* and *sl-PagingInfo-RemoteUE,* the L2 U2N Remote UE shall: | Typo, “send”-🡪 “sent” | Min.w.wang@ericsson.com |  |
| 135 | | N | ***sl-ServingCellInfo***  Indicates the Uu serving Cell related related information. | Typo, one “related” is to be deleted. | Min.w.wang@ericsson.com |  |
| 136 | | N | ***drx-HARQ-RTT-TimerUL***  Value in number of symbols of the BWP where the transport block was transmitted. *drx-HARQ-RTT-TimerDL-r17* is only applicable for SCS 480 kHz and 960 kHz. If configured, the UE shall ignore *drx-HARQ-RTT-TimerDL* (without suffix). | Typo,  *drx-HARQ-RTT-TimerDL-r17-🡪 drx-HARQ-RTT-TimerUL-r17* | Min.w.wang@ericsson.com |  |
| 137 | | N | SL-ResourcePoolConfigPS-r17 ::= SEQUENCE {  sl-ResourcePoolPS-ID-r17 SL-ResourcePoolID-r16,  sl-ResourcePoolPS-r17 SL-ResourcePool-r16 OPTIONAL, -- Need M  ...  } | no need to define new IE for R17, it has exactly same structure as R16 IE  SL-ResourcePoolConfig-r16 ::= SEQUENCE {  sl-ResourcePoolID-r16 SL-ResourcePoolID-r16,  sl-ResourcePool-r16 SL-ResourcePool-r16 OPTIONAL -- Need M  } | Min.w.wang@ericsson.com |  |
| 138 | | N | SL-TxPoolDedicatedPS-r17 ::= SEQUENCE {  sl-PoolToReleasePS-List-r17 SEQUENCE (SIZE (1..maxNrofTXPool-r16)) OF SL-ResourcePoolID-r16 OPTIONAL, -- Need N  sl-PoolToAddModPS-List-r17 SEQUENCE (SIZE (1..maxNrofTXPool-r16)) OF SL-ResourcePoolConfigPS-r17 OPTIONAL -- Need N  } | no need to define a new IE for R17, it has exactly same structure as R16 IE  SL-TxPoolDedicated-r16 ::= SEQUENCE {  sl-PoolToReleaseList-r16 SEQUENCE (SIZE (1..maxNrofTXPool-r16)) OF SL-ResourcePoolID-r16 OPTIONAL, -- Need N  sl-PoolToAddModList-r16 SEQUENCE (SIZE (1..maxNrofTXPool-r16)) OF SL-ResourcePoolConfig-r16 OPTIONAL -- Need N  } | Min.w.wang@ericsson.com |  |
| 139 | | N | ***allowedReducedConfigForOverheating***  Indicates the reduced configuration that the SCG is allowed to configure.  *reducedMaxCCs* in *allowedReducedConfigForOverheating* indicates the maximum number of downlink/uplink PSCell/SCells that the SCG is allowed to configure. This field is used in (NG)EN-DC and NR-DC.  *reducedMaxBW-FR1* and *reducedMaxBW-FR2* in *allowedReducedConfigForOverheating* indicates the maximum aggregated bandwidth across all downlink/uplink carriers of FR1 and FR2-1, respectively that the SCG is allowed to configure. *reducedMaxBW-FR2* in *allowedReducedConfigForOverheating-r17* indicates the maximum aggregated bandwidth across all downlink/uplink carriers of FR2-2 that the SCG is allowed to configure. This field is only used in NR-DC. | Typo, FR2-🡪 FR2-2 | Min.w.wang@ericsson.com |  |
| 140 | | N | ***offsetThresholdTA***  Offset for TA reporting as specified in TS 38.321. | spec reference is missing, should be “TS 38.321 [3]” | xun.tang@intel.com |  |
| 141 | | N | ***EphemerisInfo***  This field provides satellite ephemeris either in format of position and velocity state vector or in format of orbital parameters. This field is excluded when determining changes in system information, i.e. changes of XXX should neither result in system information change notifications nor in a modification of valueTag in SIB1. | XXX should be replaced by EphemerisInfo. | xun.tang@intel.com |  |
| 142 | | N | ***ta-Common***  TACommon is a network-controlled common timing advanced value and it may include any timing offset considered necessary by the network. TACommon with value of 0 is supported. The granularity of TACommon is 4.07 × 10^(-3) μs. Values are given in unit of corresponding granularity. This field is excluded when determining changes in system information, i.e. changes of XXX should neither result in system information change notifications nor in a modification of valueTag in SIB1.” | XXX should be replaced by ta-Common | xun.tang@intel.com |  |
| 143 | | N | ***taCommonDrift***  Indicate drift rate of the common TA. The granularity of TACommonDrift is 0.2 × 10^(-3) μs⁄s Values are given in unit of corresponding granularity. *This field is excluded when determining changes in system information, i.e. changes of XXX should neither result in system information change notifications nor in a modification of valueTag in SIB1.* | XXX should be replaced by taCommonDrift. And the last sentence should not be in italics. | xun.tang@intel.com |  |
| 144 | | N | ***taCommonDriftVariant***  Indicate drift rate variation of the common TA. The granularity of TACommonDriftVariation is 0.2×10^(-4) μs⁄s^2. Values are given in unit of corresponding granularity. *This field is excluded when determining changes in system information, i.e. changes of XXX should neither result in system information change notifications nor in a modification of valueTag in SIB1.* | XXX should be replaced by taCommonDriftVariant. And the last sentence should not be in italics. | xun.tang@intel.com |  |
| 145 | | N | ***referenceLocation1, referenceLocation2***  Reference locations used for location based event. The *referenceLocation1* is associated to serving cell and *referenceLocation2* is associated to candidate target cell. The value of the field is same as *Ellipsoid-Point* defined in TS37.355. The first/leftmost bit of the first octet contains the most significant bit. | spec reference is missing, should be “TS 37.355 [49]” | xun.tang@intel.com |  |
| 146 | | N | maxTAC-r17 INTEGER ::= 12 -- Maximum number of Tracking Area Codes to which a cell belongs to | The last “to” is redundant | xun.tang@intel.com |  |
| 147 | | Y | Many IEs with TCI state is missing ‘-‘ between TCI and State. E.g, ul-TCIState, ul-TCIState-ToAddModList-r17, UL-TCIState-r17,ul-TCIState-ToReleaseList-r17, r17 RefUnifiedTCIStateList-r17, followUnifiedTCIstate-r17, etc. | add ‘-‘ between TCI and State | Youn.hyoung.heo@intel.com |  |
| 148 | | N | BFD set | Change to BFD-RS set | Youn.hyoung.heo@intel.com |  |
| 149 | | N | simultaneousU-TCI-UpdateListn  List of serving cells which can be updated simultaneously for TCI relation with a MAC CE. The different lists shall not contain same serving cells. Network should configure in these lists only serving cells that are configured with unifiedtci-StateType | TCI relation should be corrected with TCI state update | Youn.hyoung.heo@intel.com |  |
| 150 | | N | ***SearchSpaceLinkingId***  This parameter is used to link two search spaces of same type. If two search spaces have the same SearchSpaceLinkingId UE assumes these search spaces are linked to PDCCH repetition REF. | No need “REF” | Youn.hyoung.heo@intel.com |  |
| 151 | | N | 5.8.9.6.1 General   **Figure 5.8.9.6.1-1: UE assistance Information Sidelink** | 1. ‘UE’ is not clear. The resolution is not high. 2. The line(<-) in the figure is red.   UE assistance Information Sidelink-> UE assistance information Sidelink | wulh5@lenovo.com |  |
| 152 | | N | UE-TxTEG-RequestUL-TDOA-Config-r17 ::= CHOICE {  oneShot-r17 NULL,  periodicReporting-r17 ENUMERATED {ms120, ms240, ms480, ms640, ms1024, ms2048, ms5120, ms10240}  }  ***ue-TxTEG\_Request-UL-TDOA-Config***  Configures the periodicty of UE reporting for the association between Tx TEG and SRS Positioning resources. When configured with *oneShot* UE reports the association only one time. When configured with *periodicReporting* value ms120 means the UE reports every 120ms, ms240 means UE reports every 240ms and so on. | The wording of ‘ue-TxTEG\_Request-UL-TDOA-Config’ is aligned with ‘UE-TxTEG-RequestUL-TDOA-Config-r17’. Should be ‘ue-TxTEG-RequestUL-TDOA-Config’ | wulh5@lenovo.com |  |
| 153 | | N | 6.3.5 Sidelink information elements …….  …… *SL-MeasResultsRelay* The IE *SL-MeasResultsSLRelay* covers measured results of L2 U2N Relay UEs.  *SL-MeasResultsRelay* information element  -- ASN1START  -- TAG-SL-MEASRESULTSRELAY-START | *SL-MeasResultsSLRelay* should be modified to SL-MeasResultsRelay | wulh5@lenovo.com |  |
| 154 | | N | 2> for each entry in the *interFreqCarrierFreqList*:  3> if the UE is not a RedCap UE or if *redcapAccessReject* is absent: | Should be updated to “redcapAccessRejected” to align with the IE name in ASN.1. | liu.jing30@zte.com.cn |  |
| 155 | | Y | RRCReconfiguration-v1700-IEs ::= SEQUENCE {  otherConfig-v1700 OtherConfig-v1700 OPTIONAL, -- Need M  ul-GapFR2-Config-r17 SetupRelease { UL-GapFR2-Config-r17 } OPTIONAL, -- Need M  sl-L2RelayUEConfig-r17 SetupRelease { SL-L2RelayUEConfig-r17 } OPTIONAL, -- Cond L2RelayUE  sl-L2RemoteUEConfig-r17 SetupRelease { SL-L2RemoteUEConfig-r17 } OPTIONAL, -- Cond L2RemoteUE  dedicatedPagingDelivery-r17 OCTET STRING (CONTAINING Paging) OPTIONAL, -- L2U2NRelay  needForNCSG-ConfigNR-r17 SetupRelease {NeedForNCSG-ConfigNR-r17} OPTIONAL, -- Need M  needForNCSG-ConfigEUTRA-r17 SetupRelease {NeedForNCSG-ConfigEUTRA-r17} OPTIONAL, -- Need M  musim-GapConfig-r17 SetupRelease {MUSIM-GapConfig-r17} OPTIONAL, -- Need M  scg-State-r17 ENUMERATED { deactivated } OPTIONAL, -- Need S  appLayerMeasConfig-r17 AppLayerMeasConfig-r17 OPTIONAL, -- Need M  nonCriticalExtension SEQUENCE {} OPTIONAL  } | NCSG, UL FR2 gap, MUSIM gap are all “gap” related features, so suggest to put those IEs together.  RRCReconfiguration-v1700-IEs ::= SEQUENCE {  otherConfig-v1700 OtherConfig-v1700 OPTIONAL, -- Need M  ~~ul-GapFR2-Config-r17 SetupRelease { UL-GapFR2-Config-r17 } OPTIONAL, -- Need M~~  sl-L2RelayUEConfig-r17 SetupRelease { SL-L2RelayUEConfig-r17 } OPTIONAL, -- Cond L2RelayUE  sl-L2RemoteUEConfig-r17 SetupRelease { SL-L2RemoteUEConfig-r17 } OPTIONAL, -- Cond L2RemoteUE  dedicatedPagingDelivery-r17 OCTET STRING (CONTAINING Paging) OPTIONAL, -- L2U2NRelay  needForNCSG-ConfigNR-r17 SetupRelease {NeedForNCSG-ConfigNR-r17} OPTIONAL, -- Need M  needForNCSG-ConfigEUTRA-r17 SetupRelease {NeedForNCSG-ConfigEUTRA-r17} OPTIONAL, -- Need M  musim-GapConfig-r17 SetupRelease {MUSIM-GapConfig-r17} OPTIONAL, -- Need M  ul-GapFR2-Config-r17 SetupRelease { UL-GapFR2-Config-r17 } OPTIONAL, -- Need M  scg-State-r17 ENUMERATED { deactivated } OPTIONAL, -- Need S  appLayerMeasConfig-r17 AppLayerMeasConfig-r17 OPTIONAL, -- Need M  nonCriticalExtension SEQUENCE {} OPTIONAL  } | liu.jing30@zte.com.cn |  |
| 156 | | N | 5.3.5.15 FR2 UL gap configuration The UE shall:  1> if ul-GapFR2-Config is set to setup:  2> if an FR2 UL gap configuration is already setup, release the FR2 UL gap configuration;  2> setup the FR2 UL gap configuration indicated by the ul-GapFR2-Config in accordance with the received gapOffset, i.e., the first subframe of each gap occurs at an SFN and subframe meeting the following condition:  SFN mod T = FLOOR (gapOffse/10);  if the UGRP is larger than 5ms:  subframe = gapOffset mod 10;  else:  subframe = gapOffset or (gapOffset +5);  with T = CEIL(UGRP/10).  1> else if ul-GapFR2-Config is set to release:  2> release the FR2 UL gap configuration. | gapOffse => gapOffset  ul-GapFR2-Config and gapOffset in section 5.3.5.15 should be *italic*. | liu.jing30@zte.com.cn |  |
| 157 | | N | Section 6.2.2:  ***srs-TimeAlignmnetTimer***  TA timer for SRS for positioning transmission during RRC\_INACTIVE State.  Editor’s Note: Range to be taken from SDT | 1. Typo of ‘alignment’ of ‘*srs-TimeAlignmnetTimer*’.  2. The value range of *srs-TimeAlignmnetTimer* is already aligned with SDT. So the editor note in the field description should be deleted. | pan.yu24@zte.com.cn |  |
| 158 | | N | ***ue-TxTEG\_Request-UL-TDOA-Config***  Configures the periodicty of UE reporting for the association between Tx TEG and SRS Positioning resources. When configured with *oneShot* UE reports the association only one time. When configured with *periodicReporting* value ms120 means the UE reports every 120ms, ms240 means UE reports every 240ms and so on. | Typo, change ‘periodicty’ to ‘periodicity’. | pan.yu24@zte.com.cn |  |
| 159 | | N | ***srs-PosRRCInactiveConfig***  SRS for positioning confifuration during RRC\_INACTIVE State. | Typo, change confifuration to configuration. | pan.yu24@zte.com.cn |  |
| 160 | | N | ***AssociatedSRS-PosResourceId***  The ID of SRS Positioning Resource (*SRS-PosResource*) which is associted to a specific UE Tx TEG.  ***AssociatedSRS-PosResourceSetID***  The ID of SRS Positioning Resource Set (*SRS-PosResourceSet*) which is associted to a specific UE Tx TEG. | Typo, change associted to associated. | pan.yu24@zte.com.cn |  |
| 161 | | Y | Section 6.2.2 (RRCRelease message)  allowedCG-List-r16 SEQUENCE (SIZE (0.. maxNrofConfiguredGrantConfigMAC-1-r16)) OF ConfiguredGrantConfigIndexMAC-r16 OPTIONAL -- Need R | Change the suffix to -r17 | eswar.vutukuri@zte.com.cn |  |
| 162 | | Y | Place 1:  QCL-Info ::= SEQUENCE {  cell ServCellIndex OPTIONAL, -- Need R  bwp-Id BWP-Id OPTIONAL, -- Cond CSI-RS-Indicated  referenceSignal CHOICE {  csi-rs NZP-CSI-RS-ResourceId,  ssb SSB-Index  },  qcl-Type ENUMERATED {typeA, typeB, typeC, typeD},  ...,  [[  additionalPCI-r17 AdditionalPCIIndex-r17 OPTIONAL -- Need R  Place 2:  UL-TCIState-r17 ::= SEQUENCE {  ul-TCIState-Id-r17 UL-TCIState-Id-r17,  servingCellId-r17 ServCellIndex OPTIONAL, -- Need S  referenceSignal-r17 CHOICE {  ssb-Index-r17 SSB-Index,  csi-RS-Index-r17 NZP-CSI-RS-ResourceId,  srs-r17 PUCCH-SRS  },  additionalPCI-r17 AdditionalPCIIndex-r17 OPTIONAL, -- Need R  ul-powerControl-r17 Uplink-powerControlId-r17 OPTIONAL, -- Need R  pathlossReferenceRS-Id-r17 PUSCH-PathlossReferenceRS-Id OPTIONAL -- Need S  -- Editor’s Note: Check if new id -r17 is needed to cover full ID range  } | The parameter name of additioalPCI-r17 have been used in a lot of other places, but all other parameters are assigned with PhysCellId only this parameter is in TCI-State assigned with AdditionalPCIIndex-r17.  We suggest to change the parameter name of additionalPCI-r17 to additionalPCIIndex-r17. | dong.fei@zte.com.cn |  |
| 163 | | N | ***sp-CSI-MultiplexingMode***  Indicates if the behavior of transmitting SP-CSI on the first PUSCH repetitions coresponding to two SRS resource sets is enabled or not. | Typo, change the ‘coresponding’ to corresponding | dong.fei@zte.com.cn |  |
| 164 | | N | **nrofReportedGroups**  Presence if this field indicates that groupBasedBeamReportingR17 is enabled and the value configures the number of reported beam groups per CSI-report. | if -> of | dong.fei@zte.com.cn |  |
| 165 | | Y | In **PhysicalCellGroupConfig**, the **MulticastConfig-r17** field descriptions table includes g-CS-RNTI-ConfigToAddModList and g-CS-RNTI-ConfigToReleaseList, that do actually not exist in MulticastConfig-r17 | In PhysicalCellGroupConfig, remove g-CS-RNTI-ConfigToAddModList and g-CS-RNTI-ConfigToReleaseList from the MulticastConfig-r17 field descriptions table | david.lecompte@hhuawei.com |  |
| 166 | | Y | In **PhysicalCellGroupConfig**, there is a **G-CS-RNTI-Config field descriptions table** but there is no G-CS-RNTI-Config defined there (it was replaced with Group-Config which is defined in MAC-CellGroupConfig and for which there is a table) | In PhysicalCellGroupConfig, remove the G-CS-RNTI-Config field descriptions table | david.lecompte@hhuawei.com |  |
| 167 | | Y | In **RadioBearerConfig**, in MRB-ToAddMod-r17, there is NEED N (with capitals) for two fields | Change to "Need N" (instead of "NEED N") | david.lecompte@hhuawei.com |  |
| 168 | | Y | In **MBS-SessionInfoList**, there is NEED N (with capitals) for 7 fields | Change to "Need N" (instead of "NEED N") | david.lecompte@hhuawei.com |  |
| 169 | | Y | In **MBS-SessionInfoList**,:  1) the MBS-SessionInfoList field descriptions table is actually a field descriptions table of MBS-SessionInfo (without "List")  2) it includes "headerCompression", "pdcp-SN-SizeDL" and "t-Reordering" that are actually fields of MRB-PDCP-ConfigBroadcast  3) it includes "sn-FieldLength" and "t-Reassembly" that are actually fields of MRB-RLC-ConfigBroadcast | 1) Change table title to "MBS-SessionInfo" (remove "List")  2) Create a field description table of MRB-PDCP-ConfigBroadcast and move the descriptions of "headerCompression", "pdcp-SN-SizeDL" and "t-Reordering" there  3) Create a field description table of MRB-RLC-ConfigBroadcast and move the descriptions of "sn-FieldLength" and "t-Reassembly" there | david.lecompte@hhuawei.com |  |
| 170 | | Y | NotificationMessageSidelink-r17-IEs ::= SEQUENCE {  indicationType-r17 ENUMERATED {  relayUE-UuRLF-r17, relayUE-HO-r17, relayUE-CellReselection-r17,  relayUE-UuRRCFailure-r17  } OPTIONAL,  lateNonCriticalExtension OCTET STRING OPTIONAL,  nonCriticalExtension SEQUENCE {} OPTIONAL  } | Missing hyphens, should be:  relayUE-Uu-RLF-r17  relayUE-Uu-RRC-Failure-r17 | nathan.tenny@mediatek.com |  |
| 171 | | Y | Uu-Relay-RLC-ChannelConfig-r17::= SEQUENCE {  uu-LogicalChannelIdentity-r17 LogicalChannelIdentity OPTIONAL, -- Cond LCH-SetupOnly  uu-Relay-RLC-ChannelID-r17 Uu-Relay-RLC-ChannelID-r17,  reestablishRLC-r17 ENUMERATED {true} OPTIONAL, -- Need N  rlc-Config-r17 RLC-Config OPTIONAL, -- Cond LCH-Setup  mac-LogicalChannelConfig-r17 LogicalChannelConfig OPTIONAL, -- Cond LCH-Setup  ...  } | Spurious hyphens, should be:  Uu-RelayRLC-ChannelConfig-r17  uu-RelayRLC-ChannelConfig-r17 | nathan.tenny@mediatek.com |  |
| 172 | | Y | UE-TimersAndConstants-RemoteUE-r17 ::= SEQUENCE {  t300-RemoteUE-r17 ENUMERATED {ms100, ms200, ms300, ms400, ms600, ms1000, ms1500, ms2000} OPTIONAL, -- Need S  t301-RemoteUE-r17 ENUMERATED {ms100, ms200, ms300, ms400, ms600, ms1000, ms1500, ms2000} OPTIONAL, -- Need S  t319-RemoteUE-r17 ENUMERATED {ms100, ms200, ms300, ms400, ms600, ms1000, ms1500, ms2000} OPTIONAL, -- Need S  ...  } | Spurious hyphen, should be:  UE-TimersAndConstantsRemoteUE-r17  (This also occurs in the field name where the IE is used in SIB1.) | nathan.tenny@mediatek.com |  |
| 173 | | Y | SL-TxResourceReq-v1700 ::= SEQUENCE {  sl-DRX-InfoFromRx-List-r17 SEQUENCE (SIZE (1..maxNrofSL-Rx-InfoSet-r17)) OF SL-DRX-ConfigUC-SemiStatic-r17 OPTIONAL  } | Spurious hyphens, should be:  sl-DRX-InfoFromRxList-r17  maxNrofSL-RxInfoSet-r17  (Historically we have not treated Tx and Rx as acronyms.) | nathan.tenny@mediatek.com |  |
| 174 | | Y | UEAssistanceInformationSidelink-r17-IEs ::= SEQUENCE {  sl-PreferredDRXConfig-r17 SL-PreferredDRXConfig-r17 OPTIONAL,  lateNonCriticalExtension OCTET STRING OPTIONAL,  nonCriticalExtension SEQUENCE {} OPTIONAL  }  SL-PreferredDRXConfig-r17 ::= SEQUENCE {  sl-PreferredDRX-onDurationTimer-r17 ENUMERATED {ffs},  sl-PreferredDRX-Cycle-r17 ENUMERATED {ffs},  sl-PreferredDRX-StartOffset-r17 ENUMERATED {ffs}  } | Missing hyphens, should be:  sl-PreferredDRX-Config-r17  SL-PreferredDRX-Config-r17 | nathan.tenny@mediatek.com |  |
| 175 | | N | Section 5.8.3.3  3> if *SIB12* including *sl-NonRelayDiscovery* and if configured by upper layers to transmit NR sidelink non-relay discovery announcements, or if *SIB12* including *sl-L2U2N-Relay* and if configured by upper layers to transmit NR sidelink L2 U2N relay discovery announcements, or if *SIB12* including *sl-L3U2N-RelayDiscovery* and if configured by upper layers to transmit NR sidelink L3 U2N relay discovery announcements:  4> include *sl-TxResourceReqListDis* and set its fields (if needed) as follows for each destination for which it requests network to assign NR sidelink discovery announcements resource:  5> set *sl-DestinationIdentityDisc* to the destination identity configured by upper layer for NR sidelink discovery announcements transmission;  5> if the UE is acting as L2 U2N Relay UE | Missing colon after “if the UE is acting as L2 U2N Relay UE” | nathan.tenny@mediatek.com |  |
| 176 | | N | Section 5.8.3.3  2> if *SIB12* including *sl-ConfigCommonNR* is provided by the PCell:  3> if configured by upper layers to receive NR sidelink communication:  4> include *sl-RxInterestedFreqList* and set it to the frequency for NR sidelink communication reception;  4> include *sl-RxDRX-ReportList* and set its fields (if needed) as follows for each destination for which it reports to network:  5> if *sl-DRX-ConfigCommon-GC-BC* is included in SIB12-IEs: | Missing italics on “SIB12-IEs” | nathan.tenny@mediatek.com |  |
| 177 | | N | Section 5.8.9.7.2  5.8.9.7.2 PC5 Relay RLC channel addition/modification  Upon PC5-RRC connection is established between the L2 U2N Relay UE and L2 U2N Relay UE, the L2 U2N Relay UE shall: | Grammar, should be either “When a PC5-RRC connection is established” or “Upon PC5-RRC connection establishment” | nathan.tenny@mediatek.com |  |
| 178 | | N | Section 5.8.9.7.2  1> else (a PC5 Relay RLC channel with the received *sl-RLC-ChannelID-PC5* was not configured before):  2> establish an sidelink RLC entity in accordance with the received *sl-RLC-ConfigPC5*; | Typo, “an sidelink” should be “a sidelink” | nathan.tenny@mediatek.com |  |
| 179 | | N | Section 5.8.9.8.3: 5.8.9.8.3 Reception of *RemoteUEInformationSidelink* message by the L2 U2N Relay UE The L2 U2N Relay UE shall:  1> if the *RemoteUEInformationSidelink* includes the *sl-PagingInfo-RemoteUE*:  2> if the UE is in RRC\_CONNECTED on an active BWP with common search space configured including *pagingSearchSpace*; or  2> if the UE is in RRC\_IDLE or RRC\_INACITIVE: | Typo, should be RRC\_INACTIVE | nathan.tenny@mediatek.com |  |
| 180 | | N | Section 5.8.15.3  NOTE 1: U2N Remote UE uses SL-RSRP measurements for relay reselection trigger evaluation when there is data transmission from U2N Relay UE to U2N Remote UE, and it is left to UE implementation whether to use SL-RSRP or SD-RSRP for relay reselection trigger evaluation in case of no data transmission from U2N Relay UE to U2N Remote UE. If SD-RSRP is used, the discovery procedure will be preformed between the U2N Remote UE and the selected U2N Relay UE. | Typo, “preformed” should be “performed” | nathan.tenny@mediatek.com |  |
| 181 | | N | RRCReconfiguration   |  |  | | --- | --- | | *L2RelayUE* | For L2 U2N Relay UE, the field is optionally present, Need M. Otherwise, it is absent. | | *L2RemoteUE* | The field is optional present for L2 U2N Remote UE, need M; otherwise it is absent. | | *L2U2NRelay* | For L2 U2N Relay UE, the field is optionally present, Need N. Otherwise, it is absent. | | Wording of the L2RemoteUE condition does not match the other conditions. Should be:  “For L2 U2N Remote UE, the field is optionally present, Need M. Otherwise, it is absent.” | nathan.tenny@mediatek.com |  |
| 182 | | N | RRCRelease  ***sl-ServingCellInfo***  Indicates the Uu serving Cell related related information. | Spurious capital, “Cell” should be “cell” | nathan.tenny@mediatek.com |  |
| 183 | | Y | SL-TxResourceReqDisc-r17 ::= SEQUENCE {  sl-DestinationIdentityDisc-r17 SL-DestinationIdentity-r16,  sl-SourceIdentity-RelayUE-r17 SL-SourceIdentity-r17 OPTIONAL,  sl-CastTypeDisc-r17 ENUMERATED {broadcast, groupcast, unicast, spare1},  sl-TxInterestedFreqListDisc-r17 SL-TxInterestedFreqList-r16,  sl-TypeTxSyncListDis-r17 SEQUENCE (SIZE (1..maxNrofFreqSL-r16)) OF SL-TypeTxSync-r16,  sl-DiscoveryType-r17 ENUMERATED {relay, non-Relay},  ...  } | Typo, “sl-TypeTxSyncListDis-r17” should be “sl-TypeTxSyncListDisc-r17” | nathan.tenny@mediatek.com |  |
| 184 | | N | Section 7.1.1, Txxx start condition  Upon reception of the *RRC reconfiguration* message indicating direct-to-indirect path switch | Typo, *RRC reconfiguration* should be *RRCReconfiguration* | nathan.tenny@mediatek.com |  |
| 185 | | N | Section 7.1.1, Txxx stop condition  Upon successfully sending *RRCReconfigurationComplete* message (i.e., PC5 RLC acknowledge is received from target L2 U2N Relay UE) | Typo, “acknowledge” should be “acknowledgement” | nathan.tenny@mediatek.com |  |
| 186 | | Y | SL-ReselectionConfig-r17::= SEQUENCE {  sl-RSRP-Thresh-r17 SL-RSRP-Range-r16 OPTIONAL, -- Need R  sl-FilterCoefficient-RSRP-r17 FilterCoefficient OPTIONAL, -- Need R  sl-HystMin-r17 Hysteresis OPTIONAL -- Need R  } | Spurious hyphen, should be sl-FilterCoefficientRSRP-r17 | nathan.tenny@mediatek.com |  |
| 187 | | Y | MeasGapConfig ::= SEQUENCE {  gapFR2 SetupRelease { GapConfig } OPTIONAL, -- Need M  ...,  [[  gapFR1 SetupRelease { GapConfig } OPTIONAL, -- Need M  gapUE SetupRelease { GapConfig } OPTIONAL -- Need M  ]],  [[  gapUEToAddModList-r17 SEQUENCE (SIZE (1..maxNrofGapId-1-r17)) OF GapConfig OPTIONAL, -- Need N  gapUEToReleaseList-r17 SEQUENCE (SIZE (1..maxNrofGapId-1-r17)) OF MeasGapId-r17 OPTIONAL, -- Need N  gapFR1ToAddModList-r17 SEQUENCE (SIZE (1..maxNrofGapId-1-r17)) OF GapConfig OPTIONAL, -- Need N  gapFR1ToReleaseList-r17 SEQUENCE (SIZE (1..maxNrofGapId-1-r17)) OF MeasGapId-r17 OPTIONAL, -- Need N  gapFR2ToAddModList-r17 SEQUENCE (SIZE (1..maxNrofGapId-1-r17)) OF GapConfig OPTIONAL, -- Need N  gapFR2ToReleaseList-r17 SEQUENCE (SIZE (1..maxNrofGapId-1-r17)) OF MeasGapId-r17 OPTIONAL -- Need N  ]]  } | Missing hyphens, should be:  gapUE-ToAddModList-r17  gapUE-ToReleaseList-r17  gapFR1-ToAddModList-r17  gapFR1-ToReleaseList-r17  gapFR2-ToAddModList-r17  gapFR2-ToReleaseList-r17  (Note: Historically we have treated FR1 and FR2 as acronyms) | nathan.tenny@mediatek.com |  |
| 188 | | Y | LogicalChannelConfig ::= SEQUENCE {  [some text snipped here for brevity]  [[  logicalChannelGroup-IAB-Ext-r17 INTEGER (8..maxLCG-ID-IAB-r17) OPTIONAL, -- Need R  allowedHARQ-mode ENUMERATED {harqModeA, harqModeB} OPTIONAL -- Need S  ]]  } OPTIONAL, -- Cond UL  ...,  [[  channelAccessPriority-r16 INTEGER (1..4) OPTIONAL, -- Need R  bitRateMultiplier-r16 ENUMERATED {x40, x70, x100, x200} OPTIONAL -- Need R  ]]  } | Spurious hyphen, should be logicalChannelGroupIAB-Ext-r17  Missing hyphens, should be harq-ModeA and harq-ModeB | nathan.tenny@mediatek.com |  |
| 189 | | Y | SRS-Resource ::= SEQUENCE {  [Text snipped for brevity]  [[  spatialRelationInfo-PDC-r17 SetupRelease { SpatialRelationInfo-PDC-r17 } OPTIONAL, -- Need M  resourceMapping-r17 SEQUENCE {  nrofSymbols-r17 ENUMERATED {n8, n10, n12, n14},  repetitionFactor-r17 ENUMERATED {n1, n2, n4, n5, n6, n7, n8, n10, n12, n14}  },  partialFreqSounding-r17 SEQUENCE {  startRBIndexFScaling-r17 CHOICE{  startRBIndexAndFreqScalingFactor2-r17 INTEGER (0..1),  startRBIndexAndFreqScalingFactor4-r17 INTEGER (0..3)  },  enableStartRBHopping-r17 ENUMERATED {enable} OPTIONAL -- Need R  } OPTIONAL, -- Need R  transmissionComb-n8-r17 SEQUENCE {  startPosition-r17 INTEGER (0..13),  combOffset-n8-r17 INTEGER (0..7),  cyclicShift-n8-r17 INTEGER (0..5)  } OPTIONAL -- Need R  ]]  } | Spurious hyphen, should be SpatialRelationInfoPDC-r17  Missing hyphens, should be:  startRB-IndexF-Scaling-r17  startRB-IndexAndFreqScalingFactor2-r17  startRB-IndexAndFreqScalingFactor4-r17  enableStartRB-Hopping-r17 | nathan.tenny@mediatek.com |  |
| 190 | | Y | SSB-MTC-AdditionalPCI-r17 ::= SEQUENCE {  additionalPCIIndex-r17 AdditionalPCIIndex-r17,  additionalPCI-r17 PhysCellId,  periodicity-r17 ENUMERATED { ms5, ms10, ms20, ms40, ms80, ms160, spare2, spare1 } OPTIONAL, -- Need S  ssb-PositionsInBurst-r17 CHOICE {  shortBitmap BIT STRING (SIZE (4)),  mediumBitmap BIT STRING (SIZE (8)),  longBitmap BIT STRING (SIZE (64))  },  ss-PBCH-BlockPower-r17 INTEGER (-60..50)  }  --Editor’s note: more RAN1 input may be coming for this IE  AdditionalPCIIndex-r17 ::= INTEGER(0..maxNrofAdditionalPCI-1-r17) | Missing hyphens, should be additionalPCI-Index-r17 and AdditionalPCI-Index-r17 | nathan.tenny@mediatek.com |  |
| 191 | | Y | UL-TCIState-r17 ::= SEQUENCE {  ul-TCIState-Id-r17 UL-TCIState-Id-r17,  servingCellId-r17 ServCellIndex OPTIONAL, -- Need S  referenceSignal-r17 CHOICE {  ssb-Index-r17 SSB-Index,  csi-RS-Index-r17 NZP-CSI-RS-ResourceId,  srs-r17 PUCCH-SRS  },  additionalPCI-r17 AdditionalPCIIndex-r17 OPTIONAL, -- Need R  ul-powerControl-r17 Uplink-powerControlId-r17 OPTIONAL, -- Need R  pathlossReferenceRS-Id-r17 PUSCH-PathlossReferenceRS-Id OPTIONAL -- Need S  -- Editor’s Note: Check if new id -r17 is needed to cover full ID range  } | Wrong hyphenation, should be:  UL-TCI-State-r17  ul-TCI-StateId-r17 | nathan.tenny@mediatek.com |  |
| 192 | | Y | UL-ExcessDelayConfig-r17 ::= SEQUENCE {  excessDelay-DRBlist-r17 SEQUENCE (SIZE(1..maxDRB)) OF ExcessDelay-DRB-IdentityInfo-r17  }  ExcessDelay-DRB-IdentityInfo-r17 ::= SEQUENCE {  drb-IdentityList SEQUENCE (SIZE (1..maxDRB)) OF DRB-Identity,  delayThreshold ENUMERATED {ms0dot25, ms0dot5, ms1, ms2, ms4, ms5, ms10, ms20, ms30, ms40, ms50, ms60, ms70,  ms80, ms90, ms100, ms150, ms300, ms500}  } | Wrong hyphenation and capitalisation, should be:  excessDelayDRB-List-r17  ExcessDelayDRB-IdentityInfo-r17 | nathan.tenny@mediatek.com |  |
| 193 | | Y | UL-GapFR2-Config-r17 ::= SEQUENCE {  gapOffset-r17 INTEGER (0..159),  ugl-r17 ENUMERATED {ms0dot125, ms0dot25, ms0dot5, ms1},  ugrp-r17 ENUMERATED {ms5, ms20, ms40, ms160},  refFR2ServCellAsyncCA-r17 ServCellIndex OPTIONAL –- Cond AsyncCA  } | Missing hyphen, should be refFR2-ServCellAsyncCA-r17 | nathan.tenny@mediatek.com |  |
| 194 | | Y | BeamFailureDetectionSet-r17 ::= SEQUENCE {  bfdRSSetId-r17 INTEGER (1..2) OPTIONAL, -- Need R  bfdResourcesToAddModList-r17 SEQUENCE (SIZE(1..maxNrofBFDResourcePerSet-r17)) OF RadioLinkMonitoringRS  OPTIONAL, -- Need N  bfdResourcesToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofBFDResourcePerSet-r17)) OF RadioLinkMonitoringRS-Id  OPTIONAL, -- Need N  beamFailureInstanceMaxCount-r17 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10} OPTIONAL, -- Need R  beamFailureDetectionTimer-r17 ENUMERATED {pbfd1, pbfd2, pbfd3, pbfd4, pbfd5, pbfd6, pbfd8, pbfd10} OPTIONAL, -- Need R  ...  --editor’s note: maxNrofBFDResourcePerSet-r17 is said in LS 64 but feature discussion might indicate just max 2 per set  } | Missing hyphens, should be:  bfd-RS-SetId-r17  bfd-ResourcesToAddModList-r17  bfd-ResourcesToReleaseList-r17  maxNrofBFD-ResourcePerSet-r17 | nathan.tenny@mediatek.com |  |
| 195 | | Y | Section 6.4  max-DLorJointTCI-r17 INTEGER ::= ffsUpperLimit -- Size is FFS | Wrong hyphenation, should be maxDL-OrJointTCI-r17 | nathan.tenny@mediatek.com |  |
| 196 | | Y | Section 6.4  maxUu-Relay-RLC-ChannelID-r17 INTEGER ::= 32 -- Maximum value of Uu Relay RLC channel ID | Spurious hyphen, should be maxUu-RelayRLC-ChannelID-r17 | nathan.tenny@mediatek.com |  |
| 197 | | Y | Section 6.4  maxNrofRbSetGroups-r17 INTEGER ::= 8 -- Maximum number of RB set groups  maxNrofRbSets-r17 INTEGER ::= 8 -- Maximum number of RB sets | Missing hyphens and wrong capitalisation, should be:  maxNrofRB-SetGroups-r17  maxNrofRB-Sets-r17 | nathan.tenny@mediatek.com |  |
| 198 | | Y | Section 6.4  maxCEFReport-r17 INTEGER ::= 4 -- Maximum number of CEF reports by the UE | Missing hyphen, should be maxCEF-Report-r17 | nathan.tenny@mediatek.com |  |
| 199 | | Y | Section 6.4  maxNeighCell-MBS-r17 INTEGER ::= 8 -- Maximum number of MBS broadcast neighbour cells | Spurious hyphen, should be maxNeighCellMBS-r17 | nathan.tenny@mediatek.com |  |
| 200 | | Y | UEAssistanceInformation-v1700-IEs ::= SEQUENCE {  ul-GapFR2-Preference-r17 UL-GapFR2-Preference-r17 OPTIONAL,  musim-Assistance-r17 MUSIM-Assistance-r17 OPTIONAL,  overheatingAssistance-r17 OverheatingAssistance-r17 OPTIONAL,  maxBW-PreferenceFR2-2-r17 MaxBW-PreferenceFR2-2-r17 OPTIONAL,  maxMIMO-LayerPreferenceFR2-2-r17 MaxMIMO-LayerPreferenceFR2-2-r17 OPTIONAL,  minSchedulingOffsetPreferenceExt-r17 MinSchedulingOffsetPreferenceExt-r17 OPTIONAL,  rlm-MeasRelaxationState-r17 BOOLEAN OPTIONAL,  bfd-MeasRelaxationState-r17 BIT STRING (SIZE (32)) OPTIONAL,  nonSDT-DataIndication-r17 SEQUENCE {  resumeCause-r17 ResumeCause OPTIONAL  } OPTIONAL,  scg-DeactivationPreference ENUMERATED { scgDeactivationPreferred, noPreferrence } OPTIONAL,  uplinkData-r17 ENUMERATED { true } OPTIONAL,  rrm-MeasRelaxationFulfilment-r17 BOOLEAN OPTIONAL,  nonCriticalExtension SEQUENCE {} OPTIONAL  } | Missing hyphen, should be scg-DeactivationPreferred (and the other codepoint should be scg-DeactivationNotPreferred—cf. item 37) | nathan.tenny@mediatek.com |  |
| 201 | |  | In 5.7.2.2.:  When F1-C related information has to be transferred, the IAB-MT shall initiate the procedure only if SBR2 or split SRB2 is established. | SBR2 🡪 SRB2 | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
| 202 | |  | The IE *DedicatedInfoF1c* is used to transfer IAB-DU specific F1-C related information between the network and the IAB node. The carried information consists of F1AP message encapsulated in SCTP/IP or F1-C related (SCTP)/IP packet, see TS 38.472 [X]. The RRC layer is transparent for this information. | IAB is also network part,, thus, “network” : 🡪”IAB donor-CU” | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
| 203 | |  | 0：  1> for the IAB-MT, if there is a need to transfer F1-C related information:  2>include the *dedicatedInfoF1c*; | We think the procedure is not finished, should add “to include F1-C related information;” as:  1> for the IAB-MT, if there is a need to transfer F1-C related information:  2>include the *dedicatedInfoF1c* to include F1-C related information | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
| 204 | | N | 5.3.10.4 RLF cause determination *(skipped)*  1> else if the UE declares radio link failure due to consistent uplink LBT failures:  2> set the *rlf-Cause* as *lbtFailure*;  1> else if the IAB-MT declares radio link failure due to the reception of a BH RLF indication on BAP entity:  2> set the *rlf-Cause* as *bh-rlfRecoveryFailure*.  1> else if the UE declares radio link failure due to T312 expiry:  2> set the *rlf-Cause* as *t312-Expiry*; | Need to update “.” to “;”  Need to update “;” to “.” | sb07.kim@samsung.com |  |
|  | | 205 | NOTE 5: A UE capable of NR sidelink communication and configured by upper layers to perform NR sidelink communication on a frequency, may acquire *SIB12* or *SystemInformationBlockType28* from a cell other than current serving cell (for RRC\_INACTIVE or RRC\_IDLE) or current PCell (for RRC\_CONNECTED), if *SIB12* of current serving cell (for RRC\_INACTIVE or RRC\_IDLE) or current PCell (for RRC\_CONNECTED) does not provide configuration for NR sidelink communication for the frequency, and if the other cell providing configuration for NR sidelink communication for the frequency meets the S-criteria as defined in TS 38.304 [20] or TS 36.304 [27]. | NOTE 5 also applies to NR sidelink discovery. Thus,  Propose to replace “NR sidelink communication” by “NR sidelink communication/discovery” | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 206 | 1> if the UE is acting as a L2 U2N Relay UE, for each of the *PagingRecord*, if any, included in the *Paging* message:  2> if the *ue-Identity* included in the *PagingRecord* in the *Paging* message matches the UE identity in *sl-PagingIdentity-RemoteUE* included in *sl-PagingInfo-RemoteUE*:  3> inititate the Uu Message transfer in sidelink as specified in 5.8.9.9; | Duplicated description with the above level 1> sentence (i.e., included in the *Paging* message.  Propose to delete the wording “in the *Paging* message” in this level 2> sentence. | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 207 | NOTE 3: For L2 U2N Remote UE in RRC\_IDLE/INACTIVE, the cell (re)selection procedure as specified in TS 38.304 [20] and relay (re)selection procedure as specified in 5.8.15.3 are performed independently and up to UE implementation to select either a cell or a L2 U2N Relay UE. | RRC\_INACTIVE should not be mentioned here this subclause for RRC connection establishment procedure.  Propose to Remove “/INACTIVE” | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 208 | The L2 U2N Relay UE shall:  1> for each *Uu-Relay-RLC-ChannelID* value included in the *uu-Relay-RLC-ChannelToReleaseList* that is part of the current configuration within the same cell group (LCH release):  2> release the RLC entity as specified in TS 38.322 [4], clause 5.1.3;  2> release the corresponding logical channel. | Editoral correction.  *~~U~~uu-Relay-RLC-ChannelID* | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 209 | 1> if *sl-RLC-ChannelToReleaseList* is included in *sl-ConfigDedicatedNR* within *RRCReconfiguration*:  2> perform PC5 Relay RLC channel release as specified in 5.8.9.1.2; | Wrong citation number.  Propose to change “5.8.9.1.2” to “5.3.5.5.12” | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 210 | 1> if *sl-RLC-ChannelToAddModList* is included in *sl-ConfigDedicatedNR* within *RRCReconfiguration*:  2> perform PC5 Relay RLC channel addition/modification as specified in 5.8.9.1.2; | Wrong citation number  Propose to change “5.8.9.1.2” to “5.3.5.5.13” | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 211 | The network configures the L2 U2N Relay UE with relay operation related configurations. For each connected L2 U2N Remote UE indicated in *sl-L2Identity-Remote*, the network provides the configuration parameters used for data relaying. | Clarify that the L2 Remote UE’s Uu singaling relaying via L2 U2N Relay UE is also supported and configured.  Propose “the network provides the configuration parameters used for Uu signalling anddata relaying” | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 212 | The purpose of this procedure is to provide synchronisation information to a UE. This procedure also applies to sidelink discovery. | Editorial change.  Propose to add “NR” as ”NR sidelink | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 213 | The purpose of this procedure is to select a synchronisation reference and used when transmitting NR sidelink communication. This procedure also applies to sidelink discovery. | Editorial change.  Propose to add “NR” as ”NR sidelink | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 214 | ul-GapFR2-Config-r17 SetupRelease { UL-GapFR2-Config-r17 } OPTIONAL, -- Need M  sl-L2RelayUEConfig-r17 SetupRelease { SL-L2RelayUEConfig-r17 } OPTIONAL, -- Cond L2RelayUE  sl-L2RemoteUEConfig-r17 SetupRelease { SL-L2RemoteUEConfig-r17 } OPTIONAL, -- Cond L2RemoteUE  dedicatedPagingDelivery-r17 OCTET STRING (CONTAINING Paging) OPTIONAL, -- L2U2NRelay  needForNCSG-ConfigNR-r17 SetupRelease {NeedForNCSG-ConfigNR-r17} OPTIONAL, -- Need M | editorial change.  Cond L2U2NRelay | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 215 | ***sl-ServingCellInfo***  Indicates the Uu serving Cell related related information. | The word ”related” is repeated twice.  Delete one ”related”. | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 216 | ***uu-Relay-RLC-ChannelToAddModList***  Configuration of the Uu RLC entities and the corresponding MAC Logical Channels to be added and modified. | Editorial change:  Better replace by “List” | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 217 | ***uu-Relay-RLC-ChannelToAddModList***  Configuration of the Uu RLC entities and the corresponding MAC Logical Channels to be added and modified. | Editorial change:  Change to “or” | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 218 | ***UE-TimersAndConstants* field descriptions** | Editorial change:  Proposes “***UE-TimersAndConstants-RemoteUE”*** | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 219 | ***sl-PagingIdentity-RemoteUE***  Indicates the L2 U2N Remote UE’s paging UE ID. | Editorial change:  Proposes “paging UE ID(s)” | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
|  | | 220 | Parameters that are specified for NR sidelink discovery, which is used for the sidelink signalling radio bearer of NR sidelink U2N relay related discovery messages (e.g., Announcement message, Solicitation message and Response message, see TS 23.304 [65]). The SL-SRB using this SCCH configuration is named as SL-SRB4. | SL-SRB4 is used for both relay and non-relay discovery messages.  Propose the following change “sidelink ~~U2N relay related~~ discovery messages” | Boubacar <[kimba@vivo.com](mailto:kimba@vivo.com)> |  |
| N | | 221 | 1> if *sdt-MAC-PHY-CG-Config* is configured:  2> if the resume procedure is initiated in a cell that is different to the PCell in which the UE received the stored *sdt-MAC-PHY-CG-Config*:  3> release the stored *sdt-MAC-PHY-CG-Config*; | 1> if *sdt-MAC-PHY-CG-Config* is configured:  2> if the resume procedure is initiated in a cell that is different from the PCell in which the UE received the stored *sdt-MAC-PHY-CG-Config*:  3> release the stored *sdt-MAC-PHY-CG-Config*; | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| N | | 222 | 2> if resume is triggered by upper layers:  3> inform upper layers about the failure to resume the RRC connection;  2> if resume istriggered due to an RNA update; or:  2> if resume is triggered for SDT and T380 is not running: | Remove the : | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| Y | | 223 | cg-SDT-Config-LCH-restrictionToAddModList-r17 SEQUENCE (SIZE(1..maxLC-ID)) OF CG-SDT-Config-LCH-restriction OPTIONAL, -- Need N | There are too many hypens in some of the parameter/IE names, e.g. cg-SDT-Config-LCH-restrictionToAddModList, cg-SDT-Config-LCH-r17, BWP-Uplink-Dedicated-SDT, cg-SDT-Config-Initial-BWP-SUL. Remove the unnecessary hyphens following the ASN.1 naming conventions. | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| Y | | 224 | CG-SDT-Config-LCH-restriction ::= SEQUENCE {  logicalChannelIdentity LogicalChannelIdentity, | Add field description; Change allowedCG-List-r16 to allowedCG-List-r17; add "r17" to field names | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| Y | | 225 | ***sdt-DRB-ContinueROHC***  Indicates whether the PDCP entity for the radio bearers configured for SDT continues or resets the ROHC header compression protocol during PDCP re-establishment during SDT procedure, as specified in TS 38.323 [5]. Value *cell* indicates that ROHC header compression continues when the UE resumes for SDT in the same cell as the PCell when the RRCRelease message is received. Value *rna* indicates that ROHC header compression continues when the UE resumes for SDT in a cell belonging to the same RNA as the PCell when the RRCRelease message is received. If the field is absent PDCP entity for the radio bearers configured for SDT reset the ROHC header compression protocol during PDCP re-establishment during SDT procedure, as specified in TS 38.323 [5]. | Editorial corrections  [Proposed change] Change “when” to “where”:  Value *cell* indicates that ROHC header compression continues when the UE resumes for SDT in the same cell as the PCell when the RRCRelease message was~~is~~ received. Value *rna* indicates that ROHC header compression continues ~~when~~ where the UE resumes for SDT in a cell belonging to the same RNA as the PCell ~~when~~ where the RRCRelease message was~~is~~ received. If the field is absent PDCP entity for the radio bearers configured for SDT reset the ROHC header compression protocol during PDCP re-establishment ~~during~~ when SDT is initiated~~procedure~~, as specified in TS 38.323 [5]. | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| Y | | 226 | ***CG-SDT-TA-ValiditationConfig***  Configuration for the RSRP based TA validation. If this IE is not configured, then the UE does not perform RSRP based TA validation. | Editorial issues  [Proposed change] Change CG-SDT-TA-ValiditationConfig to cg-SDT-TA-ValidationConfig. Change “This IE” to “This field”. Also the names in ASN.1 should be changed (“validation”, not “validitation”) | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| Y | | 227 | ***nonSDT-DataIndication***  Informs the network about the arrival of data mapped to radio bearers not configured for SDT data during SDT. | Move the field description of nonSDT-DataIndication under the description for the fields of UEAssistanceInformation  Change “*nonSDT-Data-Indication “* to “*nonSDT-DataIndication”* | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| Y | | 228 | ***AssocaitedSRS-PosResourceId***  ***The ID of SRS Positioning Resource (SRS-PosResource) which is associted to a specific UE Tx TEG.***  ***AssociatedSRS-PosResourceSetID***  ***The ID of SRS Positioning Resource Set (SRS-PosResourceSet) which is associted to a specific UE Tx TEG.*** | First letter of the field name should be in lower case | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| N | | 229 | 3> if the *halfDuplexRedCapAllowed* is not present in the acquires *SIB1* and the UE supports only half-duplex FDD operation:  4> consider the cell as barred in accordance with TS 38.304 [20];  4> consider cell re-selection to other cells on the same frequency as the barred cell as specified in TS 38.304 [20]; | acquires ->acquired | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| Y | | 230 | relaxedMeasurement-r17 SEQUENCE {  stationaryMobilityEvaluation-r17. SEQUENCE {  s-SearchDeltaP-Stationary-r17. ENUMERATED {dB3, dB6, dB9, dB12, dB15, spare3, spare2, spare1},  t-SearchDeltaP-Stationary-r17. ENUMERATED {s5, s10, s20, s30, s60, s120, s180, s240, s300, spare7, spare6, spare5,  spare4, spare3, spare2, spare1}  }, | relaxedMeasurementRedCap-r17  The “.” after the new field should be removed. | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| Y | | 231 | ***nonCellDefiningSSB-r17***  If configured, the UE operating in this BWP uses this SSB for the purposes for which it would otherwise have used the cell-defining SSB of the serving cell (e.g. obtaining sync, measurements (FFS on measurements), RLM,...). Furthermore, other parts of the BWP configuration that refer to an SSB (e.g. the “SSB” configured in the QCL-Info IE; the “ssb-Index” configured in the RadioLinkMonitoringRS; CFRA-SSB-Resource; PRACH-ResourceDedicatedBFR) refer implicitily to this NCD-SSB.  The NCD-SSB has the same values for the properties (e.g., ssb-PositionsInBurst, PCI, ssb-periodicity, ssb-PBCH-BlockPower) of the corresponding CD-SSB apart from the values of the properties configured in the *NonCellDefiningSSB-r17* IE. | “r17” should be removed in field description.  the RedCap UE operating in this BWP uses this SSB  ss~~b~~-PBCH-BlockPower | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| Y | | 232 | The IE *NonCellDefiningSSB* is used to configure a non-cell-defining SSB to be used while the UE operates in a dedicated BWP. | “The IE *NonCellDefiningSSB* is used to configure a non-cell-defining SSB to be used while the RedCap UE operates in a dedicated BWP. | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| Y | | 233 | NonCellDefiningSSB-r17 ::= SEQUENCE {  absoluteFrequencySSB-r17 ARFCN-ValueNR,  ssb-Periodicity ENUMERATED { ms5, ms10, ms20, ms40, ms80, ms160, spare2, spare1 } OPTIONAL, -- Need S  -- FFS whether additional properties may differ from the CD-SSB, e.g. time offset. If so, add them here.  ...  } | “ssb-Periodicity-r17” | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| Y | | 234 | pucch-ResourceConfig-RedCap-r17 ENUMERATED{2,3,4,6,8,9,10,12} OPTIONAL -- Need R  ]]  } | Change the naming pucch-ResourceConfig-RedCap-r17=> prb-Offset-r17 | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| Y | | 2352 | ***intra-SlotFH-r17***  In case a separate initial UL BWP is configured for RedCap UEs, the presence of this parameter indicates whether intra-slot PUCCH frequency hopping within the separate initial UL BWP in the common PUCCH resource is enabled for RedCap UEs. If this field is absent, intra-slot PUCCH frequency hopping within RedCap-specific initial UL BWP is enabled. If this field is present, intra-slot PUCCH frequency hopping within RedCap-specific initial UL BWP is disabled and each PUCCH resource is mapped to a single PRB on one side of the UL BWP and this parameter determines whether the PRB index in the PRB mapping is counted in increasing order from the lower edge or in decreasing order from the upper edge of the UL BWP. | intra-SlotFH~~-r17~~.. | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| Y | | 236 | Event X1: Seving L2 U2N Relay UE becomes worse than absolute threshold1 AND NR Cell becomes better than another absolute threshold2;  Event X2: Serving L2 U2N Relay UE becomes worse than absolute threshold; | Typo. Should be changed to Serving | Yinghao Guo  <yinghaoguo@huawei.com> |  |
| Y | | 237 | In the NTN-Config fields description table, there are field descriptions of fields of EpochTime and TA-Info | Create field description tables for EpochTime and TA-Info and move their fields there | david.lecompte@huawei.com |  |
| Y | | 238 | In PUSCH-ServingCellConfig, in the field description of nrofHARQ-ProcessesForPUSCH, there is "16HARQ processes" | Add missing space between "16" and "HARQ" | david.lecompte@huawei.com |  |
| 239 | | N | 5.8.9.5 Actions related to PC5-RRC connection release requested by upper layers or AS layer The UE initiates the procedure when upper layers request the release of the PC5-RRC connection as specified in TS 24.587 [57] or when AS layer releases the the PC5-RRC connection. The UE shall not initiate the procedure for power saving purposes. | Should add the related subclauses leading to the AS triggered PC5 RRC connection release.  Change as follows:  The UE initiates the procedure when upper layers request the release of the PC5-RRC connection as specified in TS 24.587 [57] or when AS layer releases the the PC5-RRC connection as specified in 5.3.5.5.2, 5.3.5.16.2 and 5.8.9.10.4. The UE shall not initiate the procedure for power saving purposes. | xiao.xiao@vivo.com |  |
| 240 | | N | 5.8.9.9.2 Actions related to transmission of *UuMessageTransferSidelink* message The L2 U2N Relay UE initiates the Uu message transfer procedure when one of the following conditions is met:  1> upon receiving *Paging* message related to the connected L2 U2N Remote UE from network;   1. upon acquisition of the SIBs requested by the connected L2 U2N Remote UE (as indicated in *sl-Requested-SI-List* in the *RemoteUEInformationSidelink*);   1> upon receiving the updated SIB1 and the SIBs have been requested by the connected L2 U2N Remote UE from network; […] | 1. For SIB1, request-based delivery is supported. But SIB1 is missing in the procedural text. Also add bracket for SIBs. 2. Incorrect grammar.   Suggested changes as follows:  The L2 U2N Relay UE initiates the Uu message transfer procedure when one of the following conditions is met:  1> upon receiving *Paging* message related to the connected L2 U2N Remote UE from network;   1. upon acquisition of the SIB1 and SIB(s) requested by the connected L2 U2N Remote UE (as indicated in *sl-Requested-SI-List* in the *RemoteUEInformationSidelink*);   1> upon receiving the updated SIB1 and the SIB(s) which have been requested by the connected L2 U2N Remote UE from network; | xiao.xiao@vivo.com |  |
| 241 | | N | 5.8.9.9.3 Reception of the *UuMessageTransferSidelink* Upon receiving the *UuMessageTransferSidelink* message, the L2 U2N Remote UE shall:  1> if *sl-PagingDelivery* is included:  2> perform the procedure as defined in clause 5.3.2.3;  1> if *sl-SystemInformationDeliverySidelink* is included:  2> perform the actions specified in clause 5.2.2.4; | SIB1 delivery is missing in the procedure.  Suggested change:  Upon receiving the *UuMessageTransferSidelink* message, the L2 U2N Remote UE shall:  1> if *sl-PagingDelivery* is included:  2> perform the procedure as defined in clause 5.3.2.3;  1> if *sl-SystemInformationDeliverySidelink* or *sl-SIB1-Delivery* is included:  2> perform the actions specified in clause 5.2.2.4; | xiao.xiao@vivo.com |  |
| 242 | | N | 5.8.9.10.4 Actions related to reception of *NotificationMessageSidelink* message Upon receiving the *NotificationMessageSidelink*, the U2N Remote UE shall:  1> if the *indicationType* is included:  2> if the UE is L2 U2N Remote UE in RRC\_CONNECTED:  3> initiate the RRC connection re-establishment procedure as specified in 5.3.7;2> else if the UE is L3 U2N Remote UE, or L2 U2N Remote UE in RRC\_IDLE or RRC\_INACTIVE:  3> if the PC5-RRC connection with the U2N Relay UE is determined to be released:  4> perform the PC5-RRC connection release as specified in 5.8.9.5.  3> else maintain the PC5-RRC connection;  NOTE: For L3 U2N Remote UE, or L2 U2N Remote UE in RRC\_IDLE or RRC\_INACTIVE, it is up to Remote UE implementation whether to release or keep the unicast PC5 link. | Editorial change: It is PC5-RRC connection rather than the PC5 unicast link that can be visible in RRC layer.  Change “unicast PC5 link” to “PC5-RRC connection” (wherever applied) | xiao.xiao@vivo.com |  |
| 243 | | N | SIB19 field description:  ***ntn-Config*** Provides Ephemeris data, common TA parameters, koffset, validity duration for UL sync information and epoch time when included in SIB19. | Incomplete field description.  Change to:  ***ntn-Config***  Provides Ephemeris data, common TA parameters, cell specific koffset, kmac, polarization parameters, validity duration for UL sync information and epoch time when included in SIB19. | xiao.xiao@vivo.com |  |
| 244 | | Y | In the IE of ReportConfigNR:  condEventD1-r17 SEQUENCE {  distanceThresFromReference1-r17 INTEGER(0.. 65525),  distanceThresFromReference2-r17 INTEGER(0.. 65525) OPTIONAL, --Need R  […]  },  eventD1-r17 SEQUENCE {  distanceThresFromReference1-r17 INTEGER(1.. 65525),  distanceThresFromReference2-r17 INTEGER(1.. 65525) OPTIONAL, --Need R  […]  } | This should be a typo, as the intention/agreement is to use 16 bits for this field, corresponding to 0..65535 (not 65525)  Change “65525” to “65535”. | xiao.xiao@vivo.com |  |
| 245 | | Y | Field name of *ntn-UlSyncValidityDuration-r17*. | As per related agreements, this parameter should be a validity “timer” instead of a window-like duration.  Change the name to “*ntn-UlSyncValidity~~Duration~~Timer-r17*” | xiao.xiao@vivo.com |  |
| 246 | | N | 5.5.4.19 Event D1  The UE shall:  1> consider the entering condition for this event to be satisfied when both condition D1-1 and conditionD1-2, as specified below, is fulfilled;  1> consider the leaving condition for this event to be satisfied when condition D1-3 or conditionD1-4, as specified below, is fulfilled;  […]  ***Ml1*** is the UE location, represented by the distance between UE and a reference location parameter for this event (i.e. *referenceLocation1* as defined within *reportConfigNR* for this event), not taking into account any offsets.  ***Ml2*** is the UE location, represented by the distance between UE and a reference location parameter for this event (i.e. *referenceLocation2* as defined within *reportConfigNR* for this event), not taking into account any offsets but.  […] | It should be the distance between the UE and a reference location, not between the UE and a “parameter” as in the current description.  Remove the words “parameter”. Also, remove the “but” at the end of “Ml2” description. | xiao.xiao@vivo.com |  |
| 247 | | Y | In IE: *BeamFailureRecoveryServingCellConfig*,  ***additionalPCI***  Indicates the physical cell IDs (PCI) of the SSBs in the *candidateBeamRSList2*. | In IE: *BeamFailureRecoveryServingCellConfig*, there is no corresponding IE for the below field description in current version, the below field description should be removed first.  ***additionalPCI***  Indicates the physical cell IDs (PCI) of the SSBs in the *candidateBeamRSList2*.  This IE exists in the previous version, but was removed in this version. We need further discuss whether it is needed. | Chenli5g@vivo.com |  |
| 248 | | Y | In IE TCI-state:  additionalPCI-r17 AdditionalPCIIndex-r17 OPTIONAL -- Need R | The name of “additionalPCI-r17” should be changed to “additionalPCIIndex-r17” to align with the similar one in “SSB-MTC-AdditionalPCI-r17” as below:  SSB-MTC-AdditionalPCI-r17 ::= SEQUENCE {  additionalPCIIndex-r17 AdditionalPCIIndex-r17,  additionalPCI-r17 PhysCellId, | Chenli5g@vivo.com |  |
| 249 | | Y | ***p0-PUSCH-SetList2***  For indicating per-TRP OLPC set in DCI format 0\_1/0\_2 with the legacy field, a second p0-PUSCH-SetList-r16 is used. When this field is present the p0-PUSCH-SetList2 corresponds to the first SRS resource set (see TS 38.213). | Typo:  ***p0-PUSCH-SetList2***  For indicating per-TRP OLPC set in DCI format 0\_1/0\_2 with the legacy field, a second p0-PUSCH-SetList-r16 is used. When this field is present the *p0-PUSCH-SetList~~2~~* corresponds to the first SRS resource set (see TS 38.213).  The reason is *p0-PUSCH-SetList* corresponds to the first SRS resource set. | Chenli5g@vivo.com |  |
| 250 | | Y | The name of IE:  ***sfnSchemePdsch*** | This IE should be changed to *sfnScheme~~Pdsch~~* to align with the similar IE (*sfnScheme*) in PDCCH-Config. | Chenli5g@vivo.com |  |
| 251 | | Y | ***trs-ResouceSetConfig***  RS configuration of TRS occasion(s) for idle/inactive UE(s), in terms of a list of N>=1 NZP TRS resource set(s). The maximum number of TRS resource sets configured by higher layer is 64. If a TRS resource is configured, the L1 based availability indication is always enabled based on that configuration. A UE which acquired SIB-X with a TRS configuration but did not yet receive an associated L1-based availability indication considers the configured TRS as unavailable. | Replace SIB-X with SIB 17 | david.lecompte@huawei.com |  |
| 252 | | Y | **SpCellConfig field descriptions**  ***lowMobilityEvaluationConnected***  Indicates the criterion for a UE to detect low mobility in RRC\_CONNECTED in an SpCell. The *s-SearchDeltaP-Connected* is the parameter "SSearchDeltaP-connected". And the *t-SearchDeltaP-Connected* is the parameter " TSearchDeltaP-Connected". Low mobility criterion is configured in NR Pcell for the case of NR SA/ NR CA/ NE-DC/NR-DC, and in the NR PSCell for the case of EN-DC. | Remove space between " and T | david.lecompte@huawei.com |  |
| 253 | | Y | *SubgroupConfig* field descriptions  ***subgroupsNumPerPO***  Total number of subgroups per Paging Occasion (PO) for UE to read subgroups indication from physical-layer signaling The field represents the sum of CN-assigned and UEID-based subgroups supported by the network. | Missing full stop between "signaling" and "The" | david.lecompte@huawei.com |  |
| 254 | | Y | *SubgroupConfig* field descriptions  ***subgroupsNumForUEID***  Number of subgroups per Paging Occasion (PO) for UE to read subgroups indication from physical-layer signaling, for UEID-based subgrouping method. When present, the fieldis set to an integer smaller than or equal to *subgroupsNumPerPO*s*. subgroupsNumPerPO* equals to *subgroupsNumForUEID* when the network does not support CN-assigned subgrouping. The field is absent when the network does not support UEID-based subgrouping. Both this field and *subgroupsNumPerPO* are equal to 1 when the network does not support subgrouping. | s to be deleted in field name: *subgroupsNumPerPO*s -> *subgroupsNumPerPO* | david.lecompte@huawei.com |  |
| 255 | | Y | *PDCCH-Config field descriptions*  ***pdcch-SkippingDurationList***  The UE can be configured to be indicated by DCI a value of X (i.e., skipping duration), in units of slots, among at most 3 multiple RRC configured values by scheduling DCIs indicating PDCCH schedules data. | Remove "multiple" (shown in red) | david.lecompte@huawei.com |  |
| 256 | | Y | AvailabilityCombination-r17 ::= SEQUENCE {  availabilityCombinationId-r16 AvailabilityCombinationId-r16,  rbSetGroups-r17 SEQUENCE (SIZE (1..maxNrofRbSetGroups-r17)) OF RbSetGroup-r17 OPTIONAL, -- Need M  resourceAvailability-r16 SEQUENCE (SIZE (1..maxNrofResourceAvailabilityPerCombination-r16)) OF INTEGER (0..7) OPTIONAL -- Need M  } | Wrong suffixes, should be r17 | david.lecompte@huawei.com |  |
| 257 | | Y | In 5.3.5.20  3> if *ran-VisibleParameters* is set to setup and the parameters have been received;  4> forward the *measConfigAppLayerId,* the *ran-VisiblePeriodicity*, the *numberOfBufferLevelEntries* and the *reportInitialPlayOutDelay* to upper layers considering the *serviceType*; | The end of the 3> bullet should be ":", not ";" | david.lecompte@huawei.com |  |
| 258 | | Y | In 5.7.16.2  4> set the *appLayerBufferLevel* values in the *appLayerBufferLevelLIst* to the buffer level values received from the upper layer in the order with the first *appLayerBufferLevel* value set to the newest received buffer level value, the second *appLayerBufferLevel* value set to the second newest received buffer level value, and so on until all the buffer level values received from the upper layer have been assigned or the configured maximum number of *appLayerBufferLevel* values have been set, if any; | "I" should be small case  *appLayerBufferLevelLIst -> appLayerBufferLevelList* | david.lecompte@huawei.com |  |
| 259 | | Y | In 5.7.16.2  3> submit the *MeasurementReportAppLayer* message to lower layers for transmission upon which the procedure ends. | This is the last bullet of this section, so can remove the red text. | david.lecompte@huawei.com |  |
| 260 | | Y | *MeasurementReportAppLayer message*  RAN-VisibleMeasurements-r17 ::= SEQUENCE {  appLayerBufferLevelList-r17 SEQUENCE (SIZE (1..8)) OF AppLayerBufferLevel OPTIONAL,  initialPlayoutDelay-r17 INTEGER (0..30000) OPTIONAL,  pdu-SessionIdList-r17 SEQUENCE (SIZE (1..maxNrofPDU-Sessions-r17)) OF PDU-SessionID OPTIONAL,  ...  }  AppLayerBufferLevel ::= INTEGER (0..30000) | AppLayerBufferLevel is a new Rel-17 type, it should have the -r17 suffix | david.lecompte@huawei.com |  |
| 261 | N | Section 5.8.3.2  2> if configured by upper layer to receive NR sidelink non-relay discovery announcements on the frequency included in *sl-FreqInfoList* in *SIB12* of the PCell including *sl-NonRelayDiscovery*:  3> if the UE did not transmit a *SidelinkUEInformationNR* message since last entering RRC\_CONNECTED state; or  3> if since the last time the UE transmitted a *SidelinkUEInformationNR* message the UE connected to a PCell not providing *SIB12* including *sl-ConfigCommonNR* or connected to a PCell providing *SIB12* but not including *sl-NonRelayDiscovery*; or  3> if the last transmission of the *SidelinkUEInformationNR* message did not include *sl-RxInterestedFreqListDisc*; or if the frequency configured by upper layers to receive NR sidelink discovery announcements on has changed since the last transmission of the *SidelinkUEInformationNR* message:  4> initiate transmission of the *SidelinkUEInformationNR* message to indicate the NR sidelink discovery reception frequency of interest in accordance with 5.8.3.3; | The terminology “announcements” is more related to discovery model A, but the procedure should be both applied to mode A/B. Suggest to use a more general wording to cover both model A and model B, to avoid misunderstanding.  Can change ‘discovery announcements’ to ‘discovery messages’  This terminology change, if agreed, should also be applied to other sections not listed here. | liangjing@vivo.com |  |
| 262 | N | Section 5.8.9.1a.3  1> if discovery transmission for a specific destination is terminated in upper layers:  2> release the PDCP entity, RLC entity and the logical channel of the sidelink SRB4 for discovery message of the specific destination; | Editorial change.  Reference should be added here “if discovery transmission for a specific destination is terminated in upper layers as specified in TS 24.554” | liangjing@vivo.com |  |
|  |  | Section 5.8.15.3  3> if the UE did not detect any candidate NR sidelink U2N Relay UE which SD-RSRP exceeds *sl-RSRP-Thresh* by *sl-HystMin*:  4> consider no NR sidelink U2N Relay UE to be selected; | Editorial.  Change ‘which’ to ‘for which’. | liangjing@vivo.com |  |
| 263 | Y | SL-L2RelayUEConfig-r17 ::= SEQUENCE {  sl-RemoteUE-ToAddModList-r17 SEQUENCE (SIZE (1..maxRemoteUE-r17)) OF SL-RemoteUE-ToAddMod-r17 OPTIONAL, -- Need M  sl-RemoteUE-ToReleaseList-r17 SEQUENCE (SIZE (1..maxRemoteUE-r17)) OF SL-DestinationIdentity-r16 OPTIONAL, -- Need M  ...  } | “maxRemoteUE” could be changed to “maxNrofRemoteUE” to align with the naming style for other parameters. | liangjing@vivo.com |  |
| 264 | N | Section 5.8.1  NOTE 3: All SL-DRBs related to the same PC5-RRC connection have the same activation/deactivation setting for ciphering and the same activation/deactivation setting for integrity protection as in TS 33.536 [60].  NOTE 4: When integrity check failure concerning SL-SRB1 for a specific destination is detected, the UE sends an indication to the upper layers [57]. | Align with wording for the references.  as specified in TS 33.536  upper layers as specified in TS 24.587 | liangjing@vivo.com |  |
| 265 | N | Section 5.8.3.1  is reporting, for NR sidelink groupcast or broadcast communication, the Destination Layer-2 ID and QoS profile associated with its interested services that sidelink DRX is applied, | Editorial.  Change ‘that’ to ‘to which’ (wherever applied) | liangjing@vivo.com |  |
| 266 | N | Section 5.8.3.2  3> if the UE received a sidelink DRX assistance information for NR sidelink unicast communication from the associated peer UE: | To be more aligned with stage-3 style.  ‘a sidelink DRX assistance information’ should be changed to:  ‘~~a~~ sidelink DRX assistance information in the *UEAssistanceInformationSidelink* message’ | liangjing@vivo.com |  |
| 267 | N | In 5.3.5.8.3  1> if the target L2 U2N Relay UE changes its serving PCell before path switch (i.e. the received *RRCReconfiguration* message containing *reconfigureWithSync* indicating path switch as specified in 5.3.5.5.2): | It should be reconfigurationwithsync | qianxi.lu@oppo.com |  |
| 268 | N | 9.2.4 Default sidelink RLC bearer configuration Parameters that are used for the sidelink RLC bearer for Remote UE’s SRB1 RRC message such as *RRCResume*, *RRCReestablishment*, and *RRCReconfigurationComplete* (in response to the *RRCReconfiguration* message containing *reconfigureWithSync* indicating path switch to a L2 U2N Relay UE) message. The sidelink RLC bearer using this configuration is named as SL-RLC1. | It should be reconfigurationwithsync | qianxi.lu@oppo.com |  |
| 269 | N | In 5.3.10.5  1> if the failure is detected due to reconfiguration with sync failure as described in 5.3.5.8.3, set the fields in *VarRLF-report* as follows:  2> set the *connectionFailureType* to *hof*;  2> if any DAPS bearer was configured while T304 was running:  3> set *lastHO-Type* to *daps*;  3> if radio link failure was detected in the source PCell, according to subclause 5.3.10.3:4> set *timeConnSourceDAPS-Failure* to the time between the initiation of the DAPS handover execution and the radio link failure detected in the source PCell while T304 was running;  4> set the *rlf-Cause* to the trigger for detecting the source radio link failure in accordance with clause 5.3.10.4; | The blank space before '3>' should be removed.  ‘4>’ should have a separate link.  1> if the failure is detected due to reconfiguration with sync failure as described in 5.3.5.8.3, set the fields in *VarRLF-report* as follows:  2> set the *connectionFailureType* to *hof*;  2> if any DAPS bearer was configured while T304 was running:  3> set *lastHO-Type* to *daps*;  3> if radio link failure was detected in the source PCell, according to subclause 5.3.10.3;  4> set *timeConnSourceDAPS-Failure* to the time between the initiation of the DAPS handover execution and the radio link failure detected in the source PCell while T304 was running;  4> set the *rlf-Cause* to the trigger for detecting the source radio link failure in accordance with clause 5.3.10.4; | Wulh5@lenovo.com |  |
| 270 | N | In 5.3.10.5  3> set *choCandidateCellList* to include the global cell identity and tracking area code, if available, and otherwise to the physical cell identity and carrier frequency of each of the candidate target cells for conditional handover included in *condRRCReconfig* within *VarConditionalReconfig* at the time of the failed conditional handover, excluding the candidate target cells included in *measResulNeighCells*;  ***choCandidateCellList*** This field is used to indicate the list of candidate target cells for conditional handover included in condRRCReconfig at the time of connection failure. The field does not include the candidate target cells included in measResulNeighCells. | *‘t’ is missed in measResulNeighCells IE.*  *measResulNeighCells* => *measResultNeighCells* | Wulh5@lenovo.com |  |
| 271 | N | In 5.3.10.5  2> if configuration of the conditional handover is available in *VarConditionalReconfig* at the moment of declaring the radio link failure:  3> set *timeSinceCHO-Reconfig* to the time elapsed between the detection of the radio link failure, and the reception, in the source PCell, of the last *conditionalReconfiguration* including the *condRRCReconfig* message; | Remove “message” | Wulh5@lenovo.com |  |
| 272 | N | In 5.7.10.6  3> for the source PCell in which the last *RRCReconfiguration* message including *reconfigurationWithSync* was applied:  4> set the *sourceCellID* in *sourceCellInfo* to the global cell identity and tracking area code of the source PCell; | Change *sourceCellID* to *sourcePCellId* to align with IE name in ASN.1. | Wulh5@lenovo.com |  |
| 273 | N | In 5.7.10.6  3> for the target PCell indicated in the last applied *RRCReconfiguration* message including *reconfigurationWithSync*:  4> set the *targetCellID* in *targetCellInfo* to the global cell identity and tracking area code of the target PCell; | Change *targetCellID* to *targetPCellId* to align with IE name in ASN.1. | Wulh5@lenovo.com |  |
| 274 | N | In 5.7.10.6  3> if *sourceDAPS-FailureReporting* included in the *successHO-Config* configured by the source PCell before executing the last reconfiguration with sync is set to *true*, and if the last executed handover was a DAPS handover and if an RLF occurred at the source PCell during the DAPS handover while T304 was running:  4> set *sourceDAPS-Failure* in *shr-Cause* to *true*; | Change *sourceDAPS-Failure* to *sourceDAPSFailure* to align with IE name in ASN.1. | Wulh5@lenovo.com |  |
| 275 | N | In 5.3.5.13.4  2> if the *RRCReconfiguration* within *condRRCReconfig* includes the *masterCellGroup* including the *reconfigurationWithSync*, consider the cell which has a physical cell identity matching the value indicated in the *ServingCellConfigCommon* included in the *reconfigurationWithSync* within the masterCellGroup in the received *condRRCReconfig* to be applicable cell; | Missing italics. | xiongyi3@xiaomi.com |  |
| 276 | N | In 5.3.5.13.4a  1> for each *condReconfigId* within the *VarConditionalReconfig* specified in TS 36.331[10],: | The “,” should be removed. | xiongyi3@xiaomi.com |  |
| 277 | N | In 6.3.2  ***eventId***  Choice of NR event triggered reporting criteria. If network configured eventD1 network shall configure includeCommonLocationInfo for the UE. | Missing italics in the highlighted words. | xiongyi3@xiaomi.com |  |
| 278 | N | In 5.5.6.2 Initiation NOTE 1: The UE verifies the measurement gap situation only upon receiving the indication from upper layers. If at this point in time sufficient gaps are available, the UE does not initiate the procedure. Unless it receives a new indication from upper layers, the UE is only allowed to further repeat the procedure in the same PCell once per frequency of the target RAT if the provided measurement gaps are insufficient.  1> if and only if upper layers indicate to stop performing location measurements towards E-UTRA or NR or stop subframe and slot timing detection towards E-UTRA and *preConfigGapID* is not activated:  2> initiate the procedure to indicate stop.  NOTE 2: The UE may initiate the procedure to indicate stop even if it did not previously initiate the procedure to indicate start.  1> if *preConfigGapID* is activated:  2> if a request from upper layers to transmit either a new *preConfigGapID* or to modify the current *measGapConfig* is received; or  2> if a request from upper layers indicate that the current gap is not needed:  3> trigger the lower layers to deactivate the current active measurement gap as specified in TS 38.321 [6]; | Suggest to add “using UL MAC CE”, it would be more clear and it align the text description of initiating the activation request. 5.5.6.2 Initiation …  1> if and only if upper layers indicate to stop performing location measurements towards E-UTRA or NR or stop subframe and slot timing detection towards E-UTRA and *preConfigGapID* is not activated:  2> initiate the procedure to indicate stop.  NOTE 2: The UE may initiate the procedure to indicate stop even if it did not previously initiate the procedure to indicate start.  1> if *preConfigGapID* is activated:  2> if a request from upper layers to transmit either a new *preConfigGapID* or to modify the current *measGapConfig* is received; or  2> if a request from upper layers indicate that the current gap is not needed:  3> trigger the lower layers to deactivate the current active measurement gap using UL MAC CE as specified in TS 38.321 [6]; | lixiaolong1@xiaomi.com |  |
| 279 |  |  |  |  |  |
| 280 |  |  |  |  |  |
| 281 |  |  |  |  |  |
| 282 |  |  |  |  |  |
| 283 |  |  |  |  |  |
| 284 |  |  |  |  |  |
| 285 |  |  |  |  |  |
| 286 |  |  |  |  |  |
| 287 |  |  |  |  |  |
| 288 |  |  |  |  |  |
| 289 |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |