**3GPP TSG-****RAN2 Meeting#xxx R2-24xxxxx**

**Tbd**

**Agenda Item:** XXX

**Source:** Ericsson

**Title:** NR Rel-18 38.331 ASN.1 Review, Class 0 issues

**Document for:** Discussion and decision

# Guidelines

* This file is used to log NR 38.331 ASN.1 Review Class 0 issues.
	+ **- Typo, minor wording improvement etc.**
	+ **- ASN.1 field not following naming rules (e.g. incorrect suffix, capitalization, “-“, etc).**
* Fill in the columns, see example.
	+ Make sure the inserted specification text is unique, such that the location of the issue is simple to find.
	+ Avoid indicating duplicated issues by checking if the concerned specification text is already reported in the table.
	+ Step the file name v(x) -> v(x+1) and upload to ftp server.
* The “status” column will be filled in by the RRC Spec Rapporteur.

# Class 0 issues

| **Issue**  | **ASN1?****Y/N** | **Copied existing specification text.****Text should be unique, so that it can be easily found in the specification.****If needed, add also the new text.** | **Comment/description/****correction** | **Email address**  | **Status** |
| --- | --- | --- | --- | --- | --- |
| Ex 1 | NN | 2> derive the KUPint key associated with the *integrityProtAlgorithm* indicated in the SecurityModeCommand message, as specified in TS 33.501 [11]; | Missing italics. | hakan.l.palm@ericsson.com |  |
| Ex 2 | N | PUSCH scheduled by RAR UL grant (see 38.213 clause 8.3 and 38.214 clause 6.1.2.2) and uses interlaced PUCCH Format 0, 1, 2, and 3 for cell-specific PUCCH (see TS 38.213 [13], clause 9.2.1). | Incorrect reference, should be 9.2.101. | hakan.l.palm@ericsson.com |  |
| Ex 3 | Y | RbSetGroup, rbSetGroups | RB-SetGroup, rb-SetGroups | hakan.l.palm@ericsson.com |  |
| 4 | N | maxCandidateBandIndexIndicate the maximum number of band entry index for MUSIM capability restriction reporting. | Remove this field description. As “maxCandidateBandIndex” is not a field, but a multiplicity.  | tangxun@catt.cn |  |
| 5 | N | musim-AvoidedBandsListIndicates the UE’s preference on band(s) and/or combination(s) of bands to be avoided or MUSIM purpose. | Typo, should be “for MUSIM purpose” | tangxun@catt.cn |  |
| 6 | N | musim-GapKeepIndicates the UE is allowed to use “keep solution” for collided MUSIM periodic gaps. If “keep solution” is not granted, priority based solution is used as fallback solution) as specified in TS 38.133[14]. | Typo, remove “)” in “as fallback solution)” | tangxun@catt.cn |  |
| 7 | Y | maxCandidateBandIndex -r18 INTEGER ::= 8 -- Maximum number of band entry index for MUSIM capability | The name should be “maxCandidateBand~~Index~~”, as it represents a maximum number, not an index. | tangxun@catt.cn |  |
| 8 | N | 4> select the first frequency band in the frequencyBandList (or for aerial UE frequencyBandListAerial), and frequencyBandListSUL, if present, which the UE supports and for which the UE supports at least one of the additionalSpectrumEmission values in nr-NS-PmaxList (or for aerial UE nr-NS-PmaxListAerial), if present: | No need to add “()”, i.e., “~~(~~or for aerial UE nr-NS-PmaxListAerial~~)~~”. | tangxun@catt.cn |  |
| 9 | Y | -- ASN1START-- TAG-NTN-CONFIG-STARTATG-Config-r18 ::= SEQUENCE {<omitted> }-- TAG-NTN-CONFIG-STOP-- ASN1STOP | It should be “ATG” | tangxun@catt.cn |  |
| 10 | N | suspend all multicast MRB(s) associated with multicast session(s) not configured to receive in RRC\_INACTIVE | It should be “not configured to be received in RRC\_INACTIVE” | Fangying.xiao@cn.sharp-world.com |  |
| 11 | N | indicate PDCP suspend to lower layers of all DRBs and multicast MRBs associated with multicast session(s) not configured to receive in RRC\_INACTIVE | It should be “not configured to be received in RRC\_INACTIVE” | Fangying.xiao@cn.sharp-world.com |  |
| 12 | nN | - change of its fulfilment status for RRM measurement relaxation criterion, or;- service link (specified in TS 38.300 [2]) propagation delay difference between serving cell and neighbour cell(s); or- its preference on multi-Rx operation for FR2; or- availability of flight path information for Aerial UE operation; or | Typo in use of commas, should be “xxx, or;” instead of ”xxx; or” | Helka-liina.maattanen@ericsson.com |  |
| 13 | Y | UAV-Config-r18 ::= SEQUENCE { flightPathUpdateThrConfig-r18 SEQUENCE { flightPathUpdateDistanceThr-r18 SetupRelease { FlightPathUpdateDistanceThr-r18 } OPTIONAL, -- Need M  flightPathUpdateTimeThr-r18 SetupRelease { FlightPathUpdateTimeThr-r18 } OPTIONAL -- Need M } OPTIONAL, -- Need M ...} | A “,” is missing.[Lenovo] No comma needed.[QC] agree with Lenovo, comma is not needed here | zhang.mengjie@zte.com.cn |  |
| 14 |  | 2> if the UE has flight path information available:3> if the UE had not previously provided a flight path information since last entering RRC\_CONNECTED state; or3> if at least one waypoint was not previously provided; or3> if at least one upcoming waypoint that was previously provided is being removed; or3> if *flightPathUpdateDistanceThr* is configured and for at least one waypoint, the 3D distance between the previously provided location and the new location is more than or equal to the distance threshold configured by *flightPathUpdateDistanceThr*; or | Suggest to remove “being” | zhang.mengjie@zte.com.cn |  |
| 15 |  | The reporting events concerning Aerial UE altitude are labelled H*N* with *N* equal to 1 and 2. Additionally, the reporting events concerning Aerial UE altitude and the neighboring cell measurements simultaneously are labelled A*M*H*N* with *M* equal to 3, 4, 5 and *N* equal to 1, 2.Event H1: Aerial UE altitude becomes higher than a threshold; | Change “;” to “.” | zhang.mengjie@zte.com.cn |  |
| 16 | N | 5.2.2.4.21:1> if *SatSwitchWithReSync* and *t-Service* are included, and the UE supports hard satellite switch with resynchronization;2> if *t-ServiceStart* is included and the UE supports soft satellite switch with resynchronization:3> perform the satellite switch with resynchronization as specified in 5.7.19 between the time indicated by *t-ServiceStart* and the time indicated by *t-Service* for the serving cell.2> else:3> perform the satellite switch with resynchronization as specified in 5.7.19 at the time indicated by *t-Service* for the serving cell. | * Field name *satSwitchWithReSync* instead of IE name should be used.
* Semicolon should be replaced by colon.
* Format of indentation level “3>” should be “B3”.
 | hchoi5@lenovo.com |  |
| 17 | N | 5.5.2.12:1> if effectiveMeasWindowConfig is set to setup:2> if an effective measurement window configuration is already setup:3> release the effective measurement window configuration;2> setup an effective measurement window configuration indicated by the *effectiveMeasWindowConfig* in accordance with the received *windowOffsetPeriodicity* (providing *periodicity* and *offset* for the following condition), i.e., the first subframe of each window occurs at an SFN and subframe meeting the following condition:SFN mod *T* = FLOOR(*offset*/10);subframe = *offset* mod 10;with *T* = *periodicity*/10;1> else if effectiveMeasWindowConfig is set to release:2> release the effective measurement window configuration; | * Highlighted field names/values should be set in italics.
* Last semicolon should be replaced by dot.
 | hchoi5@lenovo.com |  |
| 18 | Y | 6.2.2, Paging message:PagingRecord-v1800 ::= SEQUENCE { mt-SDT ENUMERATED {true} OPTIONAL -- Need N} | Add suffix "-r18" for field mt-SDT. | hchoi5@lenovo.com |  |
| 19 | N | 6.2.2, RRCRelease message, SRS-PosRRC-InactiveValidityAreaConfig field descriptions:***srs-PosHyperSFN-Index***Indicates whether the current SFN is even or odd SFN for SRS for Positioning transmission. If this filed is not configured, the UE assumes that SRS for positioning periodictity longer than one SFN is not configured. | In the description of srs-PosHyperSFN-Index two typos should be fixed:* filed ->field
* periodictity ->periodicity
 | hchoi5@lenovo.com |  |
| 20 | Y | 6.2.2, UEInformationResponse message:PerRASSBInfo-v1800 ::= SEQUENCE { allPreamblesBlocked ENUMERATED {true} OPTIONAL, lbt-Detected-r18 ENUMERATED {true} OPTIONAL, ...}PerRACSI-RSInfo-v1800 ::= SEQUENCE { allPreamblesBlocked ENUMERATED {true} OPTIONAL, lbt-Detected-r18 ENUMERATED {true} OPTIONAL, ...} | Add missing suffix “-r18” for field allPreamblesBlocked. | hchoi5@lenovo.com |  |
| 21 | Y | 6.2.2, UEInformationResponse message:scgFailureCause-r18 ENUMERATED {t310-Expiry, randomAccessProblem, rlc-MaxNumRetx, synchReconfigFailureSCG, scg-ReconfigFailure, srb3-IntegrityFailure, scg-lbtFailure-r16, beamFailureRecoveryFailure-r16, t312-Expiry-r16, bh-RLF-r16, beamFailure-r17, spare3, spare2, spare1 } | The scgFailureCause-r18 IE is a new R18 type. Therefore, the suffices "-r16" and "-r17" can be removed from the values. Furthermore, two spare values ("spare5, spare4") should be added to fully use the 4-bit value range. | hchoi5@lenovo.com |  |
| 22 | N | 6.3.1, SIB19:***satSwitchWithReSync* field descriptions** | In the title of field descriptions table the letter “s” should be set to capital letter. | hchoi5@lenovo.com |  |
| 23 | Y | 6.3.2, IE CandidateTCI-UL-State:CandidateTCI-UL-State-r18 ::= SEQUENCE { tci-UL-StateId-r18 TCI-UL-StateId-r17, referenceSignal-r18 CHOICE { ssb-Index SSB-Index, csi-RS-Index NZP-CSI-RS-ResourceId }, pathlossReferenceRS-Id-r18 PathlossReferenceRS-Id-r17 OPTIONAL, -- Need R …}***Tci-UL-StateID***The ID number of the uplink TCI state. | * In ASN.1 the format of the ellipsis should be fixed.
* In field description in name Tci-UL-StateID the letter “T” should be set in lowercase letter.
 | hchoi5@lenovo.com |  |
| 24 | Y | 6.3.2, IE CodebookConfig:typeII-CJT-PortSelection-r18 SEQUENCE { paramCombination-CJT-PS-r18 INTEGER (1..5), paramCombination-CJT-PS-alpha-r18 SEQUENCE (SIZE (1..4)) OF INTEGER (1..8) OPTIONAL, -- Need R  | In IE type of typeII-CJT-PortSelection-r18 a line break should be added after “SEQUENCE {“. | hchoi5@lenovo.com |  |
| 25 | Y | 6.3.2, IE CSI-ReportSubConfig:nzp-CSI-RS-ResourceList-r18 SEQUENCE (SIZE (1..maxNrofNZP-CSI-RS-ResourcesPerSet)) OF NZP-CSI-RS-ResourceIndex NZP-CSI-RS-ResourceIndex ::= INTEGER (0..maxNrofNZP-CSI-RS-ResourcesPerSet-1-r18)**CSI-ReportSubConfig field descriptions:*****port-subsetIndicator***Indicates the number of ports of the NZP CSI-RS resources indicated in *nzp-CSI-RS-resourceList* (the value is the same like portNumber of these NZP CSI-RS resources) and the (sub)set of CSI-RS antenna ports used for CSI calculation of the sub-configuration. …***nzp-CSI-RS-resourceList***… | ASN.1: Suffix “-r18” missing for IE NZP-CSI-RS-ResourceIndex.Field descriptions: field names should be aligned with ASN.1.* *port-subsetIndicator ->portSubsetIndicator*
* *nzp-CSI-RS-resourceList ->nzp-CSI-RS-ResourceList*
 | hchoi5@lenovo.com |  |
| 26 | Y | 6.3.2, IE LTM-Candidate:ltm-NoResetID-r18 INTEGER (1..maxNrofLTM-Configs-r18-plus-1)  ltm-UE-MeasuredTA-ID-r18 INTEGER (1..maxNrofLTM-Configs-r18-plus-1) 6.3.2, IE LTM-Config:ltm-ServingCellNoResetID-r18 INTEGER (1..maxNrofLTM-Configs-r18-plus-1) ltm-ServingCellUE-MeasuredTA-ID-r18 INTEGER (1..maxNrofLTM-Configs-r18-plus-1)  | For constant maxNrofLTM-Configs-r18-plus-1 the format of suffix is wrong, should be “maxNrofLTM-ConfigsPlus1-r18". | hchoi5@lenovo.com |  |
| 27 | Y | 6.3.2, IE LTM-CSI-ResourceConfigId:LTM-CSI-ResourceConfigId-r18 ::= INTEGER (0..maxNrofLTM-CSI-ResourceConfigurations-r18-1) | For constant maxNrofLTM-CSI-ResourceConfigurations-r18-1 the format of suffix is wrong, should be “-1-r18". | hchoi5@lenovo.com |  |
| 28 | Y | 6.3.2, IE MeasObjectNR-SL:MeasObjectNR-SL-v1800 ::= SEQUENCE { sl-Frequency INTEGER (1..maxNrofFreqSL-r16), tx-PoolMeasToRemoveList-r16 Tx-PoolMeasList-r16 OPTIONAL, -- Need N tx-PoolMeasToAddModList-r16 Tx-PoolMeasList-r16 PTIONAL -- Need N} | * Suffix “-r18” missing for field sl-Frequency.
* Suffix for fields tx-PoolMeasToRemoveList-r16 and tx-PoolMeasToAddModList-r16 should be “-r18”.
 | hchoi5@lenovo.com |  |
| 29 | Y | 6.3.2, IE MeasWindowConfig:MeasWindowConfig-r18 ::= SEQUENCE { windowOffsetPeriodicity CHOICE { periodicityMs40 INTEGER (0..39), periodicityMs80 INTEGER (0..79), ... }, windowDuration ENUMERATED {ms2, ms5, ms5dot5, spare1}, ...} | Suffix “-r18” missing for fields windowOffsetPeriodicity and windowDuration. | hchoi5@lenovo.com |  |
| 30 | N | 6.3.2, IE PDSCH-Config:

|  |
| --- |
| **Conditional Presence** |
| DCI-1-3 |

 | The name of condition “DCI-1-3” should be set in italics. | hchoi5@lenovo.com |  |
| 31 | Y | 6.3.2, IE ReportConfigNR:ReportOnScellActivation-r18 ::= SEQUENCE { rsType NR-RS-Type, reportQuantityRS-Indexes MeasReportQuantity, maxNrofRS-IndexesToReport INTEGER (1..maxNrofIndexesToReport), includeBeamMeasurements BOOLEAN} | Suffix “-r18” missing for the fields inside ReportOnScellActivation-r18. | hchoi5@lenovo.com |  |
| 32 | Y | 6.3.2, IE ResumeCause:ResumeCause ::= ENUMERATED {emergency, highPriorityAccess, mt-Access, mo-Signalling, mo-Data, mo-VoiceCall, mo-VideoCall, mo-SMS, rna-Update, mps-PriorityAccess, mcs-PriorityAccess, mt-SDT, srs-PosConfigOrActivationReq-v1800, spare3, spare2, spare1 } | Suffix “-v1800” missing for new value “mt-SDT”. | hchoi5@lenovo.com |  |
| 33 | N | 6.3.2, IE SchedulingRequestResourceConfig:***periodicityAndOffset***…UE indicates support of the following SR periodicities in *additionalSR-Periodicities* (see TS 38.306, clause 4.2.6): | The UE capability “additionalSR-Periodicities” has been defined in TS 38.306 in PHY-Parameters. Therefore, in the description of periodicityAndOffset the highlighted part should be revised to:"TS 38.306 [26], clause 4.2.7.10". | hchoi5@lenovo.com |  |
| 34 | Y | 6.3.2, IE ServingCellConfig:tag2-r18 SEQUENCE { tag2-Id TAG-Id, tag2-flag BOOLEAN}  | For the two fields inside tag2-r18 IE, the suffix “-r18” is missing. | hchoi5@lenovo.com |  |
| 35 | Y | 6.3.2, IE SRS-Config:TxHoppingConfig-r18 ::= SEQUENCE { overlapValue-r18 ENUMERATED {zeroRB, oneRB, twoRB, fourRB}, numberOfHops INTEGER(1..6), slotOffsetForRemainingHopsList-r18 SEQUENCE (SIZE (1..maxNrofHops-r18-1) ) OF SlotOffsetForRemainingHops-r18, ...}TxHoppingConfig field descriptions:***slotOffsetForRemainingHopsList***This field specifies the starting slot offset and starting symbol for the SRS resource with tx hopping for different resource types (aperiodic, semi-persistent or periodic SRS transmission). Each hop is configured with the same periodcity. | * For field numberOfHops the suffix “-r18” is missing.
* For constant maxNrofHops-r18-1 the format of the suffix is wrong, should be “-1-r18”.
* In the description of slotOffsetForRemainingHopsList the typo in “periodcity” should be fixed (should be “periodicity”).
 | hchoi5@lenovo.com |  |
| 36 | N | 6.3.2, IE SRS-Config, SRS-Resource, SRS-PosResource field descriptions + SRS-ResourceSet, SRS-PosResourceSet field descriptions:***srs-PosHyperSFN-Index***Indicates whether the current SFN is even or odd SFN for SRS for Positioning transmission. If this filed is not configured, the UE assumes that SRS for positioning periodictity longer than one SFN is not configured. | In the description of srs-PosHyperSFN-Index two typos should be fixed:* filed ->field
* periodictity ->periodicity
 | hchoi5@lenovo.com |  |
| 37 | Y | 6.3.2, IE SRS-PosResourceSetLinkedForAggBW:-- ASN1START-- TAG- SRS-POSRESOURCESETLINKEDFORAGGBW-START-- TAG- SRS-POSRESOURCESETLINKEDFORAGGBW-STOP-- ASN1STOP | Redundant space in the START/STOP tag name should be removed. | hchoi5@lenovo.com |  |
| 38 | Y | 6.3.5, IE SL-BWP-PRS-PoolConfig: SL-PRS-TxPoolDedicated-r18 ::= SEQUENCE { sl-PRS-PoolToReleaseList-r1 SEQUENCE (SIZE (1..maxNrofSL-PRS-TxPool-r18)) OF SL-PRS-ResourcePoolID-r18 OPTIONAL, -- Need N | Suffix of field sl-PRS-PoolToReleaseList-r1 should be “-r18”. | hchoi5@lenovo.com |  |
| 39 | Y | 6.3.5, IE SL-CBR-CommonTxDedicated-SL-PRS-RP-List:*SL-CBR-CommonTxDedicated-SL-PRS-RP-List*The IE *SL-CBR-CommonTxConfigListDedicated-SL-PRS-RP* indicates the list of SL PRS transmission parameters…-- ASN1START-- TAG- SL-CBR-COMMONTXDEDICATEDSL-PRS-RP-LIST-STARTSL-CBR-CommonTxDedicatedSL-PRS-RP-List-r18 ::= SEQUENCE { | * In the IE name the redundant dash should be removed to be aligned with ASN.1.
* In the description the highlighetd IE name should be corrected to *SL-CBR-CommonTxDedicatedSL-PRS-RP-List*.
* In ASN.1 the redundant space in the START tag name should be removed.
 | hchoi5@lenovo.com |  |
| 40 | N | 6.3.5, IE SL-ConfiguredGrantConfig-Dedicated-SL-PRS-RP:– *SL-ConfiguredGrantConfigDedicated-SL-PRS-RP*The IE *SL-ConfiguredGrantConfig-Dedicated-SL-PRS-RP* specifies the configured grant configuration information for NR sidelink positioning in a dedicated SL-PRS resource pool..***SL-ConfiguredGrantConfigDedicated-SL-PRS-RP* information element*****SL-ConfiguredGrantConfig* field descriptions** | * In the description redundant dashes in the IE name should be removed to be aligned with ASN.1.
* Title of field descriptions table should be replaced by “*SL-ConfiguredGrantConfigDedicatedSL-PRS-RP*”.
 | hchoi5@lenovo.com |  |
| 41 | Y | 6.3.5, IE SL-LBT-FailureRecoveryConfig:The IE *SL-LBT-FailureRecoveryConfig-r18* is used to configure the parameters used for detection and cancellation of sidelink consistent LBT failures for operation with shared spectrum channel access, as specified in TS 38.321 [3].SL-LBT-FailureRecoveryConfig-r18 ::= SEQUENCE { sl-lbt-FailureInstanceMaxCount-r18 ENUMERATED {n4, n8, n16, n32, n64, n128} OPTIONAL, -- Need M sl-lbt-FailureDetectionTimer-r18 ENUMERATED {ms10, ms20, ms40, ms80, ms160, ms320} OPTIONAL, -- Need M sl-LBT-RecoveryTimer-r18 ENUMERATED {ms10, ms20, ms40, ms80, ms160, ms320} OPTIONAL, -- Need M ...} | * In the description the suffix “-r18” is not needed.
* In ASN.1 the part “LBT” in field name sl-LBT-RecoveryTimer-r18 should be set in lowercase letters to be consistent with the naming of the other fields.
 | hchoi5@lenovo.com |  |
| 42 | N | 6.3.5, IE SL-ResourcePool:***sl-A2X-Service***Presence of this field indicates the resource pool is dedicated for A2X service, i.e., not to be used for other than A2X service. Value *brid* indicates the resource pool is for BRID, value *daa* indicates the resource pool is for DAA, and value *bridAndDAA* indicates the resource poos is for both BRID and DAA. If this field is absent in all the configured resource pools, the UE may choose non-dedidcated resource pool for A2X service. | In the decription of sl-A2X-Service two typos should be fixed:* poos ->pool
* non-dedidcated ->non-dedicated
 | hchoi5@lenovo.com |  |
| 43 | Y | 6.4:maxNrofHops-r18-1maxNrofLTM-Configs-r18-plus-1 maxNrofLTM-CSI-ResourceConfigurations-r18-1 maxNrofCandidateTCI-State-r18-1 maxNrofCandidateUL-TCI-r18-1  | The wrong format of suffices for the concerned constants should be corrected as follows:* maxNrofHops-r18-1 ->maxNrofHops-1-r18
* maxNrofLTM-Configs-r18-plus-1 ->maxNrofLTM-ConfigsPlus1-r18
* maxNrofLTM-CSI-ResourceConfigurations-r18-1 ->

maxNrofLTM-CSI-ResourceConfigurations-1-r18* maxNrofCandidateTCI-State-r18-1 ->maxNrofCandidateTCI-State-1-r18
* maxNrofCandidateUL-TCI-r18-1 ->maxNrofCandidateUL-TCI-1-r18

It should be noted that the constants maxNrofCandidateTCI-State-r18-1and maxNrofCandidateUL-TCI-r18-1 are defined in 6.4 but not used elsewhere. | hchoi5@lenovo.com |  |
| 44 | Y | 6.6.2, NotificationMessageSidelink message:-- TAG-NOTIFICATIONMESSAGESIDELINK -STOP-- ASN1STOP | Redundant space in the STOP tag name should be removed. | hchoi5@lenovo.com |  |
| 44 | N | 6.6.2, UEInformationRequestSidelink field descriptions:***SL-E2E-QoS-ConnectionListPC5***Indicates the QoS info for a list of end-to-end PC5 connections with each connection indicated by the destination L2 ID of the peer L2 U2U Remote UE. | To be aligned with ASN.1 the prefix “SL” should be set in lowercase letters. | hchoi5@lenovo.com |  |
| 45 | N | 7.4:– *VarAppLayerPLMN-LisConfig* | In the variable name the letter “t” is missing, should say “*VarAppLayerPLMN-ListConfig*”. | hchoi5@lenovo.com |  |
| 46 | N | 7.4:– *VarLTM-Config*The IE *VarLTM-Config* is used to store the reference configuration and the LTM candidate configurations.– *VarLTM-ServingCellNoResetID*The IE *VarLTM-ServingCellNoResetID* is used to store the serving cell ID based on which the UE determines whether a L2 reset is needed or not upon an LTM cell switch procedure.– *VarLTM-ServingCellUE-MeasuredTA-ID*The IE *VarLTM-ServingCellUE-MeasuredTA-ID* is used to store the serving cell ID based on which the UE determines whether UE-based TA measurements are needed or not upon an LTM cell switch procedure. | In the description of the concerned variables “IE” should be replaced by “UE”. | hchoi5@lenovo.com |  |
| 47 | N | 7.4:***VarSuccessPSCell-Report* variable** | In the title of the variable the “UE” is missing, i.e. should say “*VarSuccessPSCell-Report* UE variable”. | hchoi5@lenovo.com |  |
| 48 | N | 9.1.1.4, last table:

|  |  |
| --- | --- |
| MAC configuration |  |
| *>priority* | 1 |
| *>proritisedBitRate* | Inifinity |

 | Typos in the table should be fixed:* “proritisedBitRate” ->prioritisedBitRate
* “Inifinity” ->”infinity”
 | hchoi5@lenovo.com |  |
| 49 | Y | 11.2.2, CG-Config message:CG-Config-v1800-IEs ::= SEQUENCE { candidateServingFreqRangeListNR-r18 CandidateServingFreqRangeListNR-r18 OPTIONAL, candidateServingFreqListNR-r16 CandidateServingFreqListNR-r16 OPTIONAL, idc-TDM-AssistanceConfig-r18 ENUMERATED {enabled} OPTIONAL, candidateCellInfoListSubsequentCPC-r18 CandidateCellInfoListCPC-r17 OPTIONAL, scpac-ReferenceConfigurationSCG-r18 ReferenceConfiguration-r18 OPTIONAL, nonCriticalExtension SEQUENCE {} OPTIONAL}CG-Config field descriptions:***candidateServingFreqListNR, candidateServingFreqListEUTRA***Indicates frequencies of candidate serving cells for In-Device Co-existence Indication (see TS 36.331 [10]).***candidateServingFreqListNR-r16***indicates the candidate frequencies configured by SN for IDC. This field is only used in NR-DC. | * In ASN.1 and field description the suffix of field candidateServingFreqListNR-r16 should be “-r18”.
* In field description of candidateServingFreqListNR-r16 the word “indicates” should start with capital letter.
 | hchoi5@lenovo.com |  |
| 50 | N | 5.2.2.4.25Upon receiving *SIBXX*, the UE shall:1> if *sl-FreqInfoList* is included in *sl-PosConfigCommonNR*:2> if configured to receive sidelink control information for SL-PRS measurement:3> use the resource pool(s) indicated by *sl-RxPool* and/or *sl-PRS-RxPool* for sidelink control information reception for SL-PRS , as specified in 5.8.X.2; | No need to mention the SCI reception in the RRC procedure, since SCI reception is the PHY operation, in order to achieve SL-PRS reception. Change the highlight part into “SL-PRS”. | yuanli@vivo.com |  |
| 51 | N | 5.3.5.142> if configured to receive sidelink control information for SL-PRS measurement:3> use the resource pool(s) indicated by *sl-RxPool* and/or *sl-PRS-RxPool* for SL-PRS reception, as specified in 5.8.18.2; | Same reason to Issue 50.Change the highlight part into “SL-PRS”. | yuanli@vivo.com |  |
| 52 | N | 5.8.3.1Figure 5.8.3.1-1: Sidelink UE information for NR sidelink communication/discovery | The figure describes SUI transmission procedure, which includes SUI triggered by SIB23 reception. Thus NR sidelink positioning is included.Besides, SIBXX should be correctly named as SIB23. | yuanli@vivo.com |  |
| 53 | N | 5.8.3.2A UE capable of NR sidelink communication or NR sidelink discovery or NR sidelink U2N relay operation or NR sidelink U2U relay operation or NR sidelink positioning that is in RRC\_CONNECTED may initiate the procedure to indicate it is (interested in) receiving or transmitting NR sidelink communication or NR sidelink discovery or NR sidelink U2N relay operation or NR sidelink U2U relay operation or SL-PRS transmission/reception in several cases including upon successful connection establishment or resuming, upon change of interest, upon changing QoS profile(s), upon receiving *UECapabilityInformationSidelink* from the associated peer UE, upon RLC mode information updated from the associated peer UE or upon change to a PCell providing *SIB12* including *sl-ConfigCommonNR,* or upon change to a PCell providing *SIB23* including *sl-PosConfigCommonNR*. | Editor problem.Delete “transmission/reception”. | yuanli@vivo.com |  |
| 54 | N | 5.8.3.2A UE capable of NR sidelink positioning may initiate the procedure to request it is interested or no longer interested in either transmitting SL-PRS or receiving sidelink control information for SL-PRS. | Make no sense on UE to “request” on its interest. UE use UAI to indicate NW about its preference on frequency to receive/transmit Sl-PRS.Change “request” into “indicate”. | yuanli@vivo.com |  |
| 55 | N | 5.8.3.2A UE capable of NR sidelink positioning may initiate the procedure to request it is interested or no longer interested in either transmitting SL-PRS or receiving sidelink control information for SL-PRS. | Same reason to Issue 50.Change the highlight part into “SL-PRS”. | yuanli@vivo.com |  |
| 56 | N | 5.8.3.21> if *SIB23* including *sl-PosConfigCommonNR* is provided by the PCell:2> if configured to receive sidelink control information for SL-PRS on the frequency included in *sl-FreqInfoList* in *SIB23* of the PCell: | Same reason to Issue 50.Change the highlight part into “SL-PRS”. | yuanli@vivo.com |  |
| 57 | N | 5.8.3.33> if configured to receive sidelink control information for SL-PRS measurements;4> include *sl-PosRxInterestedFreqList* and set it to the frequency for NR sidelink positioning reception. | Same reason to Issue 50.Change the highlight part into “SL-PRS”. | yuanli@vivo.com |  |
| 58 | N | 5.8.18.32> else:3> configure lower layers to perform the sidelink resource allocation scheme 2 based on resource selection operation according to *sl-PosAllowedResourceSelectionConfig* (as defined in TS 38.321 [3] and TS 38.214 [19]) using the pools of resources indicated by *sl-PRS-TxPoolSelectedNormal* in *SL-PosPreconfigurationNR* for the concerned frequency or based on *sl-AllowedResourceSelectionConfig* (as defined in TS 38.321 [3] and TS 38.214 [19]) using the pools of resources indicated by *sl-TxPoolSelectedNormal* in *SidelinkPreconfigNR* for the concerned frequency.. | Repeat input of the period. Delete one. | yuanli@vivo.com |  |
| 59 | N | 6.3.5 *SL-ConfiguredGrantConfigDedicated-SL-PRS-RP*

| *SL-ConfiguredGrantConfig* field descriptions |
| --- |

 | Typo, change the fielf name in the table as” *SL-ConfiguredGrantConfigDedicated-SL-PRS-RP*”.[Lenovo] Covered by #40. | yuanli@vivo.com |  |
| 60 | N | si-RequestConfigMSG1-Repetitionsi-RequestConfigSUL-MSG1-Repetitionsi-RequestConfigRedCap-MSG1-RepetitionposSI-RequestConfigMSG1-RepetitionposSI-RequestConfigSUL-MSG1-RepetitionposSI-RequestConfigRedCap-MSG1-Repetitionrsrp-ThresholdMsg1-RepetitionNum2rsrp-ThresholdMsg1-RepetitionNum4rsrp-ThresholdMsg1-RepetitionNum8preambleTransMax-Msg1-Repetition | The naming of these has been done in singular (repetition). However, other mentions for similar functionality uses plural, e.g. “repetitions”:msg1-Repetitions-r18msg1-Repetitions-Priority-r18Also older examples exists:msg3-Repetitions-r17numberOfMsg3-RepetitionsList-r17In the procedural text, it is also referred to in plural, e.g. “if msg1-Repetitions is included”In some cases, it seems correct to use singular, since they point to a specific repetition number, like 2, 4 or 8, and not a true/false, range or similar:msg1-RepetitionNummsg1-RepetitionTimeOffsetROGroupConsider to rename to plural, e.g. using Repetitions. | oskar.myrberg@ericsson.com |  |
| 61 | N | msg1-RepetitionTimeOffsetROGroup | Correct naming should be msg1-RepetitionTimeOffsetRO-Group | oskar.myrberg@ericsson.com |  |
| 62 | N | 5.8.3.3 Actions related to transmission of *SidelinkUEInformationNR* message5> include *sl-U2U-InfoList* and set its fields (if needed) for each entry as follows, to report the related information of the connected L2 Remote UEs:6> include the source L2 U2U Remote UE’s source L2 destination in *sl-TargetUE-Identity*; | The L2 U2U Relay UE shall “include the source L2 U2U Remote UE’s source L2 destination in *sl-TargetUE-Identity*”, which instead should be *sl-SourceUE-Identity*.Thus, it should be corrected to *sl-SourceUE-Identity*. | lider\_pan@asus.com |  |
| 63 | N | 5.8.3.3 Actions related to transmission of *SidelinkUEInformationNR* message5> set *sl-CapabilityInformationSidelink* to include *UECapabilityInformationSidelink* message(s) received from L2 U2U Relay UE and the peer L2 U2U Remote UE, if any; | The L2 U2U Remote UE shall “set *sl-CapabilityInformationSidelink* to include *UECapabilityInformationSidelink* message received from L2 U2U Relay UE and the peer L2 U2U Remote UE, if any”. Since two *UECapabilityInformationSidelink* messages may be received from L2 U2U Relay UE and the peer L2 U2U Remote UE, it is more precise to use “message(s)” to replace “message”. | lider\_pan@asus.com |  |
| 64 | N | 5.8.3.3 Actions related to transmission of *SidelinkUEInformationNR* message6> set *sl-PerSLRB-QoS-InfoList* to include the first-hop split PDB of the sidelink QoS flow(s) received from the *sl-SplitQoS-InfoListPC5* in *UEInformationResponseSidelink* message for the associated destination in accordance with the received *sl-TargetUE-Identity*; | *sl-PerHop-QoS-InfoList* should be used instead of *sl-PerSLRB-QoS-InfoList*. | lider\_pan@asus.com |  |
| 65 | N | 5.8.9.2.1 GeneralThis clause describes how the UE compiles and transfers its (end-to-end) sidelink UE capability information for unicast to the initiating UE. | It was confirmed in RAN2#124 that the E2E UE capability transfer AS layer procedure should be performed to support L2 U2U Relay. And, the end-to-end sidelink UE capability transfer was captured in Figure 16.12.7-1: Procedure for L2 U2U Remote UE connection establishment in TS 38.300-i00. However, this agreement is missing in the current RRC specification. We think this agreement should also be reflected in the RRC specification. | lider\_pan@asus.com |  |
| 66 | N | 6.3.4 Other information elements***ran-VisibleReportingSRB***The field indicates the SRB to be used for transmission of RAN visible application layer measurement reports. | The description for *ran-VisibleReportingSRB* should be moved down under RAN-VisibleParameters field description (instead of under AppLayerMeasConfig field descriptions) because RAN-VisibleParameters is the parent IE of the *VisibleReportingSRB*. | ping.1.yuan@nokia-sbell.com |  |
| 67 | N | ***idleInactiveReportAllowed***The field indicates whether transmission of application layer measurement reports collected in RRC\_IDLE and/or RRC\_INACTIVE is allowed and if transmission of application layer measurement configurations applicable to RRC\_IDLE and/or RRC\_INACTIVE is allowed. If fhe field is not configured, transmission of application layer measurement reports and/or configurations for RRC\_IDLE/RRC\_INACTIVE are not allowed. | Typo:fhe -> the | ping.1.yuan@nokia-sbell.com |  |
| 68 | N | mce-Id-r18 OCTET STRING (SIZE (1))  ***mce-id***The field contains the Measurement Collection Entity Id, see TS 28.405 [55].AppLayerIdleInactiveConfig-r18 ::= SEQUENCE { configForRRC-IdleInactive-r18 ENUMERATED {true} OPTIONAL, -- Need M1> if *idleInactiveReportAllowed* is not included in the *RRCReconfiguration* message:2> for each application layer measurement configuration with *configforRRC-IdleInactive* set to *true*:1> for each stored application layer measurement configuration with *configforRRC-IdleInactive* set to *true* and for which *appLayerIdleInactiveConfig* has not been transmitted since the UE entered RRC\_CONNECTED*:****measConfigReportAppLayerAvailable***Indication that the UE has stored one or more application layer measurement reports while the UE was in RRC\_IDLE/RRC\_INACTIVE state and/or that the UE is configured with at least one application layer measurement configuration with *configforRRC-IdleInactive* set to *true*. | Field description for mce-id should be corrected as mce-Id to align with ASN.1.The *configforRRC-IdleInactive* should be configForRRC-IdleInactive to align with ASN.1. | ping.1.yuan@nokia-sbell.com |  |
| 69 | Y | 6.3.2EventTriggerConfig::= | Space is needed before ::=Note: this is not an issue introduced in Rel-18. There is same issue for Rel-15 to Rel-17 versions. | zhangyujian@xiaomi.com |  |
| 70 | N | 6.3.2Field description for *pagingPTWLength*Value *ms1280* corresponds to 1280 miliseconds, value *ms2560* corresponds to 2560 miliseconds and so on.Field description for *remainingTimeThreshold*Remaining time threshold used for triggering DSR for the Logical Channel Group, as specified in TS 38.321 [3]. Value in number of miliseconds. | Typo, miliseconds should be milliseconds. | zhangyujian@xiaomi.com |  |
| 71 | N | Naming of T346x (there are 7 instances of T346x) | Should be changed to T346l (as defined in clause 7.1.1). | zhangyujian@xiaomi.com |  |
| 72 | N | 5.10.3.2 Multicast MRB establishmentUpon establishment of a multicast MRB, the UE shall:1> establish a PDCP entity and an RLC entity i n accordance with *MRB-InfoBroadcast* for this multicast MRB included in the *MBSMulticastConfiguration* message and the configuration specified in 9.1.1.7; | The following ‘space’ should be removed.an RLC entity i n accordance | daimz4@Lenovo.com |  |
| 73 | N | 5.10.3.2 Multicast MRB establishmentUpon establishment of a multicast MRB, the UE shall:1> establish a PDCP entity and an RLC entity i n accordance with *MRB-InfoBroadcast* for this multicast MRB included in the *MBSMulticastConfiguration* message and the configuration specified in 9.1.1.7; | ‘MRB-InfoBroadcast’ should be changed to ‘MRB-InfoMulticast’ as follows.accordance with *MRB-InfoMulticast* for this multicast MRB included in | daimz4@Lenovo.com |  |
| 74 | N | 5.7.10.31> if the *successHO-ReportReq* is set to *true* and if the UE has successful handover related information available in *VarSuccessHO-Report* and if the current registered SNPN is included in *snpn-IdentityList* if stored in the *VarSuccessHO-Report*: | Unnecessary “if” before stored1> if the *successHO-ReportReq* is set to *true* and if the UE has successful handover related information available in *VarSuccessHO-Report* and if the current registered SNPN is included in *snpn-IdentityList* ~~if~~ stored in the *VarSuccessHO-Report*: | gyorgy.wolfner@nokia.com |  |
| 75 | N | 5.7.10.31> if the *successPSCell-ReportReq* is set to *true* and if the UE has successful PSCell change or addition information available in *VarSuccessPSCell-Report* and if the current registered SNPN is included in *snpn-IdentityList* if stored in the *VarSuccessPSCell-Report*: | Unnecessary “if” before stored1> if the *successPSCell-ReportReq* is set to *true* and if the UE has successful PSCell change or addition information available in *VarSuccessPSCell-Report* and if the current registered SNPN is included in *snpn-IdentityList* if stored in the *VarSuccessPSCell-Report*: | gyorgy.wolfner@nokia.com |  |
| 76 | N | 5.7.10.41> if the registered SNPN or the SNPN selected by upper layers (see TS24.501 [23]) from the list of SNPN(s) included in the *NPN-IdentityInfoList* in *SIB1*is not included in *plmn-IdentityList* stored in a non-empty *VarRA-Report*: | Space is missing after SIB11> if the registered SNPN or the SNPN selected by upper layers (see TS24.501 [23]) from the list of SNPN(s) included in the *NPN-IdentityInfoList* in *SIB1* is not included in *plmn-IdentityList* stored in a non-empty *VarRA-Report*: | gyorgy.wolfner@nokia.com |  |
| 77 | N | 5.8.9.7.11> for unicast in L2 U2U relay operation, if there is no end-to-end sidelink DRB(s) associated with this RLC channel: | Rewording proposal to make the text cleaner:1> for ~~unicast in~~ L2 U2U relay ~~operation~~, if there is no end-to-end sidelink DRB~~(s)~~ associated with ~~this~~ the PC5 Relay RLC channel: | gyorgy.wolfner@nokia.com |  |
| 78 | N | 5.8.9.7.12> for each *SL-RLC-ChannelID* in *sl-RLC-ChannelToReleaseList* received in *sl-ConfigDedicatedNR* within *RRCReconfiguration,* or for each *SL-RLC-ChannelID* included in the received *sl-RLC-ChannelToReleaseListPC5* that is part of the current UE sidelink configuration, or for the RLC channel to be released: | Rewording proposal, as the current text is not very clear:2> for each *SL-RLC-ChannelID* in *sl-RLC-ChannelToReleaseList* received in *sl-ConfigDedicatedNR* within *RRCReconfiguration,* or for each *SL-RLC-ChannelID* included in the received *sl-RLC-ChannelToReleaseListPC5* that is part of the current UE sidelink configuration, or for the SL-RLC ChannelID in L2 U2U relay that has no associated end-to-end sidelink DRB~~channel to be released~~: | gyorgy.wolfner@nokia.com |  |
| 79 | N | 5.8.15.32> if the UE has a selected NR sidelink U2N Relay UE, and upper layers request the release of the PC5-RRC connection; or | Additional clarification to make to text unambiguous:2> if the UE has a selected NR sidelink U2N Relay UE, and upper layers request the release of the PC5-RRC connection to the selected NR sidelink U2N Relay UE; or | gyorgy.wolfner@nokia.com |  |
| 80 | N | 5.3.13.1c:2> if the frequency on which the UE is configured to transmit NR sidelink positioning is included in *sl-FreqInfoList* within *SIB25* provided by the cell on which the UE camps; and if the valid version of *SIB25* does not include *sl-PRS-TxPoolSelectedNormal* for the concerned frequency; | * The two references to SIB25 should be replaced by "*SIB23*".
* Semicolon should be replaced by dot.
 | hchoi5@lenovo.com |  |
| 81 | N | 5.3.13.6:1> else if cell reselection occurs when *srs-PosRRC-InactiveValidityAreaConfig* is configured and if the cell is included in the *srs-PosRRC-InactiveValidityAreaConfig*:2> if *autonomousTA-AdjustmentEnabled* is configured;3> indicate to the lower layer to update Timing Advance and stored RSRP. | Replace semicolon by colon. | hchoi5@lenovo.com |  |
| 82 | N | 5.8.18.3:6> if sl-TxPoolExceptional or sl-PRS-TxPoolExceptional for the concerned frequency is included in RRCReconfiguration; or6> if the PCell provides SIB25 including sl-TxPoolExceptional or sl-PRS-TxPoolExceptional in sl-FreqInfoList for the concerned frequency:…6> configure lower layers to perform the sidelink resource allocation scheme 2 based on resource selection operation according to *sl-PosAllowedResourceSelectionConfig* (as defined in TS 38.321 [3] and TS 38.214 [19]) using the pools of resources indicated by *sl-PRS-TxPoolSelectedNormalNormal* for the concerned frequency, or based on resource selection operation according to *sl-AllowedResourceSelectionConfig* (as defined in TS 38.321 [3] and TS 38.214 [19]) using the pools of resources indicated by *sl-TxPoolSelectedNormal* for the concerned frequency; | * References to field names and RRC message should be set in italics.
* Reference to SIB25 should be replaced by “*SIB23*”.
* Remove redundant “Normal” from name sl-PRS-TxPoolSelectedNormalNormal.
 | hchoi5@lenovo.com |  |
| 83 | Y | 6.3.2, SRS-PosTx-Hopping:-- ASN1START-- TAG- SRS-PosTx-Hopping-START***SRS-PosUplinkTransmissionWindowConfig* field descriptions** | * Redundant space in the START tag name should be removed.
* In the title of field descriptions “*SRS-PosUplinkTransmissionWindowConfig*” should be replaced by “*SRS-PosTx-Hopping*”.
 | hchoi5@lenovo.com |  |
| 84 | Y | 6.3.5, SL-ReportConfigList:SL-RS-Type-r16 ::= ENUMERATED {dmrs, sl-prs, spare2, spare1} | In SL-RS-Type-r16 the suffix “-v1800” should be added to new value “sl-prs”. | hchoi5@lenovo.com |  |
| 85 | Y | 6.3.5, SL-ResourcePool:sl-SCI-based-SL-PRS-Tx-Trigger-SCI2-D-r18 BOOLEAN OPTIONAL, -- Need M sl-TriggerConditionRequest-r17 INTEGER (0..1) OPTIONAL -- Need M | Suffix of field sl-TriggerConditionRequest-r17 should be “-r18”. | hchoi5@lenovo.com |  |
| 86 | N | 6.2.2, DLInformationTransfer:

|  |
| --- |
| Conditional Presence |
| ***clockQualityDetailsLevel*** |

 | Name of condition “clockQualityDetailsLevel” should not be set in bold. | hchoi5@lenovo.com |  |
| 87 | N | ***eDRX-AllowedInactive***The presence of *eDRX-AllowedInactive-r17* this field indicates that extended DRX cycle equal to or shorter than 10.24 s for RAN paging is allowed in the cell for UEs in RRC\_INACTIVE. The UE shall stop using extended DRX cycle equal to or shorter than 10.24 s for RAN paging in RRC\_INACTIVE if *eDRX-AllowedInactive-r17* is not present. The presence of *eDRX-AllowedInactive-r18* indicates that extended DRX cycle longer than 10.24 s for RAN paging is allowed in the cell for UEs in RRC\_INACTIVE. The UE shall stop using extended DRX cycle longer than 10.24 s for RAN paging in RRC\_INACTIVE if *eDRX-AllowedInactive-r18* is not present. | Typo“this field” should be removed | lihaitao@oppo.com |  |
| 88 | N | 5.3.2.3Existing text:2> if the UE is not configured to receive multicast in RRC\_INACTIVE or if *inactiveReceptionAllowed* is not included for at least one of the MBS session (s) indicated by the *TMGI(s)* that the UE has joined:New text:2> if the UE is not configured to receive multicast in RRC\_INACTIVE or if *inactiveReceptionAllowed* is not included for at least one of the MBS sessions indicated by the *TMGI(s)* that the UE has joined: | When you say “for at least one”, it should be MBS sessions. Otherwise, it should be “for one or more MBS session(s)”. My understanding is, here we intended to say for at least one of the MBS sessions. | mani.thyagarajan@nokia.com |  |
| 89 | N | 5.3.2.3Existing text:3> start monitoring the G-RNTI(s) corresponding to the *TMGI(s),* if configured;New text:3> start monitoring the G-RNTI(s), if configured, corresponding to the *TMGI(s)*; | I believe "if configured" is about G-RNTI(s). If so, it should be moved closer to G-RNTI. If it is about TMGI(s), then the current text is fine. | mani.thyagarajan@nokia.com |  |
| 90 | N | 5.3.13.1dExisting text:5.3.13.1d RRC connection resume for multicast receptionNew text:5.3.13.1d Conditions for resuming RRC connection ~~resume~~ for multicast reception | To align with other subsections under this section, the heading can be changed to say “Conditions for resuming RRC connection for multicast reception” | mani.thyagarajan@nokia.com |  |
| 91 | N | 5.3.13.1dExisting text:1> if the PTM configuration is not available in the cell after cell selection or reselection for a multicast session that the UE has joined for which the UE is not indicated to stop monitoring the G-RNTI; orNew text:1> if the PTM configuration is not available in the cell after cell selection or reselection, for a multicast session that the UE has joined and for which the UE is not indicated to stop monitoring the G-RNTI; or | Difficult to read this bullet. Some punctuation and addition of text can make it readable | mani.thyagarajan@nokia.com |  |
| 92 | N | 5.9.4.2Existing text:2> ensure having a valid version of *SIB21* for the PCell, if present;New text:2> ensure having a valid version of *SIB21* for the PCell, if provided by the PCell; | Align the wording to the wording used in the condition in first level bullet where it says:1> if *SIB21* is provided by the PCell; or | mani.thyagarajan@nokia.com |  |
| 93 | N | 5.9.4.2Existing text:3> if the set of MBS broadcast frequencies of interest for MBS broadcast reception on non-serving cell, determined in accordance with 5.9.4.3, is different from the list of MBS broadcast frequencies of interest for MBS broadcast reception on non-serving cell included in the last transmission of the MBS Interest Indication; orNew text:3> if the set of MBS broadcast frequencies of interest for MBS broadcast reception on non-serving cell, determined in accordance with 5.9.4.3, is different from ~~the list of MBS broadcast frequencies of interest for MBS broadcast reception on non-serving cell~~ *freqInfoMBS* included in the last transmission of the MBS Interest Indication; or | A long text can be made concise by replacing it by "*freqInfoMBS*" | mani.thyagarajan@nokia.com |  |
| 94 | N | 5.10.1.1Existing text:UE configured to receive MBS multicast service(s) in RRC\_INACTIVE that the UE has joined applies MBS multicast procedures described in this clause.New text:A UE configured to receive MBS multicast service~~(s)~~ in RRC\_INACTIVE ~~that~~ for multicast service(s) that the UE has joined applies MBS multicast procedures described in this clause. | Some text improvement suggestions here | mani.thyagarajan@nokia.com |  |
| 95 | N | 5.10.1.1Existing text:Optionally, the *MBSMulticastConfiguration* message may also contain a list of neighbour cells providing the same MBS multicast service(s) for RRC\_INACTIVE as provided in the current cell.New text:Optionally, the *MBSMulticastConfiguration* message may also contain a list of neighbour cells providing the same MBS multicast service(s) for reception in RRC\_INACTIVE as provided in the current cell. | Some text improvement suggestions here | mani.thyagarajan@nokia.com |  |
| 96 | Y | 6.2.2Field name: mbs-NonServingInfoList-r18New name: mbs-NonServingCellInfoList-r18 | Suggestion to change the field name | mani.thyagarajan@nokia.com |  |
| 97 | N | 6.2.2Field description for ***mbs-SessionInfoList***Existing text:Provides the configuration of each MBS session provided by MBS multicast in the current cell.New text:Provides the configuration of multicast MBS session(s) in the current cell | Some text improvement suggestions here | mani.thyagarajan@nokia.com |  |
| 98 | Y | 6.2.2Field name: ***nonServingCellMII***New name: ***miiForNonServingCellBroadcast*** | Suggestion to change the field name | mani.thyagarajan@nokia.com |  |
| 99 | Y | 6.3.6Field name: *MBS-NonServingInfoList*New name: *MBS-NonServingCellInfoList* | Suggestion to change the field name | mani.thyagarajan@nokia.com |  |
| 100 | Y | 6.3.6Field name: cfr-Bandwidth-r18. But in the field description it says cfr-BandwidthMBSNew name: cfr-BandwidthMBS-r18 | Here the field name in ASN.1 and in the field description are not aligned | mani.thyagarajan@nokia.com |  |
| 101 | N | 5.3.5.13.4NOTE 3: For CHO with candidate SCGs, up to 2 MeasId can be configured for condExecutionCond and up to 2 MeasId can be configured for condExecutionCondPSCell for each condReconfigId. | Should be “SCG(s)”. | zhang.mengjie@zte.com.cn |  |
| 102 | N | 5.3.5.13.81> use the default values specified in 9.2.3 for timers T310, T311 and constants N310, N311 associate to cell group for which the LTM cell switch procedure is triggered; | Should be “associated” | zhang.mengjie@zte.com.cn |  |
| 103 | N | 5.3.5.18.62> replace the value of ltm-ServingCellUE-MeasuredTA-ID in VarLTM-ServingCellUE-MeasuredTA-ID with the value received within ltm-UE-MeasuredTA-ID; | Missing italics. | zhang.mengjie@zte.com.cn |  |
| 104 | N | 5.3.5.18.71> release from current UE configuration all entries of ltm-CSI-ReportConfigToAddModList.1> release ltm-Config; | Wrong indentation. It should be:1> release from current UE configuration all entries of ltm-CSI-ReportConfigToAddModList.1> release ltm-Config; | zhang.mengjie@zte.com.cn |  |
| 105 | N | 5.5.2.2 Measurement identity removalThe UE shall:1> for each *measId* included in the received *measIdToRemoveList* that is part of the current UE configuration in *VarMeasConfig*:2> remove the entry with the matching *measId* from the *measIdList* within the *VarMeasConfig*;2> remove the measurement reporting entry for this *measId* from the *VarMeasReportList*, if included;2> stop the periodical reporting timer or timer T321 or timer T322, whichever one is running, and reset the associated information (e.g. *timeToTrigger*) for this *measId*.2> if the *reportType* is set to *reportOnActivation* in the *reportConfig* associated with this *measId*:… | Incorrect signaling name. According to the ASN.1, the correct name is *reportOnScellActivation* | song.xiaohui@zte.com.cn |  |
| 106 | N | 5.5.2.3 Measurement identity addition/modification... 2> if the *reportType* is set to *reportOnActivation* in the *reportConfig* associated with this *measId*:3> indicate to lower layer to enable the measurement reporting for fast unknown SCell activation. | Same as above：Incorrect signaling name. According to the ASN.1, the correct name is *reportOnScellActivation* | song.xiaohui@zte.com.cn |  |
| 107 | N | 5.5.4.14> if the eventH1 or eventH2 is configured in the corresponding reportConfig:5> for all the events of the same type for which simulMultiTriggerSingleMeasReport is set to true and the entry condition applicable for the event has been satisfied:6> consider only the event with the smallest value between the altitude of the UE and the corresponding altitude threshold to be applicable;4> else if the eventA3H1 or eventA3H2 or eventA4H1 or eventA4H2 or eventA5H1 or eventA5H2 is configured in the corresponding reportConfig:5> for all the events of the same type associated with the same measObjectNR for which simulMultiTriggerSingleMeasReport is set to true and the entry conditions applicable for the event has been satisfied:6> consider only the event with the smallest value between the altitude of the UE and the corresponding altitude threshold to be applicable; | Unclear description. For all events, each event needs to satisfy the entry condition.“…the entry condition applicable for each event has been satisfied” | yuanli@vivo.com |  |
| 108 | N | 6.2.2

|  |
| --- |
| ***flightPathInfoReq***This field is used to indicate whether the UE can report information about the flight path information, if available, and to specify the flight path information report configuration. |

 | Redundant description.“information about” should be removed. | yuanli@vivo.com |  |
| 109 | No | 5.7.10.73> include *sn-InitiatedPSCellChange* if *sn-InitiatedPSCellChange* is included in the *RRCReconfiguration* including the applied *RRCReconfiguration* message with *reconfigurationWithSync* for the SCG; | It would be cleaner to put the condition 1st and then the action as a separate step:3> ~~include~~ *~~sn-InitiatedPSCellChange~~* if *sn-InitiatedPSCellChange* is included in the *RRCReconfiguration* including the applied *RRCReconfiguration* message with *reconfigurationWithSync* for the SCG~~;~~:4> include *sn-InitiatedPSCellChange*; | gyorgy.wolfner@nokiacom |  |
| 110 | N |

|  |
| --- |
| *CSI-AssociatedReportConfigInfo* field descriptions |
| ***applyIndicatedTCI-State,*** ***applyIndicatedTCI-State2***This field indicates, for an aperiodic CSI-RS resource set (perSet) or for CSI-RS resource (perResource), if UE applies the first or the second "indicated" DL only TCI or joint TCI as specified in TS 38.214 [19], clause 5.1.5. If more than one value for the field *coresetPoolIndex* is configured in the DL BWP used to trigger the CSI report, the value 'first' corresponds to the "indicated" joint/DL TCI states specific to *coresetPoolIndex* value 0 and the value 'second' correspond to the value 1, respectively. The *applyIndicatedTCI-State* is for *ResourcesForChannel*, and *applyIndicatedTCI-State2* is for *ResourcesForChannels2.* |

 | The first letter of *ResourcesForChannel* should be lowercase.The name of *ResourcesForChannels2* is incorrect. According to the ASN.1, the correct name is *resourcesForChannel2*. | wangda@catt.cn |  |
| 111 | N |

|  |
| --- |
| ***tci-SelectionPresentIn-DCI***Indicates if a [TCI selection field] is present or absent in DCI format 1\_1 and DCI format 1\_2 for a DL BWP, see reference XXX. |

 | The reference should be added as TS38.212 [17] clause 7.3.1.2 and TS38.214[19] clause 5.1.5. | wangda@catt.cn |  |
| 112 | N |

|  |
| --- |
| ***reportingMode***Configures the UE with reporting mode for group based reporting.(see TS XXXXXX) |

 | The reference should be added as TS38.214 [19] clause 5.2.1.4.2. | wangda@catt.cn |  |
| 113 | Y | CodebookConfig-r18 ::= SEQUENCE { codebookType CHOICE { type2 SEQUENCE { typeII-CJT-r18 SEQUENCE { | The codebookType should add suffix “-r18”. | wangda@catt.cn |  |
| 114 | Y | tci-SelectionPresentIn-DCI-r18 ENUMERATED { enabled } OPTIONAL, -- Need RapplyIndicatedTCI-StateDCI-1-0-r18 ENUMERATED {first, second, both} OPTIONAL -- Need R

|  |
| --- |
| ***tci-SelectionPresentIn-DCI***Indicates if a [TCI selection field] is present or absent in DCI format 1\_1 and DCI format 1\_2 for a DL BWP, see reference XXX. |

 | The name of “tci-SelectionPresentIn-DCI-r18” should be “tci-SelectionPresentInDCI-r18”. | wangda@catt.cn |  |
| 115 | Y | DelayD ::= ENUMERATED { symb4, slot1, slot2, slot3, slot4, slot5, slot6, slot10 } | The IE DelayD should add suffix “-r18”. | wangda@catt.cn |  |
| 116 | N |

|  |
| --- |
| ***srs-ResourceSetId***Indicates the associated SRS resource set for PUSCH+PUSCH simultaneous uplink transmsision for CG-type 1 PUSCH. |

 | Typo. It should be “transmission”. | wangda@catt.cn |  |
| 117 | N |

|  |
| --- |
| ***tag2-flag***If this field is set to *true*, the *tag2-Id* is associated to value 0 and *tag-Id* is associated to value 1 of field TI bit in RAR , fallbackRAR and in the absolute TAC MAC CE, see TS 38.321 [3]. Otherwise, the *tag2-Id* is associated to value 1 and tag-Id is associated to value 0 of field R bit in RAR, fallbackRAR and in the absolute TAC MAC CE, see TS 38.321 [3]. |

 | In RAR, the R bit is already defined as TI bit. Thus, the “R bit” in second sentence should be “TI bit”, which is the same as first sentence. | wangda@catt.cn |  |
| 118 | Y |

|  |
| --- |
| ***n-TimingAdvanceOffset***The N\_TA-Offset to be applied for all uplink transmissions on this serving cell if *n-TimingAdvanceOffset* is not configured. If *tag2* is configured for this serving cell, this field is to be applied to all uplink transmissions associated to *tag-id* configured for this serving cell. If the field is absent, the UE applies the value defined for the duplex mode and frequency range of this serving cell. See TS 38.133 [14], table 7.1.2-2. |

 | In the first sentence, “*n-TimingAdvanceOffset*” should be “*n-TimingAdvanceOffset2*”, since this field description is applied for *n-TimingAdvanceOffset*. | wangda@catt.cn |  |
| 119 | N | 5.3.8.3 Reception of the *RRCRelease* by the UE2> if *srs-PosRRC-InactiveValidityAreaConfig* is configured:3> apply the configuration and instruct MAC to start the *inactivePosSRS-ValidityAreaTAT*;[...]2> if the *multicastConfigInactive* is configured:3> if the multicast PTM configuration is provided for a multicast session for which the UE is not indicated to stop monitoring the G-RNTI and the UE selects the same cell as the one on which it received *RRCRelease*:5.3.5.3 Reception of an RRCReconfiguration by the UE1> if the *RRCReconfiguration* message includes the *uav-Config*:2> (re)configure the UAV parameters in accordance with the included *uav-Config*;(Note that above is not a full list, and the problem may also exist in other places of the Spec.) | All the fields included in the highlighted sentences are with "SetupRelease" signalling structure, but they are now described with the wording like “Is configured” or “include”. Such wording does not align with the guideline in A3.8 on how to describe the "SetupRelease" related operations, and may lead to wrong UE behaviour. 1> if *field-rX* is set to "setup":2> do something;1> else (*field-rX* is set to "release"):2> release *field-rX* (if appropriate).So we suggest aligning the wording used in the procedure wherever the "SetupRelease" parameter is involved.[Lenovo] This issue is not editorial. Since it affects different features, it should be better discussed and resolved in the WI-specific sessions. | xiaoxiao@catt.cn |  |
| 120 | N | ***interFreqCarrierFreqList***List of neighbouring carrier frequencies and frequency specific cell re-selection information. If *interFreqCarrierFreqList-v1610, interFreqCarrierFreqList-v1700, interFreqCarrierFreqList-v1720*, *interFreqCarrierFreqList-v1730,* *interFreqCarrierFreqList-v1760* or *InterFreqCarrierFreqInfo-v1800* are present, they shall contain the same number of entries, listed in the same order as in *interFreqCarrierFreqList* (without suffix). | Need changing to "*InterFreqCarrierFreq~~Info~~List-v1800*".[Lenovo] Agree but capital letter “I” in “Inter” should be set in lowercase letter. | xiaoxiao@catt.cn |  |
| 121 | Y | [[ pdu-SessionIdList-r18 SEQUENCE (SIZE (1..maxNrofPDU-Sessions-r17)) OF QFI-List-r18 OPTIONAL ]] | Suffix should be “-v18xy” but not "-r18" (since it is an NCE, not an revision)[Lenovo] This issue has been already raised in RIL by I107. | xiaoxiao@catt.cn |  |
| 122 | Y | SEQUENCE { successHO-Config-r18 SetupRelease {SuccessHO-Config-r17} OPTIONAL, nonCriticalExtension SEQUENCE {} OPTIONAL} | Lack of Need Code. Should be "Need M".[Lenovo] This issue is not editorial. Furthermore, it has been already raised in RIL by Z523. | xiaoxiao@catt.cn |  |
| 123 | Y | InterFreqCarrierFreqInfo... [[ mobileIAB-Freq ENUMERATED {true} OPTIONAL -- Need R ]] | Move the field into InterFreqCarrierFreqInfo-v1800, and add suffix "-r18".[Lenovo] This issue is not editorial. Furthermore, it has been already raised in RIL by B002. | xiaoxiao@catt.cn |  |
| 124 | N | 5.8.9.11.34> set *sl-SplitQoS-InfoListPC5* to include the split PDB value for each QoS flow on the fisrt PC5 hop between L2 U2U Relay UE and L2 U2U Remote UE; | Typo4> set *sl-SplitQoS-InfoListPC5* to include the split PDB value for each QoS flow on the first PC5 hop between L2 U2U Relay UE and L2 U2U Remote UE; | kawano.takuma@sharp.co.jp |  |
| 125 | N | 5.8.9.34> initiate the RRC connection re-establishment procedure as specified in 5.3.7. | Typo4> initiate the RRC connection re-establishment procedure as specified in 5.3.7; | kawano.takuma@sharp.co.jp |  |
| 126 | Y | 6.2.2 sl-MeasResultServingRelay-r18 OCTET STRING OPTIONAL, -- Contains PC5 SL-MeasResultRelay-r17 sl-MeasResultsCandRelay-r18 OCTET STRING OPTIONAL, | Similar to *sl-MeasResultServingRelay-r18*, we need a description of what's included in *sl-MeasResultsCandRelay-r18*. sl-MeasResultServingRelay-r18 OCTET STRING OPTIONAL, -- Contains PC5 SL-MeasResultRelay-r17 sl-MeasResultsCandRelay-r18 OCTET STRING OPTIONAL, -- Contains PC5 SL-MeasResultRelay-r17 | kawano.takuma@sharp.co.jp |  |
| 127 | N | 6.2.2Existing text:***inactivePosSRS-ValidityAreaTAT***Time alignment timer value for SRS for positioning transmission during RRC\_INACTIVE state which is applicable in a validity area.New text:***inactivePosSRS-ValidityAreaTAT***Validity area-specific Time alignment timer value for SRS for positioning transmission during RRC\_INACTIVE state. | Some text improvements suggested. | mani.thyagarajan@nokia.com |  |
| 128 | Y | 6.2.2Existing text:srs-PosResourceSetLinkedForAggBWListNew text:srs-PosLinkedResSetsBWA-List | Suggestion for renaming a field. | mani.thyagarajan@nokia.com |  |
| 129 | Y | 6.2.2Existing text:srs-PosResSetLinkedForAggBWInactiveList New text:srs-PosLinkedResSetsBWA-Inactive-List | Suggestion for renaming a field. Keeping the same name and differentiating by adding “Inactive” at the end before -List is easy to read and differentiate the connected state and inactive state fields. | mani.thyagarajan@nokia.com |  |
| 130 | Y | 6.2.2Existing text:srs-PosRRC-AggBW-InactiveConfigListNew text:srs-PosConfigBWA-Inactive-List | Suggestion for renaming a field. | mani.thyagarajan@nokia.com |  |
| 131 | N | 6.3.2 *SRS-PosResourceSetLinkedForAggBW* field descriptionsExisting text:***freqInfo***Indicates the SRS Positioning Resource set carrier frequency that is linked for bandwidth aggregation.New text:***freqInfo***Indicates the carrier frequency of the SRS for Positioning Resource set that is linked for bandwidth aggregation. | Some text improvements suggested. | mani.thyagarajan@nokia.com |  |
| 132 | N | 6.3.2 *SRS-PosResourceSetLinkedForAggBW* field descriptionsExisting text:***ul-bwp-ID***Indicates the SRS Positioning Resource set uplink bandwidth ID that is linked for bandwidth aggregation.New text:***ul-bwp-ID***Indicates the uplink BWP of the SRS for Positioning Resource set that is linked for bandwidth aggregation | Some text improvements suggested. | mani.thyagarajan@nokia.com |  |
| 133 | N | 6.3.1, SIB4, the field description of interFreqCarrierFreqList has a typo. It should refer to the frequency list, and not the entry within the list. | ***interFreqCarrierFreqList***List of neighbouring carrier frequencies and frequency specific cell re-selection information. If *interFreqCarrierFreqList-v1610*, *interFreqCarrierFreqList-v1700*, *interFreqCarrierFreqList-v1720*, *interFreqCarrierFreqList-v1730*, *interFreqCarrierFreqList-v1760* or *~~I~~interFreqCarrierFreqList~~Info~~-v1800* are present, they shall contain the same number of entries, listed in the same order as in *interFreqCarrierFreqList* (without suffix).[Lenovo] Agree, see also #120. | pradeep.jose@mediatek.com |  |
| 134 | N | 6.3.3, BandCombinationList, there is an IE name typo in the field description of BandCombinationList-UplinkTxSwitch (with suffix). | ***BandCombinationList-UplinkTxSwitch-r16***, ***BandCombinationList-UplinkTxSwitch-v1630***, ***BandCombinationList-UplinkTxSwitch-v1640***, ***BandCombinationList-UplinkTxSwitch-v1650***, ***BandCombinationList-UplinkTxSwitch-v1690***, ***BandCombinationList-UplinkTxSwitch-v16a0***, ***BandCombinationList-UplinkTxSwitch-v16e0***, ***BandCombinationList-UplinkTxSwitch-v1700***, ***BandCombinationList-UplinkTxSwitch-v1720***, ***BandCombinationList-UplinkTxSwitch-v1730***, ***BandCombinationList-UplinkTxSwitch-v1760***, ***BandCombinationList-UplinkTxSwitch-v1770***, ***BandCombinationList-UplinkTxSwitch-v1800*** | morton.lin@mediatek.com |  |
| 135 | Y | 6.4, Multiplicity and type constraints definitions, there is a typo. | maxULTxSwitchingBetweenBandPairs-r18 INTEGER ::= 32 -- Maximum number of combinations of a band pair and another band pair/band -- between which ~~dyanmic~~dynamic UL Tx switching requires additional switching -- period. | morton.lin@mediatek.com |  |
| 136 | Y | 6.3, RF-ParametersMRDC, there is wrong definition IE. |  ]], [[ supportedBandCombinationList-v1800 BandCombinationList-v1800 OPTIONAL, supportedBandCombinationList-UplinkTxSwitch-v1800 BandCombinationList-UplinkTxSwitch-v1800 OPTIONAL ]] | morton.lin@mediatek.com |  |
| 137 | N | 5.3.5.18.6, wrong indentation in bulleted list. The bullet 2> replace the value of *ltm-ServingCellNoResetID* in *VarLTM-ServingCellNoResetID* … should be indented more. | 4> after the end of this procedure, trigger the PDCP entity of this DRB to perform data recovery as specified in TS 38.323 [5], after applying the LTM configuration in *ltm-CandidateConfig* within *LTM-Candidate IE* in *VarLTM-Config*;2> replace the value of *ltm-ServingCellNoResetID* in *VarLTM-ServingCellNoResetID* with the value of *ltm-NoResetID* in the *LTM-Candidate* in *VarLTM-Config* indicated by lower layers or for the selected cell in accordance with 5.3.7.3;1> if the *LTM-Candidate IE* in *VarLTM-Config* indicated by lower layers or for the selected cell in accordance with 5.3.7.3 contains the field *ltm-UE-MeasuredTA-ID*:2> replace the value of ltm-ServingCellUE-MeasuredTA-ID in VarLTM-ServingCellUE-MeasuredTA-ID with the value received within ltm-UE-MeasuredTA-ID; | li-chuan.tseng@mediatek.com |  |
| 138 | N | 5.3.5.18.3, the entry of *ltm-DL-OrJointTCI-StateToReleaseList* does not contain field named as *tci-StateId*. The entry itself is a TCI state ID (of type *TCI-StateId*). | 2> if the received *LTM-Candidate* includes *ltm-DL-OrJointTCI-StateToReleaseList*: 3> for each *TCI-StateId~~tci-StateId~~* in the *ltm-DL-OrJointTCI-StateToReleaseList*: 4> if the current *VarLTM-Config* includes a *CandidateTCI-State* within an *LTM-Candidate* with the *ltm-CandidateId* value that is associated with the *TCI-StateId~~tci-StateId~~* value: 5> remove the entry related to *CandidateTCI-State* within the *LTM-Candidate* from *VarLTM-Config*. | li-chuan.tseng@mediatek.com |  |
| 139 | N | 5.3.5.18.3, Handling of *ltm-DL-OrJointTCI-StateToAddModList* could be written in clearer way. |  4> if the current *VarLTM-Config* includes a *CandidateTCI-State* within an *LTM-Candidate* with the *ltm-CandidateId* value that is associated with the *tci-StateId* value: 5> replace the *CandidateTCI-State* within *LTM-Candidate* in the current *VarLTM-Config* with the received *CandidateTCI-State*~~entry related to~~ *~~CandidateTCI-State~~* ~~within the~~ *~~LTM-Candidate~~* ~~from~~ *~~VarLTM-Config~~*. 4> else: 5> add the received *CandidateTCI-State* within *LTM-Candidate* to *VarLTM-Config*; | li-chuan.tseng@mediatek.com |  |
| 140 | N | 5.3.5.18.3, Handling of *ltm-UL-TCI-StatesToAddModList* could be written in clearer way. |  4> if the current *VarLTM-Config* includes an *CandidateTCI-UL-State* within an *LTM-Candidate* with the *ltm-CandidateId* value that is associated with the *tci-StateId* value: 5> replace the *CandidateTCI-UL-State* within *LTM-Candidate* in the current *VarLTM-Config* with the received *CandidateTCI-UL-State*~~entry related to~~ *~~CandidateTCI-UL-State~~* ~~within the~~ *~~LTM-Candidate~~* ~~from~~ *~~VarLTM-Config~~*. 4> else: 5> add the received *CandidateTCI-UL-State* within *LTM-Candidate* to *VarLTM-Config*. | li-chuan.tseng@mediatek.com |  |
| 141 | N | 5.3.5.18.3, The entry of *ltm-nzp-CSI-RS-ResourceToReleaseList* does not contain field named as *nzp-CSI-RS-ResourceId*. The entry itself is a NZP-CSI-RS resource ID (of type *NZP-CSI-RSI-ResourceId*). | 2> if the received *LTM-Candidate* includes *ltm-nzp-CSI-RS-ResourceToReleaseList*: 3> for each *NZP-CSI-RSI-ResourceId~~nzp-CSI-RS-ResourceId~~* in the *ltm-nzp-CSI-RS-ResourceToReleaseList*: 4> if the current *VarLTM-Config* includes an *NZP-CSI-RS-Resource* within an *LTM-Candidate* with the *ltm-CandidateId* value that is associated with the *NZP-CSI-RSI-ResourceId~~nzp-CSI-RS-ResourceId~~* value: 5> remove the entry related to *NZP-CSI-RS-Resource* within the *LTM-Candidate* from *VarLTM-Config*. | li-chuan.tseng@mediatek.com |  |
| 142 | N | 5.3.5.18.3, Handling of *ltm-nzp-CSI-RS-ResourceToAddModList* could be written in clearer way. | 4> if the current *VarLTM-Config* includes an *NZP-CSI-RS-Resource* within an *LTM-Candidate* with the *ltm-CandidateId* value that is associated with the *nzp-CSI-RS-ResourceId* value: 5> replace the *NZP-CSI-RS-Resource* within *LTM-Candidate* in the current *VarLTM-Config* with the received *NZP-CSI-RS-Resource*~~entry related to NZP-CSI-RS-Resource within the LTM-Candidate from VarLTM-Config~~. 4> else: 5> add the received *NZP-CSI-RS-Resource* within *LTM-Candidate* to *VarLTM-Config*. | li-chuan.tseng@mediatek.com |  |
| 143 | N | 5.3.5.18.3, The entry of *ltm-nzp-CSI-RS-ResourceSetToReleaseList* does not contain field named as *nzp-CSI-RS-ResourceSetId*. The entry itself is a NZP-CSI-RS resource set ID (of type *NZP-CSI-RSI-ResourceSetId*). | 2> if the received *LTM-Candidate* includes *ltm-nzp-CSI-RS-ResourceSetToReleaseList*: 3> for each *NZP-CSI-RSI-ResourceSetId~~nzp-CSI-RS-ResourceSetId~~* in the *ltm-nzp-CSI-RS-ResourceSetToReleaseList*: 4> if the current *VarLTM-Config* includes an *NZP-CSI-RS-ResourceSet* within an *LTM-Candidate* with the *ltm-CandidateId* value that is associated with the *NZP-CSI-RSI-ResourceSetId~~nzp-CSI-RS-ResourceSetId~~* value: 5> remove the entry related to *NZP-CSI-RS-ResourceSet* within the *LTM-Candidate* from *VarLTM-Config*. | li-chuan.tseng@mediatek.com |  |
| 144 | N | 5.3.5.18.3, Handling of *ltm-nzp-CSI-RS-ResourceSetToAddModList* could be written in clearer way. | 4> if the current *VarLTM-Config* includes an *NZP-CSI-RS-ResourceSet* within an *LTM-Candidate* with the *ltm-CandidateId* value that is associated with the *nzp-CSI-RS-ResourceSetId* value: 5> replace the *NZP-CSI-RS-ResourceSet* within *LTM-Candidate* in the current *VarLTM-Config* with the received *NZP-CSI-RS-ResourceSet*~~entry related to~~ *~~NZP-CSI-RS-ResourceSet~~* ~~within the~~ *~~LTM-Candidate~~* ~~from~~ *~~VarLTM-Config~~*. 4> else: 5> add the received *NZP-CSI-RS-ResourceSet* within *LTM-Candidate* to *VarLTM-Config*. | li-chuan.tseng@mediatek.com |  |
| 145 | N | 5.3.5.18.3, The entry of *pathlossReferenceRS-ToReleaseList* does not contain field named as *pathlossReferenceRS-Id*. The entry itself is a pathloss reference RS ID (of type *PathlossReferenceRS-Id*). | 2> if the received *LTM-Candidate* includes *pathlossReferenceRS-ToReleaseList*: 3> for each *PathlossReferenceRS-Id~~pathlossReferenceRS-Id~~* in the *pathlossReferenceRS-ToReleaseList*: 4> if the current *VarLTM-Config* includes an *PathlossReferenceRS* within an *LTM-Candidate* with the *ltm-CandidateId* value that is associated with the *PathlossReferenceRS-Id~~pathlossReferenceRS-Id~~* value: 5> remove the entry related to *PathlossReferenceRS* within the *LTM-Candidate* from *VarLTM-Config*. | li-chuan.tseng@mediatek.com |  |
| 146 | N | 5.3.5.18.3, Handling of *pathlossReferenceRS-ToAddModList* could be written in clearer way. | 4> if the current *VarLTM-Config* includes an *PathlossReferenceRS* within an *LTM-Candidate* with the *ltm-CandidateId* value that is associated with the *pathlossReferenceRS-Id* value: 5> replace the *PathlossReferenceRS* within *LTM-Candidate* in the current *VarLTM-Config* with the received *PathLossReferenceRS*~~entry related to~~ *~~PathlossReferenceRS~~* ~~within the~~ *~~LTM-Candidate~~* ~~from~~ *~~VarLTM-Config~~*. 4> else: 5> add the received *PathlossReferenceRS* within *LTM-Candidate* to *VarLTM-Config*. | li-chuan.tseng@mediatek.com |  |
| 147 | N | 5.3.5.18.4, The entry of ltm-CSI-ResourceConfigToReleaseList does not contain field named as ltm-CSI-ResourceConfigId. The entry itself is a LTM CSI resource config ID (of type LTM-CSI-ResourceConfigId). | 1> for each *LTM-CSI-ResourceConfigId~~ltm-CSI-ResourceConfigId~~* value included in the *ltm-CSI-ResourceConfigToReleaseList* for which there is an entry in *ltm-CSI-ResourceConfigList* in *VarLTM-Config*: 2> remove the entry related to the *LTM-CSI-ResourceConfig* from *VarLTM-Config*. | li-chuan.tseng@mediatek.com |  |
| 148 | Y | 6.3.2: IE LTM-Candidate,5.3.5.18.3Some field names within LTM-Candidate IE do not follow naming convention.(Also update to procedural text in 5.3.5.18.3 is needed) | LTM-Candidate-r18 ::= SEQUENCE {***<omit other fields>*** ltm-NZP~~nzp~~-CSI-RS-ResourceToAddModList-r18 SEQUENCE (SIZE (1..maxNrofNZP-CSI-RS-Resources)) OF NZP-CSI-RS-Resource OPTIONAL, -- Need N ltm-NZP~~nzp~~-CSI-RS-ResourceToReleaseList-r18 SEQUENCE (SIZE (1..maxNrofNZP-CSI-RS-Resources)) OF NZP-CSI-RS-ResourceId OPTIONAL, -- Need N ltm-NZP~~nzp~~-CSI-RS-ResourceSetToAddModList-r18 SEQUENCE (SIZE (1..maxNrofNZP-CSI-RS-ResourceSets)) OF NZP-CSI-RS-ResourceSet OPTIONAL, -- Need N ltm-NZP~~nzp~~-CSI-RS-ResourceSetToReleaseList-r18 SEQUENCE (SIZE (1..maxNrofNZP-CSI-RS-ResourceSets)) OF NZP-CSI-RS-ResourceSetId OPTIONAL, -- Need N***<omit other fields>***} | li-chuan.tseng@mediatek.com |  |
| 149 | Y | 6.3.2: IE LTM-CandidateOne field name within *LTM-SSB-Config* IE does not follow naming convention. | LTM-SSB-Config-r18 ::= SEQUENCE { ssb-Frequency-r18 ARFCN-ValueNR, subcarrierSpacing-r18 SubcarrierSpacing, ssb-Periodicity-r18 ENUMERATED {ms5, ms10, ms20, ms40, ms80, ms160, spare2, spare1} OPTIONAL, -- Need R ssb-PositionsInBurst-r18 CHOICE { shortBitmap BIT STRING (SIZE (4)), mediumBitmap BIT STRING (SIZE (8)), longBitmap BIT STRING (SIZE (64)) } OPTIONAL, -- Need R ss-PBCH-BlockPower-r18 INTEGER (-60..50) OPTIONAL, -- Need R ...} | li-chuan.tseng@mediatek.com |  |
| 150 | Y | 6.3.2: IE EarlyUL-SyncConfigOne field name within EarlyUL-SyncConfig IE does not follow naming convention. | EarlyUL-SyncConfig-r18 ::= SEQUENCE { frequencyInfoUL-r18 FrequencyInfoUL, rach-ConfigGeneric-r18 RACH-ConfigGeneric, bwp-GenericParameters-r18 BWP, ssb-PerRACH-Occasion-r18 ENUMERATED {oneEighth, oneFourth, oneHalf, one, two, four, eight, sixteen} OPTIONAL, -- Need M prach-RootSequenceIndex-r18 CHOICE { l839 INTEGER (0..837), l139 INTEGER (0..137) }, ltm-PRACH~~prach~~-SubcarrierSpacing-r18 SubcarrierSpacing, n-TimingAdvanceOffset-r18 ENUMERATED { n0, n25600, n39936 } OPTIONAL, -- Need R ...} | li-chuan.tseng@mediatek.com |  |
| 151 | Y | 6.3.2: IE LTM-Candidate,5.3.5.18.3Fields ltm-UL-TCI-StatesToReleaseList / ToAddModList could be renamed (States -> State) to be in line with other lists (singular form is used).(Also update to procedural text in 5.3.5.18.3 is needed) | ltm-UL-TCI-State~~s~~ToAddModList-r18 SEQUENCE (SIZE (1..maxNrofCandidateUL-TCI-r18)) OF CandidateTCI-UL-State-r18 OPTIONAL, -- Need N ltm-UL-TCI-State~~s~~ToReleaseList-r18 SEQUENCE (SIZE (1.. maxNrofCandidateUL-TCI-r18)) OF TCI-UL-StateId-r17 OPTIONAL, -- Need N | li-chuan.tseng@mediatek.com |  |
| 152 | N | 6.3.2: IE LTM-CandidateRRCReconfiguration for LTM execution may configure also SCells. However, field description does not capture it properly. | ***ltm-CandidateConfig***This field includes an *RRCReconfiguration* message used to configure an LTM candidate ~~cell~~configuration. | li-chuan.tseng@mediatek.com |  |
| 153 | N | 6.3.2: IE LTM-CandidateIncorrect field description | ***pathlossReferenceRS-ToReleaseList***A list of Reference Signals to be used for path loss estimation for unified TCI state for LTM to remove~~add and/or modify~~. | li-chuan.tseng@mediatek.com |  |
| 154 | N | 5.3.5.18.6, Italic font should be used | 2> replace the value of *ltm-ServingCellUE-MeasuredTA-ID*~~ltm-ServingCellUE-MeasuredTA-ID~~ in *VarLTM-ServingCellUE-MeasuredTA-ID*~~VarLTM-ServingCellUE-MeasuredTA-ID~~ with the value received within *ltm-UE-MeasuredTA-ID*~~ltm-UE-MeasuredTA-ID~~; | li-chuan.tseng@mediatek.com |  |
| 155 | N | 5.3.5.18.6, Message name typo correction | NOTE 2: When *ltm-ConfigComplete* is not included for an LTM candidate configuration, before an LTM cell switch is triggered a UE implementation may generate and store an *RRCReconfiguration*~~RRC reconfiguration~~ message by applying the received LTM candidate configuration on top of the LTM reference configuration, and the stored *RRCReconfiguration*~~RRC reconfiguration~~ message is applied when the LTM cell switch is triggered. | li-chuan.tseng@mediatek.com |  |
| 156 | N | 5.3.5.17.2.2Format typo in value of T421 in second level 2 bullet | timer value set to ~~T421~~ *t421* | nathan.tenny@mediatek.com |  |
| 157 | N | 5.5.4.20bSubject-verb disagreement | Hys ~~are~~is expressed in dB | nathan.tenny@mediatek.com |  |
| 158 | N | 5.5.5.1Enumerated values of sl-MeasQuantity should be lowercase. | set the sl-MeasQuantity to ~~SL-RSRP~~*sl-rsrp*set the sl-MeasQuantity to ~~SD-RSRP~~*sd-rsrp* | nathan.tenny@mediatek.com |  |
| 159 | N | 5.7.3c.1Typo "NR RAN" for "NG-RAN" | Procedure is to inform ~~NR~~ NG-RAN | nathan.tenny@mediatek.com |  |
| 160 | N | 5.7.3c.2Typo "receiption" in first bullet | rece~~i~~ption of *NotificationMessageSidelink* | nathan.tenny@mediatek.com |  |
| 161 | N | 5.7.3c.4Missing word "in" in second level 2 bullet | for each measObjectRelay included in MeasConfig | nathan.tenny@mediatek.com |  |
| 162 | N | 5.8.3.2Misplaced "or" in level 2 bullets | 2> if configured by upper layer to receive NR sidelink L2 U2N relay discovery messages on the frequency included in *sl-FreqInfoList* in *SIB12* of the PCell including *sl-L2U2N-Relay*; or if configured by upper layer to receive NR sidelink L3 U2N relay discovery messages on the frequency included in *sl-FreqInfoList* in *SIB12* of the PCell including *sl-L3U2N-RelayDiscovery*; or2> ~~or~~ if configured by upper layer to receive NR sidelink U2U relay discovery messages on the frequency included in *sl-FreqInfoList* in *SIB12* of the PCell including [*FFS gNB capability indication*]: | nathan.tenny@mediatek.com |  |
| 163 | N | 5.8.9.10.4Misformatted section number in first level 5 bullet | 5> initiate the indirect path failure information procedure as specified in 5.7.3c to report indirect path failure; | nathan.tenny@mediatek.com |  |
| 164 | N | 5.8.9.10.4Missing italics on enumerated value relayUE-PC5-RLF in last level 2 bullet. | 2> if sl-IndicationType is ~~relayUE-PC5-RLF~~*relayUE-PC5-RLF*: | nathan.tenny@mediatek.com |  |
| 165 | N | 5.8.9.11Unfortunate section title; there is already a "Sidelink UE information" procedure on Uu (section 5.8.3). | 5.8.9.11 ~~Sidelink~~ UE information transfer on sidelink | nathan.tenny@mediatek.com |  |
| 166 | Y | 6.2.3, IE N3C-IndirectPathAddChangeIndentation error on field n3c-C-RNTI-r18 impairs ASN.1 readability. |  n3c-RelayIdentification-r18 SEQUENCE { n3c-CellGlobalId-r18 SEQUENCE { n3c-PLMN-Id-r18 PLMN-Identity, n3c-CellIdentity-r18 CellIdentity }, n3c-C-RNTI-r18 RNTI-Value } OPTIONAL, -- Cond N3CIndirectPathAddChange | nathan.tenny@mediatek.com |  |
| 167 | N | 6.2.3, IE PDCP-ConfigTypo "optional present" in conditional presence table for condition SplitBearerMP. | the field is optionally present, need M, when MP is configured. | nathan.tenny@mediatek.com |  |
| 168 | N | 6.2.3, IE ReportConfigInterRATRedundant sentences in IE description regarding events for L2 U2N relay UE. | The measurement reporting events for L2 U2N relay UE are labelled Y*N* with *N* equal to 1, 2 and so on~~. The measurement reporting events for L2 U2N relay UE are labelled~~, and Z1. | nathan.tenny@mediatek.com |  |
| 169 | N | 6.3.5, IE SL-PHY-MAC-RLC-Config (under SL-ConfigDedicatedNR heading)Typo "optional present" in conditional presence table for condition L2U2U. | The field is optionally present for L2 U2U Relay UE and L2 U2U Remote UE, need N | nathan.tenny@mediatek.com |  |
| 170 | Y | 6.3.5, IE SL-L2RemoteUE-Config"UE" omitted from field name sl-L2IdentityRelay-r18. |  sl-L2IdentityRelayUE-r18 SL-DestinationIdentity-r16, | nathan.tenny@mediatek.com |  |
| 171 | Y | 6.3.5, IE SL-RelayUE-ConfigU2USpurious hyphens in field names sl-RSRP-Thresh-DiscConfig-r18 and sd-RSRP-Thresh-DiscConfig-r18. |  sl-RSRP-Thresh~~-~~DiscConfig-r18 SL-RSRP-Range-r16 OPTIONAL, -- Need R sl-hystMaxRelay-r18 Hysteresis OPTIONAL, -- Cond SL-RSRP-ThreshRelay sd-RSRP-Thresh~~-~~DiscConfig-r18 SL-RSRP-Range-r16 OPTIONAL, -- Need R sd-hystMaxRelay-r18 Hysteresis OPTIONAL -- Cond SD-RSRP-ThreshRelay | nathan.tenny@mediatek.com |  |
| 172 | N | 6.3.5, IE SL-SRAP-ConfigU2UMissing word "between" in field description of sl-MappingToRelease-U2U-List | Indicates the list of mappings between the end-to-end | nathan.tenny@mediatek.com |  |
| 173 | N | 6.3.5, IE SL-SRAP-ConfigU2URedundant "identity" in field description of sl-RemoteUE-SLRB-Identity. | Identity of the end-to-end sidelink bearer ~~identity~~ | nathan.tenny@mediatek.com |  |
| 174 | N | 5.8.3.3Missing semicolon after a level 5 bullet | 5> set sl-RLC-ModeIndication to include the RLC mode(s); | nathan.tenny@mediatek.com |  |
| 175 | N | 5.8.3.3Full stop instead of semicolon after a level 4 bullet | 4> include sl-PosRxInterestedFreqList and set it to the frequency for NR sidelink positioning reception~~.~~; | nathan.tenny@mediatek.com |  |
| 176 | N | 5.8.18.2Missing "shall" in first line of section | A UE capability of NR sidelink positioning that is configured by upper layers for reception of SL-PRS shall: | nathan.tenny@mediatek.com |  |
| 177 | N | 5.8.18.3Typo in field name in level 6 bullet | Change sl-PRS-TxPoolSelectedNormalNormal to sl-PRS-TxPoolSelectedNormal[Lenovo] Agree but already covered by #82. | nathan.tenny@mediatek.com |  |
| 178 | N | 5.8.18.3Missing italics in level 5 bullet "else, if the sl-PRS-TxPoolSelectedNormal or sl-TxPoolSelectedNormal for the concerned frequency is included in the sl-ConfigDedicatedNR within RRCReconfiguration" | else, if the *sl-PRS-TxPoolSelectedNormal* or *sl-TxPoolSelectedNormal* for the concerned frequency is included in the *sl-ConfigDedicatedNR* within *RRCReconfiguration* | nathan.tenny@mediatek.com |  |
| 179 | Y | 6.2.2, Message RRCReleaseTypo in IE name in field description of srs-PosRRC-InactiveValidityAreaConfigList | SRS-PosRes~~e~~ourceSet | nathan.tenny@mediatek.com |  |
| 180 | N | 6.3.2, IE SRS-ConfigTypo in field description of srs-PosHyperSFN-Index in the table ***SRS-Resource, SRS-PosResource* field descriptions** | Change "filed" to "field"[Lenovo] Agree but already covered by #36. | nathan.tenny@mediatek.com |  |
| 181 | N | 6.3.2, IE SRS-ConfigTypo in field description of srs-PosHyperSFN-Index in the table ***SRS-ResourceSet, SRS-PosResourceSet* field descriptions** | Change "filed" to "field"[Lenovo] Agree but already covered by #36. | nathan.tenny@mediatek.com |  |
| 182 | N | 6.3.2, IE SRS-ConfigSpurious italics throughout field definition of overlapValue (under IE TxHoppingConfig) | This field specifies the overlap during SRS transmission in terms of number of resource blocks. Value *zeroRB* implies *0* PRB, value *oneRB* corresponds to *1* PRB, value *twoRB* corresponds to *2* PRBs and so on. The same value for the *overlapValue* is configured to all the hops. | nathan.tenny@mediatek.com |  |
| 183 | Y | 6.3.5, IE SL-CBR-CommonTxDedicated-SL-PRS-RP-ListHyphenation error in section title for this IE (should have no hyphen after “Dedicated”) | *SL-CBR-CommonTxDedicated~~-~~SL-PRS-RP-List*[Lenovo] Agree but is already covered by #39. | nathan.tenny@mediatek.com |  |
| 184 | N | 6.3.5, IE SL-CBR-CommonTxDedicated-SL-PRS-RP-ListHyphenation and capitalization errors in fields of SL-CBR-SL-PRS-TxConfig-r18 |  sl-PRS-CR-Limit-r18 INTEGER(0..10000) OPTIONAL, -- Need M sl-PRS-MaxTx~~-p~~P~~ower~~-r18 INTEGER (-30..33) OPTIONAL, -- Need M sl-PRS-MaxNum~~-~~Transmissions-r18 INTEGER(1..32) OPTIONAL -- Need M | nathan.tenny@mediatek.com |  |
| 185 | N | 5.7.4.21> if configured to report relay UE information with non-3GPP connection(s);2> if the UE did not transmit a *UEAssistanceInformation* message with *n3c-relayUE-InfoList* since it was configured to report available relay UE information with non-3GPP connection(s); or2> if the UE has new available non-3GPP conection(s); or2> if the non-3GPP connection(s) with the reported relay UE(s) is not available:3> initiate transmission of the *UEAssistanceInformation* message in accordance with 5.7.4.3 to report relay UE information with non-3GPP connection(s) included in the *n3c-relayUE-InfoList*; | 1. “;” should be “:”2. should be connection(s) | wang.mengzhen@zte.com.cn |  |
| 186 | N | 5.8.9.1.24> according to association between User Info and L2 ID as specified in TS 23.304 [65], set *sl-PeerRemoteUE-LocalIdentity* to include the new local UE ID, and and set *sl-PeerRemoteUE-L2Identity* to include the destination L2 ID of peer L2 U2U Remote UE in the *SL-SRAP-ConfigPC5*, if needed;2> else if the local ID pair is to be released for an end-to-end PC5 connetion: | 1. remove the redundant “and”.2. typo | wang.mengzhen@zte.com.cn |  |
| 187 | N | 5.8.9.11.1This purpose of this procedure is to transfer the UE information in sidelink. The L2 U2U Remote UE informs its end-to-end QoS information to its connected L2 U2U Relay UE in the *UEInformationRequestSidelink* message, and the L2 U2U Relay UE delivers the split QoS information of the first-hop to the Remote UE in the *UEInformationResponseSidelink* message. | Change “This” to “The” | wang.mengzhen@zte.com.cn |  |
| 188 | N | 5.8.9.11.33> set the contents of *UEInformationResponseSidelink* message as follows:4> set *sl-SplitQoS-InfoListPC5* to include the split PDB value for each QoS flow on the fisrt PC5 hop between L2 U2U Relay UE and L2 U2U Remote UE; | typo | wang.mengzhen@zte.com.cn |  |
| 189 | N | 5.8.17.3A UE capable of NR sidelink U2U Remote UE operation shall initiate NR sidelink U2U Relay (re)slection procedure as specified in 5.8.17.4 when one of the following conditions is met: | Typo, should be “(re)selection” | wang.mengzhen@zte.com.cn |  |
| 190 | Y | 6.2.2 IE UEAssistanceInformationN3C-RelayUE-Info-r18::= SEQUENCE { n3c-RelayIdentification-r18 SEQUENCE { n3c-CellGlobalId-r18 SEQUENCE { n3c-PLMN-Id-r18 PLMN-Identity, n3c-CellIdentity-r18 CellIdentity }, n3c-C-RNTI-r18 RNTI-Value }} | Format. Add blank before “n3c-C-RNTI” to keep align with “n3c-CellGlobalId” in vertical. | wang.mengzhen@zte.com.cn |  |
| 191 | Y | 6.3.2 IE, *N3C-IndirectPathAddChange*N3C-IndirectPathAddChange-r18 ::= SEQUENCE { n3c-RelayIdentification-r18 SEQUENCE { n3c-CellGlobalId-r18 SEQUENCE { n3c-PLMN-Id-r18 PLMN-Identity, n3c-CellIdentity-r18 CellIdentity }, n3c-C-RNTI-r18 RNTI-Value } OPTIONAL, -- Cond N3CIndirectPathAddChange ...} | The same issue as above. Add blank before “n3c-C-RNTI” to keep align with “n3c-CellGlobalId” in vertical. | wang.mengzhen@zte.com.cn |  |
| 192 | Y | 6.2.2 IE, SidelinkUEInformation***sl-U2U-Identity***This field is to identify a the end-to-end PC5 link. When a L2 U2U Remote UE reports info for the first hop, it includes *sl-TargetUE-Identity* to indicate the peer L2 Remote UE on the second hop, and when a L2 U2U Relay UE reports info for the second hop, it includes *sl-SourceUE-Identity* to indicate the source L2 U2U Remote UE on the first hop. | Change “a the” to “an”. | wang.mengzhen@zte.com.cn |  |
| 193 | N | 6.3.2***DRX-Config* field descriptions*****drx-NonIntegerShortCycle***Value in non-integer number of ms, e.g. ms25over3 corresponds to 25/3 ms, ms100over9 corresponds to 100/9 ms and so on). | Remove “)” [Lenovo] Agree but the description can be further improved by starting with the first two values:“Value in non-integer number of ms. Value ms1001over240 corresponds to 1001/240 ms, value ms25over6 corresponds to 25/6 ms and so on.” | hisashi.futaki@nec.com  |  |
| 194 | Y | 7.4*VarServingSecurityCellSetID* UE variable-- ASN1START-- TAG-VARCONDITIONALRECONFIG-STARTVarServingSecurityCellSetID ::= SEQUENCE { servingSecurityCellSetId-r18 INTEGER (1.. maxSecurityCellSet-r18)}-- TAG-VARCONDITIONALRECONFIG-STOP-- ASN1STOP | TAG name is wrong, which should be VARSERVINGSECURITYCELLSETID. | hisashi.futaki@nec.com  |  |
| 195 | Y | 6.2.2*UEInformationResponse message*< skip >RA-InformationCommon-r16 ::= SEQUENCE { absoluteFrequencyPointA-r16 ARFCN-ValueNR,< skip >  [[ usedFeatureCombination-r18 ReportedFeatureCombination-r18 OPTIONAL, triggeredFeatureCombination-r18 ReportedFeatureCombination-r18 OPTIONAL, attemptedBWP-InfoList-r18 SEQUENCE (SIZE (1..maxNrofBWPs)) OF AttemptedBWP-Info-r18 OPTIONAL, numberOfLBTFailures-r18 INTEGER (1..128) OPTIONAL, perRAInfoList-v1800 PerRAInfoList-v1800 OPTIONAL, sdt-Failed-r18 ENUMERATED {true} OPTIONAL ]]}***numberOfLBTFailures***This field is used to indicate the total number of preamble transmission attempts for which LBT failure indication is received in the RA procedure. < … > | field name shold be "numberOfLBT-Failures-r18" to avoid abbreviation followed by capital letter. The same correction should be applied to the field description as well.Additional comment: Same issue found for "perRAInfoList-v1800" (->perRA-InfoList), but the field name reuses one in the earlier release (R16) unfortunately. No change is proposed here. Similar situation for perRASSBInfoList-v18 (->perRA-SSB-InfoList) and perRACSI-RSInfoList-v18 (->perRA-CSI-RS-InfoList), where both are introduced in R16. Probably can consider misc from earlier releases. | hisashi.futaki@nec.com  |  |
| 196 | N | 5.7.10.5 RA information determination< skip >1> if at least one LBT failure indication has been received from lower layers during the random-access procedure:2> set the *numberOfLBTFailures* to indicate the total number of random-access attempts for which LBT failure indications have been received from lower layers in the random-access procedure. | following the same correction as the previous one. Referred field name should be "numberOfLBT-Failures-r18" | hisashi.futaki@nec.com  |  |
| 197 | Y | 6.2.2*UEAssistanceInformation message*< skip >MUSIM-GapPriorityPreferenceList-r18 ::= SEQUENCE (SIZE (1..3)) OF GapPriority-r17[ ]MUSIM-CapRestriction-r18 ::= SEQUENCE { musim-Cell-SCG-ToRelease-r18 MUSIM-Cell-SCG-ToRelease-r18 OPTIONAL, musim-CellToAffectList-r18 MUSIM-CellToAffectList-r18 OPTIONAL, musim-AffectedBandsList-r18 MUSIM-AffectedBandsList-r18 OPTIONAL, musim-AvoidedBandsList-r18 MUSIM-AvoidedBandsList-r18 OPTIONAL, musim-MaxCC-r18 MUSIM-MaxCC-r18 OPTIONAL} | Unnecessary space exists in front of MUSIM-CapRestriction-r18. Should remove it. | hisashi.futaki@nec.com  |  |
| 198 | N | 5.3.5.18.6<skipped text>1> release the radio bearer(s) and the logical channel(s) that are part of the current UE configuration but not part of the LTM candidate configuration either indicated by lower layers or for the selected cell in accordance with 5.3.7.3, or the LTM reference configuration (in case the LTM candidate configuration does not include *ltm-ConfigComplete*). | The construct with “either” and “or” is not clearly describing the intention.It can be written as:1> release the radio bearer(s) and the logical channel(s) that are part of the current UE configuration but not part of the LTM candidate configuration for a cell indicated by lower layers or for the selected cell in accordance with 5.3.7.3, in the LTM reference configuration (in case the LTM candidate configuration does not include *ltm-ConfigComplete*). | pmallick@lenovo.com |  |
| 199 | N | 5.3.5.13.4<skipped text>4> if NES mode indication is received from lower layers, indicating that the NES-specific CHO execution condition is enabled; and4> if the entry condition(s) applicable for this event associated with the *condReconfigId*, i.e. the event corresponding with the *condEventId(s)* of the corresponding *condTriggerConfig* within *VarConditionalReconfig*, is fulfilled for the applicable cells for all measurements after layer 3 filtering taken during the corresponding *timeToTrigger* defined for this event within the *VarConditionalReconfig*:5> consider the event associated to that *measId* to be fulfilled;4> if the *measId* for this event associated with the *condReconfigId* has been modified; or4> if NES mode indication is received from lower layers, indicating that the NES-specific CHO execution condition is disabled; or | “NES mode indication” should be called “NES-mode indication” in compliance with L1 specification. | pmallick@lenovo.com |  |
| 200 | N | The field is mandatory present when dynamic grant is used for initial uplink transmission in RACH-less handover in NTN. Otherwise, it is absent, Need R. | remove "Need R" --> The field is mandatory present when dynamic grant is used for initial uplink transmission in RACH-less handover in NTN. Otherwise, it is absent.[Lenovo] Disagree since it defines the UE behaviour when once the field has been configured but is absent in a subsequent configuration. | shiyang.leng@samsung.com |  |
| 201 | Y | tn-DistanceRadius-r18 INTEGER(0..65536 ) | typo in upper limit of the integer range, should be up to 65535, i.e., INTEGER(0..65535) | shiyang.leng@samsung.com |  |
| 202 | Y | distanceThreshFromReference1-r18 INTEGER(0.. 65525 ), | condEventD2, typo in upper limit of the integer range, should be up to 65535, i.e., INTEGER(0..65535) | shiyang.leng@samsung.com |  |
| 203 | Y | distanceThreshFromReference2-r18 INTEGER(0.. 65525 ), | condEventD2, typo in upper limit of the integer range, should be up to 65535, i.e., INTEGER(0..65535) | shiyang.leng@samsung.com |  |
| 204 | N | ***tci-SelectionPresentIn-DCI***Indicates if a [TCI selection field] is present or absent in DCI format 1\_1 and DCI format 1\_2 for a DL BWP, see reference XXX. | Need reference. TS 38.212 7.3.1.2.2 and 7.3.1.2.3 | Youn.heo@samsung.com |  |
| 205 | Y | vectorLengthDD-r18 ENUMERATED {n1,n2,n4,n8 }, | Unnecessary space. | Youn.heo@samsung.com |  |
| 206 | Y |  tdCQI-r18 ENUMERATED {n11,n12,n2 } OPTIONAL -- Need R | Unnecessary space | Youn.heo@samsung.com |  |
| 207 | N | ***valueOfN-CJT-r18***Field describes the size of the window of FD bases for Rel-18 Type II CJT PS codebook. For M=2, N=2,4 (see TS 38.214 [19], clause 5.2.2.2.9) | Bases=> basis | Youn.heo@samsung.com |  |
| 208 | N | valueOfN-Doppler-r18Field describes the size of the window of FD bases for Rel-18 Type II Doppler PS codebook. For M=2, N=2,4 (see TS 38.214 [19], clause 5.2.2.2.9) | Bases=> basis | Youn.heo@samsung.com |  |
| 209 | N | The IE *RACH-ConfigTwoTA* is used to specify random access parameters for each additional PCI configured for the serving cell. | Double space | Youn.heo@samsung.com |  |
| 210 | N | additionalRACH-perPCI-ToAddModListList of RACH configurations for the additional PCIs. The RACH configuration for an additional PCI is applied for Random Access procedure initiated by PDCCH order towards to the additional PCI, as specified in TS 38.321 clause 5.1.1b. This configuration may be different for different UEs. |  Extra space | shiyang.leng@samsung.com |  |
| 211 | N | 2TA-OnlyThe field is optionally present, Need N in the BWP-UplinkCommon if additionalPCI-ToAddModList is present in spCellConfigDedicated or sCellConfigDedicated and it has the same number of entries as the additionalPCI-ToAddModList . It is absent otherwise. |  Extra spaces | shiyang.leng@samsung.com |  |
| 212 | N | stx2-Panel | Parameter name should be sTx-2Panel-r18  | Youn.heo@samsung.com |  |
| 213 | N | reportingModeConfigures the UE with reporting mode for group based reporting.(see TS XXXXXX ) | reference TS 38.214 clause 5.2.1.4.2 | shiyang.leng@samsung.com |  |
| 214 | Y | dmrs-UplinkTransformPrecoding-r16 SetupRelease {DMRS-UplinkTransformPrecoding-r16} OPTIONAL -- Need M ]] } OPTIONAL, -- Need R ... ,  |  Editorial: remove redundant spacing | seungri.jin@samsung.com |  |
| 215 | Y | timeDensityTransformPrecoding ENUMERATED {d2} OPTIONAL -- Need S } OPTIONAL, -- Need R ... ,  |  Editorial: remove the redundant space. | seungri.jin@samsung.com |  |
| 216 | N | multipanelSFN-SchemeParameter to configure multiple panel simultaneous uplink transmission SFN scheme for PUCCH resources Ref XXX . |  reference TS 38.213 9.2.6 | shiyang.leng@samsung.com |  |
| 217 | Y | Change the field name or make it clear in a field description that the field is for RACH-less, to be consistent with NTN RACH-less configuration or unify the RACH-less for IAB/LTM/NTN framework under one IE | CG-mIAB-Configuration-r18 | m.tesanovic@samsung.com |  |
| 218 | N | CHO with target SCG or CHO with candidate SCG(s) is taken as conditional reconfiguration for UE, therefore the definition of the condReconfigId IE should be modified. | 6.3.2 Radio resource control information elements– CondReconfigIdThe IE CondReconfigId is used to identify a CHO, CPA or CPC configuration.=>The IE CondReconfigId is used to identify a CHO, CPA, CPC, CHO with target SCG or CHO with candidate SCG configuration. | yu1.pan@samsung.com, ww1016.wang@samsung.com |  |
| 219 | N | According to the agreement in RAN2#124: The target MN provides an reportConfigNR instance to the source MN with only the condEventA4 related parameters (a4-Threshold, hysteresis, timeToTrigger and rsType),add clarification in the filed description.For the parameters of the execution condition for PSCell in CHO with candidate SCG(s) is provided by the candidate MN not by the source MN, it needs to be clairified in the specification clearly. | 6.3.2 Radio resource control information elements– CondReconfigToAddModList……CondReconfigToAddMod field descriptionscondExecutionCondPSCellThe execution condition that needs to be fulfilled for the associated PSCell in order to trigger the execution of a conditional reconfiguration for CHO with candidate SCG(s). The Meas Ids refer to the measConfig associated with the MCG. When configuring 2 triggering events (Meas Ids) for a candidate cell, network ensures that both refer to the same measObject. The network only indicates MeasId(s) associated with condEventA4.=>The execution condition that needs to be fulfilled for the associated PSCell in order to trigger the execution of a conditional reconfiguration for CHO with candidate SCG(s), and the parameters of the execution condition are provided by the candidate MN. The Meas Ids refer to the measConfig associated with the MCG. When configuring 2 triggering events (Meas Ids) for a candidate cell, network ensures that both refer to the same measObject. The network only indicates MeasId(s) associated with condEventA4. | yu1.pan@samsung.com, ww1016.wang@samsung.com |  |
| 220 | N | **(See section 4.2.1 page 37)**- If configured by upper layers for MBS broadcast reception, acquires MCCH change notification and MBS broadcast control information and data. | Replace "and" by ","- If configured by upper layers for MBS broadcast reception, acquires MCCH change notification, ~~and~~ MBS broadcast control information and data. | shrivastava@samsung.com |  |
| 221 | N | **(see section 5.3.13.1d page 190)**1> if mbs-NeighbourCellList acquired in the previous cell indicates that a multicast session that the UE has joined for which the UE is not indicated to stop monitoring the G-RNTI is not provided for RRC\_INACTIVE in the current serving cell; or1> if the measured RSRP or RSRQ for serving cell as specified in TS 38.304 [20] is below the threshold indicated by thresholdIndex for a multicast session that the UE has joined: 2> initiate RRC connection resume procedure in 5.3.13.2 with resumeCause set to mt-Access.  | Made 3 changes as below:1> if mbs-NeighbourCellList acquired in the previous cell indicates that a multicast session that the UE has joined and for which the UE is not indicated to stop monitoring the G-RNTI, is not provided for RRC\_INACTIVE in the current serving cell; or1> if the measured RSRP or RSRQ for serving cell as specified in TS 38.304 [20] is below the threshold indicated by thresholdIndex for a multicast session that the UE has joined: 2> initiate the RRC connection resume procedure in 5.3.13.2 with resumeCause set to mt-Access.  | shrivastava@samsung.com |  |
| 222 | N | **(see section 5.10.3.2 page 434)**1> establish a PDCP entity and an RLC entity i n accordance with MRB-InfoBroadcast for this multicast MRB included in the MBSMulticastConfiguration message and the configuration specified in 9.1.1.7 ; | Remove space in-between as:1> establish a PDCP entity and an RLC entity in accordance with MRB-InfoBroadcast for this multicast MRB included in the MBSMulticastConfiguration message and the configuration specified in 9.1.1.7 ; | shrivastava@samsung.com |  |
| 223 | N | **(Section 5.3.11)**1> for each application layer measurement configuration for which configForRRC-IdleInactive is not set to true:2> inform upper layers about the release of all application layer measurement configurations;2> discard any application layer measurement reports which were not yet submitted to lower layers for transmission; | Remove "all" since this bullet is performed per each application layer measurement configuration(Section 5.3.11)1> for each application layer measurement configuration for which configForRRC-IdleInactive is not set to true:2> inform upper layers about the release of ~~all~~ application layer measurement configuration~~s~~;2> discard any application layer measurement reports which were not yet submitted to lower layers for transmission; | s90.jeong@samsung.com |  |
| 224 | N | Field description of offsetThresholdTA in TAG-Config***offsetThresholdTA***Offset for TA reporting as specified in TS 38.321 [3]. Network only configures this parameter for MCG. For ATG, network only configures offsetThresholdTA-r18 in unit of symbols | Editorial: Add “which is” i.e. For ATG, network only configures offsetThresholdTA-r18, which is in unit of symbols. | j.sedin@samsung.com |  |
| 225 | N | **5.3.7.2**2>  if MR-DC is configured:3>  perform MR-DC release, as specified in clause 5.3.5.10;2>  perform the LTM configuration release procedure for the MCG and the SCG as specified in clause 5.3.5.18.7;**5.3.7.3**2>  remove all the entries within the MCG*VarConditionalReconfig*, if any;2>  perform the LTM configuration release procedure for the MCG and the SCG as specified in clause 5.3.5.18.7;**5.3.8.3**2>  perform the LTM configuration release procedure for the MCG and the SCG as specified in clause 5.3.5.18.7;2>  remove all the entries within the MCG and the SCG*VarConditionalReconfig*, if any;**5.3.11**1>  release the *uav-Config*, if configured;1>  perform LTM configuration release procedure for the MCG and SCG as specified in clause 5.3.5.18.7; | When these conditions are evaluated, the UE may not be configured with LTM configuration.Suggest to add ‘if configured’ or something similar in all 4 cases.Additionally, add ‘the’ in the last instance (5.3.11) before ‘SCG’ to align with the rest. | uphuyal@qti.qualcomm.com |  |
| 226 | N | CellGroupConfig > uplinkTxSwitchingAssociatedBandDualUL-List field description. | The clause number for TS38.214 is incorrect. "6.16" should be changed to "6.1.6". | uphuyal@qti.qualcomm.com |  |
| 227 | N | 5.8.9.1.21> if the UE is acting as L2 U2U Remote UE (i.e. Tx UE), and if the procedure is initiated to configure the first hop PC5 Relay RLC channel of an end-to-end sidelink DRB to the connected L2 U2N Relay UE (i.e. Rx UE), based on configuration in *SIB12* or *SidelinkPreconfigNR*; or1> if the UE is acting as L2 U2U Relay UE (i.e. Tx UE) and is in RRC\_IDLE or in RRC\_INACTIVE or OoC, and if the procedure is initiated to configure the second hop PC5 Relay RLC channel to the connected L2 U2N Remote UE (i.e. Rx UE) based on configuration in *SIB12* or *SidelinkPreconfigNR*: | Change “U2N” to “U2U” | wulh5@lenovo.com |  |
| 228 | Y | SRS-PosRRC-InactiveValidityAreaConfigList-r18 ::= SEQUENCE SIZE(1..maxNrOfVA-r18) OF SRS-PosRRC-InactiveValidityAreaConfig-r18 | SRS-PosRRC-InactiveValidityAreaConfigList-r18 ::= SEQUENCE (SIZE(1..maxNrOfVA-r18)) OF SRS-PosRRC-InactiveValidityAreaConfig-r18[Lenovo] Is not editorial and it has been already raised in RIL by B010. | qiangli3@huawei.com |  |
| 229 | Y | ***CandidateTCI-UL-State* information element**-- ASN1START-- TAG-CANDIDATETCI-UL-STATE-STARTCandidateTCI-UL-State-r18 ::= SEQUENCE { tci-UL-StateId-r18 TCI-UL-StateId-r17, referenceSignal-r18 CHOICE { ssb-Index SSB-Index, csi-RS-Index NZP-CSI-RS-ResourceId }, pathlossReferenceRS-Id-r18 PathlossReferenceRS-Id-r17 OPTIONAL, -- Need R …}-- TAG-CANDIDATETCI-UL-STATE-STOP-- ASN1STOP | ***CandidateTCI-UL-State* information element**-- ASN1START-- TAG-CANDIDATETCI-UL-STATE-STARTCandidateTCI-UL-State-r18 ::= SEQUENCE { tci-UL-StateId-r18 TCI-UL-StateId-r17, referenceSignal-r18 CHOICE { ssb-Index SSB-Index, csi-RS-Index NZP-CSI-RS-ResourceId }, pathlossReferenceRS-Id-r18 PathlossReferenceRS-Id-r17 OPTIONAL, -- Need R ...}-- TAG-CANDIDATETCI-UL-STATE-STOP-- ASN1STOP[Lenovo] Covered by #23. | qiangli3@huawei.com |  |
| 230 | N | Clause 5.2.2.4.211> if *SatSwitchWithReSync* and *t-Service* are included, and the UE supports hard satellite switch with resynchronization;2> if *t-ServiceStart* is included and the UE supports soft satellite switch with resynchronization: | “SatSwitchWithReSync” should start with lower case: satSwitchWithReSync[Lenovo] Covered by #16. | zhenglili4@huawei.com |  |
| 231 | N | Clause 5.7.19:1> start re-synchronising to the DL of the SpCell served by the satellite indicated by *ntn-Config* in *SatSwitchWithReSync*;1> start timer T430 with the timer value set to *ntn-UlSyncValidityDuration* from the subframe indicated by *epochTime* in *ntn-Config* in *SatSwitchWithReSync*;1> inform lower layers when UL synchronisation is obtained. | Same issue with above. “SatSwitchWithReSync” should be changed to “satSwitchWithReSync” | zhenglili4@huawei.com |  |
| 232 | N | Clause 6.3.1:***interFreqCarrierFreqList***List of neighbouring carrier frequencies and frequency specific cell re-selection information. If *interFreqCarrierFreqList-v1610, interFreqCarrierFreqList-v1700, interFreqCarrierFreqList-v1720*, *interFreqCarrierFreqList-v1730,* *interFreqCarrierFreqList-v1760* or *InterFreqCarrierFreqInfo-v1800* are present, they shall contain the same number of entries, listed in the same order as in *interFreqCarrierFreqList* (without suffix). | InterFreqCarrierFreqInfo-v1800 should start with lower case[Lenovo] Covered by #120 and #133. | zhenglili4@huawei.com |  |
| 233 | Y | Clause 6.3.2:ntn-cg-RACH-less-RetransmissionTimer INTEGER (1..64) OPTIONAL, -- Need R | An “-r18” suffix is needed. | zhenglili4@huawei.com |  |
| 244 | N | Clause 5.3.3.43> if at least one stored application layer measurement configuration or application layer measurement report container has not been released:4> include *measConfigReportAppLayerAvailable* in the *RRCSetupComplete* message | Here the wording “has not been released” is applied for both configuration and report container, but usually this spec uses “has not been discarded” for report container.Change “if at least one stored application layer measurement configuration or application layer measurement report container has not been released” into:if at least one stored application layer measurement configuration has not been released or application layer measurement report container has not been ~~released~~discarded | jun.chen@huawei.com |  |
| 245 | N | 3> if *configForRRC-IdleInactive* is set to *true*:4> store the received *qoe-Reference*, *measConfigAppLayerId*, *serviceType*, *qoe-MeasurementType*, *qoe-AeaScope*, *mce-Id*, *configForRRC-IdleInactive*, *appLayerMeasPriority*, if included, in *VarAppLayerIdleConfig*;4> if the *qoe-AreaScope* includes *plmn-IdentityList*: | Here “if included” refers to appLayerMeasPriority as all other info seem mandatory for Idle/INACTIVE QoE config, so the obje for “if included” is unclear. Suggest to put “if included” in brackets. | Jun.chen@huawei.com |  |
| 246 | Y | Qoe-AreaScope-r18 ::= CHOICE { cellGlobalIdList CellGlobalIdList-r16, trackingAreaCodeList TrackingAreaCodeList-r16, trackingAreaIdentityList TrackingAreaIdentityList-r16, plmn-IdentityList PLMN-IdentityList2-r16, ...} | Should be QoE instead of Qoe | Jun.chen@huawei.com |  |
| 247 | Y | ***mce-id***The field contains the Measurement Collection Entity Id, see TS 28.405 [55]. | the clause information is missing here.Like the clause information fo r the above IE qoe-Reference, the clause information can be added.[Lenovo] Not needed since no MCE ID is defined in TS 28.405 but “QoE collection entity address” in clause 5.1. The “QoE collection entity address” is a IPv4 or IPv6 address that is not the same as the MCE ID. | Jun.chen@huawei.com |  |
| 248 | N | Clause 5.5.2.12:The UE shall:1> if effectiveMeasWindowConfig is set to setup:2> if an effective measurement window configuration is already setup:3> release the effective measurement window configuration;2> setup an effective measurement window configuration indicated by the *effectiveMeasWindowConfig* in accordance with the received *windowOffsetPeriodicity* (providing *periodicity* and *offset* for the following condition), i.e., the first subframe of each window occurs at an SFN and subframe meeting the following condition:SFN mod *T* = FLOOR(*offset*/10);subframe = *offset* mod 10;with *T* = *periodicity*/10;1> else if effectiveMeasWindowConfig is set to release:2> release the effective measurement window configuration; | Missing italics | zhenglili4@huawei.com |  |
| 249 | N | 1> if the received otherConfig includes the multiRx-PreferenceReportingConfigFR2:2> if the *multiRx-PreferenceReportingConfigFR2* is set to *setup*: | Missing italics | zhenglili4@huawei.com |  |
| 250 | Y | RRCReconfiguration-v1800-IEs ::= SEQUENCE { needForInterruptionConfigNR-r18 ENUMERATED { enabled, disabled } OPTIONAL, -- Need M uav-Config-r18 SetupRelease { UAV-Config-r18 } OPTIONAL, -- Need M sl-IndirectPathAddChange-r18 SetupRelease { SL-IndirectPathAddChange-r18 } OPTIONAL, -- Need M n3c-IndirectPathAddChange-r18 SetupRelease { N3C-IndirectPathAddChange-r18 } OPTIONAL, -- Need M n3c-IndirectPathConfigRelay-r18 SetupRelease { N3C-IndirectPathConfigRelay-r18 } OPTIONAL, -- Need M otherConfig-v1800 OtherConfig-v1800 OPTIONAL, -- Need M srs-PosResourceSetLinkedForAggBWList-r18 SetupRelease { SRS-PosResourceSetLinkedForAggBWList-r18 } OPTIONAL, -- Need M ltm-Config-r18 SetupRelease {LTM-Config-r18} OPTIONAL, -- Need M nonCriticalExtension SEQUENCE {} OPTIONAL} | The indentation of the fields should be aligned (sl-IndirectPathAddChange-r18, n3c-IndirectPathAddChange-r18, n3c-IndirectPathConfigRelay-r18, otherConfig-v1800 are “earlier” than other fields) | zhenglili4@huawei.com |  |
| 251 | N | 4> if the *needForInterruptionConfigNR* is enabled and the *NeedForInterruptionInfoNR* information is changed compared to last time the UE reported this information: | Lower case | zhenglili4@huawei.com |  |