**3GPP TSG CT WG3 Meeting #138 *C3-246374***

**Orlando, US, 18 - 22 November, 2024 was C3-246118**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **549** | **CR** | **0342** | **rev** | **-** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Define SS\_SLPositioningManagement API procedures |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | eLSAPP |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Stage-2 (SA6) agreed CR S6-244617 (TS 23.434 CR#337) defines new API - SS\_SLPositioningManagement API, where SEAL LMS (SL positioning enabler capability) provides support to the provisioning/delivery of ranging services in an area to the subscribed VAL server (SL Positioning / Ranging Server). |
|  |  |
| ***Summary of change:*** | New API procedure is defined to support SS\_SLPositioningManagement API.  |
|  |  |
| ***Consequences if not approved:*** | Stage-2 requirements not supported. |
|  |  |
| ***Clauses affected:*** | 5.2.8 (new) and sub clauses. |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS/TR 23.434 CR 0337  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact open API defined in this specification |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* First Change \*\*\*

## 5.1 Introduction of SEAL services

The table 5.1-1 lists the SEAL server APIs below the service name. A service description clause for each API gives a general description of the related API.

Table 5.1-1: List of SEAL Service APIs

|  |  |  |  |
| --- | --- | --- | --- |
| Service Name | Service Operations | Operation Semantics | Consumer(s) |
| SS\_LocationReporting | Create\_Trigger\_Location\_Reporting | Request/ Response | VAL server |
| Fetch\_Location\_Report\_Trigger | Request/Response | VAL server |
| Update\_Trigger\_Location\_Reporting | Request/ Response | VAL server |
| Cancel\_Trigger\_Location\_Reporting | Request/ Response | VAL server |
| Notify\_Trigger\_Location\_Reporting | Notify | VAL server |
| SS\_LocationInfoEvent | Subscribe\_Location\_Info | Subscribe/Notify | VAL server |
| Update\_Location\_Info\_Subscription | VAL server |
| Unsubscribe\_Location\_Info | VAL server |
| Notify\_Location\_Info | VAL server |
| SS\_LocationInfoRetrieval | Obtain\_Location\_Info | Request/ Response | VAL server |
| SS\_LocationAreaInfoRetrieval | Obtain\_UEs\_Info | Request/ Response | VAL server |
| SS\_LocationMonitoring | Subscribe\_Location\_Monitoring | Subscribe/Notify | VAL server |
| Update\_Location\_Monitoring\_Subscription |
| Unsubscribe\_Location\_Monitoring |
| Notify\_Location\_Monitoring\_Events |
| SS\_LocationAreaMonitoring | Subscribe\_Location\_Area\_Monitoring | Subscribe/Notify | VAL server |
| Notify\_Location\_Area\_Monitoring\_Events |
| Update\_Location\_Area\_Monitoring\_Subscribe |
| Unsubscribe\_Location\_Area\_Monitoring |
| SS\_VALServiceAreaConfiguration | Configure\_VAL\_Service\_Area | Request/Response | VAL server |
| Obtain\_VAL\_Service\_Area | Request/Response | VAL server |
| Update\_VAL\_Service\_Area | Request/Response | VAL server |
| Delete\_VAL\_Service\_Area | Request/Response | VAL server |
| Subscribe\_VAL\_Service\_Area\_Change\_Event | Subscribe/Notify | SEAL server |
| Update\_Subscription\_VAL\_Service\_Area\_Change\_Event |
| Unsubscribe\_VAL\_Service\_Area\_Change\_Event |
| Notify\_VAL\_Service\_Area\_Change\_Event |
| SS\_SLPositioningManagement | Subscribe | Subscribe/Notify | VAL server |
| Notify |
| SS\_GroupManagement | Query\_Group\_Info | Request/ Response | VAL server |
| Update\_Group\_Info | Request/ Response | VAL server |
| Create\_Group | Request/ Response | VAL server |
| Delete\_Group | Request/Response | VAL server |
| SS\_GroupManagementEvent | Subscribe\_Group\_Info\_Modification | Subscribe/Notify | VAL server |
| Notify\_Group\_Info\_Modification | VAL server |
| Notify\_Group\_Creation | VAL server |
| SS\_UserProfileRetrieval | Obtain\_User\_Profile | Request/ Response | VAL server |
| SS\_VALServiceData | Obtain\_VAL\_Service\_Data | Request/Response | SEAL server |
| SS\_UserProfileEvent | Subscribe\_User\_Profile\_Update | Subscribe/Notify | VAL server |
| Notify\_User\_Profile\_Update | VAL server |
| SS\_NetworkResourceAdaptation(NOTE 3) | Reserve\_Network\_Resource | Request/Response | VAL server |
| Request\_Unicast\_Resource | Request/Response | VAL server |
| Update\_Unicast\_Resource | Request/Response | VAL server |
| Request\_Multicast\_Resource | Request/Response | VAL server |
| Notify\_UP\_Delivery\_Mode | Subscribe/Notify | VAL server |
| Discover\_TSC\_Stream\_Availability | Request/Response | VAL server |
| Create\_TSC\_Stream | Request/Response | VAL server |
| Delete\_TSC\_Stream | Request/Response | VAL server |
| Create\_MBS\_Resource | Request/Response | VAL server |
| Update\_MBS\_Resource | Request/Response | VAL server |
| Delete\_MBS\_Resource | Request/Response | VAL server |
| Activate\_MBS\_Resource | Request/Response | VAL server |
| Deactivate\_MBS\_Resource | Request/Response | VAL server |
| Reliable\_Transmission\_Request | Request/Response | e.g., SEALDD Server, VAL Server |
| Subscribe\_Unified\_Traffic\_Pattern\_and\_Monitoring\_Management | Subscribe/Notify | VAL server |
| Update\_Unified\_Traffic\_Pattern\_and\_Monitoring\_Management\_Subscription |
| Unsubscribe\_Unified\_Traffic\_Pattern\_and\_Monitoring\_Management |
| Notify\_Unified\_Traffic\_Pattern\_Update |
| SS\_EventsMonitoring | Subscribe\_Monitoring\_Events | Subscribe/Notify | VAL server |
| Notify\_Monitoring\_Events |
| SS\_Events | Subscribe\_Event | Subscribe/Notify | VAL server |
| Notify\_Event | VAL server |
| Unsubscribe\_Event | VAL server |
| Update\_Subscription | VAL server |
| SS\_KeyInfoRetrieval | Obtain\_Key\_Info | Request/Response | VAL server |
| SS\_KMParametersProvisioning | Request | Request/Response | VAL server |
| SS\_NetworkResourceMonitoring | Subscribe\_Unicast\_QoS\_Monitoring\_Data | Subscribe/Notify | VAL server |
| Unsubscribe\_Unicast\_QoS\_Monitoring\_Data | VAL server |
| Notify\_Unicast\_QoS\_Monitoring\_Data | VAL server |
| Obtain\_Unicast\_QoS\_Monitoring\_Data | Request/Response | VAL server |
| Update\_Unicast\_QoS\_Monitoring\_Subscription | VAL server |
| SS\_IdmParameterProvisioning | Provide\_Configuration | Request/Response | VAL server |
| Get\_Configuration |
| Update\_Configuration |
| Delete\_Configuration |
| SS\_ADAE\_VALPerformanceAnalytics | Subscribe\_VAL\_Performance\_Analytics | Subscribe/Notify | VAL server |
| Notify\_VAL\_Performance\_Analytics |
| Unsubscribe\_VAL\_Performance\_Analytics |
| SS\_ADAE\_SlicePerformanceAnalytics API | Subscribe\_Slice\_Performance\_Analytics | Subscribe/Notify | VAL server |
| Notify\_Slice\_Performance\_Analytics |
| Unsubscribe\_Slice\_Performance\_Analytics |
| SS\_ADAE\_Ue2UePerformanceAnalytics | UE-to-UE\_Performance\_Analytics\_Subscribe | Subscribe/Notify | VAL server |
| UE-to-UE\_Performance\_Analytics\_Notify |
| UE-to-UE\_Performance\_Analytics\_Unsubscribe |
| SS\_ADAE\_LocationAccuracyAnalytics | Subscribe\_Location\_Accuracy\_Analytics | Subscribe/Notify | VAL server |
| Notify\_Location\_Accuracy\_Analytics |
| Unsubscribe\_Location\_Accuracy\_Analytics |
| SS\_ADAE\_ServiceApiAnalytics | Subscribe\_Service\_API\_Analytics | Subscribe/Notify | VAL server |
| Notify\_Service\_API\_Analytics |
| Unsubscribe\_Service\_API\_Analytics |
| SS\_ADAE\_SliceUsagePatternAnalytics | Subscribe\_Slice\_Usage\_Pattern\_Analytics | Subscribe/Notify | VAL server, NSCE server |
| Notify\_Slice\_Usage\_Pattern\_Analytics |
| Unsubscribe\_Slice\_Usage\_Pattern\_Analytics |
| Get\_Slice\_Usage\_Stats | Request/Response | VAL server, NSCE server |
| SS\_ADAE\_EdgeLoadAnalytics | Subscribe\_Edge\_Load | Subscribe/Notify | VAL server, EAS, EESVAL server, EAS, EESVAL server, EAS, EES |
| Notify\_Edge\_Load |
| Unsubscribe\_Edge\_Load |
| Get\_Edge\_Load\_Data | Request/Response | VAL server, EAS, EES |
| SS\_AADRF\_DataManagement | SS\_AADRF\_DataManagement\_Subscribe | Subscribe/Notify | ADAE server |
| SS\_AADRF\_DataManagement\_Unsubscribe |
| SS\_AADRF\_DataManagement\_Notify |
| NOTE 1: The service operations of SS\_Events API are reused by the SS\_LocationInfoEvent, SS\_LocationMonitoring, SS\_LocationAreaMonitoring, SS\_GroupManagementEvent, SS\_UserProfileEvent and SS\_EventsMonitoring for events related services.NOTE 2: The service APIs exposed by the SEALDD Server and the corresponding service operations, operation semantics and service consumers are specified in clause 5 of 3GPP TS 29.548 [35].NOTE 3: The "Create\_MBS\_Resource", "Update\_MBS\_Resource", "Delete\_MBS\_Resource", "Activate\_MBS\_Resource" and "Deactivate\_MBS\_Resource" service operations correspond to the stage 2 "Request\_Multicast/Broadcast\_Resource", "Update\_Multicast/Broadcast\_Resource", "Delete\_Multicast/Broadcast\_Resource", "Activate\_Multicast\_Resource" and "Deactivate\_Multicast\_Resource" service operations defined in clause 14.4.2 of 3GPP TS 23.434 [2].NOTE 4: The service APIs exposed by the NSCE Server and the corresponding service operations, operation semantics and service consumers are specified in clause 5 of 3GPP TS 29.435 [42]. |

Table 5.1-2 summarizes the corresponding APIs defined in this specification.

Table 5.1-2: API Descriptions

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Service Name** | **Clause** | **Description** | **OpenAPI Specification File** | **apiName** | **Annex** |
| SS\_LocationReporting | 7.1.1 | Report Location Information Service. | TS29549\_SS\_LocationReporting.yaml | ss-lr | A.2 |
| SS\_GroupManagement | 7.2 | Group Management Service | TS29549\_SS\_GroupManagement.yaml | ss-gm | A.3 |
| SS\_UserProfileRetrieval | 7.3 | User Profile Retrieval Service | TS29549\_SS\_UserProfileRetrieval.yaml | ss-upr | A.4 |
| SS\_NetworkResourceAdaptation | 7.4 | Network Resource Adaptation Service | TS29549\_SS\_NetworkResourceAdaptation.yaml | ss-nra | A.5 |
| SS\_Events | 7.5 | Events Notify Service | TS29549\_SS\_Events.yaml | ss-events | A.6 |
| SS\_KeyInfoRetrieval(NOTE 2) | 7.6 | Key Information Retrieval Service | TS29549\_SS\_KeyInfoRetrieval.yaml | ss-kir | A.7 |
| SS\_LocationAreaInfoRetrieval | 7.1.2 | Location Area Info Retrieval Service | TS29549\_SS\_LocationAreaInfoRetrieval.yaml | ss-lair | A.8 |
| SS\_NetworkResourceMonitoring | 7.4 | Network Resource Monitoring | TS29549\_SS\_NetworkResourceMonitoring.yaml | ss-nrm | A.10 |
| SS\_VALServiceData | 7.3 | VAL Service Data Service | TS29549\_SS\_VALServiceData.yaml | ss-vsd | A.11 |
| SS\_VALServiceAreaConfiguration | 7.1.3 | VAL Service Area Configuration Service | TS29549\_SS\_VALServiceAreaConfiguration.yaml | ss-vsac | A.12 |
| SS\_KMParametersProvisioning(NOTE 3) | 7.6 | Key Management Parameters Provisioning Service | TS29549\_SS\_KMParametersProvisioning.yaml | ss-kpp | A.14 |
| SS\_ADAE\_VALPerformanceAnalytics | 7.10 | ADAE VAL performance analytics service | TS29549\_SS\_ADAE\_VALPerformanceAnalytics.yaml | ss-adae-pa | A.15 |
| SS\_ADAE\_SlicePerformanceAnalytics | 7.10 | ADAE slice specific application performance analytics service | TS29549\_SS\_ADAE\_SlicePerformanceAnalytics.yaml | ss-adae-sspa | A.16 |
| SS\_ADAE\_Ue2UePerformanceAnalytics | 7.10 | ADAE UE-to-UE PerformanceAnalytics Service | TS29549\_SS\_ADAE\_Ue2UePerformanceAnalytics.yaml | ss-adae-uupa | A.17 |
| SS\_ADAE\_LocationAccuracyAnalytics | 7.10 | ADAE location accuracy performance analytics service | TS29549\_SS\_ADAE\_LocationAccuracyAnalytics.yaml | ss-adae-laa | A.18 |
| SS\_ADAE\_ServiceApiAnalytics | 7.10 | ADAE service API analytics service | TS29549\_SS\_ADAE\_ServiceApiAnalytics.yaml | ss-adae-sa | A.19 |
| SS\_ADAE\_SliceUsagePatternAnalytics | 7.10 | ADAE slice usage pattern analytics service | TS29549\_SS\_ADAE\_SliceUsagePatternAnalytics.yaml | ss-adae-sup | A.20 |
| SS\_ADAE\_EdgeLoadAnalytics | 7.10.7 | Edge load analytics service | TS29549\_SS\_ADAE\_EdgeLoadAnalytics.yaml | ss-adae-el | A.21 |
| SS\_AADRF\_DataManagement | 7.10.8 | A-ADRF Data Management Service | TS29549\_SS\_AADRF\_DataManagement.yaml | ss-aadrf-datamanagement | A.22 |
| SS\_SLPositioningManagement | 7.1.4 | SL Positioning Management service | TS29549\_SS\_SLPositioningManagement.yaml | ss-slpm | A.23 |
| NOTE 1: The APIs exposed by the SEALDD Server are specified in clause 5 of 3GPP TS 29.548 [35].NOTE 2: The stage 2 requirements for this API are defined in clause 5.3 of 3GPP TS 33.434 [26].NOTE 3: The stage 2 requirements for this API are defined in clause 5.8 of 3GPP TS 33.434 [26].NOTE 4: The APIs exposed by the NSCE Server are specified in clause 5 of 3GPP TS 29.435 [42]. |

\*\*\* Next Change \*\*\*

### 5.2.8 SS\_SLPositioningManagement API

#### 5.2.8.1 Service Description

The SS\_SLPositioningManagement API, as defined 3GPP TS 23.434 [2], enables a service consumer to:

- create/update/delete a SL Positioning Management Subscription; and

- receive SL Positioning related event(s) reporting.

#### 5.2.8.2 Service Operations

##### 5.2.8.2.1 Introduction

The service operations defined for the SS\_SLPositioningManagement API are shown in the table 5.2.8.2.1-1.

Table 5.2.8.2.1-1: Service operations of the SS\_SLPositioningManagement API

|  |  |  |
| --- | --- | --- |
| Service operation name | Description | Initiated by |
| SS\_SLPositioningManagement\_Subscribe | This service operation is used by a service consumer to create/update/delete a SL Positioning Management Subscription. | VAL Server |
| SS\_SLPositioningManagement\_Notify | This service operation is used by the LM Server to notify on SL Positioning related event(s). | SEAL Server |
|  |  |  |
|  |  |  |

##### 5.2.8.2.2 SS\_SLPositioningManagement\_Subscribe

###### 5.2.8.2.2.1 General

This service operation is used by a service consumer to request the creation of a SL Positioning Management Subscription at the LM Server.

The following procedures are supported by the "SS\_SLPositioningManagement\_Subscribe" service operation:

- SL Positioning Management Subscription Creation.

- SL Positioning Management Subscription Update.

- SL Positioning Management Subscription Deletion.

###### 5.2.8.2.2.2 SL Positioning Management Subscription Creation

This procedure is used by a service consumer to request the LM Server to create a SL Positioning Management Subscription.

1. In order to request the creation of a SL Positioning Management Subscription, the service consumer shall send an HTTP POST request to the LM Server targeting the "SL Positioning Management Subscriptions" collection resource, with the request body including the SlPositionMgmtSubsc data structure.

2a. Upon success, the LM Server shall respond with an HTTP "201 Created" status code with the response body containing a representation of the created "Individual SL Positioning Management Subscription" resource within the SlPositionMgmtSubsc data structure.

2b. On failure, the appropriate HTTP status code indicating the error shall be returned and appropriate additional error information should be returned in the HTTP POST response body, as specified in clause 7.1.4.7.

###### 5.2.8.2.2.3 SL Positioning Management Subscription Update

This procedure is used by a service consumer to request the LM Server to update an existing SL Positioning Management Subscription Subscription.

1. In order to request the update/modification of an existing SL Positioning Management Subscription, the service consumer shall send an HTTP PUT/PATCH request to the LM Server targeting the corresponding "Individual SL Positioning Management Subscription" resource, with the request body including either:

- the updated representation of the resource within the SlPositionMgmtSubsc data structure, in case the HTTP PUT method is used; or

- the requested modifications to the resource within the SlPositionMgmtSubscPatch data structure, in case the HTTP PATCH method is used.

If the LM Server is not able to handle the request, it may respond with an HTTP "307 Temporary Redirect" status code or an HTTP "308 Permanent Redirect" status code including an HTTP "Location" header containing an alternative URI of the resource located in an alternative LM Server, as defined in clause 5.2.10 of 3GPP TS 29.122 [3].

2a. Upon success, the LM Server shall respond with either:

- an HTTP "200 OK" status code with the response body containing a representation of the updated/modified "Individual SL Positioning Management Subscription" resource within the SlPositionMgmtSubsc data structure; or

- an HTTP "204 No Content" status code.

2b. On failure, the appropriate HTTP status code indicating the error shall be returned and appropriate additional error information should be returned in the HTTP PUT/PATCH response body, as specified in clause 7.1.4.7.

###### 5.2.8.2.2.4 SL Positioning Management Subscription Deletion

This procedure is used by a service consumer to request the LM Server to delete an existing SL Positioning Management Subscription.

1. In order to request the deletion of an existing SL Positioning Management Subscription, the service consumer shall send an HTTP DELETE request to the LM Server targeting the corresponding "Individual SL Positioning Management Subscription" resource.

2a. Upon success, the LM Server shall respond with an HTTP "204 No Content" status code.

2b. On failure, the appropriate HTTP status code indicating the error shall be returned and appropriate additional error information should be returned in the HTTP DELETE response body, as specified in clause 7.1.4.7.

\*\*\* Next Change \*\*\*

##### 5.2.8.2.3 SS\_SLPositioningManagement\_Notify

###### 5.2.8.2.3.1 General

This service operation is used by the LM Server to notify on SL Positioning related event(s).

The following procedures are supported by the "SS\_SLPositioningManagement\_Notify" service operation:

- SL Positioning Management Event Notification.

###### 5.2.8.2.3.2 SL Positioning Management Event Notification

This procedure is used by the LM Server to notify on SL Positioning related event(s).

1. In order to notify a previously subscribed service consumer on SL Positioning related event(s), the LM Server shall send an HTTP POST request to the service consumer with the request URI set to "{notifUri}", where the "notifUri" variable is set to the value received from the service consumer during the creation/update of the corresponding SL Positioning Management Subscription using the procedures defined in clauses 5.2.8.2.2, and the request body including the SlPositionMgmtNotif data structure.

2a. Upon success, the service consumer shall respond to the LM Server with an HTTP "204 No Content" status code to acknowledge the reception of the notification.

2b. On failure, the appropriate HTTP status code indicating the error shall be returned and appropriate additional error information should be returned in the HTTP POST response body, as specified in clause 7.1.4.7.

\*\*\* End of Changes \*\*\*