**3GPP TSG RAN WG4 Meeting # *R4-2417642r1***

**, 18th – 22nd November 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **2525** | **rev** | **-** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | (5G\_V2X\_NRSL-Core) CR to 38.101-1 Rel-17 Cat-A for 7.6E.3.1 Out-of-band blocking for V2X non-concurrent operation |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | 5G\_V2X\_NRSL-Core |  | ***Date:*** | 8 |
|  |  |  |  |  |
| ***Category:*** | **A** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Interference frequency step size and exceptions allowed for spurious response frequencies are missing in 7.6E.3.1. |
|  |  |
| ***Summary of change:*** | Interference frequency step size and exceptions allowed for spurious response frequencies were added in 7.6E.3.1. |
|  |  |
| ***Consequences if not approved:*** | 1. Interference frequency step size will remain missing in 7.6E.3.1
2. 7.7E.1 will be not needed if no exceptions are allowed for spurious response frequencies in 7.6E.3.1.
 |
|  |  |
| ***Clauses affected:*** | 7.6E.3.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **x** |  |  Test specifications | TS 38.521-1 |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<< Unchanged sections omitted >>

### 7.6E.3 Out-of-band blocking

#### 7.6E.3.1 General

For NR V2X bands out-of-band band blocking is defined for an unwanted CW interfering signal falling outside a frequency range 30 MHz below or above the UE receive band. When UE is configured for NR V2X reception non-concurrent with NR uplink transmissions for NR V2X operating bands specified in Table 5.2E.1-1, the throughput of the wanted signal shall be ≥ 95% of the maximum throughput of the reference measurement channels as specified in Annexes A.7.2 with parameters specified in Table 7.6E.3.1-1 and Table 7.6E.3.1-2. The relative throughput requirement shall be met for any SCS specified for the channel bandwidth of the wanted signal.

For interferer frequencies across ranges 1, 2 and 3 in Table 7.6E.3.1-2, a maximum of

 

exceptions are allowed for spurious response frequencies in each assigned frequency channel when measured using a step size of MHz withthe number of resource blocks in the downlink transmission bandwidth configuration, BWChannelthe bandwidth of the frequency channel in MHz and *n* = 1, 2, 3 for SCS = 15, 30, 60 kHz, respectively. For these exceptions, the requirements in clause 7.7E.1 apply.Table 7.6E.3.1-1: Out-of-band blocking parameters for NR V2X

|  |  |  |
| --- | --- | --- |
| RX parameter | Units | Channel bandwidth |
|  |  | 5 MHz2 | 10 MHz | 20 MHz | 30 MHz | 40 MHz |
| Power in transmission bandwidth configuration | dBm | PREFSENS\_V2X + channel bandwidth specific value below |
|  | dB | 6 | 6 | 9 | 11 | 12 |
| NOTE 1: Reference measurement channel is A.7.2.NOTE 2: The CBW is only applicable for PS UE in n14. |

Table 7.6E.3.1-2: Out of-band blocking for NR V2X

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NR band | Parameter | Units | Range 1 | Range 2 | Range 3 |
| n14 | Pinterferer | dBm | -44 | -30 | -15 |
| Finterferer (CW) | MHz | -60 < f – FDL\_low < -15or15 < f – FDL\_high < 60 | -85 < f – FDL\_low ≤ -60or60 ≤ f – FDL\_high < 85 | 1 ≤ f ≤ FDL\_low – 85orFDL\_high + 85 ≤ f≤ 12750 |
| n47 | Pinterferer | dBm | -44 | -30 | -15 |
|  | Finterferer (CW) | MHz | FDL\_low -30 toFDL\_low -60 | FDL\_low -60 toFDL\_low -85 | FDL\_low -85 to1 MHz |
|  |  |  | FDL\_high +30 toFDL\_high + 60 | FDL\_high +60 toFDL\_high +85 | FDL\_high +85 to+12750 MHz |
| n38 | Pinterferer | dBm | -44 | -30 | -15 |
|  | Finterferer (CW) | MHz | FDL\_low -30 toFDL\_low -60 | FDL\_low -60 toFDL\_low -85 | FDL\_low -85 to1 MHz |
| NOTE 1: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm for FInterferer > 4400 MHz. |

#### 7.6E.3.2 Out-of-band blocking for V2X concurrent operation

For the inter-band concurrent NR V2X operation, the requirements specified in clause 7.6E.3.1 shall apply for the NR sidelink reception in Band n47 and the requirements specified in clause 7.6.3 shall apply for the NR downlink reception in licensed band while all downlink carriers are active.

<< End of changes >>