**3GPP TSG-RAN WG4 Meeting #113 R4-2420394**

**Orlando, US, 18th – 22nd November, 2024**

**Agenda item:** 7.23.5

**Source:** Moderator (vivo)

**Title:** WF on UE RF requirements for LP-WUS

**Document for:** Approval

# Introduction

This is WF for Rel-19 LP-WUS UE RF.

# Topic #1: General and system parameters

### Sub-topic 1-1 General

**Issue 1-1-3: General issue on how to introduce LP-WUS feature into core specs 38.101-x**

Agreements:

* + **Add a new suffix “M” as “LP-WUS/WUR”**

**Issue 1-1-4: views on which requirements should be updated in core spec**

Agreements:

* + **The part should be updated for LP-WUS/WUR in spec.**
		- **The additional requirements are not precluded, if needed.**

|  |  |
| --- | --- |
| **Sections or requirements** | **Needed or not?** |
| Operation bands | FFS |
| UE channel bandwidth | FFS |
| Channel raster | FFS |
| REFSENS | YES |
| Maximum input level | YES |
| ACS | YES |
| ASCS | YES |
| In-band blocking | YES |
| Out-of-band blocking | YES |
| Narrow band blocking | YES |
| Spurious response | FFS |
| Wide band Intermodulation | FFS |
| Spurious emissions | FFS |
| Annex A Measurement channels | YES |

### Sub-topic 1-2 System parameters

**Issue 1-2-1: Channel raster for LP-WUR**

Agreements:

* + **No new channel raster is introduced dedicated for LP-WUS/WUR.**
		- **FFS on whether there is need of the limited set of frequencies supported by LP-WUS to reduce the receiver complexity and cost**

# Topic #2: REFSENS, ASCS and ACS requirements

### Sub-topic 2-1 SNR simulation and values

**Issue 2-1-1: Target FR1 SNR value for LP-WUS/WUR**

Agreements:

* + **Agree generally that for OOK-based, use worst case waveform of OOK-4 M=4 to derive SNR.**
		- **Some detailed aspects should be also confirmed, e.g., CRC bit (8), sequence length (8, 16), codepoint length of known part of the sequence)**

**Issue 2-1-3: Link level simulation assumption for FR2 LP-WUR**

Agreements:

* + **Further discussions and alignment on FR2 RF simulation assumption is needed.**

### Sub-topic 2-2 NF and REFSENS requirements

**Issue 2-2-1: General views on REFSENS for LP-WUS**

Agreements:

* + **Discuss REFSENS for the two types of receivers respectively, and then check if one single value or two values are specified pending on the final REFSENS values.**

**Issue 2-2-3: companies input on SNR, NF and IM value for FR1 OOK-based LR**

* Proposals
	+ **Proposal 1: check the following input from companies and converge the range for OOK-based LR. (Moderator)**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **FR1 OOK-based receiver** | **Huawei** | **Sony** | **Spread****trum** | **Apple** | **vivo** | **QC** | **Samsung** | **LGE** | **CMCC** | **ZTE** | **Nokia** | **E//** |
| IM(dB) | 2.5 | 2.5 | 2.5 | >=2.5 | 2.5 | 2.5 | 3 | 2.5 | 2.5 | 2.5 | 1 | 2.5 |
| NF(dB) (assume MR=9dB) | 17 | 10 | 17 | 16 | 15 | 11.5 | 15 | 16 | 12 | 14 | 12 | 12 |
| SNR(dB) | -2 | -7~-2 | -3 |  | -2 | -1 for sequence length of 18 | -2 |  | -2.5 | -2 |  | -1.5~-5 |
| RFESENS(dB) |  |  | -90.5 |  |  |  |  |  |  | -93.5/-96.5 |  |  |

Agreements:

* + **Use 2.5dB IM as a starting point, encourage companies to report the difference aspects due to OOK waveform receiver. Tighten or relaxed values are not precluded. The corresponding band should also be reported.**
	+ **The total value of NF+IM can be considered.**
	+ **On how to handle the NF values:**
		- **Option 1: For NF whether average value can be adopted.**
		- **Option 2: two sets NFs for different LP-WUR types with different power consumption target**
		- **Option 3: also consider coverage**
	+ **Capture the table in WF as background information**

**Issue 2-2-4: companies input on SNR, NF and IM value for FR1 OFDM-based LR**

* Proposals
	+ **Proposal 1: check the following input from companies and converge the range for OFDM-based LR. (Moderator)**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **FR1 OFDM-based receiver** | **Huawei** | **Sony** | **Spread****trum** | **Apple** | **vivo** | **QC** | **Samsung** | **LGE** | **CMCC** | **ZTE** | **Nokia** | **E//** |
| IM(dB) | 2.5 | 2.5 | 2.5 | >=2.5 | 2.5 |  |  | 2.5 | 2.5 | 2.5 | 1 | 2.5 |
| NF(dB)(assume MR=9dB) | 11 | 10 | 11 | 16 | 11 |  |  | 12 | 9 | 11 | 12 | 12~13 |
| SNR(dB) | -2 | -7~-2 | -3 |  | -2 or -5 |  |  |  | -4.7 | -5 |  | -3.2 |
| RFESENS(dB) |  |  | -96.5 |  |  |  |  |  |  | -99.5/-102.5 |  |  |

Agreements:

* + **Further discuss next meeting**

**Issue 2-2-6: Baseline OFDM-based architecture for FR2 LP-WUR**

Agreements:

* + **FR2 LPWUR adopts zero-IF topology baseline assumption. FFS details**
		- **Multiple frequency conversion in RF domain is not precluded**
	+ **For deriving a sensitivity requirement, the baseline OFDM-based FR2 LPWUR architecture is assumed to have the following features:**
		- **It comprises 2 Rx chains, and the antennas attached to the respective chains are mutually orthogonally polarized**
		- **FFS on whether and how to combine two Rx chains**
		- **Antenna gain is that of a single element**
		- **Coverage target should be considered**

### Sub-topic 2-3 ASCS simulation and requirements

**Issue 2-3-1: Required number of guard RB for ASCS**

Agreements:

* + **[0RB] as guard RB for ASCS.**

**Issue 2-3-2: Detailed Test case for ASCS**

WF:

* + **RAN4 further discuss the test case next meeting**

### Sub-topic 2-4 ACS simulation and requirements

**Issue 2-4-1: Phase noise for simulation assumption**

Agreements:

* + **Companies can use different phase noise assumptions, the phase noise assumption should be reported**

 **Issue 2-4-2: General ACS requirements value and guard RB**

Agreements:

* + **For ACS evaluation, companies are encouraged to provide the simulation results by assuming**
		- **Baseline: the same interference experienced by LP-WUR and main radio.**
		- **Optional: the different interference level for LP-WUR and main radio**

**Issue 2-4-4: Test parameters for LP-WUR ACS case**

WF:

* + **RAN4 further discuss detailed test parameters table and how to modify spec.**

# Topic #3: Other RF requirements

### Sub-topic 3-1 IBB, OBB and Intermodulation requirements for UE RF

**Issue 3-1-1: IBB, OBB requirements**

* Proposals
	+ **Option 1: the interference levels for IBB could be relaxed compared to the values defined for MR (at least for the LP-WUR type which targets ultra-low power consumption). OBB could be kept unchanged at least for LP-WUR type which targets moderate power consumption, FFS for ultra-low power consumption LP-WUR.**
	+ **Option 2: In-band blocking requirement for legacy UE could be reused. the OBB requirement for legacy UE in TS 38.101-1 could be reused.**

WF:

* + Further discuss IBB and OBB requirements

**Issue 3-1-3: detailed table for test parameters of IBB and OBB test case**

* Proposals
	+ **Proposal 1: further discuss detailed test parameters table and how to modify spec, after concluding IBB and OBB requirements value and guard RBs.**

WF:

* + FFS

### Sub-topic 3-2 Other Rx requirements

**Issue 3-2-1: spurious response requirements**

* Proposals
	+ **Option 1: spurious response should be relaxed at least for the LP-WUR type which targets ultra-low power consumption. (Huawei)**
	+ **Option 2: Reuse the spurious response requirements from TS 38.101-1 for LP-WUR. (ZTE)**

WF:

* + FFS whether spurious response can be relaxed

**Issue 3-2-2: Maximum input level requirements**

Agreements:

* + **For maximum input power level, further discuss**
		- **Option 1: use legacy -25dBm**
		- **Option 2: scaled to -26.5dBm.**

# Topic #4: Testability issues

### Sub-topic 4-1 Testability for UE RF requirements

**Issue 4-1-1: alignment of common understanding on LP-WUS requirements and corresponding testing**

Agreements:

* + **The same LP-WUS RF requirements for all three RRC states are assumed. But only one RRC state needs to be tested.**

**Issue 4-1-2: General framework of** **interface between the MR and the LR to verify RF performance**

Agreements:

* + **Group discuss and conclude the general framework for LP-WUS performance verification, consider the following as starting point:**
		- **Option 1: Counter the detection rate without waking up the MR would be enough to verify LP-WUS RF performance. The MR should only be woken up when data transfer the system simulator is needed.**
		- **Other options are not precluded.**
		- **NOTE: FFS on [During the test, it is expected that only the intended WUS sequence will be counted, if the intended WUS sequence, WUS sequence not intended for UE under test, and/or missing WUS during monitoring occasion are transmitted during the test].**