**3GPP TSG RAN WG4 Meeting # *R4-24XXXXX***

**, 18th – 22nd November 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **0048** | **rev** | **-** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | (LTE\_NBIoT\_eMTC\_NTN\_req-Perf) CR to 36.102 Rel-18 Cat-F for the Note in Table 8.2.1.2-1 |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | LTE\_NBIoT\_eMTC\_NTN\_req-Perf |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Note in Table 8.2.1.2-1 leads to the misunderstanding that the requirements in TS36.101[7] Clause 8 and Clause 9 apply to testing under NTN access mode. |
|  |  |
| ***Summary of change:*** | Note in Table 8.2.1.2-1 was revised to carify that UE that supports NTN access (ntn-Connectivity-EPC-r17) shall also support TN access. The requirements in TS36.101[7] Clause 8 and Clause 9 only apply to testing under TN access mode. |
|  |  |
| ***Consequences if not approved:*** | It will lead to the misunderstanding that the requirements in TS36.101[7] Clause 8 and Clause 9 apply to testing under NTN access mode. |
|  |  |
| ***Clauses affected:*** | 8.2.1.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **x** |  |  Test specifications | TS 36.521-4 |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<< Unchanged sections omitted >>

8.2.1.2 Applicability of requirements for optional UE features

The performance requirements in Table 8.2.1.2-1 shall apply for UEs which support optional UE features only. If same test is listed for different UE features/capabilities in Clauses 8.2.1.2, then this test shall apply for UEs which support all corresponding UE features/capabilities.

**Table 8.2.1.2-1: Requirements applicability for optional UE features**

|  |  |  |
| --- | --- | --- |
| **UE feature/capability** | **Test list** | **Applicability notes** |
| NTN access (ntn-Connectivity-EPC-r17) | Clause 8.2.1.1 (Test 1, Test 2, Test 3) | The requirements apply only for UE Category M1 |
| Clause 8.3.1.1 (Test 1, Test 2) | The requirements apply only for UE Category NB1, NB2 |
| NTN scenario support (ntn-ScenarioSupport-r17) | Clause 8.2.1.1 (Test 1, Test 2, Test 3) | The requirements apply only for UE Category M1, and only when ntn-ScenarioSupport-r17 is “ngso” or is not included |
| Clause 8.3.1.1 (Test 1, Test 2) | The requirements apply only for UE Category NB1, NB2, and only when ntn-ScenarioSupport-r17 is “ngso” or is not included |
| Operation in coverage enhancement mode A (ce-ModeA-r13) | Clause 8.2.1.1 (Test 1, Test 2) | The requirements apply only for UE Category M1 |
| Operation in coverage enhancement mode B (ce-ModeB-r13) | Clause 8.2.1.1 (Test 3) | The requirements apply only for UE Category M1 |
| Note: UE that supports NTN access (ntn-Connectivity-EPC-r17) shall also support TN access. For the UE supporting NTN access (*ntn-Connectivity-EPC-r17*), the requirements in TS36.101 Clause 8 and Clause 9 also apply to UE according to the UE category and capability. |

<< End of changes >>