**3GPP TSG-CT WG1 Meeting #124-eC1-20aabb**

**Electronic meeting, 2-10 June 2020 was C1-203373**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **24.301** | **CR** | **3386** | **rev** | **1** | **Current version:** | **16.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction to implementation of CR #3338 |
|  |  |
| ***Source to WG:*** | MediaTek Inc. |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | PARLOS |  | ***Date:*** | 2020-06-05 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | In CR #3338 (approved in meeting #122-e), the below highlighted corrections has been modified for EMM-REGISTERED.LIMITED-SERVICE state:5.2.3.2.3 LIMITED-SERVICEThe UE:- shall perform cell selection/reselection according to 3GPP TS 36.304 [21]; - may respond to paging (with IMSI);- may detach locally and initiate attach for emergency bearer services;- may detach locally and initiate attach for access to RLOS; and- if configured for eCall only mode as specified in 3GPP TS 31.102 [17], shall perform the eCall inactivity procedure at expiry of timer T3444 or T3445 (see subclause 5.5.4).But while writing CR#3338 in current specification , the below highlighted modifications has been made which looks to be incorrectly written as per suggested in CR#3338:5.2.3.2.3 LIMITED-SERVICEThe UE:- shall perform cell selection/reselection according to 3GPP TS 36.304 [21]; - may detach locally and respond to paging (with IMSI);- may detach locally and initiate attach for emergency bearer services;- may initiate attach for access to RLOS; and- if configured for eCall only mode as specified in 3GPP TS 31.102 [17], shall perform the eCall inactivity procedure at expiry of timer T3444 or T3445 (see subclause 5.5.4).It need to correction in current specification so that CR#3338 will written correctly. |
|  |  |
| ***Summary of change:*** | Need correction in current specification as per CR#3338 |
|  |  |
| ***Consequences if not approved:*** | Wrong implementation may lead to unexpected results. |
|  |  |
| ***Clauses affected:*** | 5.2.3.2.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Rev#2:"may" removed in rev#1 is unremoved. |

##### 5.2.3.2.3 LIMITED-SERVICE

The UE:

- shall perform cell selection/reselection according to 3GPP TS 36.304 [21];

- may respond to paging (with IMSI);

- may detach locally and initiate attach for emergency bearer services;

- may detach locally and may initiate attach for access to RLOS; and

- if configured for eCall only mode as specified in 3GPP TS 31.102 [17], shall perform the eCall inactivity procedure at expiry of timer T3444 or T3445 (see subclause 5.5.4).