**3GPP TSG-CT WG1 Meeting #126-eC1-20xxxx**

**Electronic meeting, 15-23 October 2020 was C1-205994**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **24.486** | **CR** | **0029** | **rev** | **1** | **Current version:** | **16.1.0**  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Update to server procedure of V2X service discovery procedure |
|  |  |
| ***Source to WG:*** | Huawei, Hisilicon |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | V2XAPP |  | ***Date:*** | 2020-10-01 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The HTTP response message of the server procedure of V2X service discovery procedure is unclear, quote of Clause 6.6.2:*6.6.2 Server procedure**Upon reception of an HTTP POST request message containing:**a) a Content-Type header field set to "application/vnd.3gpp.vae-info+xml"; and**b) an application/vnd.3gpp.vae-info+xml MIME body with a <service-discovery-info> element in the <VAE-info> root element, the VAE-S:**1) shall reply with a HTTP response with a <result> element of the <service-discovery-info> element set to a value "success" or "fail", and may include a <service-discovery-data> element which provides the V2X UE service discovery data.*The HTTP response needs to be detailed. |
|  |  |
| ***Summary of change:*** | 1. Specify the HTTP response message;
 |
|  |  |
| ***Consequences if not approved:*** | The HTTP response message of the server procedure of V2X service discovery procedure is unclear. |
|  |  |
| ***Clauses affected:*** | 6.6.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

### 6.6.2 Server procedure

Upon reception of an HTTP POST request message containing:

a) a Content-Type header field set to "application/vnd.3gpp.vae-info+xml"; and

b) an application/vnd.3gpp.vae-info+xml MIME body with a <service-discovery-info> element in the <VAE-info> root element,

the VAE-S:

a) shall generate an HTTP 200 (OK) response according to IETF RFC 2616 [19]. In the HTTP 200 (OK) response message, the VAE-S:

1) shall include a Content-Type header field set to "application/vnd.3gpp.vae-info+xml"; and

2) shall include an application/vnd.3gpp.vae-info+xml MIME body with a <service-discovery-info> element in the <VAE-info> root element:

i) shall include a <result> child element set to the value "success" or "failure" indicating success or failure of getting the service discovery information; and

ii) if <result> element is set to “success”, shall include a <service-discovery-data> element with one or more <V2X-service-mapping> elements, each <V2X-service-mapping> shall include:

A) one or more <V2X-service-id> element(s) set to the identities of the available V2X service IDs; and

B) a <V2X-AS-address> element set to the V2X AS address; and

b) shall send the HTTP 200 (OK) response towards the VAE-C.

\* \* \* End of Change \* \* \* \*