**3GPP TSG-CT WG1 Meeting #126-eC1-20xxxx**

**Electronic meeting, 15-23 October 2020 was C1-206003**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **24.486** | **CR** | **0038** | **rev** | **1** | **Current version:** | **16.1.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | XML schema for V2X USD provisioning procedure | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, Hisilicon | | | | | | | | | |
| ***Source to TSG:*** | C1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | V2XAPP | | | | |  | ***Date:*** | | | 2020-10-01 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The specification needs to define the XML scheme for V2X USD provisioning procedure. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | 1. Add the XML scheme for V2X USD provisioning procedure; | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The XML scheme for V2X USD provisioning procedure is missing. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 8.4.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* First Change \* \* \* \*

### 8.4.2 XML schema

<?xml version="1.0" encoding="UTF-8"?>

<xs:schema xmlns:xs=<http://www.w3.org/2001/XMLSchema>

targetNamespace="urn:3gpp:ns:vaeInfo:1.0"

xmlns:vaeinfo="urn:3gpp:ns:vaeInfo:1.0"

elementFormDefault="qualified"

attributeFormDefault="unqualified"

xmlns:xenc="http://www.w3.org/2001/04/xmlenc#">

<!-- root XML element -->

<xs:element name="vae-info" type="vaeinfo:vaeinfo-Type" id="info"/>

<xs:complexType name="vaeinfo-Type">

<xs:sequence>

<xs:element name="registration-info" type="vaeinfo:tRegistrationType" minOccurs="0"/>

<xs:element name="V2XUSDAnouncement" type="vaeinfo:tV2XUSDAnouncementType"/>

</xs:sequence>

<xs:anyAttribute namespace="##any" processContents="lax"/>

</xs:complexType>

<xs:complexType name="tRegistrationType">

<xs:sequence>

<xs:element name="v2x-ue-id" type="vaeinfo:contentType" minOccurs="0" maxOccurs="1"/>

<xs:element name="v2x-service-id" type="xs:string" minOccurs="0" maxOccurs="unbounded"/>

<xs:element name="result" type="xs:string" minOccurs="0" maxOccurs="1"/>

<xs:any namespace="##other" processContents="lax"/>

</xs:sequence>

<xs:anyAttribute namespace="##any" processContents="lax"/>

</xs:complexType>

<xs:complexType name="tV2XUSDAnouncementType">

<xs:sequence>

<xs:element name="v2x-ue-id" type="vaeinfo:contentType" minOccurs="0" maxOccurs="1"/>

<xs:element name="v2xUSDConfigurationData" type="vaeinfo:tUSDType" minOccurs="1" maxOccurs="1"/>

<xs:element name="anyExt" type="vaeinfo:anyExtType" minOccurs="0"/>

</xs:sequence>

<xs:anyAttribute namespace="##any" processContents="lax"/>

</xs:complexType>

<xs:complexType name="contentType">

<xs:choice>

<xs:element name="vaeURI" type="xs:anyURI"/>

<xs:element name="vaeString" type="xs:string"/>

<xs:element name="vaeBoolean" type="xs:boolean"/>

<xs:any namespace="##other" processContents="lax"/>

</xs:choice>

<xs:anyAttribute namespace="##any" processContents="lax"/>

</xs:complexType>

</xs:schema>

\* \* \* End of Change \* \* \* \*