**3GPP TSG-CT WG1 Meeting #130-eC1-213310**

**Electronic meeting, 20-28 May 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **23.122** | **CR** |  0723 | **rev** | **-** | **Current version:** | **17.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | InterSystem handling of Tsor-CM timers. |
|  |  |
| ***Source to WG:*** | Samsung |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | eCPSOR\_CON |  | ***Date:*** | 2021-05-10 |
|  |  |  |  |  |
| ***Category:*** |  **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)...Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** |  During the last meeting Tsor-CM timer behavior for intersystem change case was proposed we think following behavior is appropriate:1) During network controlled intersystem change like HO or redirection there is no impact to Tsor-CM timer. i.e. if the Tsor-CM timer is running they continue to run. 2) When the timers expire or stopped action defined in C.4.2 is applicable only on 5GS.3) If the timer stops or expires when UE is not in 5GS for e.g. UE is in EPS then no actions are performed by the UE.  |
|  |  |
| ***Summary of change:*** | Tsor-CM timer expiry or stop event is ignored by the UE when it is not in the 5GS.  |
|  |  |
| ***Consequences if not approved:*** | UE behavior w.r.t Tsor-CM timer for intersystem change not available. |
|  |  |
| ***Clauses affected:*** | C.4.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\*\*\* First change \*\*\*\*\*

## C.4.2 Applying SOR-CMCI in the UE

During SOR procedure and while applying SOR-CMCI, the UE shall determine the time to release the PDU session(s) as follows:

- If the UE has a configured "user controlled list of services exempted from release due to SOR" and a matching criterion is found for a service included in the "user controlled list of services exempted from release due to SOR", the UE shall set the Tsor-cm timer associated to the service to infinity;

- If one or more SOR-CMCI rules are included in SOR-CMCI, where for each criterion:

a) DNN of the PDU session:

 the UE shall check whether it has a PDU session with a DNN matching to the DNN included in SOR-CMCI, and if any, the UE shall set the associated timer Tsor-cm to the value included in the SOR-CMCI;

b) S-NSSAI of the PDU session:

 the UE shall check whether it has a PDU session with a S-NSSAI matching the S-NSSAI included in SOR-CMCI, and if any, the UE shall set the associated timer Tsor-cm to the value included in the SOR-CMCI;

c) IMS registration related signalling:

 the UE shall check whether IMS registration related signalling is ongoing as specified in 3GPP TS 24.501 [64], and if it is ongoing, the UE shall set the associated timer Tsor-cm to the value included in the SOR-CMCI;

d) MMTEL voice call:

 the UE shall check whether MMTEL voice call is ongoing as specified in 3GPP TS 24.501 [64], and if it is ongoing, the UE shall set the associated timer Tsor-cm to the value included in the SOR-CMCI;

e) MMTEL video call:

 the UE shall check whether MMTEL video call is ongoing as specified in 3GPP TS 24.501 [64], and if it is ongoing, the UE shall set the associated timer Tsor-cm to the value included in the SOR-CMCI;

f) MO SMS over NAS or MO SMSoIP:

 the UE shall check whether MO SMS over NAS or MO SMSoIP services is ongoing as specified in TS 24.501 [64], and if it is ongoing, the UE shall set the associated timer Tsor-cm to the value included in the SOR-CMCI; or

g) match all:

 the UE shall set the associated timer Tsor-cm to the value included in the SOR-CMCI;

- otherwise, the UE shall consider the timer value for Tsor-cm equal to zero.

The UE shall start all applicable Tsor-cm timers.

While one or more Tsor-cm timers are running, the UE shall check the newly established PDU session or service for a matching criterion in the SOR-CMCI:

- If the UE has a configured "user controlled list of services exempted from release due to SOR" and a matching criterion is found for a service included in the "user controlled list of services exempted from release due to SOR", the UE shall set the Tsor-cm timer associated to the service to infinity;

- If a matching criterion is found and the applicable Tsor-cm timer indicated the value "infinity" then the UE shall set the Tsor-cm timer associated to the PDU session to infinity; or

- For all other cases, if a matching criterion is found then the UE shall set the Tsor-cm timer associated to the newly established PDU session, or service, with the exception that if the value of the Tsor-cm timer exceeds the highest value among the current values of all running Tsor-cm timers, then the value of the Tsor-cm timer for the new PDU session or service shall be set to the highest value among the current values of all running Tsor-cm timers.

NOTE 1: For newly established PDU session or service as described above, the timer is set irrespective of whether other ongoing PDU sessions or services that match the same criteria exist and for which corresponding Tsor-cm timers are running.

NOTE 2: NAS 5GMM layer will receive an explicit indication from the upper layers that a service is started or stopped. When a service is started, it is handled as a new service in the procedures described in this subclause.

NOTE 3: While one or more Tsor-cm timers are running, the UE can trigger any 5GSM procedure or start new services.

While one or more Tsor-cm timers are running, upon receiving a new SOR-CMCI as described in annex C.3, the UE shall check if there is a matching criterion found for any ongoing PDU session or service in the new SOR-CMCI:

- if the UE has a configured "user controlled list of services exempted from release due to SOR" and a matching criterion is found for a service included in the "user controlled list of services exempted from release due to SOR", the UE shall set the Tsor-cm timer associated to the service to infinity;

- if a matching criterion is found and the value of Tsor-cm timer in the new SOR-CMCI indicates the value "infinity", then the Tsor-cm timer value for the associated PDU session or service shall be set to infinity;

- if a matching criterion is found and the value of Tsor-cm timer in the new SOR-CMCI is other than infinity and is smaller than the current value of the running Tsor-cm timer for the associated PDU session or service, then the Tsor-cm timer value for the associated PDU session or service shall be replaced with the value in the new SOR-CMCI without stopping and restarting the timer; or

- for all other cases, the running Tsor-cm timers for the associated PDU sessions or services are kept unchanged.

The timer Tsor-cm stops when the associated PDU session is released or the associated service is stopped.

If the UE enters idle mode or 5GMM-CONNECTED mode with RRC inactive indication (see 3GPP TS 24.501 [64]), while one or more Tsor-cm timers are running, then the UE stops the timer(s). In this case, if:

a) the UE has a list of available and allowable PLMNs in the area and based on this list or any other implementation specific means, the UE determines that there is a higher priority PLMN than the selected VPLMN; or

b) the UE does not have a list of available and allowable PLMNs in the area and is unable to determine whether there is a higher priority PLMN than the selected VPLMN using any other implementation specific means;

then the UE attempts to obtain service on a higher priority PLMN as specified in subclause 4.4.3.3 by acting as if timer T that controls periodic attempts has expired.

If the UE performs inter-system change due to network controlled inter RAT mobility (see 3GPP TS 36.331 [42] and 3GPP TS 38.331 [65]) the Tsor-cm timer(s) if running are not stopped. If the UE is not in 5GS, when the last running Tsor-cm timer stops or expires no actions are performed by the UE.

If the UE is in 5GS, when the last running Tsor-cm timer stops or expires not due to UE entering idle mode or 5GMM-CONNECTED mode with RRC inactive indication, if:

i) the UE has a list of available and allowable PLMNs in the area and based on this list or any other implementation specific means, the UE determines that there is a higher priority PLMN than the selected VPLMN; or

ii) the UE does not have a list of available and allowable PLMNs in the area and is unable to determine whether there is a higher priority PLMN than the selected VPLMN using any other implementation specific means;

then the UE shall perform the deregistration procedure (see clause 4.2.2.3 of 3GPP TS 23.502 [63]) that releases all the established PDU sessions and the UE enters idle mode and attempts to obtain service on a higher priority PLMN as specified in subclause 4.4.3.3 by acting as if timer T that controls periodic attempts has expired.

NOTE 4: The list of available and allowable PLMNs in the area is implementation specific.

The UE which has an emergency PDU session, receives a request from the upper layers to establish an emergency PDU session or perform emergency services fallback, registers for emergency services, or is configured for high priority access in the selected PLMN is not required to enter idle mode the last running Tsor-cm timer stops or expires. The UE shall attempt to perform the PLMN selection after the emergency PDU session or the high priority service is released, if any Tsor-cm timer was running and the last running Tsor-cm timer stopped or expired when the emergency PDU session or the high priority service was established and after the UE enters idle mode or 5GMM-CONNECTED mode with RRC inactive indication (see 3GPP TS 24.501 [64]).

\*\*\*\*\* End change \*\*\*\*\*