**3GPP TSG-CT WG1 Meeting #135-eC1-22xxxx**

**E-Meeting, 6th – 12th April 2022 *was* C1-222845**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **24.555** | **CR** | **0003** | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | ZTE, Nokia, Nokia Shanghai Bell | | | | | | | | | |
| ***Source to TSG:*** | C1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5G\_ProSe | | | | |  | ***Date:*** | | | 2022-04-08 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | According to TS 33.503, 5G PKMF addressing information may be provisioned by the PCF to the 5G ProSe layer-3 remote UE or the 5G ProSe layer-3 UE-to-network relay UE.  However, 5G PKMF addressing information is not defined in the UE policies for 5G ProSe UE-to-network relay UE and remote UE. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Define encoding of 5G PKMF addressing information in UE policies for 5G ProSe UE-to-network relay UE, and UE policies for 5G ProSe remote UE respectively. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Provisioning of 5G PKMF addressing information by PCF is not supported. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 3.2, 5.5.2, 5.6.2. | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**\*\*\*\*\*\*\***

\* \* \* First Change \* \* \* \*

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5G ProSe 5G Proximity-based Services

5G PKMF 5G ProSe Key Management Function

ProSeP 5G ProSe Policy

\* \* \* Next Change \* \* \* \*

### 5.5.2 Information elements coding

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| 0 | 0 | 0 | PAI | ProSeP info type = {UE policies for 5G ProSe UE-to-network relay UE} | | | | octet k |
| Spare | | |  |
| Length of ProSeP info contents | | | | | | | | octet k+1  octet k+2 |
| Validity timer | | | | | | | | octet k+3  octet k+7 |
| Served by NG-RAN | | | | | | | | octet k+8  octet o1 |
| Not served by NG-RAN | | | | | | | | octet o1+1  octet o2 |
| Default destination layer-2 IDs for sending the discovery signalling for announcement and additional information and for receiving the discovery signalling for solicitation | | | | | | | | octet o2+1  octet o3 |
| User info ID for discovery | | | | | | | | octet o3+1  octet o3+6 |
| RSC info list | | | | | | | | octet o3+7  octet o4 |
| 5QI to PC5 QoS parameters mapping rules | | | | | | | | octet o4+1  octet o5 |
| ProSe identifier to ProSe application server address mapping rules | | | | | | | | octet o5+1  octet o6 |
| 5G PKMF addressing information | | | | | | | | octet (o6+1)\*  octet l\* |

Figure 5.5.2.1: ProSeP Info = {UE policies for 5G ProSe UE-to-network relay UE}

Table 5.5.2.1: ProSeP Info = {UE policies for 5G ProSe UE-to-network relay UE}

|  |
| --- |
| ProSeP info type (bit 1 to 4 of octet k) shall be set to "0011" (UE policies for 5G ProSe UE-to-network relay UE) |
| PKMF address indication (PAI) (bit 5 of octet k) |
| The PAI indicates whether the PKMF addressing information is included in the IE or not |
| Bit |
| **5** |
| 0 PKMF addressing information is not included |
| 1 PKMF addressing information is included |
|  |
| Length of ProSeP info contents (octets k+1 to k+2) indicates the length of ProSeP info contents. |
|  |
| Validity timer (octet k+3 to k+7):  The validity timer field provides the expiration time of validity of the UE policies for 5G ProSe UE-to-network relay UE. The validity timer field is a binary coded representation of a UTC time, in seconds since midnight UTC of January 1, 1970 (not counting leap seconds). |
|  |
| Served by NG-RAN (octet k+8 to o1):  The served by NG-RAN field is coded according to figure 5.5.2.2 and table 5.5.2.2, and contains configuration parameters for 5G ProSe UE-to-network relay UE when the UE is served by NG-RAN. |
|  |
| Not served by NG-RAN (octet o1+1 to o2):  The not served by NG-RAN field is coded according to figure 5.5.2.5 and table 5.5.2.5, and contains configuration parameters for 5G ProSe UE-to-network relay discovery and communication when the UE is not served by NG-RAN. |
|  |
| Default destination layer-2 IDs for sending the discovery signalling for announcement and additional information and for receiving the discovery signalling for solicitation (octet o2+1 to o3):  The default destination layer-2 IDs for sending the discovery signalling for announcement and additional information and for receiving the discovery signalling for solicitation is coded according to figure 5.5.2.11a and table 5.5.2.11a and contains a list of the default destination layer-2 IDs for the initial UE-to-network relay discovery signalling. |
|  |
| User info ID for discovery (octet o3+1 to o3+6):  The value of the User info ID parameter is a 48-bit long bit string. The format of the User info ID parameter is out of scope of this specification. |
|  |
| RSC info list (octet o3+7 to o4):  The RSC info list field is coded according to figure 5.5.2.12 and table 5.5.2.12 and contains the RSCs related paramters. |
|  |
| 5QI to PC5 QoS parameters mapping rules (octet o4+1 to o5):  The 5QI to PC5 QoS parameters mapping rules field is coded according to figure 5.5.2.17 and table 5.5.2.17 and contains the 5QI to PC5 QoS parameters mapping rules. |
|  |
| ProSe identifier to ProSe application server address mapping rules (octet o5+1 to o6):  The ProSe identifier to ProSe application server address mapping rules field is coded according to figure 5.5.2.19 and table 5.5.2.19 and contains the ProSe identifier to ProSe application server address mapping rules. |
|  |
| If the length of ProSeP info contents field is bigger than indicated in figure 5.5.2.1, receiving entity shall ignore any superfluous octets located at the end of the ProSeP info contents. |
| 5G PKMF addressing information (octet o6+1 to l)  5G PKMF addressing information contains the IPv4 address(es), IPv6 address(es) and/or FQDN of the 5G PKMF and is coded according to figure 5.5.2.x, figure 5.5.2.y, figure 5.5.2.z and table 5.5.2.x. At least one of the addressing parameters (FQDN, IPv4 address list or IPv6 address list) shall be included. |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of served by NG-RAN contents | | | | | | | | octet k+8  octet k+9 |
| Authorizated PLMN list for layer-3 relay UE | | | | | | | | octet (k+10)\*  octet o50\* |
| Authorizated PLMN list for layer-2 relay UE | | | | | | | | octet (o50+1)\*  octet o1\* |

Figure 5.5.2.2: Served by NG-RAN

Table 5.5.2.2: Served by NG-RAN

|  |
| --- |
| Authorizated PLMN list for layer-3 relay UE:  The authorizated PLMN list for layer-3 relay UE field is coded according to figure 5.5.2.3 and table 5.5.2.3. |
|  |
| Authorizated PLMN list for layer-2 relay UE:  The authorizated PLMN list for layer-2 relay UE field is coded according to figure 5.5.2.3 and table 5.5.2.3. |

|  |  |
| --- | --- |
| Length of authorized PLMN list contents | octet k+10  octet k+11 |
| Authorized PLMN 1 | octet (k+12)\*  octet (k+14)\* |
| Authorized PLMN 2 | octet (k+15)\*  octet (k+17)\* |
| ... | octet (k+18)\*  octet (o50-3)\* |
| Authorized PLMN n | octet (o50-2)\*  octet o50\* |

Figure 5.5.2.3: Authorized PLMN list

Table 5.5.2.3: Authorized PLMN list

|  |
| --- |
| Authorized PLMN:  The authorized PLMN field is coded according to figure 5.5.2.4 and table 5.5.2.4. |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| MCC digit 2 | | | | MCC digit 1 | | | | octet k+15 |
| MNC digit 3 | | | | MCC digit 3 | | | | octet k+16 |
| MNC digit 2 | | | | MNC digit 1 | | | | octet k+17 |

Figure 5.5.2.4: PLMN ID

Table 5.5.2.4: PLMN ID

|  |
| --- |
| Mobile country code (MCC) (octet k+15, octet k+16 bit 1 to 4):  The MCC field is coded as in ITU-T Recommendation E.212 [5], annex A. |
|  |
| Mobile network code (MNC) (octet k+16 bit 5 to 8, octet k+17):  The coding of MNC field is the responsibility of each administration but BCD coding shall be used. The MNC shall consist of 2 or 3 digits. If a network operator decides to use only two digits in the MNC, MNC digit 3 shall be coded as "1111". |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of not served by NG-RAN contents | | | | | | | | octet o1+1  octet o1+2 |
| NR radio parameters per geographical area list for UE-to-network relay discovery | | | | | | | | octet o1+3  octet o51 |
| NR radio parameters per geographical area list for UE-to-network relay communication | | | | | | | | octet o51+1  octet o2 |

Figure 5.5.2.5: Not served by NG-RAN

Table 5.5.2.5: Not served by NG-RAN

|  |
| --- |
| NR radio parameters per geographical area list for UE-to-network relay discovery (octet o1+3 to o51):  The NR radio parameters per geographical area list for UE-to-network relay discovery field is coded according to figure 5.5.2.6 and table 5.5.2.6. |
|  |
| NR radio parameters per geographical area list for UE-to-network relay communication (octet o51+1 to o2):  The NR radio parameters per geographical area list for UE-to-network relay communication field is coded according to figure 5.5.2.7 and table 5.5.2.7. |
| If the length of not served by NG-RAN contents field is bigger than indicated in figure 5.5.2.5, receiving entity shall ignore any superfluous octets located at the end of the not served by NG-RAN contents. |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of NR radio parameters per geographical area list for UE-to-network relay discovery contents | | | | | | | | octet o1+3  octet o1+4 |
| Radio parameters per geographical area info 1 | | | | | | | | octet o1+5  octet o510 |
| Radio parameters per geographical area info 2 | | | | | | | | octet (o510+1)\*  octet o511\* |
| ... | | | | | | | | octet (o511+1)\*  octet o512\* |
| Radio parameters per geographical area info n | | | | | | | | octet (o512+1)\*  octet o51\* |

Figure 5.5.2.6: NR radio parameters per geographical area list for UE-to-network relay discovery

Table 5.5.2.6: NR radio parameters per geographical area list for UE-to-network relay discovery

|  |
| --- |
| Radio parameters per geographical area info:  The radio parameters per geographical area info field is coded according to figure 5.5.2.8 and table 5.5.2.8. |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of NR radio parameters per geographical area list for UE-to-network relay communication contents | | | | | | | | octet o51+1  octet o51+2 |
| Radio parameters per geographical area info 1 | | | | | | | | octet o51+3  octet o513 |
| Radio parameters per geographical area info 2 | | | | | | | | octet (o513+1)\*  octet o514\* |
| ... | | | | | | | | octet (o514+1)\*  octet o515\* |
| Radio parameters per geographical area info n | | | | | | | | octet (o515+1)\*  octet o2\* |

Figure 5.5.2.7: NR radio parameters per geographical area list for UE-to-network relay communication

Table 5.5.2.7: NR radio parameters per geographical area list for UE-to-network relay communication

|  |
| --- |
| Radio parameters per geographical area info:  The radio parameters per geographical area info field is coded according to figure 5.5.2.8 and table 5.5.2.8. |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of radio parameters per geographical area contents | | | | | | | | octet o510+1  octet o510+2 |
| Geographical area | | | | | | | | octet o510+3  octet o5100 |
| Radio parameters | | | | | | | | octet o5100+1  octet o511-1 |
| MI | 0  Spare | 0  Spare | 0  Spare | 0  Spare | 0  Spare | 0  Spare | 0  Spare | octet o511 |

Figure 5.5.2.8: Radio parameters per geographical area info

Table 5.5.2.8: Radio parameters per geographical area info

|  |
| --- |
| Geographical area (octet o510+3 to o5100):  The geographical area field is coded according to figure 5.5.2.9 and table 5.5.2.9. |
|  |
| Radio parameters (octet o5100+1 to o511-1):  The radio parameters field is coded according to figure 5.3.2.11 and table 5.3.2.11, applicable in the geographical area indicated by the geographical area field when not served by NG-RAN. |
|  |
| Managed indicator (MI) (octet o511 bit 8):  The managed indicator indicates how the radio parameters indicated in the radio parameters field in the geographical area indicated by the geographical area field are managed.  Bit  **8**  0 Non-operator managed  1 Operator managed |
|  |
| If the length of radio parameters per geographical area contents field is bigger than indicated in figure 5.5.2.8, receiving entity shall ignore any superfluous octets located at the end of the radio parameters per geographical area contents. |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of geographical area contents | | | | | | | | octet o510+3  octet o510+4 |
| Coordinate 1 | | | | | | | | octet (o510+5)\*  octet (o510+10)\* |
| Coordinate 2 | | | | | | | | octet (o510+11)\*  octet (o510+16)\* |
| ... | | | | | | | | octet (o510+17)\*  octet (o510-2+6\*n)\* |
| Coordinate n | | | | | | | | octet (o510-1+6\*n)\*  octet (o510+4+6\*n)\* = octet o5100\* |

Figure 5.5.2.9: Geographical area

Table 5.5.2.9: Geographical area

|  |
| --- |
| Coordinate:  The coordinate field is coded according to figure 5.5.2.10 and table 5.5.2.10. |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Latitude | | | | | | | | octet o510+11  octet o510+13 |
| Longitude | | | | | | | | octet o510+14  octet o510+17 |

Figure 5.5.2.10: Coordinate area

Table 5.5.2.10: Coordinate area

|  |
| --- |
| Latitude (octet o510+11 to o510+13):  The latitude field is coded according to clause 6.1 of 3GPP TS 23.032 [6]. |
|  |
| Longitude (octet o510+14 to o510+17):  The longitude field is coded according to clause 6.1 of 3GPP TS 23.032 [6]. |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of radio parameters contents | | | | | | | | octet o5100+1  octet o5100+2 |
| Radio parameters contents | | | | | | | | octet o5100+3  octet o511-1 |

Figure 5.5.2.11: Radio parameters

Table 5.5.2.11: Radio parameters

|  |
| --- |
| Radio parameters contents:  Radio parameters are defined as *SL-PreconfigurationNR* in clause 9.3 of 3GPP TS 38.331 [7]. |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of default destination layer-2 IDs for sending the discovery signalling for announcement and additional information and for receiving the discovery signalling for solicitation contents | | | | | | | | octet o2+1  octet o2+2 |
| Default destination layer-2 ID 1 | | | | | | | | octet o2+3  octet o2+5 |
| Default destination layer-2 ID 2 | | | | | | | | octet (o2+6)\*  octet (o2+8)\* |
| ... | | | | | | | | octet (o2+9)\*  octet (o3-3)\* |
| Default destination layer-2 ID n | | | | | | | | octet (o3-2)\*  octet o3\* |

Figure 5.5.2.11a: Default destination layer-2 IDs for sending the discovery signalling for announcement and additional information and for receiving the discovery signalling for solicitation

Table 5.5.2.11a: Default destination layer-2 IDs for sending the discovery signalling for announcement and additional information and for receiving the discovery signalling for solicitation

|  |
| --- |
| Default destination layer-2 ID (octet o2+3 to o2+5):  The default destination layer-2 ID is a 24-bit long bit string. |
|  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  | |
| Length of RSC info list contents | | | | | | | | | octet o3+7  octet o3+8 | |
| RSC info 1 | | | | | | | | | octet o3+9  octet o52 | |
| RSC info 2 | | | | | | | | | octet (o52+1)\*  octet (o53)\* | |
| ... | | | | | | | | | octet (o53+1)\*  octet (o54)\* | |
| RSC info n | | | | | | | | | octet (o54+1)\*  octet o4\* | |

Figure 5.5.2.12: RSC info list

Table 5.5.2.12: RSC info list

|  |
| --- |
| RSC info:  The RSC info field is coded according to figure 5.5.2.13 and table 5.5.2.13. |
|  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | | 6 | | 5 | | 4 | | 3 | | 2 | | 1 |  | |
| Length of RSC info contents | | | | | | | | | | | | | | | octet o52+1  octet o52+2 | |
| RSC list | | | | | | | | | | | | | | | octet o52+3  octet o520 | |
| Security related parameters for discovery | | | | | | | | | | | | | | | octet o520+1  octet o511 | |
| 0  Spare | | 0  Spare | | 0  Spare | | 0  Spare | | 0  Spare | | 0  Spare | | Layer indication | | | octet o511+1 | |
| PDU session parameters for layer-3 relay UE | | | | | | | | | | | | | | | octet (o511+2)  octet o530 | |
| NR-PC5 UE-to-network relay security policies | | | | | | | | | | | | | | | octet (o530+1)  octet o53 | |

Figure 5.5.2.13: RSC info

Editor's note: How to define the Security related parameters for discovery is FFS and depends on SA3 final requirements

Table 5.5.2.13: RSC info

|  |
| --- |
| RSC list (octet o52+3 to o520):  The RSC list field is coded according to figure 5.5.2.14 and table 5.5.2.14. |
|  |
| Security related parameters for discovery (octet o520+1 to o511):  The security related parameters for discovery field is coded according to figure 5.5.2.15 and table 5.5.2.15. |
|  |
| Layer indication (octet o511+1):  Bits  2 1  0 1 Layer 3  1 0 Layer 2  The other values are reserved. |
|  |
| PDU session parameters for layer-3 relay UE (octet o511+2 to o53):  The PDU session parameters for layer-3 relay UE field is coded according to figure 5.5.2.16 and table 5.5.2.16. |
|  |
| NR-PC5 UE-to-network relay security policies (octet o530+1 to octet o53)  The NR-PC5 UE-to-network relay security policies is coded as the NR-PC5 unicast security policies defined in figure 5.4.2.34 and table 5.4.2.34. |
|  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  | |
| Length of RSC list contents | | | | | | | | | octet o52+3  octet o52+4 | |
| RSC 1 | | | | | | | | | octet o52+5  octet o52+7 | |
| RSC 2 | | | | | | | | | octet (o52+8)\*  octet (o52+10)\* | |
| … | | | | | | | | | octet (o52+11)\*  octet (o520-3)\* | |
| RSC n | | | | | | | | | octet (o520-2)\*  octet o520\* | |

Figure 5.5.2.14: RSC list

Table 5.5.2.14: RSC list

|  |
| --- |
| RSC (octet o52+5 to o52+7):  The RSC identifies a connectivity service the UE-to-Network relay provides. The value of the RSC is a 24-bit long bit string. The values of the RSC from "000001" to "00000F" in hexadecimal representation are spare and shall not be used in this release of specification. The UE shall ignore the spare value of the RSC in this release of specification. For all other values, the format of the RSC is out of scope of this specification. |
|  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | | 6 | | | 5 | | 4 | | 3 | | | 2 | 1 |  | |
| Length of PDU session parameters for layer-3 relay UE contents | | | | | | | | | | | | | | | | octet o511+2  octet o511+3 | |
| Spare | | PATP | | PSSCM | | | PSNSSAI | | PDNN | | PDU session type | | | | | octet o511+4 | |
| DNN | | | | | | | | | | | | | | | | octet (o511+5)\*  octet o512\* | |
| S-NSSAI | | | | | | | | | | | | | | | | octet (o512+1)\*  octet (o53-1)\* | |
| Spare | | | | | Access type preference | | | | | | | SSC mode | | | | octet o53\* | |

Figure 5.5.2.16: PDU session parameters for layer-3 relay UE

Table 5.5.2.16: PDU session parameters for layer-3 relay UE

|  |  |
| --- | --- |
| PDU session type (bits 3 to 1 of octet o511+4):  The PDU session type field shall be encoded as the PDU session type value part of the PDU session type information element defined in clause 9.11.4.11 of 3GPP TS 24.501 [4]. | |
|  | |
| Presence of DNN (PDNN) (bit 4 of octet o511+4) | |
| PDNN indicates whether the DNN field is present or not. | |
| Bit | |
| **4** |  |
| 0 | DNN field is not included |
| 1 | DNN field is included |
|  | |
| Presence of S-NSSAI (PSNSSAI) (bit 5 of octet o511+4) | |
| PSNSSAI indicates whether the S-NSSAI field is present or not. | |
| Bit | |
| **5** |  |
| 0 | S-NSSAI field is not included |
| 1 | S-NSSAI field is included |
|  | |
| Presence of SSC mode (PSSCM) (bit 6 of octet o511+4) | |
| PSSCM indicates whether the SSC mode field is present or not. | |
| Bit | |
| **6** |  |
| 0 | SSC mode field is not included (NOTE) |
| 1 | SSC mode field is included |
|  |  |
| Presence of access type preference (PATP) (bit 7 of octet o511+4) | |
| PATP indicates whether the access type preference mode field is present or not. | |
| Bit | |
| **7** |  |
| 0 | Access type preference field is not included (NOTE) |
| 1 | Access type preference field is included |
|  | |
| DNN (octet o511+5 to o512):  The DNN field shall be encoded as a sequence of a one octet DNN length field and a DNN value field of a variable size. The DNN value contains an APN as defined in 3GPP TS 23.003 [10]. | |
|  | |
| S-NSSAI (octet o512+1 to o53-1):  The S-NSSAI field shall be encoded as a sequence of a one octet S-NSSAI length field and an S-NSSAI value field of a variable size. The S-NSSAI value shall be encoded as the value part of the S-NSSAI information element defined in clause 9.11.2.8 of 3GPP TS 24.501 [4]. | |
|  | |
| SSC mode (bits 3 to 1 of octet o53):  The SSC mode field shall be encoded as the value part of the SSC mode information element defined in clause 9.11.4.16 of 3GPP TS 24.501 [4]. | |
|  | |
| Access type preference (bits 5 to 4 of octet o53):  The access type preference field shall be encoded as the value part of the access type information element defined in clause 9.11.2.1A of 3GPP TS 24.501 [4]. | |
|  | |
| NOTE: Since SSC mode field and access type preference field are coded in the same octet, this octet is not included only when both PSSCM and PATP are set to 0. | |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  | |
| Length of 5QI to PC5 QoS parameters mapping rules contents | | | | | | | | | octet o4+1  octet o4+2 | |
| 5QI to PC5 QoS parameters mapping rule 1 | | | | | | | | | octet o4+3  octet o55 | |
| 5QI to PC5 QoS parameters mapping rule 2 | | | | | | | | | octet (o55+1)\*  octet o56\* | |
| … | | | | | | | | | octet (o56+1)\*  octet o57\* | |
| 5QI to PC5 QoS parameters mapping rule n | | | | | | | | | octet (o57+1)\*  octet o5\* | |

Figure 5.5.2.17: 5QI to PC5 QoS parameters mapping rules

Table 5.5.2.17: 5QI to PC5 QoS parameters mapping rules

|  |
| --- |
| 5QI to PC5 QoS parameters mapping rule:  The 5QI to PC5 QoS parameters mapping rule field is coded according to figure 5.5.2.18 and table 5.5.2.18 and contains the 5QI to PC5 QoS parameters mapping rule. |
|  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  | |
| Length of 5QI to PC5 QoS parameters mapping rule contents | | | | | | | | | octet o55+1  octet o55+2 | |
| 5QI | | | | | | | | | octet o55+3 | |
| PQI | | | | | | | | | octet o55+4 | |
| PDB adjustment factor | | | | | | | | | octet o55+5 | |
| RSC list | | | | | | | | | octet (o55+6)\*  octet o56\* | |

Figure 5.5.2.18: 5QI to PC5 QoS parameters mapping rule

Table 5.5.2.18: 5QI to PC5 QoS parameters mapping rule

|  |
| --- |
| 5QI (octet o55+3):  Bits  **8 7 6 5 4 3 2 1**  0 0 0 0 0 0 0 0 Reserved  0 0 0 0 0 0 0 1 5QI 1  0 0 0 0 0 0 1 0 5QI 2  0 0 0 0 0 0 1 1 5QI 3  0 0 0 0 0 1 0 0 5QI 4  0 0 0 0 0 1 0 1 5QI 5  0 0 0 0 0 1 1 0 5QI 6  0 0 0 0 0 1 1 1 5QI 7  0 0 0 0 1 0 0 0 5QI 8  0 0 0 0 1 0 0 1 5QI 9  0 0 0 0 1 0 1 0 5QI 10  0 0 0 0 1 0 1 1  to Spare  0 1 0 0 0 0 0 0  0 1 0 0 0 0 0 1 5QI 65  0 1 0 0 0 0 1 0 5QI 66  0 1 0 0 0 0 1 1 5QI 67  0 1 0 0 0 1 0 0 Spare  0 1 0 0 0 1 0 1 5QI 69  0 1 0 0 0 1 1 0 5QI 70  0 1 0 0 0 1 1 1 5QI 71  0 1 0 0 1 0 0 0 5QI 72  0 1 0 0 1 0 0 1 5QI 73  0 1 0 0 1 0 1 0 5QI 74  0 1 0 0 1 0 1 1 5QI 75  0 1 0 0 1 1 0 0 5QI 76  0 1 0 0 1 1 0 1  to Spare  0 1 0 0 1 1 1 0  0 1 0 0 1 1 1 1 5QI 79  0 1 0 1 0 0 0 0 5QI 80  0 1 0 1 0 0 0 1 Spare  0 1 0 1 0 0 1 0 5QI 82  0 1 0 1 0 0 1 1 5QI 83  0 1 0 1 0 1 0 0 5QI 84  0 1 0 1 0 1 0 1 5QI 85  0 1 0 1 0 1 1 0 5QI 86  0 1 0 1 0 1 1 1  to Spare  0 1 1 1 1 1 1 1  1 0 0 0 0 0 0 0  to Operator-specific 5QIs  1 1 1 1 1 1 1 0  1 1 1 1 1 1 1 1 Reserved |
|  |
| PQI (octet o55+4):  Bits  **8 7 6 5 4 3 2 1**  0 0 0 0 0 0 0 0 Reserved  0 0 0 0 0 0 0 1  to Spare  0 0 0 1 0 1 0 0  0 0 0 1 0 1 0 1 PQI 21  0 0 0 1 0 1 1 0 PQI 22  0 0 0 1 0 1 1 1 PQI 23  0 0 0 1 1 0 0 0 PQI 24  0 0 0 1 1 0 0 1 PQI 25  0 0 0 1 1 0 1 0 PQI 26  0 0 0 1 1 0 1 1  to Spare  0 0 1 1 0 1 1 0  0 0 1 1 0 1 1 1 PQI 55  0 0 1 1 1 0 0 0 PQI 56  0 0 1 1 1 0 0 1 PQI 57  0 0 1 1 1 0 1 0 PQI 58  0 0 1 1 1 0 1 1 PQI 59  0 0 1 1 1 1 0 0 PQI 60  0 0 1 1 1 1 0 1 PQI 61  0 0 1 1 1 1 1 0  to Spare  0 1 0 1 1 0 0 1  0 1 0 1 1 0 1 0 PQI 90  0 1 0 1 1 0 1 1 PQI 91  0 1 0 1 1 1 0 0 PQI 92  0 1 0 1 1 1 0 1 PQI 93  0 1 0 1 1 1 1 0  to Spare  0 1 1 1 1 1 1 1  1 0 0 0 0 0 0 0  to Operator-specific PQIs  1 1 1 1 1 1 1 0  1 1 1 1 1 1 1 1 Reserved |
|  |
| PDB adjustment factor (octet o55+5):  The PDB adjustment factor field is a binary coded representation of a percentage of the standardized PDB identified by the PQI. |
|  |
| RSC list (octet o55+6 to o56):  The RSC list field is coded according to figure 5.5.2.14 and table 5.5.2.14. |
|  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  | |
| Length of ProSe identifier to ProSe application server address mapping rules contents | | | | | | | | | octet o5+1  octet o5+2 | |
| ProSe identifier to ProSe application server address mapping rule 1 | | | | | | | | | octet (o5+3)\*  octet o150\* | |
| ProSe identifier to ProSe application server address mapping rule 2 | | | | | | | | | octet (o150+1)\*  octet o151\* | |
| ... | | | | | | | | | octet (o151+1)\*  octet o152\* | |
| ProSe identifier to ProSe application server address mapping rule n | | | | | | | | | octet (o152+1)\*  octet o6\* | |

Figure 5.5.2.19: ProSe identifier to ProSe application server address mapping rules

Table 5.5.2.19: ProSe identifier to ProSe application server address mapping rules

|  |
| --- |
| ProSe identifier to ProSe application server address mapping rule:  The ProSe identifier to ProSe application server address mapping rule field is coded according to figure 5.5.2.20 and table 5.5.2.20. |
|  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | | 6 | | 5 | | 4 | | 3 | | 2 | 1 |  | |
| Length of ProSe identifier to ProSe application server address mapping rule contents | | | | | | | | | | | | | | octet o150+1  octet o150+2 | |
| ProSe identifiers | | | | | | | | | | | | | | octet o150+3  octet o1500 | |
| 0  Spare | | 0  Spare | | 0  Spare | | 0  Spare | | 0  Spare | | AT | | | | octet o1500+1 | |
| ProSe application server address | | | | | | | | | | | | | | octet o1500+2  octet o6 | |

Figure 5.5.2.20: ProSe identifier to ProSe application server address mapping rule

Table 5.5.2.20: ProSe identifier to ProSe application server address mapping rule

|  |
| --- |
| ProSe identifiers (o150+3 to o1500):  The ProSe identifiers field is coded according to figure 5.3.2.14 and table 5.3.2.14. |
|  |
| Address type (AT) (octet o1500+1 bit 1 to 3):  The AT field indicates the ProSe application server address type.  Bits  **3 2 1**  0 0 1 IPv4  0 1 0 IPv6  0 1 1 FQDN  The other values are reserved. |
|  |
| If the AT indicates IPv4, then the ProSe application server address field contains an IPv4 address in 4 octets.  If the AT indicates IPv6, then the ProSe application server address field contains an IPv6 address in 16 octets.  If the AT indicates FQDN, then the ProSe application server address field contains a sequence of one octet FQDN length field and a FQDN value of variable size. The FQDN value field shall be encoded as defined in clause 28.3.2.1 in 3GPP TS 23.003 [10]. |
|  |
| If the length of ProSe identifier to ProSe application server address mapping rule contents field is bigger than indicated in figure 5.5.2.19, receiving entity shall ignore any superfluous octets located at the end of the ProSe identifier to ProSe application server address mapping rule contents. |
|  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | | 6 | | 5 | | 4 | | 3 | | 2 | | | 1 |  | |
| Length of 5G PKMF addressing information | | | | | | | | | | | | | | | | octet o6+1  octet o6+2 | |
| 0  Spare | | 0  Spare | | 0  Spare | | 0  Spare | | 0  Spare | | FQDN | | IPv6add | IPv4add | | | octet o6+3 | |
| IPv4 address list | | | | | | | | | | | | | | | | octet (o6+4)\*  octet o160\* | |
| IPv6 address list | | | | | | | | | | | | | | | | octet (o160+1)\*  octet (o161)\* | |
| FQDN | | | | | | | | | | | | | | | | octet (o161+1)\*  octet l\* | |

Figure 5.5.2.x: 5G PKMF addressing information

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  | |
| Number of IPv4 addresses | | | | | | | | | octet o6+4 | |
| IPv4 address 1 | | | | | | | | | octet o6+5  octet o6+8 | |
| IPv4 address 2 | | | | | | | | | octet o6+9  octet o6+12 | |
| … … | | | | | | | | |  | |
| IPv4 address N | | | | | | | | | octet o160-3  octet o160 | |

Figure 5.5.2.y: IPv4 address list

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  | |
| Number of IPv6 addresses | | | | | | | | | octet o160+1 | |
| IPv6 address 1 | | | | | | | | | octet o160+2  octet o160+17 | |
| IPv6 address 2 | | | | | | | | | octet o160+18  octet o160+33 | |
| … … | | | | | | | | |  | |
| IPv6 address N | | | | | | | | | octet o161-15  octet o161 | |

Figure 5.5.2.z: IPv6 address list

Table 5.5.2.x: 5G PKMF addressing information

|  |
| --- |
| IPv4 addresses (IPv4add) (o6+2 bit 1): (NOTE 1)  Bit  **1**  0 IPv4 address list is not present  1 IPv4 address list is present |
| IPv6 addresses (IPv6add) (octet o6+2 bit 2): (NOTE 1)  Bit  **2**  0 IPv6 address list is not present  1 IPv6 address list is present  FQDN (octet o6+3 bit 3): (NOTE 2)  Bit  **3**  0 FQDN is not present  1 FQDN is present |
| IPv4 address list (octet o6+4 to octet o160) |
| IPv4 address list contains the IPv4 address(es) of the 5G PKMF and shall be encoded as defined in figure 5.5.2.y.  IPv6 address list (octet o160+1 to octet o161)  IPv6 address list contains the IPv6 address(es) of the 5G PKMF and shall be encoded as defined in figure 5.5.2.z.  FQDN (octet o161+1 to l)  FQDN field contains a sequence of one octet FQDN length field and a FQDN value of variable size. The FQDN value field shall be encoded as defined in clause 28.3.2.1 in 3GPP TS 23.003 [10]. |
| NOTE 1: If multiple IPv4 addresses and/or IPv6 addresses are included, which one of these addresses is selected is implementation dependent.  NOTE 2: If the 5G PKMF supports the 5G PKMF Services with "https" URI scheme (i.e use of TLS is mandatory), then the FQDN shall be used to construct the target URI. |

\* \* \* Next Change \* \* \* \*

### 5.6.2 Information elements coding

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| 0 | 0 | 0 | 0 | ProSeP info type = {UE policies for 5G ProSe remote UE} | | | | octet k |
| Spare | | | |
| Length of ProSeP info contents | | | | | | | | octet k+1  octet k+2 |
| Validity timer | | | | | | | | octet k+3  octet k+7 |
| Served by NG-RAN | | | | | | | | octet k+8  octet o1 |
| Not served by NG-RAN | | | | | | | | octet o1+1  octet o2 |
| Default destination layer-2 IDs for sending the discovery signalling for solicitation and for receiving the discovery signalling for announcement and additional information | | | | | | | | octet o2+1  octet o3 |
| User info ID for discovery | | | | | | | | octet o3+1  octet o3+6 |
| RSC info list | | | | | | | | octet o3+7  octet l |
| N3IWF selection information for 5G ProSe layer-3 remote UE | | | | | | | | octet l+1  octet m |
| 5G PKMF addressing information | | | | | | | | octet m+1  octet p |

Figure 5.6.2.1: ProSeP Info = {UE policies for 5G ProSe remote UE}

Editor's note: How to define the security parameters used for UE-to-network relay depends on SA3 final requirements.

Table 5.6.2.1: ProSeP Info = {UE policies for 5G ProSe remote UE}

|  |
| --- |
| ProSeP info type (bit 1 to 4 of octet k) shall be set to "0100" (UE policies for 5G ProSe remote UE) |
|  |
| Length of ProSeP info contents (octets k+1 to k+2) indicates the length of ProSeP info contents. |
|  |
| Validity timer (octet k+3 to k+7):  The validity timer field provides the expiration time of validity of the UE policies for 5G ProSe remote UE. The validity timer field is a binary coded representation of a UTC time, in seconds since midnight UTC of January 1, 1970 (not counting leap seconds). |
|  |
| Served by NG-RAN (octet k+8 to o1):  The served by NG-RAN field is coded according to figure 5.6.2.2 and table 5.6.2.2, and contains configuration parameters for 5G ProSe remote UE when the UE is served by NG-RAN. |
|  |
| Not served by NG-RAN (octet o1+1 to o2):  The not served by NG-RAN field is coded according to figure 5.6.2.5 and table 5.6.2.5, and contains configuration parameters for 5G ProSe UE-to-network relay discovery and communication when the UE is not served by NG-RAN. |
|  |
| Default destination layer-2 IDs for sending the discovery signalling for solicitation and for receiving the discovery signalling for announcement and additional information (octet o2+1 to o3):  The default destination layer-2 IDs for sending the discovery signalling for solicitation and for receiving the discovery signalling for announcement and additional information is coded according to figure 5.6.2.11a and table 5.6.2.11a and contains a list of the default destination layer-2 IDs for the initial UE-to-network relay discovery signalling. |
|  |
| User info ID for discovery (octet o3+1 to o3+6):  The value of the User info ID parameter is a 48-bit long bit string. The format of the User info ID parameter is out of scope of this specification. |
|  |
| RSC info list (octet o3+7 to l):  The RSC info list field is coded according to figure 5.6.2.12 and table 5.6.2.12 and contains the RSCs related paramters. |
|  |
| N3IWF selection information for 5G ProSe layer-3 remote UE (octet l+1 to m):  The N3IWF selection information for 5G ProSe layer-3 remote UE field is coded according to figure 5.6.2.17 and table 5.6.2.17, and contains two parts: 1) N3IWF identifier configuration (either FQDN or IP address) for 5G ProSe layer-3 remote UE; 2) 5G ProSe layer-3 UE-to-network relay access node selection information. |
|  |
| If the length of ProSeP info contents field is bigger than indicated in figure 5.6.2.1, receiving entity shall ignore any superfluous octets located at the end of the ProSeP info contents.  5G PKMF addressing information (octet m+1 to p) |
| 5G PKMF addressing information contains the IPv4 address(es), IPv6 address(es) and/or FQDN of the 5G PKMF and is coded according to figure 5.5.2.x, figure 5.5.2.y, figure 5.5.2.z and table 5.5.2.x. At least one of the addressing parameters (FQDN, IPv4 address list or IPv6 address list) shall be included. |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of served by NG-RAN contents | | | | | | | | octet k+8  octet k+9 |
| 0  Spare | 0  Spare | 0  Spare | 0  Spare | 0  Spare | 0  Spare | 0  Spare | L3RI | octet (k+10)\* |
| Authorized PLMN list for layer-2 remote UE | | | | | | | | octet (k+11)\*  octet o1\* |

Figure 5.6.2.2: Served by NG-RAN

Table 5.6.2.2: Served by NG-RAN

|  |
| --- |
| Layer-3 remote UE authorization indication (L3RI) (octet k+10, bit 1):  The layer-3 remote UE authorization indication field indicates whether the UE is authorized to act as a layer-3 remote UE.  Bits  1  0 Not authorized to act as a layer-3 remote UE  1 Authorized to act as a layer-3 remote UE |
|  |
| Authorized PLMN list for layer-2 remote UE (octet k+11 to o1):  The authorized PLMN list for layer-2 remote UE field is coded according to figure 5.6.2.3 and table 5.6.2.3. |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  | |
| Length of authorized PLMN list contents | | | | | | | | | octet k+11  octet k+12 | |
| Authorized PLMN 1 | | | | | | | | | octet (k+13)\*  octet (k+15)\* | |
| Authorized PLMN 2 | | | | | | | | | octet (k+16)\*  octet (k+18)\* | |
| ... | | | | | | | | | octet (k+19)\*  octet (o50-3)\* | |
| Authorized PLMN n | | | | | | | | | octet (o50-2)\*  octet o50\* | |

Figure 5.6.2.3: Authorized PLMN list

Table 5.6.2.3: Authorized PLMN list

|  |
| --- |
| Authorized PLMN:  The authorized PLMN field is coded according to figure 5.6.2.4 and table 5.6.2.4. |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| MCC digit 2 | | | | MCC digit 1 | | | | octet k+16 |
| MNC digit 3 | | | | MCC digit 3 | | | | octet k+17 |
| MNC digit 2 | | | | MNC digit 1 | | | | octet k+18 |

Figure 5.6.2.4: PLMN ID

Table 5.6.2.4: PLMN ID

|  |
| --- |
| Mobile country code (MCC) (octet k+16, octet k+17 bit 1 to 4):  The MCC field is coded as in ITU-T Recommendation E.212 [5], annex A. |
|  |
| Mobile network code (MNC) (octet k+17 bit 5 to 8, octet k+18):  The coding of MNC field is the responsibility of each administration but BCD coding shall be used. The MNC shall consist of 2 or 3 digits. If a network operator decides to use only two digits in the MNC, MNC digit 3 shall be coded as "1111". |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of not served by NG-RAN contents | | | | | | | | octet o1+1  octet o1+2 |
| NR radio parameters per geographical area list for UE-to-network relay discovery | | | | | | | | octet o1+3  octet o51 |
| NR radio parameters per geographical area list for UE-to-network relay communication | | | | | | | | octet o51+1  octet o2 |

Figure 5.6.2.5: Not served by NG-RAN

Table 5.6.2.5: Not served by NG-RAN

|  |
| --- |
| NR radio parameters per geographical area list for UE-to-network relay discovery (octet o1+3 to o51):  The NR radio parameters per geographical area list for UE-to-network relay discovery field is coded according to figure 5.6.2.6 and table 5.6.2.6. |
|  |
| NR radio parameters per geographical area list for UE-to-network relay communication (octet o51+1 to o2):  The NR radio parameters per geographical area list for UE-to-network relay communication field is coded according to figure 5.6.2.7 and table 5.6.2.7. |
| If the length of not served by NG-RAN contents field is bigger than indicated in figure 5.6.2.5, receiving entity shall ignore any superfluous octets located at the end of the not served by NG-RAN contents. |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of NR radio parameters per geographical area list for UE-to-network relay discovery contents | | | | | | | | octet o1+3  octet o1+4 |
| Radio parameters per geographical area info 1 | | | | | | | | octet o1+5  octet o510 |
| Radio parameters per geographical area info 2 | | | | | | | | octet (o510+1)\*  octet o511\* |
| ... | | | | | | | | octet (o511+1)\*  octet o512\* |
| Radio parameters per geographical area info n | | | | | | | | octet (o512+1)\*  octet o51\* |

Figure 5.6.2.6: NR radio parameters per geographical area list for UE-to-network relay discovery

Table 5.6.2.6: NR radio parameters per geographical area list for UE-to-network relay discovery

|  |
| --- |
| Radio parameters per geographical area info:  The radio parameters per geographical area info field is coded according to figure 5.6.2.8 and table 5.6.2.8. |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of NR radio parameters per geographical area list for UE-to-network relay communication contents | | | | | | | | octet o51+1  octet o51+2 |
| Radio parameters per geographical area info 1 | | | | | | | | octet o51+3  octet o513 |
| Radio parameters per geographical area info 2 | | | | | | | | octet (o513+1)\*  octet o514\* |
| ... | | | | | | | | octet (o514+1)\*  octet o515\* |
| Radio parameters per geographical area info n | | | | | | | | octet (o515+1)\*  octet o2\* |

Figure 5.6.2.7: NR radio parameters per geographical area list for UE-to-network relay communication

Table 5.6.2.7: NR radio parameters per geographical area list for UE-to-network relay communication

|  |
| --- |
| Radio parameters per geographical area info:  The radio parameters per geographical area info field is coded according to figure 5.6.2.8 and table 5.6.2.8. |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of radio parameters per geographical area contents | | | | | | | | octet o510+1  octet o510+2 |
| Geographical area | | | | | | | | octet o510+3  octet o5100 |
| Radio parameters | | | | | | | | octet o5100+1  octet o511-1 |
| MI | 0  Spare | 0  Spare | 0  Spare | 0  Spare | 0  Spare | 0  Spare | 0  Spare | octet o511 |

Figure 5.6.2.8: Radio parameters per geographical area info

Table 5.6.2.8: Radio parameters per geographical area info

|  |
| --- |
| Geographical area (octet o510+3 to o5100):  The geographical area field is coded according to figure 5.6.2.9 and table 5.6.2.9. |
|  |
| Radio parameters (octet o5100+1 to o511-1):  The radio parameters field is coded according to figure 5.3.2.11 and table 5.3.2.11, applicable in the geographical area indicated by the geographical area field when not served by NG-RAN. |
|  |
| Managed indicator (MI) (octet o511 bit 8):  The managed indicator indicates how the radio parameters indicated in the radio parameters field in the geographical area indicated by the geographical area field are managed.  Bit  **8**  0 Non-operator managed  1 Operator managed |
|  |
| If the length of radio parameters per geographical area contents field is bigger than indicated in figure 5.6.2.8, receiving entity shall ignore any superfluous octets located at the end of the radio parameters per geographical area contents. |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of geographical area contents | | | | | | | | octet o510+3  octet o510+4 |
| Coordinate 1 | | | | | | | | octet (o510+5)\*  octet (o510+10)\* |
| Coordinate 2 | | | | | | | | octet (o510+11)\*  octet (o510+16)\* |
| ... | | | | | | | | octet (o510+17)\*  octet (o510-2+6\*n)\* |
| Coordinate n | | | | | | | | octet (o510-1+6\*n)\*  octet (o510+4+6\*n)\* = octet o5100\* |

Figure 5.6.2.9: Geographical area

Table 5.6.2.9: Geographical area

|  |
| --- |
| Coordinate:  The coordinate field is coded according to figure 5.6.2.10 and table 5.6.2.10. |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Latitude | | | | | | | | octet o510+11  octet o510+13 |
| Longitude | | | | | | | | octet o510+14  octet o510+17 |

Figure 5.6.2.10: Coordinate area

Table 5.6.2.10: Coordinate area

|  |
| --- |
| Latitude (octet o510+11 to o510+13):  The latitude field is coded according to clause 6.1 of 3GPP TS 23.032 [6]. |
|  |
| Longitude (octet o510+14 to o510+17):  The longitude field is coded according to clause 6.1 of 3GPP TS 23.032 [6]. |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of radio parameters contents | | | | | | | | octet o5100+1  octet o5100+2 |
| Radio parameters contents | | | | | | | | octet o5100+3  octet o511-1 |

Figure 5.6.2.11: Radio parameters

Table 5.6.2.11: Radio parameters

|  |
| --- |
| Radio parameters contents (octet o5100+3 to o511-1):  Radio parameters are defined as *SL-PreconfigurationNR* in clause 9.3 of 3GPP TS 38.331 [7]. |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of default destination layer-2 IDs for sending the discovery signalling for solicitation and for receiving the discovery signalling for announcement and additional information contents | | | | | | | | octet o2+1  octet o2+2 |
| Default destination layer-2 ID 1 | | | | | | | | octet o2+3  octet o2+5 |
| Default destination layer-2 ID 2 | | | | | | | | octet (o2+6)\*  octet (o2+8)\* |
| ... | | | | | | | | octet (o2+9)\*  octet (o3-3)\* |
| Default destination layer-2 ID n | | | | | | | | octet (o3-2)\*  octet o3\* |

Figure 5.6.2.11a: Default destination layer-2 IDs for sending the discovery signalling for solicitation and for receiving the discovery signalling for announcement and additional information

Table 5.6.2.11a: Default destination layer-2 IDs for sending the discovery signalling for solicitation and for receiving the discovery signalling for announcement and additional information

|  |
| --- |
| Default destination layer-2 ID (octet o2+3 to o2+5):  The default destination layer-2 ID is a 24-bit long bit string. |
|  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  | |
| Length of RSC info list contents | | | | | | | | | octet o3+7  octet o3+8 | |
| RSC info 1 | | | | | | | | | octet o3+9  octet o52 | |
| RSC info 2 | | | | | | | | | octet (o52+1)\*  octet o53\* | |
| ... | | | | | | | | | octet (o53+1)\*  octet o54\* | |
| RSC info n | | | | | | | | | octet (o54+1)\*  octet o4\* | |

Figure 5.6.2.12: RSC info list

Table 5.6.2.12: RSC info list

|  |
| --- |
| RSC info:  The RSC info field is coded according to figure 5.6.2.13 and table 5.6.2.13. |
|  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | | 6 | | 5 | | 4 | | 3 | | 2 | | 1 |  | |
| Length of RSC info contents | | | | | | | | | | | | | | | octet o52+1  octet o52+2 | |
| RSC list | | | | | | | | | | | | | | | octet o52+3  octet o520 | |
| Security related parameters for discovery | | | | | | | | | | | | | | | octet o520+1  octet o511 | |
| 0  Spare | | 0  Spare | | 0  Spare | | 0  Spare | | 0  Spare | | NSI | | LI | | | octet o511+1 | |
| PDU session parameters for layer-3 remote UE | | | | | | | | | | | | | | | octet (o511+2)\*  octet o53\* | |

Figure 5.6.2.13: RSC info

Table 5.6.2.13: RSC info

|  |
| --- |
| RSC list (octet o52+3 to o520):  The RSC list field is coded according to figure 5.6.2.14 and table 5.6.2.14. |
|  |
| Security related parameters for discovery (octet o520+1 to o511):  The security related parameters for discovery field is coded according to figure 5.6.2.15 and table 5.6.2.15. |
|  |
| Layer indication (LI) (octet o511+1 bit 1 to 2):  Bits  2 1  0 1 Layer 3  1 0 Layer 2  The other values are reserved. |
|  |
| N3IWF support indication (NSI) (octet o511+1 bit 3):  Bit  5  0 Using N3IWF access for the relayed traffic is not supported  1 Using N3IWF access for the relayed traffic is supported  The NSI is set to "Using N3IWF access for the relayed traffic is supported" only when the LI is set to "Layer 3". |
|  |
| PDU session parameters for layer-3 remote UE (octet o511+2 to o53):  The PDU session parameters for layer-3 remote UE field is coded according to figure 5.6.2.16 and table 5.6.2.16. |
|  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  | |
| Length of RSC list contents | | | | | | | | | octet o52+3  octet o52+4 | |
| RSC 1 | | | | | | | | | octet o52+5  octet o52+7 | |
| RSC 2 | | | | | | | | | octet (o52+8)\*  octet (o52+10)\* | |
| … | | | | | | | | | octet (o52+11)\*  octet (o520-3)\* | |
| RSC n | | | | | | | | | octet (o520-2)\*  octet o520\* | |

Figure 5.6.2.14: RSC list

Table 5.6.2.14: RSC list

|  |
| --- |
| RSC (octet o52+5 to o52+7):  The RSC identifies a connectivity service that the remote UE wants. The value of the RSC is a 24-bit long bit string. The values of the RSC from "000001" to "00000F" in hexadecimal representation are spare and shall not be used in this release of the specification. The UE shall ignore the spare value of the RSC in this release of specification. For all other values, the format of the RSC is out of scope of this specification. |
|  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | | 6 | | | 5 | | 4 | | 3 | | | 2 | 1 |  | |
| Length of PDU session parameters for layer-3 relay contents | | | | | | | | | | | | | | | | octet o511+2  octet o511+3 | |
| Spare | | PATP | | PSSCM | | | PSNSSAI | | PDNN | | PDU session type | | | | | octet o511+4 | |
| DNN | | | | | | | | | | | | | | | | octet (o511+5)\*  octet o512\* | |
| S-NSSAI | | | | | | | | | | | | | | | | octet (o512+1)\*  octet (o53-1)\* | |
| Spare | | | | | Access type preference | | | | | | | SSC mode | | | | octet o53\* | |

Figure 5.6.2.16: PDU session parameters for layer-3 relay

Table 5.6.2.16: PDU session parameters for layer-3 relay

|  |  |
| --- | --- |
| PDU session type (bits 3 to 1 of octet o511+4):  The PDU session type field shall be encoded as the PDU session type value part of the PDU session type information element defined in clause 9.11.4.11 of 3GPP TS 24.501 [4]. | |
|  | |
| Presence of DNN (PDNN) (bit 4 of octet o511+4) | |
| PDNN indicates whether the DNN field is present or not. | |
| Bit | |
| **4** |  |
| 0 | DNN field is not included |
| 1 | DNN field is included |
|  | |
| Presence of S-NSSAI (PSNSSAI) (bit 5 of octet o511+4) | |
| PSNSSAI indicates whether the S-NSSAI field is present or not. | |
| Bit | |
| **5** |  |
| 0 | S-NSSAI field is not included |
| 1 | S-NSSAI field is included |
|  | |
| Presence of SSC mode (PSSCM) (bit 6 of octet o511+4) | |
| PSSCM indicates whether the SSC mode field is present or not. | |
| Bit | |
| **6** |  |
| 0 | SSC mode field is not included (NOTE) |
| 1 | SSC mode field is included |
|  |  |
| Presence of access type preference (PATP) (bit 7 of octet o511+4) | |
| PATP indicates whether the access type preference mode field is present or not. | |
| Bit | |
| **7** |  |
| 0 | Access type preference field is not included (NOTE) |
| 1 | Access type preference field is included |
|  | |
| DNN (octet o511+5 to o512):  The DNN field shall be encoded as a sequence of a one octet DNN length field and a DNN value field of a variable size. The DNN value contains an APN as defined in 3GPP TS 23.003 [10]. | |
|  | |
| S-NSSAI (octet o512+1 to o53-1):  The S-NSSAI field shall be encoded as a sequence of a one octet S-NSSAI length field and an S-NSSAI value field of a variable size. The S-NSSAI value shall be encoded as the value part of the S-NSSAI information element defined in clause 9.11.2.8 of 3GPP TS 24.501 [4]. | |
|  | |
| SSC mode (bits 3 to 1 of octet o53):  The SSC mode field shall be encoded as the value part of the SSC mode information element defined in clause 9.11.4.16 of 3GPP TS 24.501 [4]. | |
|  | |
| Access type preference (bits 5 to 4 of octet o53):  The access type preference field shall be encoded as the value part of the access type information element defined in clause 9.11.2.1A of 3GPP TS 24.501 [4]. | |
|  | |
| NOTE: Since SSC mode field and access type preference field are coded in the same octet, this octet is not included only when both PSSCM and PATP are set to 0. | |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  | |
| Length of N3IWF selection information for 5G ProSe layer-3 remote UE | | | | | | | | | octet l+1  octet l+2 | |
| N3IWF identifier configuration for 5G ProSe layer-3 remote UE | | | | | | | | | octet l+3\*  octet l0\* | |
| 5G ProSe layer-3 UE-to-network relays access node selection information | | | | | | | | | octet l0+1\*  octet m | |

Figure 5.6.2.17: N3IWF selection information for 5G ProSe layer-3 remote UE

Table 5.6.2.17: N3IWF selection information for 5G ProSe layer-3 remote UE

|  |
| --- |
| N3IWF identifier configuration for 5G ProSe layer-3 remote UE (octet l+3\* to l0\*):  The N3IWF identifier configuration for 5G ProSe layer-3 remote UE contains a list of home N3IWF identifier entries and is coded according to figure 5.6.2.18 and table 5.6.2.18.  5G ProSe layer-3 UE-to-network relays access node selection information (octet l0+1\* to m): |
| The 5G ProSe layer-3 UE-to-network relays access node selection information contains a sequence of the N3AN node selection information entries and is coded according to figure 5.6.2.19 and table 5.6.2.19. |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  | |
| Length of N3IWF identifier configuration for 5G ProSe layer-3 remote UE | | | | | | | | | octet l+3\*  octet l+4\* | |
| Contents of N3IWF identifier configuration for 5G ProSe layer-3 remote UE | | | | | | | | | octet l+5\*  octet l01\* | |

Figure 5.6.2.18: N3IWF identifier configuration for 5G ProSe layer-3 remote UE

Table 5.6.2.18: N3IWF identifier configuration for 5G ProSe layer-3 remote UE

|  |
| --- |
| Contents of N3IWF identifier configuration for 5G ProSe layer-3 remote UE (octet l+5\* to l01\*):  The contents of N3IWF identifier configuration for 5G ProSe layer-3 remote UE shall be encoded as the encoding of home N3IWF identifier configuration defined in clause 5.3.3.3 of 3GPP TS 24.526 [11]. |
|  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  | |
| Length of 5G ProSe layer-3 UE-to-network relays access node selection information | | | | | | | | | octet l0+1\*  octet l0+2\* | |
| Contents of 5G ProSe layer-3 UE-to-network relays access node selection information | | | | | | | | | octet l0+3\*  octet m\* | |

Figure 5.6.2.19: 5G ProSe layer-3 UE-to-network relays access node selection information

Table 5.6.2.19: 5G ProSe layer-3 UE-to-network relays access node selection information

|  |
| --- |
| Contents of 5G ProSe layer-3 UE-to-network relays access node selection information (octet l0+3\* to m\*):  The contents of 5G ProSe layer-3 UE-to-network relays access node selection information shall be encoded as the encoding of N3AN node selection information defined in clause 5.3.3.2 of 3GPP TS 24.526 [11]. |
| NOTE: In this release of specification, the "preference" bit (as shown in figure 5.3.3.2.2 of 3GPP TS 24.526 [11]) is always set to "0". |

\* \* \* End of Changes \* \* \* \*