**3GPP TSG-CT WG1 Meeting #137-eC1-225000**

**E-Meeting, 18th – 26th August 2022**

Title: LS on setting RRC establishment cause value when relay UE has its own service

Response to:

Release: Release 17

Work Item: 5G\_ProSe

Source: CT1

To: RAN2

Cc:

**Contact Person:**

Name: Yizhong Zhang

E-mail Address: yizhong.zhang@vivo.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

Attachments: C1-225069

**1. Overall Description:**

CT1 has discussed how to set RRC establishment cause value for the case when the access attempt is simultaneously triggered by both the own service of the 5G ProSe layer-2 UE-to-network relay UE in 5GMM-IDLE mode and the 5G ProSe layer-2 remote UE, and achieved the following consensus (see attachment):

the RRC establishment cause is selected according to table 4.5.6.1 and table 4.5.6.2 of clause 4.5.6, 3GPP TS 24.501 in this case. However, it is possible for the lower layer to decide an applicable RRC establishment cause according to the request from of the 5G ProSe layer-2 remote UE.

**2. Actions:**

**To RAN2 group.**

**ACTION: CT1 kindly asks RAN2 to take the above information into consideration.**

**3. Date of Next CT1 Meetings:**

CT1#138e 10th - 14th October 2022 e-meeting