**3GPP TSG-CT WG1 Meeting #137-eC1-225031**

**E-Meeting, 18th – 26th August 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **24.501** | **CR** | **4627** | **rev** | **-** | **Current version:** | **17.7.1** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Addition of the length value of the Negotiated eDRX parameters IE | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | LG Electronics Inc. | | | | | | | | | |
| ***Source to TSG:*** | C1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | ARCH\_NR\_REDCAP | | | | |  | ***Date:*** | | | 2022-08-11 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | According to C1-224525 (LS on the maximum PTW length of IDLE eDRX), RAN2 agreed to support the maximum PTW length 40.96s.  <RAN2 agreements>   1. The maximum PTW length is 40.96s when IDLE eDRX cycle is longer than 10.24s. 2. The minimum PTW length is 1.28s and the step length/granularity of PTW length is 1.28 when IDLE eDRX cycle is longer than 10.24s.     To support this, TS 24.008 introduced extended PTW length values in the extened DRX parameters IE, and as the result, the length of Negotiated extended DRX parameters can be 4. So, this should be reflected in the specification accordingly. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The length of the Negotiated eDRX parameters IE can be 4. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The UE cannot successfully decode the Negotiated eDRX parameters IE that includes extended PTW length values. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 8.2.7.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 24.008 CR 3314 | | |
| ***affected:*** | |  |  | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  |  | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* First Change \* \* \* \*

### 8.2.7 Registration accept

#### 8.2.7.1 Message definition

The REGISTRATION ACCEPT message is sent by the AMF to the UE. See table 8.2.7.1.1.

Message type: REGISTRATION ACCEPT

Significance: dual

Direction: network to UE

Table 8.2.7.1.1: REGISTRATION ACCEPT message content

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| IEI | Information Element | Type/Reference | Presence | Format | Length |
|  | Extended protocol discriminator | Extended protocol discriminator  9.2 | M | V | 1 |
|  | Security header type | Security header type  9.3 | M | V | 1/2 |
|  | Spare half octet | Spare half octet  9.5 | M | V | 1/2 |
|  | Registration accept message identity | Message type  9.7 | M | V | 1 |
|  | 5GS registration result | 5GS registration result  9.11.3.6 | M | LV | 2 |
| 77 | 5G-GUTI | 5GS mobile identity  9.11.3.4 | O | TLV-E | 14 |
| 4A | Equivalent PLMNs | PLMN list  9.11.3.45 | O | TLV | 5-47 |
| 54 | TAI list | 5GS tracking area identity list  9.11.3.9 | O | TLV | 9-114 |
| 15 | Allowed NSSAI | NSSAI  9.11.3.37 | O | TLV | 4-74 |
| 11 | Rejected NSSAI | Rejected NSSAI  9.11.3.46 | O | TLV | 4-42 |
| 31 | Configured NSSAI | NSSAI  9.11.3.37 | O | TLV | 4-146 |
| 21 | 5GS network feature support | 5GS network feature support  9.11.3.5 | O | TLV | 3-5 |
| 50 | PDU session status | PDU session status  9.11.3.44 | O | TLV | 4-34 |
| 26 | PDU session reactivation result | PDU session reactivation result  9.11.3.42 | O | TLV | 4-34 |
| 72 | PDU session reactivation result error cause | PDU session reactivation result error cause  9.11.3.43 | O | TLV-E | 5-515 |
| 79 | LADN information | LADN information  9.11.3.30 | O | TLV-E | 12-1715 |
| B- | MICO indication | MICO indication  9.11.3.31 | O | TV | 1 |
| 9- | Network slicing indication | Network slicing indication  9.11.3.36 | O | TV | 1 |
| 27 | Service area list | Service area list  9.11.3.49 | O | TLV | 6-114 |
| 5E | T3512 value | GPRS timer 3  9.11.2.5 | O | TLV | 3 |
| 5D | Non-3GPP de-registration timer value | GPRS timer 2  9.11.2.4 | O | TLV | 3 |
| 16 | T3502 value | GPRS timer 2  9.11.2.4 | O | TLV | 3 |
| 34 | Emergency number list | Emergency number list  9.11.3.23 | O | TLV | 5-50 |
| 7A | Extended emergency number list | Extended emergency number list  9.11.3.26 | O | TLV-E | 7-65538 |
| 73 | SOR transparent container | SOR transparent container  9.11.3.51 | O | TLV-E | 20-n |
| 78 | EAP message | EAP message  9.11.2.2 | O | TLV-E | 7-1503 |
| A- | NSSAI inclusion mode | NSSAI inclusion mode  9.11.3.37A | O | TV | 1 |
| 76 | Operator-defined access category definitions | Operator-defined access category definitions  9.11.3.38 | O | TLV-E | 3-8323 |
| 51 | Negotiated DRX parameters | 5GS DRX parameters  9.11.3.2A | O | TLV | 3 |
| D- | Non-3GPP NW policies | Non-3GPP NW provided policies  9.11.3.36A | O | TV | 1 |
| 60 | EPS bearer context status | EPS bearer context status  9.11.3.23A | O | TLV | 4 |
| 6E | Negotiated extended DRX parameters | Extended DRX parameters  9.11.3.26A | O | TLV | 3-4 |
| 6C | T3447 value | GPRS timer 3  9.11.2.5 | O | TLV | 3 |
| 6B | T3448 value | GPRS timer 2  9.11.2.4 | O | TLV | 3 |
| 6A | T3324 value | GPRS timer 3  9.11.2.5 | O | TLV | 3 |
| 67 | UE radio capability ID | UE radio capability ID  9.11.3.68 | O | TLV | 3-n |
| E- | UE radio capability ID deletion indication | UE radio capability ID deletion indication  9.11.3.69 | O | TV | 1 |
| 39 | Pending NSSAI | NSSAI  9.11.3.37 | O | TLV | 4-146 |
| 74 | Ciphering key data | Ciphering key data  9.11.3.18C | O | TLV-E | 34-n |
| 75 | CAG information list | CAG information list  9.11.3.18A | O | TLV-E | 3-n |
| 1B | Truncated 5G-S-TMSI configuration | Truncated 5G-S-TMSI configuration  9.11.3.70 | O | TLV | 3 |
| 1C | Negotiated WUS assistance information | WUS assistance information  9.11.3.71 | O | TLV | 3-n |
| 29 | Negotiated NB-N1 mode DRX parameters | NB-N1 mode DRX parameters  9.11.3.73 | O | TLV | 3 |
| 68 | Extended rejected NSSAI | Extended rejected NSSAI  9.11.3.75 | O | TLV | 5-90 |
| 7B | Service-level-AA container | Service-level-AA container  9.11.2.10 | O | TLV-E | 6-n |
| 33 | Negotiated PEIPS assistance information | PEIPS assistance information  9.11.3.80 | O | TLV | 3-n |
| 34 | 5GS additional request result | 5GS additional request result  9.11.3.81 | O | TLV | 3 |
| 70 | NSSRG information | NSSRG information  9.11.3.82 | O | TLV-E | 7-65538 |
| 14 | Disaster roaming wait range | Registration wait range  9.11.3.84 | O | TLV | 4 |
| 2C | Disaster return wait range | Registration wait range  9.11.3.84 | O | TLV | 4 |
| 13 | List of PLMNs to be used in disaster condition | List of PLMNs to be used in disaster condition  9.11.3.83 | O | TLV | 2-n |
| 1D | Forbidden TAI(s) for the list of "5GS forbidden tracking areas for roaming" | 5GS tracking area identity list  9.11.3.9 | O | TLV | 9-114 |
| 1E | Forbidden TAI(s) for the list of "5GS forbidden tracking areas for regional provision of service" | 5GS tracking area identity list  9.11.3.9 | O | TLV | 9-114 |
| 71 | Extended CAG information list | Extended CAG information list  9.11.3.86 | O | TLV-E | 3-n |
| TBD | NSAG information | NSAG information  9.11.3.87 | O | TLV-E | 10-n |

\* \* \* End of Changes \* \* \* \*