**3GPP TSG-CT WG1 Meeting #146C1-24xxxx**

**Online, 22– 26 January 2024 Revision of C1-240113**

**Source: China Mobile, China Southern Power Grid Co**

**Title: Solve the EN to the IMS AS in 8.2**

**Spec: 3GPP TS 24.186 v1.0.0**

**Agenda item: 18.3.8**

**Document for: Decision**

**1. Introduction**

This p-CR proposes to solve the the EN to the IMS AS in 8.2.

**2. Reason for Change**

In TS 23.228 AC.7.2, P2P/P2A/P2A2P use cases are mentioned. IMS AS controlling media resource and handling SDP differently in different use cases which related to a data channel application using the ADC.

It is suggested to add the requirement to IMS AS to support usage of data channel applications.

**3. Proposal**

It is proposed to agree the following changes to 3GPP TS 24.186 v1.0.0.

\* \* \* First Change \* \* \* \*

## 8.2 Procedures at IMS AS

After the bootstrap data channels have been established, based on the SDP offer in the received re-INVITE message, IMS AS will notify the DCSF, may trigger the reservation or update of corresponding application data channel media resources upon the instruction from the DCSF and shall include an SDP offer in the sending re-INVITE message for the requested application data channel and related bootstrap data channel according to the specific data channel application use case (e.g. P2P/P2A/P2A2P), following the procedures in 3GPP TS 23.228 [3] and clause 9.3.2.2 and  9.3.3.2.2.

\* \* \* End of Changes \* \* \* \*