**3GPP TSG-CT3 Meeting #119bis-e *C3-220157***

**E-Meeting, 17th – 21th January 2022 (Revision of C3-22xxxx)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.522** | **CR** | 0484 | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Capability of 5G Access Stratum Time resource | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | IIoT | | | | |  | ***Date:*** | | | 2022-01-21 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | As defined in Table 5.2.6.25.8-1 of 23.502, capability of 5G Access Stratum Time resource can be notified. As defined 5.27.1.8 of TS 23.501, the TSCTSF exposes the 5GS and/or UE availability and capabilities for synchronization service to the AF. The exposed information includes the list of UE identities and may include the supported time synchronization distribution methods or 5G access stratum time distribution, (g)PTP grandmaster capable, 5G Clock quality. It means the (g)PTP grandmaster capability is not mandatory if the 5G Clock quality is reported. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | 5G AS time resource is included in the Time Synchronization Capability reported by the NEF. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | 5G AS time resource can’t be report. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.15.4.3.3, 5.15.4.4x, A.13 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backward compatible feature to the OpenAPI file of TimeSyncExposure API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

##### 5.15.4.3.3 Type: TimeSyncCapability

Table 5.15.4.3.3-1: Definition of type TimeSyncCapability

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| upNodeId | Uint64 | M | 1 | Identifies the applicable NW-TT. Contains a TSC user plane node Id. If integrated with TSN, the user plane node Id is a bridge Id defined in IEEE 802.1Q [51] clause 14.2.5. |  |
| gmCapables | array(GmCapable) | O | 1..N | Indicates whether user plane node supports acting as a gPTP and/or PTP grandmaster. |  |
| asTimeRes | AsTimeResource | O | 0..1 | Indicates the supported 5G clock quality (i.e. the source of time used by the 5GS). |  |
| ptpCapForUes | map(PtpCapabilitiesPerUe) | O | 1..N | Contains the PTP capabilities supported by the list of UE(s). The key of the map is the gpsi. |  |

\*\*\* Next Change \*\*\*

##### 5.15.4.4.x Enumeration: AsTimeResource

The enumeration AsTimeResource represents the supported 5G clock quality (i.e. the source of time used by the 5GS). It shall comply with the provisions defined in table 5.15.4.4.x -1.

Table 5.15.4.4.x-1: Enumeration AsTimeResource

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| ATOMIC\_CLOCK | Indicates atomic clock is supported. |  |
| GNSS | Indicates Global Navigation Satellite System is supported. |  |
| TERRESTRIAL\_RADIO | Indicates terrestrial radio is supported. |  |
| SERIAL\_TIME\_CODE | Indicates serial time code is supported. |  |
| PTP | Indicates PTP is supported. |  |
| NTP | Indicates NTP is supported. |  |
| HAND\_SET | Indicates hand set is supported. |  |
| INTERNAL\_OSCILLATOR | Indicates internal oscillator is supported. |  |
| OTHER | Indicates other source of time is supported. |  |

\*\*\* Next Change \*\*\*

# A.13 TimeSyncExposure API

openapi: 3.0.0

info:

title: 3gpp-time-sync-exposure

version: 1.0.0-alpha.3

description: |

API for time synchronization exposure.

© 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.522 V17.4.0; 5G System; Network Exposure Function Northbound APIs.

url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.522/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-time-sync/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

/{afId}/subscriptions:

get:

summary: read all of the active subscriptions for the AF

tags:

- Time Synchronization Exposure Subscriptions

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get all of the active subscriptions for the AF)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

minItems: 0

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource

tags:

- Time Synchronization Exposure Subscriptions

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

requestBody:

description: new subscription creation

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

responses:

'201':

description: Created (Successful creation)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

callbacks:

timeSyncSubsNotification:

'{$request.body#/subsNotifUri}':

post:

requestBody:

description: Notification for Time Synchronization Capability for a list of UEs.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsNotif'

responses:

'204':

description: Expected response to a successful callback processing without a body

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}:

get:

summary: read an active subscription for the AF and the subscription Id

tags:

- Individual Time Synchronization Exposure Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing subscription

tags:

- Individual Time Synchronization Exposure Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}/configurations:

get:

summary: read all of the active configurations for the AF

tags:

- Time Synchronization Exposure Configurations

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

description: String identifying the individual synchronization Exposure Subscription resource in the NEF

in: path

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get all of the active configurations for the AF)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/TimeSyncExposureConfig'

minItems: 0

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new configuration resource

tags:

- Time Synchronization Exposure Configurations

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

description: String identifying the individual synchronization Exposure Subscription resource in the NEF

in: path

required: true

schema:

type: string

requestBody:

description: new configuration creation

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

responses:

'201':

description: Created (Successful creation)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

callbacks:

timeSyncConfigNotification:

'{$request.body#/configNotifUri}':

post:

requestBody:

description: Notification for Time Synchronization Service status.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfigNotif'

responses:

'204':

description: Expected response to a successful callback processing without a body

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}/configurations/{instanceReference}:

get:

summary: read an active subscription for the AF and the subscription Id

tags:

- Individual Time Synchronization Exposure Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

- name: instanceReference

in: path

description: Identifier of the configuration resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Updates/replaces an existing configuration resource

tags:

- Individual Time Synchronization Exposure Configuration

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

- name: instanceReference

in: path

description: Identifier of the configuration resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing configuration

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

responses:

'200':

description: OK (Successful deletion of the existing configuration)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

'204':

description: Successful case. The resource has been successfully updated and no additional content is to be sent in the response message.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing configuration

tags:

- Individual Time Synchronization Exposure Configuration

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

- name: instanceReference

in: path

description: Identifier of the configuration resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing configuration)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

TimeSyncExposureSubsc:

description: Contains requested parameters for the subscription to the notification of time synchronization capability.

type: object

properties:

exterGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

gpsis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minItems: 1

description: Contains a list of UE for which the time synchronization capabilities is requested.

anyUeInd:

type: boolean

description: Any UE indication. This IE shall be present if the event subscription is applicable to any UE. Default value "false" is used, if not present.

afServiceId:

type: string

description: Identifies a service on behalf of which the AF is issuing the request.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

subsNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

subsNotifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

subscribedEvents:

type: array

items:

$ref: '#/components/schemas/SubscribedEvent'

minItems: 1

description: Subscribed events

eventFilters:

type: array

items:

$ref: '#/components/schemas/EventFilter'

minItems: 1

description: Contains the filter conditions to match for notifying the event(s) of time synchronization capabilities for a list of UE(s).

notifMethod:

$ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/NotificationMethod'

maxReportNbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

expiry:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

repPeriod:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

requestTestNotification:

type: boolean

description: Set to true by the SCS/AS to request the SCEF to send a test notification as defined in subclause 5.2.5.3 of 3GPP TS 29.122. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- subsNotifUri

- subsNotifId

TimeSyncCapability:

description: Contains time synchronization capability.

type: object

properties:

upNodeId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

gmCapables:

type: array

items:

$ref: '#/components/schemas/GmCapable'

asTimeRes:

$ref: '#/components/schemas/AsTimeResource'

ptpCapForUes:

type: object

additionalProperties:

$ref: '#/components/schemas/PtpCapabilitiesPerUe'

minProperties: 1

description: Contains the PTP capabilities supported by each of the UE(s). The key of the map is the gpsi.

required:

- upNodeId

TimeSyncExposureConfig:

description: Contains the Time Synchronization Configuration parameters.

type: object

properties:

upNodeId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

reqPtpIns:

$ref: '#/components/schemas/PtpInstance'

gmEnable:

type: boolean

description: Indicates that the AF requests 5GS to act as a grandmaster for PTP or gPTP if it is included and set to true.

gmPrio:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

timeDom:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

configNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

configNotifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

tempValidity:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TemporalValidity'

required:

- upNodeId

- reqPtpIns

- timeDom

- configNotifId

- configNotifUri

TimeSyncExposureSubsNotif:

description: Contains the notification of time synchronization capability.

type: object

properties:

subsNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

eventNotifs:

type: array

items:

$ref: '#/components/schemas/SubsEventNotification'

minItems: 1

required:

- subsNotifId

- eventNotifs

SubsEventNotification:

description: Notifications about subscribed Individual Events.

type: object

properties:

event:

$ref: '#/components/schemas/SubscribedEvent'

timeSyncCapas:

type: array

items:

$ref: '#/components/schemas/TimeSyncCapability'

minItems: 1

required:

- event

TimeSyncExposureConfigNotif:

description: Contains the notification of time synchronization service state.

type: object

properties:

configNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

stateOfConfig:

type: string

required:

- configNotifId

- stateOfConfig

PtpCapabilitiesPerUe:

description: Contains the supported PTP capabilities per UE.

type: object

properties:

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

ptpCaps:

type: array

items:

$ref: '#/components/schemas/EventFilter'

minItems: 1

required:

- gpsi

- ptpCaps

EventFilter:

description: Contains the filter conditions to match for notifying the event(s) of time synchronization capabilities.

type: object

properties:

instanceTypes:

type: array

items:

$ref: '#/components/schemas/InstanceType'

minItems: 1

transProtocols:

type: array

items:

$ref: '#/components/schemas/Protocol'

minItems: 1

ptpProfiles:

type: array

items:

type: string

minItems: 1

PtpInstance:

description: Contains PTP instance configuration and activation requested by the AF.

type: object

properties:

instanceType:

$ref: '#/components/schemas/InstanceType'

protocol:

$ref: '#/components/schemas/Protocol'

ptpProfile:

type: string

required:

- instanceType

- protocol

- ptpProfile

Protocol:

anyOf:

- type: string

enum:

- ETH

- IPV4

- IPV6

- type: string

description: >

This string identifies supported protocol.

description: >

Possible values are

- ETH: Indicates Ethernet as defined in IEEE Std 1588 [45] Annex E is supported.

- IPV4: Indicates IPv4 as defined in IEEE Std 1588 [45] Annex C is supported.

- IPV6: Indicates IPv6 as defined in IEEE Std 1588 [45] Annex D is supported.

GmCapable:

anyOf:

- type: string

enum:

- GPTP

- PTP

- type: string

description: >

This string identifies supported grandmaster.

description: >

Possible values are

- GPTP: gPTP grandmaster is supported.

- PTP: PTP grandmaste is supported.

InstanceType:

anyOf:

- type: string

enum:

- BOUNDARY\_CLOCK

- E2E\_TRANS\_CLOCK

- P2P\_TRANS\_CLOCK

- P2P\_RELAY\_INSTANCE

- type: string

description: >

This string identifies supported PTP instance type.

description: >

Possible values are

- BOUNDARY\_CLOCK: Indicates Boundary Clock as defined in IEEE Std 1588.

- E2E\_TRANS\_CLOCK: Indicates End-to-End Transparent Clock as defined in IEEE Std 1588.

- P2P\_TRANS\_CLOCK: Indicates Peer-to-Peer Transparent Clock as defined in IEEE Std 1588.

- P2P\_RELAY\_INSTANCE: Indicates PTP Relay instance as defined in IEEE Std 802.1AS.

SubscribedEvent:

anyOf:

- type: string

enum:

- AVAILABILITY\_FOR\_TIME\_SYNC\_SERVICE

- type: string

description: >

This string identifies supported event.

description: >

Possible values are

- AVAILABILITY\_FOR\_TIME\_SYNC\_SERVICE: The UE is availability for time synchronization service.

AsTimeResource:

anyOf:

- type: string

enum:

- ATOMIC\_CLOCK

- GNSS

- TERRESTRIAL\_RADIO

- SERIAL\_TIME\_CODE

- PTP

- NTP

- HAND\_SET

- INTERNAL\_OSCILLATOR

- OTHER

- type: string

description: >

This string identifies the supported 5G clock quality.

description: >

Possible values are

- ATOMIC\_CLOCK: Indicates atomic clock is supported.

- GNSS: Indicates Global Navigation Satellite System is supported.

- TERRESTRIAL\_RADIO: Indicates terrestrial radio is supported.

- SERIAL\_TIME\_CODE: Indicates serial time code is supported.

- PTP: Indicates PTP is supported.

- NTP: Indicates NTP is supported.

- HAND\_SET: Indicates hand set is supported.

- INTERNAL\_OSCILLATOR: Indicates internal oscillator is supported.

- OTHER: Indicates other source of time is supported.

\*\*\* End of Changes \*\*\*