**3GPP TSG-CT3 Meeting #120e C3-221670**

**E-Meeting, 17th – 25th February 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  |  Update of info and externalDocs fields  |
|  |  |
| ***Source to WG:*** | China Mobile |
| ***Source to TSG:*** | C3 |
|  |  |
| ***Work item code:*** | TEI17 |  | ***Date:*** | 2022-03-01 |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | CRs modifying the Nnwdaf\_EventsSubscription API and Nnwdaf\_AnalyticsInfo API have been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in 3GPP TS 29.501, clause 4.3.1.The following agreed CRs update the OpenAPI file for Nnwdaf\_EventsSubscription API for the present release:* CR#0359 impacts the OpenAPI file with a backwards compatible feature.
* CR#0365 impacts the OpenAPI file with a backwards compatible feature.
* CR#0367 impacts the OpenAPI file with a backwards compatible feature.
* CR#0369 impacts the OpenAPI file with a backwards compatible feature.
* CR#0371 impacts the OpenAPI file with a backwards compatible feature.
* CR#0386 impacts the OpenAPI file with a backwards compatible feature.
* CR#0387 impacts the OpenAPI file with a backwards compatible feature.
* CR#0391 impacts the OpenAPI file with a backwards compatible feature.
* CR#0392 impacts the OpenAPI file with a backwards compatible feature.
* CR#0393 impacts the OpenAPI file with a backwards compatible feature.
* CR#0394 impacts the OpenAPI file with a backwards compatible feature.
* CR#0395 impacts the OpenAPI file with a backwards compatible feature.
* CR#0400 impacts the OpenAPI file with a backwards compatible feature.
* CR#0403 impacts the OpenAPI file with a backwards compatible feature.
* CR#0405 impacts the OpenAPI file with a backwards compatible feature.
* CR#0406 impacts the OpenAPI file with a backwards compatible feature.
* CR#0411 impacts the OpenAPI file with a backwards compatible correction.
* CR#0417 impacts the OpenAPI file with a backwards compatible feature.
* CR#0420 impacts the OpenAPI file with a backwards compatible feature.
* 3GPP TS 29.571 CR#0332 impacts the OpenAPI file with a backwards compatible correction.

As some backward compatible corrections and features (but no backward incompatible changes or backward compatible new features) are added of the present release, the draft version number needs to be increased.The following agreed CRs update the OpenAPI file for Nnwdaf\_AnalyticsInfo API for the present release:* CR#0368 impacts the OpenAPI file with a backwards compatible feature.
* CR#0370 impacts the OpenAPI file with a backwards compatible feature.
* CR#0372 impacts the OpenAPI file with a backwards compatible feature.
* CR#0373 impacts the OpenAPI file with a backwards compatible correction.
* CR#0375 impacts the OpenAPI file with a backwards compatible correction.
* CR#0388 impacts the OpenAPI file with a backwards compatible feature.
* CR#0391 impacts the OpenAPI file with a backwards compatible feature.
* CR#0392 impacts the OpenAPI file with a backwards compatible feature.
* CR#0395 impacts the OpenAPI file with a backwards compatible feature.
* CR#0400 impacts the OpenAPI file with a backwards compatible feature.
* CR#0406 impacts the OpenAPI file with a backwards compatible feature.
* 3GPP TS 29.571 CR#0332 impacts the OpenAPI file with a backwards compatible correction.

As some backward compatible corrections and features (but no backward incompatible changes or backward compatible new features) are added of the present release, the draft version number needs to be increased.The following agreed CRs update the OpenAPI file for Nnwdaf\_MLModelProvision API for the present release:* CR#0389 impacts the OpenAPI file with a backwards compatible feature.

As some backward compatible corrections and features (but no backward incompatible changes or backward compatible new features) are added of the present release, the draft version number needs to be increased.In addition, the description field covering TS information is updated to cover proper line breaks structure, and the URL of the External Docs field is updated to https. |
|  |  |
| ***Summary of change:*** | The Nnwdaf\_EventsSubscription API version incremented from value "1.2.0-alpha.6" to value "1.2.0-alpha.7", and the TS version in the externalDocs field from 17.5.0 to 17.6.0.The Nnwdaf\_AnalyticsInfo API version incremented from value "1.2.0-alpha.5" to value "1.2.0-alpha.6", and the TS version in the externalDocs field from 17.5.0 to 17.6.0.The Nnwdaf\_MLModelProvision API version incremented from value "1.2.0-alpha.1" to value "1.2.0-alpha.2", and the TS version in the externalDocs field from 17.5.0 to 17.6.0.Update of the line breaks in the description field of TS information, and of the URL of the External Docs Field. |
|  |  |
| ***Consequences if not approved:*** | Incorrect API version number and TS version in externalDocs field. |
|  |  |
| ***Clauses affected:*** | A.2, A.3, A.5 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces backward compatible changes to Nnwdaf\_EventsSubscription API, Nnwdaf\_AnalyticsInfo and Nnwdaf\_MLModelProvision API. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**…**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

# A.2 Nnwdaf\_EventsSubscription API

openapi: 3.0.0

info:

 version: 1.2.0-alpha.7

 title: Nnwdaf\_EventsSubscription

 description: |

 Nnwdaf\_EventsSubscription Service API.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.520 V17.6.0; 5G System; Network Data Analytics Services.

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.520/'

security:

 - {}

 - oAuth2ClientCredentials:

 - nnwdaf-eventssubscription

servers:

 - url: '{apiRoot}/nnwdaf-eventssubscription/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

paths:

 /subscriptions:

 post:

 summary: Create a new Individual NWDAF Events Subscription

 operationId: CreateNWDAFEventsSubscription

 tags:

 - NWDAF Events Subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 responses:

 '201':

 description: Create a new Individual NWDAF Event Subscription resource.

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nnwdaf-eventssubscription/v1/subscriptions/{subscriptionId}'

 required: true

 schema:

 type: string

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 myNotification:

 '{$request.body#/notificationURI}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/NnwdafEventsSubscriptionNotification'

 minItems: 1

 responses:

 '204':

 description: The receipt of the Notification is acknowledged.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /subscriptions/{subscriptionId}:

 delete:

 summary: Delete an existing Individual NWDAF Events Subscription

 operationId: DeleteNWDAFEventsSubscription

 tags:

 - Individual NWDAF Events Subscription (Document)

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying a subscription to the Nnwdaf\_EventsSubscription Service

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. The Individual NWDAF Event Subscription resource matching the subscriptionId was deleted.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 description: The Individual NWDAF Event Subscription resource does not exist.

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '501':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/501'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 summary: Update an existing Individual NWDAF Events Subscription

 operationId: UpdateNWDAFEventsSubscription

 tags:

 - Individual NWDAF Events Subscription (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying a subscription to the Nnwdaf\_EventsSubscription Service

 required: true

 schema:

 type: string

 responses:

 '200':

 description: The Individual NWDAF Event Subscription resource was modified successfully and a representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 '204':

 description: The Individual NWDAF Event Subscription resource was modified successfully.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 description: The Individual NWDAF Event Subscription resource does not exist.

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '501':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/501'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /transfers:

 post:

 summary: Provide information about requested analytics subscriptions transfer and potentially create a new Individual NWDAF Event Subscription Transfer resource.

 operationId: CreateNWDAFEventSubscriptionTransfer

 tags:

 - NWDAF Event Subscription Transfers (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AnalyticsSubscriptionsTransfer'

 responses:

 '201':

 description: Create a new Individual NWDAF Event Subscription Transfer resource.

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nnwdaf-eventssubscription/v1/transfers/{transferId}'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /transfers/{transferId}:

 delete:

 summary: Delete an existing Individual NWDAF Event Subscription Transfer

 operationId: DeleteNWDAFEventSubscriptionTransfer

 tags:

 - Individual NWDAF Event Subscription Transfer (Document)

 parameters:

 - name: transferId

 in: path

 description: String identifying a request for an analytics subscription transfer to the Nnwdaf\_EventsSubscription Service

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. The Individual NWDAF Event Subscription Transfer resource matching the transferId was deleted.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '501':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/501'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 summary: Update an existing Individual NWDAF Event Subscription Transfer

 operationId: UpdateNWDAFEventSubscriptionTransfer

 tags:

 - Individual NWDAF Event Subscription Transfer (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AnalyticsSubscriptionsTransfer'

 parameters:

 - name: transferId

 in: path

 description: String identifying a request for an analytics subscription transfer to the Nnwdaf\_EventsSubscription Service

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The Individual NWDAF Event Subscription Transfer resource was modified successfully.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '501':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/501'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 nnwdaf-eventssubscription: Access to the Nnwdaf\_EventsSubscription API

 schemas:

 NnwdafEventsSubscription:

 description: Represents an Individual NWDAF Event Subscription resource.

 type: object

 properties:

 eventSubscriptions:

 type: array

 items:

 $ref: '#/components/schemas/EventSubscription'

 minItems: 1

 description: Subscribed events

 evtReq:

 $ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

 notificationURI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 eventNotifications:

 type: array

 items:

 $ref: '#/components/schemas/EventNotification'

 minItems: 1

 failEventReports:

 type: array

 items:

 $ref: '#/components/schemas/FailureEventInfo'

 minItems: 1

 prevSub:

 $ref: 'TS29520\_Nnwdaf\_AnalyticsInfo.yaml#/components/schemas/SpecificAnalyticsSubscription'

 consNfInfo:

 $ref: '#/components/schemas/ConsumerNfInformation'

 required:

 - eventSubscriptions

 EventSubscription:

 description: Represents a subscription to a single event.

 type: object

 properties:

 anySlice:

 $ref: '#/components/schemas/AnySlice'

 appIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 minItems: 1

 description: Identification(s) of application to which the subscription applies.

 dnns:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 minItems: 1

 description: Identification(s) of DNN to which the subscription applies.

 dnais:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 minItems: 1

 event:

 $ref: '#/components/schemas/NwdafEvent'

 extraReportReq:

 $ref: '#/components/schemas/EventReportingRequirement'

 loadLevelThreshold:

 type: integer

 description: Indicates that the NWDAF shall report the corresponding network slice load level to the NF service consumer where the load level of the network slice identified by snssais is reached.

 notificationMethod:

 $ref: '#/components/schemas/NotificationMethod'

 matchingDir:

 $ref: '#/components/schemas/MatchingDirection'

 nfLoadLvlThds:

 type: array

 items:

 $ref: '#/components/schemas/ThresholdLevel'

 minItems: 1

 description: Shall be supplied in order to start reporting when an average load level is reached.

 nfInstanceIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 nfSetIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 minItems: 1

 nfTypes:

 type: array

 items:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/NFType'

 minItems: 1

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 maxTopAppUlNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 description: Indicates the requested maximum number of top applications that contribute the most to the traffic in Uplink direction.

 maxTopAppDlNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 description: Indicates the requested maximum number of top applications that contribute the most to the traffic in Downlink direction.

 nsiIdInfos:

 type: array

 items:

 $ref: '#/components/schemas/NsiIdInfo'

 minItems: 1

 nsiLevelThrds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 minItems: 1

 qosRequ:

 $ref: '#/components/schemas/QosRequirement'

 qosFlowRetThds:

 type: array

 items:

 $ref: '#/components/schemas/RetainabilityThreshold'

 minItems: 1

 ranUeThrouThds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 minItems: 1

 repetitionPeriod:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 snssaia:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 description: Identification(s) of network slice to which the subscription applies. It corresponds to snssais in the data model definition of 3GPP TS 29.520.

 tgtUe:

 $ref: '#/components/schemas/TargetUeInformation'

 congThresholds:

 type: array

 items:

 $ref: '#/components/schemas/ThresholdLevel'

 minItems: 1

 nwPerfRequs:

 type: array

 items:

 $ref: '#/components/schemas/NetworkPerfRequirement'

 minItems: 1

 bwRequs:

 type: array

 items:

 $ref: '#/components/schemas/BwRequirement'

 minItems: 1

 excepRequs:

 type: array

 items:

 $ref: '#/components/schemas/Exception'

 minItems: 1

 exptAnaType:

 $ref: '#/components/schemas/ExpectedAnalyticsType'

 exptUeBehav:

 $ref: 'TS29503\_Nudm\_SDM.yaml#/components/schemas/ExpectedUeBehaviourData'

 ratTypes:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 minItems: 1

 frequency:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ArfcnValueNR'

 minItems: 1

 listOfAnaSubsets:

 type: array

 items:

 $ref: '#/components/schemas/AnalyticsSubset'

 minItems: 1

 required:

 - event

 NnwdafEventsSubscriptionNotification:

 description: Represents an Individual NWDAF Event Subscription Notification resource.

 type: object

 properties:

 eventNotifications:

 type: array

 items:

 $ref: '#/components/schemas/EventNotification'

 minItems: 1

 description: Notifications about Individual Events

 subscriptionId:

 type: string

 description: String identifying a subscription to the Nnwdaf\_EventsSubscription Service

 required:

 - eventNotifications

 - subscriptionId

 EventNotification:

 description: Represents a notification on events that occurred.

 type: object

 properties:

 event:

 $ref: '#/components/schemas/NwdafEvent'

 start:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 expiry:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeStampGen:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 failNotifyCode:

 $ref: '#/components/schemas/NwdafFailureCode'

 rvWaitTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 anaMetaInfo:

 $ref: '#/components/schemas/AnalyticsMetadataInfo'

 nfLoadLevelInfos:

 type: array

 items:

 $ref: '#/components/schemas/NfLoadLevelInformation'

 minItems: 1

 nsiLoadLevelInfos:

 type: array

 items:

 $ref: '#/components/schemas/NsiLoadLevelInfo'

 minItems: 1

 sliceLoadLevelInfo:

 $ref: '#/components/schemas/SliceLoadLevelInformation'

 svcExps:

 type: array

 items:

 $ref: '#/components/schemas/ServiceExperienceInfo'

 minItems: 1

 qosSustainInfos:

 type: array

 items:

 $ref: '#/components/schemas/QosSustainabilityInfo'

 minItems: 1

 ueComms:

 type: array

 items:

 $ref: '#/components/schemas/UeCommunication'

 minItems: 1

 ueMobs:

 type: array

 items:

 $ref: '#/components/schemas/UeMobility'

 minItems: 1

 userDataCongInfos:

 type: array

 items:

 $ref: '#/components/schemas/UserDataCongestionInfo'

 minItems: 1

 abnorBehavrs:

 type: array

 items:

 $ref: '#/components/schemas/AbnormalBehaviour'

 minItems: 1

 nwPerfs:

 type: array

 items:

 $ref: '#/components/schemas/NetworkPerfInfo'

 minItems: 1

 dnPerfInfos:

 type: array

 items:

 $ref: '#/components/schemas/DnPerfInfo'

 minItems: 1

 required:

 - event

 ServiceExperienceInfo:

 description: Represents service experience information.

 type: object

 properties:

 svcExprc:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/SvcExperience'

 svcExprcVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 nsiId:

 $ref: 'TS29531\_Nnssf\_NSSelection.yaml#/components/schemas/NsiId'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 frequency:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ArfcnValueNR'

 required:

 - svcExprc

 BwRequirement:

 description: Represents bandwidth requirements.

 type: object

 properties:

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 marBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 marBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 mirBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 mirBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 required:

 - appId

 SliceLoadLevelInformation:

 description: Contains load level information applicable for one or several slices.

 type: object

 properties:

 loadLevelInformation:

 $ref: '#/components/schemas/LoadLevelInformation'

 snssais:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 description: Identification(s) of network slice to which the subscription applies.

 numOfUes:

 $ref: '#/components/schemas/NumberAverage'

 numOfPduSess:

 $ref: '#/components/schemas/NumberAverage'

 exceedLoadLevelThrInd:

 type: boolean

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - loadLevelInformation

 - snssais

 NsiLoadLevelInfo:

 description: Represents the network slice and optionally the associated network slice instance and the load level information.

 type: object

 properties:

 loadLevelInformation:

 $ref: '#/components/schemas/LoadLevelInformation'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 nsiId:

 $ref: 'TS29531\_Nnssf\_NSSelection.yaml#/components/schemas/NsiId'

 resUsage:

 $ref: '#/components/schemas/ResourceUsage'

 numOfExceedLoadLevelThr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 exceedLoadLevelThrInd:

 type: boolean

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 timePeriod:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 numOfUes:

 $ref: '#/components/schemas/NumberAverage'

 numOfPduSess:

 $ref: '#/components/schemas/NumberAverage'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - loadLevelInformation

 - snssai

 NsiIdInfo:

 description: Represents the S-NSSAI and the optionally associated Network Slice Instance(s).

 type: object

 properties:

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 nsiIds:

 type: array

 items:

 $ref: 'TS29531\_Nnssf\_NSSelection.yaml#/components/schemas/NsiId'

 minItems: 1

 required:

 - snssai

 EventReportingRequirement:

 description: Represents the type of reporting that the subscription requires.

 type: object

 properties:

 accuracy:

 $ref: '#/components/schemas/Accuracy'

 startTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 offsetPeriod:

 type: integer

 description: Offset period in units of seconds to the reporting time, if the value is negative means statistics in the past offset period, otherwise a positive value means prediction in the future offset period. May be present if the "repPeriod" attribute is included within the "evtReq" attribute.

 sampRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 maxObjectNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 maxSupiNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 timeAnaNeeded:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 anaMeta:

 type: array

 items:

 $ref: '#/components/schemas/AnalyticsMetadata'

 minItems: 1

 anaMetaInd:

 $ref: '#/components/schemas/AnalyticsMetadataIndication'

 TargetUeInformation:

 description: Identifies the target UE information.

 type: object

 properties:

 anyUe:

 type: boolean

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 intGroupIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 UeMobility:

 description: Represents UE mobility information.

 type: object

 properties:

 ts:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 recurringTime:

 $ref: 'TS29122\_CpProvisioning.yaml#/components/schemas/ScheduledCommunicationTime'

 duration:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 durationVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 locInfos:

 type: array

 items:

 $ref: '#/components/schemas/LocationInfo'

 minItems: 1

 required:

 - duration

 - locInfos

 LocationInfo:

 description: Represents UE location information.

 type: object

 properties:

 loc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - loc

 UeCommunication:

 description: Represents UE communication information.

 type: object

 properties:

 commDur:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 commDurVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 perioTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 perioTimeVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 ts:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 tsVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 recurringTime:

 $ref: 'TS29122\_CpProvisioning.yaml#/components/schemas/ScheduledCommunicationTime'

 trafChar:

 $ref: '#/components/schemas/TrafficCharacterization'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - commDur

 - trafChar

 TrafficCharacterization:

 description: Identifies the detailed traffic characterization.

 type: object

 properties:

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 fDescs:

 type: array

 items:

 $ref: '#/components/schemas/IpEthFlowDescription'

 minItems: 1

 maxItems: 2

 ulVol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 ulVolVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 dlVol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 dlVolVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 UserDataCongestionInfo:

 description: Represents the user data congestion information.

 type: object

 properties:

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 congestionInfo:

 $ref: '#/components/schemas/CongestionInfo'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 CongestionInfo:

 description: Represents the congestion information.

 type: object

 properties:

 congType:

 $ref: '#/components/schemas/CongestionType'

 timeIntev:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 nsi:

 $ref: '#/components/schemas/ThresholdLevel'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 topAppListUl:

 type: array

 items:

 $ref: '#/components/schemas/TopApplication'

 minItems: 1

 topAppListDl:

 type: array

 items:

 $ref: '#/components/schemas/TopApplication'

 minItems: 1

 required:

 - congType

 - timeIntev

 - nsi

 TopApplication:

 description: Top application that contributes the most to the traffic.

 type: object

 properties:

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 ipTrafficFilter:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 QosSustainabilityInfo:

 description: Represents the QoS Sustainability information.

 type: object

 properties:

 areaInfo:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 startTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 qosFlowRetThd:

 $ref: '#/components/schemas/RetainabilityThreshold'

 ranUeThrouThd:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 QosRequirement:

 description: Represents the QoS requirements.

 type: object

 properties:

 5qi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

 gfbrUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 gfbrDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 resType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/QosResourceType'

 pdb:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 per:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketErrRate'

 ThresholdLevel:

 description: Represents a threshold level.

 type: object

 properties:

 congLevel:

 type: integer

 nfLoadLevel:

 type: integer

 nfCpuUsage:

 type: integer

 nfMemoryUsage:

 type: integer

 nfStorageUsage:

 type: integer

 NfLoadLevelInformation:

 description: Represents load level information of a given NF instance.

 type: object

 properties:

 nfType:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/NFType'

 nfInstanceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 nfSetId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 nfStatus:

 $ref: '#/components/schemas/NfStatus'

 nfCpuUsage:

 type: integer

 nfMemoryUsage:

 type: integer

 nfStorageUsage:

 type: integer

 nfLoadLevelAverage:

 type: integer

 nfLoadLevelpeak:

 type: integer

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - nfType

 - nfInstanceId

 NfStatus:

 description: Contains the percentage of time spent on various NF states.

 type: object

 properties:

 statusRegistered:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 statusUnregistered:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 statusUndiscoverable:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 AnySlice:

 type: boolean

 description: FALSE represents not applicable for all slices. TRUE represents applicable for all slices.

 LoadLevelInformation:

 type: integer

 description: Load level information of the network slice and the optionally associated network slice instance.

 AbnormalBehaviour:

 description: Represents the abnormal behaviour information.

 type: object

 properties:

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 excep:

 $ref: '#/components/schemas/Exception'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 addtMeasInfo:

 $ref: '#/components/schemas/AdditionalMeasurement'

 required:

 - excep

 Exception:

 description: Represents the Exception information.

 type: object

 properties:

 excepId:

 $ref: '#/components/schemas/ExceptionId'

 excepLevel:

 type: integer

 excepTrend:

 $ref: '#/components/schemas/ExceptionTrend'

 required:

 - excepId

 AdditionalMeasurement:

 description: Represents additional measurement information.

 type: object

 properties:

 unexpLoc:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 unexpFlowTeps:

 type: array

 items:

 $ref: '#/components/schemas/IpEthFlowDescription'

 minItems: 1

 unexpWakes:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 minItems: 1

 ddosAttack:

 $ref: '#/components/schemas/AddressList'

 wrgDest:

 $ref: '#/components/schemas/AddressList'

 circums:

 type: array

 items:

 $ref: '#/components/schemas/CircumstanceDescription'

 minItems: 1

 IpEthFlowDescription:

 description: Contains the description of an Uplink and/or Downlink Ethernet flow.

 type: object

 properties:

 ipTrafficFilter:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/FlowDescription'

 ethTrafficFilter:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

 AddressList:

 description: Represents a list of IPv4 and/or IPv6 addresses.

 type: object

 properties:

 ipv4Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 minItems: 1

 ipv6Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 minItems: 1

 CircumstanceDescription:

 description: Contains the description of a circumstance.

 type: object

 properties:

 freq:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 tm:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 locArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 vol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 RetainabilityThreshold:

 description: Represents a QoS flow retainability threshold.

 type: object

 properties:

 relFlowNum:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 relTimeUnit:

 $ref: '#/components/schemas/TimeUnit'

 relFlowRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 NetworkPerfRequirement:

 description: Represents a network performance requirement.

 type: object

 properties:

 nwPerfType:

 $ref: '#/components/schemas/NetworkPerfType'

 relativeRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 absoluteNum:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - nwPerfType

 NetworkPerfInfo:

 description: Represents the network performance information.

 type: object

 properties:

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 nwPerfType:

 $ref: '#/components/schemas/NetworkPerfType'

 relativeRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 absoluteNum:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - networkArea

 - nwPerfType

 FailureEventInfo:

 description: Contains information on the event for which the subscription is not successful.

 type: object

 properties:

 event:

 $ref: '#/components/schemas/NwdafEvent'

 failureCode:

 $ref: '#/components/schemas/NwdafFailureCode'

 required:

 - event

 - failureCode

 AnalyticsMetadataIndication:

 description: Contains analytics metadata information requested to be used during analytics generation.

 type: object

 properties:

 dataWindow:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 dataStatProps:

 type: array

 items:

 $ref: '#/components/schemas/DatasetStatisticalProperty'

 minItems: 1

 strategy:

 $ref: '#/components/schemas/OutputStrategy'

 aggrNwdafIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 AnalyticsMetadataInfo:

 description: Contains analytics metadata information required for analytics aggregation.

 type: object

 properties:

 numSamples:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 dataWindow:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 dataStatProps:

 type: array

 items:

 $ref: '#/components/schemas/DatasetStatisticalProperty'

 minItems: 1

 strategy:

 $ref: '#/components/schemas/OutputStrategy'

 accuracy:

 $ref: '#/components/schemas/Accuracy'

 NumberAverage:

 description: Represents average and variance information.

 type: object

 properties:

 number:

 type: integer

 variance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 required:

 - number

 - variance

 AnalyticsSubscriptionsTransfer:

 description: Contains information about a request to transfer analytics subscriptions.

 type: object

 properties:

 subsTransInfos:

 type: array

 items:

 $ref: '#/components/schemas/SubscriptionTransferInfo'

 minItems: 1

 required:

 - subsTransInfos

 SubscriptionTransferInfo:

 description: Contains information about subscriptions that are requested to be transferred.

 type: object

 properties:

 transReqType:

 $ref: '#/components/schemas/TransferRequestType'

 nwdafEvSub:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 consumerId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 contextId:

 $ref: '#/components/schemas/AnalyticsContextIdentifier'

 sourceNfIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 sourceSetIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 minItems: 1

 modelInfo:

 type: array

 items:

 $ref: '#/components/schemas/ModelInfo'

 minItems: 1

 modelProvIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 required:

 - transReqType

 - nwdafEvSub

 - consumerId

 ModelInfo:

 description: Contains information about an ML model.

 type: object

 properties:

 analyticsId:

 $ref: '#/components/schemas/NwdafEvent'

 mlFileAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 required:

 - analyticsId

 - mlFileAddr

 AnalyticsContextIdentifier:

 description: Contains information about available analytics contexts.

 type: object

 properties:

 subscriptionId:

 type: string

 description: The identifier of a subscription.

 nfAnaCtxts:

 type: array

 items:

 $ref: '#/components/schemas/NwdafEvent'

 minItems: 1

 description: List of analytics types for which NF related analytics contexts can be retrieved.

 ueAnaCtxts:

 type: array

 items:

 $ref: '#/components/schemas/UeAnalyticsContextDescriptor'

 minItems: 1

 description: List of objects that indicate for which SUPI and analytics types combinations analytics context can be retrieved.

 allOf:

 - anyOf:

 - required: [nfAnaCtxts]

 - required: [ueAnaCtxts]

 - required: [subscriptionId]

 UeAnalyticsContextDescriptor:

 description: Contains information about available UE related analytics contexts.

 type: object

 properties:

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 anaTypes:

 type: array

 items:

 $ref: '#/components/schemas/NwdafEvent'

 minItems: 1

 description: List of analytics types for which UE related analytics contexts can be retrieved.

 required:

 - supi

 - anaTypes

 DnPerfInfo:

 description: Represents DN performance information.

 type: object

 properties:

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 dnPerf:

 type: array

 items:

 $ref: '#/components/schemas/DnPerf'

 minItems: 1

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - dNPerf

 DnPerf:

 description: Represents DN performance information.

 type: object

 properties:

 appServerInsAddr:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/AddrFqdn'

 upfId:

 type: string

 description: Identifies the UPF.

 dnai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 perfData:

 $ref: '#/components/schemas/PerfData'

 spatialValidCon:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 temporalValidCon:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 PerfData:

 description: Represents DN performance data.

 type: object

 properties:

 avgTrafficRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 maxTrafficRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 avePacketDelay:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 maxPacketDelay:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 avgPacketLossRate:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRate'

#

# ENUMERATIONS DATA TYPES

#

 ResourceUsage:

 description: The current usage of the virtual resources assigned to the NF instances belonging to a particular network slice instance.

 type: object

 properties:

 cpuUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 memoryUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 storageUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 ConsumerNfInformation:

 description: Represents the analytics consumer NF Information.

 type: object

 properties:

 nfId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 taiList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

 minItems: 1

 anyOf:

 - required: [nfId]

 - required: [taiList]

 NotificationMethod:

 anyOf:

 - type: string

 enum:

 - PERIODIC

 - THRESHOLD

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - PERIODIC: The subscribe of NWDAF Event is periodically. The periodic of the notification is identified by repetitionPeriod defined in subclause 5.1.6.2.3.

 - THRESHOLD: The subscribe of NWDAF Event is upon threshold exceeded. The threshold of the notification is identified by loadLevelThreshold defined in subclause 5.1.6.2.3.

 NwdafEvent:

 anyOf:

 - type: string

 enum:

 - SLICE\_LOAD\_LEVEL

 - NETWORK\_PERFORMANCE

 - NF\_LOAD

 - SERVICE\_EXPERIENCE

 - UE\_MOBILITY

 - UE\_COMMUNICATION

 - QOS\_SUSTAINABILITY

 - ABNORMAL\_BEHAVIOUR

 - USER\_DATA\_CONGESTION

 - NSI\_LOAD\_LEVEL

 - DN\_PERFORMANCE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - SLICE\_LOAD\_LEVEL: Indicates that the event subscribed is load level information of Network Slice

 - NETWORK\_PERFORMANCE: Indicates that the event subscribed is network performance information.

 - NF\_LOAD: Indicates that the event subscribed is load level and status of one or several Network Functions.

 - SERVICE\_EXPERIENCE: Indicates that the event subscribed is service experience.

 - UE\_MOBILITY: Indicates that the event subscribed is UE mobility information.

 - UE\_COMMUNICATION: Indicates that the event subscribed is UE communication information.

 - QOS\_SUSTAINABILITY: Indicates that the event subscribed is QoS sustainability.

 - ABNORMAL\_BEHAVIOUR: Indicates that the event subscribed is abnormal behaviour.

 - USER\_DATA\_CONGESTION: Indicates that the event subscribed is user data congestion information.

 - NSI\_LOAD\_LEVEL: Indicates that the event subscribed is load level information of Network Slice and the optionally associated Network Slice Instance

 - DN\_PERFORMANCE: Indicates that the event subscribed is DN performance information.

 Accuracy:

 anyOf:

 - type: string

 enum:

 - LOW

 - HIGH

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - LOW: Low accuracy.

 - HIGH: High accuracy.

 CongestionType:

 anyOf:

 - type: string

 enum:

 - USER\_PLANE

 - CONTROL\_PLANE

 - USER\_AND\_CONTROL\_PLANE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - USER\_PLANE: The congestion analytics type is User Plane.

 - CONTROL\_PLANE: The congestion analytics type is Control Plane.

 - USER\_AND\_CONTROL\_PLANE: The congestion analytics type is User Plane and Control Plane.

 ExceptionId:

 anyOf:

 - type: string

 enum:

 - UNEXPECTED\_UE\_LOCATION

 - UNEXPECTED\_LONG\_LIVE\_FLOW

 - UNEXPECTED\_LARGE\_RATE\_FLOW

 - UNEXPECTED\_WAKEUP

 - SUSPICION\_OF\_DDOS\_ATTACK

 - WRONG\_DESTINATION\_ADDRESS

 - TOO\_FREQUENT\_SERVICE\_ACCESS

 - UNEXPECTED\_RADIO\_LINK\_FAILURES

 - PING\_PONG\_ACROSS\_CELLS

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - UNEXPECTED\_UE\_LOCATION: Unexpected UE location

 - UNEXPECTED\_LONG\_LIVE\_FLOW: Unexpected long-live rate flows

 - UNEXPECTED\_LARGE\_RATE\_FLOW: Unexpected large rate flows

 - UNEXPECTED\_WAKEUP: Unexpected wakeup

 - SUSPICION\_OF\_DDOS\_ATTACK: Suspicion of DDoS attack

 - WRONG\_DESTINATION\_ADDRESS: Wrong destination address

 - TOO\_FREQUENT\_SERVICE\_ACCESS: Too frequent Service Access

 - UNEXPECTED\_RADIO\_LINK\_FAILURES: Unexpected radio link failures

 - PING\_PONG\_ACROSS\_CELLS: Ping-ponging across neighbouring cells

 ExceptionTrend:

 anyOf:

 - type: string

 enum:

 - UP

 - DOWN

 - UNKNOW

 - STABLE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - UP: Up trend of the exception level.

 - DOWN: Down trend of the exception level.

 - UNKNOW: Unknown trend of the exception level.

 - STABLE: Stable trend of the exception level.

 TimeUnit:

 anyOf:

 - type: string

 enum:

 - MINUTE

 - HOUR

 - DAY

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - MINUTE: Time unit is per minute.

 - HOUR: Time unit is per hour.

 - DAY: Time unit is per day.

 NetworkPerfType:

 anyOf:

 - type: string

 enum:

 - GNB\_ACTIVE\_RATIO

 - GNB\_COMPUTING\_USAGE

 - GNB\_MEMORY\_USAGE

 - GNB\_DISK\_USAGE

 - NUM\_OF\_UE

 - SESS\_SUCC\_RATIO

 - HO\_SUCC\_RATIO

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - GNB\_ACTIVE\_RATIO: Indicates that the network performance requirement is gNodeB active (i.e. up and running) rate. Indicates the ratio of gNB active (i.e. up and running) number to the total number of gNB

 - GNB\_COMPUTING\_USAGE: Indicates gNodeB computing resource usage.

 - GNB\_MEMORY\_USAGE: Indicates gNodeB memory usage.

 - GNB\_DISK\_USAGE: Indicates gNodeB disk usage.

 - NUM\_OF\_UE: Indicates number of UEs.

 - SESS\_SUCC\_RATIO: Indicates ratio of successful setup of PDU sessions to total PDU session setup attempts.

 - SESS\_SUCC\_RATIO: Indicates Ratio of successful handovers to the total handover attempts.

 ExpectedAnalyticsType:

 anyOf:

 - type: string

 enum:

 - MOBILITY

 - COMMUN

 - MOBILITY\_AND\_COMMUN

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - MOBILITY: Mobility related abnormal behaviour analytics is expected by the consumer.

 - COMMUN: Communication related abnormal behaviour analytics is expected by the consumer.

 - MOBILITY\_AND\_COMMUN: Both mobility and communication related abnormal behaviour analytics is expected by the consumer.

 MatchingDirection:

 anyOf:

 - type: string

 enum:

 - ASCENDING

 - DESCENDING

 - CROSSED

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - ASCENDING: Threshold is crossed in ascending direction.

 - DESCENDING: Threshold is crossed in descending direction.

 - CROSSED: Threshold is crossed either in ascending or descending direction.

 NwdafFailureCode:

 anyOf:

 - type: string

 enum:

 - UNAVAILABLE\_DATA

 - BOTH\_STAT\_PRED\_NOT\_ALLOWED

 - UNSATISFIED\_REQUESTED\_ANALYTICS\_TIME

 - OTHER

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - UNAVAILABLE\_DATA: Indicates the requested statistics information for the event is rejected since necessary data to perform the service is unavailable.

 - BOTH\_STAT\_PRED\_NOT\_ALLOWED: Indicates the requested analysis information for the event is rejected since the start time is in the past and the end time is in the future, which means the NF service consumer requested both statistics and prediction for the analytics.

 - UNSATISFIED\_REQUESTED\_ANALYTICS\_TIME: Indicates that the requested event is rejected since the analytics information is not ready when the time indicated by the "timeAnaNeeded" attribute (as provided during the creation or modification of subscription) is reached.

 - OTHER: Indicates the requested analysis information for the event is rejected due to other reasons.

 AnalyticsMetadata:

 anyOf:

 - type: string

 enum:

 - NUM\_OF\_SAMPLES

 - DATA\_WINDOW

 - DATA\_STAT\_PROPS

 - STRATEGY

 - ACCURACY

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - NUM\_OF\_SAMPLES: Number of data samples used for the generation of the output analytics.

 - DATA\_WINDOW: Data time window of the data samples.

 - DATA\_STAT\_PROPS: Dataset statistical properties of the data used to generate the analytics.

 - STRATEGY: Output strategy used for the reporting of the analytics.

 - ACCURACY: Level of accuracy reached for the analytics.

 DatasetStatisticalProperty:

 anyOf:

 - type: string

 enum:

 - UNIFORM\_DIST\_DATA

 - NO\_OUTLIERS

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - UNIFORM\_DIST\_DATA: Indicates the use of data samples that are uniformly distributed according to the different aspects of the requested analytics.

 - NO\_OUTLIERS: Indicates that the data samples shall disregard data samples that are at the extreme boundaries of the value range.

 OutputStrategy:

 anyOf:

 - type: string

 enum:

 - BINARY

 - GRADIENT

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - BINARY: Indicates that the analytics shall only be reported when the requested level of accuracy is reached within a cycle of periodic notification.

 - GRADIENT: Indicates that the analytics shall be reported according with the periodicity irrespective of whether the requested level of accuracy has been reached or not.

 TransferRequestType:

 anyOf:

 - type: string

 enum:

 - PREPARE

 - TRANSFER

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - PREPARE: Indicates that the request is for analytics subscription transfer preparation.

 - TRANSFER: Indicates that the request is for analytics subscription transfer execution.

 AnalyticsSubset:

 anyOf:

 - type: string

 enum:

 - NUM\_OF\_UE\_REG

 - NUM\_OF\_PDU\_SESS\_ESTBL

 - RES\_USAGE

 - NUM\_OF\_EXCEED\_RES\_USAGE\_LOAD\_LEVEL\_THR

 - PERIOD\_OF\_EXCEED\_RES\_USAGE\_LOAD\_LEVEL\_THR

 - EXCEED\_LOAD\_LEVEL\_THR\_IND

 - LIST\_OF\_TOP\_APP\_UL

 - LIST\_OF\_TOP\_APP\_DL

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - NUM\_OF\_UE\_REG: The number of UE registered. This value is only applicable to NSI\_LOAD\_LEVEL event.

 - NUM\_OF\_PDU\_SESS\_ESTBL: The number of PDU sessions established. This value is only applicable to NSI\_LOAD\_LEVEL event.

 - RES\_USAGE: The current usage of the virtual resources assigned to the NF instances belonging to a particular network slice instance. This value is only applicable to NSI\_LOAD\_LEVEL event.

 - NUM\_OF\_EXCEED\_RES\_USAGE\_LOAD\_LEVEL\_THR: The number of times the resource usage threshold of the network slice instance is reached or exceeded if a threshold value is provided by the consumer. This value is only applicable to NSI\_LOAD\_LEVEL event.

 - PERIOD\_OF\_EXCEED\_RES\_USAGE\_LOAD\_LEVEL\_THR: The time interval between each time the threshold being met or exceeded on the network slice (instance). This value is only applicable to NSI\_LOAD\_LEVEL event.

 - EXCEED\_LOAD\_LEVEL\_THR\_IND: Whether the Load Level Threshold is met or exceeded by the statistics value. This value is only applicable to NSI\_LOAD\_LEVEL event.

 - LIST\_OF\_TOP\_APP\_UL: The list of applications that contribute the most to the traffic in the UL direction. This value is only applicable to USER\_DATA\_CONGESTION event.

 - LIST\_OF\_TOP\_APP\_DL: The list of applications that contribute the most to the traffic in the DL direction. This value is only applicable to USER\_DATA\_CONGESTION event.

\*\*\* 2nd Change \*\*\*

# A.3 Nnwdaf\_AnalyticsInfo API

openapi: 3.0.0

info:

 version: 1.2.0-alpha.6

 title: Nnwdaf\_AnalyticsInfo

 description: |

 Nnwdaf\_AnalyticsInfo Service API.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.520 V17.6.0; 5G System; Network Data Analytics Services.

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.520/'

security:

 - {}

 - oAuth2ClientCredentials:

 - nnwdaf-analyticsinfo

servers:

 - url: '{apiRoot}/nnwdaf-analyticsinfo/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

paths:

 /analytics:

 get:

 summary: Read a NWDAF Analytics

 operationId: GetNWDAFAnalytics

 tags:

 - NWDAF Analytics (Document)

 parameters:

 - name: event-id

 in: query

 description: Identify the analytics.

 required: true

 schema:

 $ref: '#/components/schemas/EventId'

 - name: ana-req

 in: query

 description: Identifies the analytics reporting requirement information.

 required: false

 content:

 application/json:

 schema:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/EventReportingRequirement'

 - name: event-filter

 in: query

 description: Identify the analytics.

 required: false

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventFilter'

 - name: supported-features

 in: query

 description: To filter irrelevant responses related to unsupported features

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 - name: tgt-ue

 in: query

 description: Identify the target UE information.

 required: false

 content:

 application/json:

 schema:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/TargetUeInformation'

 responses:

 '200':

 description: Containing the analytics with parameters as relevant for the requesting NF service consumer.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AnalyticsData'

 '204':

 description: No Content (The request NWDAF Analytics data does not exist)

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 description: Indicates that the NWDAF Analytics resource does not exist.

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 description: The request is rejected by the NWDAF and more details (not only the ProblemDetails) are returned.

 content:

 application/problem+json:

 schema:

 $ref: '#/components/schemas/ProblemDetailsAnalyticsInfoRequest'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /context:

 get:

 summary: Get context information related to analytics subscriptions.

 operationId: GetNwdafContext

 tags:

 - NWDAF Context (Document)

 parameters:

 - name: context-ids

 in: query

 description: Identifies specific context information related to analytics subscriptions.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ContextIdList'

 - name: req-context

 in: query

 description: Identfies the type(s) of the analytics context information the consumer wishes to receive.

 required: false

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/RequestedContext'

 responses:

 '200':

 description: Contains context information related to analytics subscriptions corresponding with one or more context identifiers.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ContextData'

 '204':

 description: No Content (No context information could be retrieved for the requested context identifiers).

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 nnwdaf-analyticsinfo: Access to the Nnwdaf\_AnalyticsInfo API

 schemas:

 AnalyticsData:

 description: Represents the description of analytics with parameters as relevant for the requesting NF service consumer.

 type: object

 properties:

 start:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 expiry:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeStampGen:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 anaMetaInfo:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/AnalyticsMetadataInfo'

 sliceLoadLevelInfos:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/SliceLoadLevelInformation'

 minItems: 1

 description: The slices and their load level information.

 nsiLoadLevelInfos:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NsiLoadLevelInfo'

 minItems: 1

 nfLoadLevelInfos:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NfLoadLevelInformation'

 minItems: 1

 nwPerfs:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NetworkPerfInfo'

 minItems: 1

 svcExps:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/ServiceExperienceInfo'

 minItems: 1

 qosSustainInfos:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/QosSustainabilityInfo'

 minItems: 1

 ueMobs:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/UeMobility'

 minItems: 1

 ueComms:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/UeCommunication'

 minItems: 1

 userDataCongInfos:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/UserDataCongestionInfo'

 minItems: 1

 abnorBehavrs:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/AbnormalBehaviour'

 minItems: 1

 smccExps:

 type: array

 items:

 $ref: '#/components/schemas/SmcceInfo'

 minItems: 1

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 EventFilter:

 description: Represents the event filters used to identify the requested analytics.

 type: object

 properties:

 anySlice:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/AnySlice'

 snssais:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 description: Identification(s) of network slice to which the subscription belongs.

 appIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 minItems: 1

 dnns:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 minItems: 1

 dnais:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 minItems: 1

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 maxTopAppUlNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 description: Indicates the requested maximum number of top applications that contribute the most to the traffic in Uplink direction.

 maxTopAppDlNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 description: Indicates the requested maximum number that the list of top applications that contribute the most to the traffic in Downlink direction.

 nfInstanceIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 nfSetIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 minItems: 1

 nfTypes:

 type: array

 items:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/NFType'

 minItems: 1

 nsiIdInfos:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NsiIdInfo'

 minItems: 1

 qosRequ:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/QosRequirement'

 nwPerfTypes:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NetworkPerfType'

 minItems: 1

 bwRequs:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/BwRequirement'

 minItems: 1

 excepIds:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/ExceptionId'

 minItems: 1

 exptAnaType:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/ExpectedAnalyticsType'

 exptUeBehav:

 $ref: 'TS29503\_Nudm\_SDM.yaml#/components/schemas/ExpectedUeBehaviourData'

 ratTypes:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 minItems: 1

 freqs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ArfcnValueNR'

 minItems: 1

 not:

 required: [anySlice, snssais]

 ProblemDetailsAnalyticsInfoRequest:

 description: Extends ProblemDetails to indicate more details why the analytics request is rejected.

 allOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/AdditionInfoAnalyticsInfoRequest'

 AdditionInfoAnalyticsInfoRequest:

 description: Indicates additional information why the analytics request is rejected.

 type: object

 properties:

 rvWaitTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 ContextData:

 description: Contains context information related to analytics subscriptions corresponding with one or more context identifiers.

 type: object

 properties:

 contextElems:

 type: array

 items:

 $ref: '#/components/schemas/ContextElement'

 minItems: 1

 description: List of items that contain context information corresponding with a context identifier.

 required:

 - contextElems

 ContextElement:

 description: Contains context information corresponding with a specific context identifier.

 type: object

 properties:

 contextId:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/AnalyticsContextIdentifier'

 pendAnalytics:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/EventNotification'

 minItems: 1

 description: Output analytics for the analytics subscription which have not yet been sent to the analytics consumer.

 histAnalytics:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/EventNotification'

 minItems: 1

 description: Historical output analytics.

 lastOutputTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 aggrSubs:

 type: array

 items:

 $ref: '#/components/schemas/SpecificAnalyticsSubscription'

 minItems: 1

 description: Information about analytics subscriptions that the NWDAF has with other NWDAFs to perform aggregation.

 histData:

 type: array

 items:

 $ref: '#/components/schemas/HistoricalData'

 minItems: 1

 description: Historical data related to the analytics subscription.

 adrfId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 adrfDataTypes:

 type: array

 items:

 $ref: '#/components/schemas/AdrfDataType'

 minItems: 1

 description: Type(s) of data stored in the ADRF by the NWDAF.

 aggrNwdafIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 description: NWDAF identifiers of NWDAF instances used by the NWDAF service consumer when aggregating multiple analytics subscriptions.

 modelProvIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 description: Identifiers of NWDAFs that provide ML models used by the NF service consumer.

 required:

 - contextId

 ContextIdList:

 description: Contains a list of context identifiers of context information of analytics subscriptions.

 type: object

 properties:

 contextIds:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/AnalyticsContextIdentifier'

 minItems: 1

 required:

 - contextIds

 HistoricalData:

 description: Contains historical data related to an analytics subscription.

 type: object

 properties:

 startTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 subsWithSources:

 type: array

 items:

 type: string

 minItems: 1

 description: Information about subscriptions with the data sources.

 data:

 type: array

 items:

 type: string

 minItems: 1

 description: Historical data related to the analytics.

 required:

 - data

 SpecificAnalyticsSubscription:

 description: Represents an existing subscription for a specific type of analytics to a specific NWDAF.

 type: object

 properties:

 subscriptionId:

 type: string

 producerId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 producerSetId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 nwdafEvSub:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NnwdafEventsSubscription'

 allOf:

 - anyOf:

 - required: [producerId]

 - required: [producerSetId]

 - required: [subscriptionId]

 - required: [nwdafEvSub]

 RequestedContext:

 description: Contains types of analytics context information.

 type: object

 properties:

 contexts:

 type: array

 items:

 $ref: '#/components/schemas/ContextType'

 minItems: 1

 description: List of analytics context types.

 required:

 - contexts

 SmcceInfo:

 description: Represents the Session Management congestion control experience information.

 type: object

 properties:

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 smcceUeList:

 type: array

 items:

 $ref: '#/components/schemas/SmcceUeList'

 minItems: 1

 SmcceUeList:

 description: Represents the List of UEs classified based on experience level of Session Management congestion control.

 type: object

 properties:

 highLevel:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 mediumLevel:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 lowLevel:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 EventId:

 anyOf:

 - type: string

 enum:

 - LOAD\_LEVEL\_INFORMATION

 - NETWORK\_PERFORMANCE

 - NF\_LOAD

 - SERVICE\_EXPERIENCE

 - UE\_MOBILITY

 - UE\_COMMUNICATION

 - QOS\_SUSTAINABILITY

 - ABNORMAL\_BEHAVIOUR

 - USER\_DATA\_CONGESTION

 - NSI\_LOAD\_LEVEL

 - SM\_CONGESTION

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - LOAD\_LEVEL\_INFORMATION: Represent the analytics of load level information of corresponding network slice.

 - NETWORK\_PERFORMANCE: Represent the analytics of network performance information.

 - NF\_LOAD: Indicates that the event subscribed is NF Load.

 - SERVICE\_EXPERIENCE: Represent the analytics of service experience information of the specific applications.

 - UE\_MOBILITY: Represent the analytics of UE mobility.

 - UE\_COMMUNICATION: Represent the analytics of UE communication.

 - QOS\_SUSTAINABILITY: Represent the analytics of QoS sustainability information in the certain area.

 - ABNORMAL\_BEHAVIOUR: Indicates that the event subscribed is abnormal behaviour information.

 - USER\_DATA\_CONGESTION: Represent the analytics of the user data congestion in the certain area.

 - NSI\_LOAD\_LEVEL: Represent the analytics of Network Slice and the optionally associated Network Slice Instance.

 - SM\_CONGESTION: Represent the analytics of Session Management congestion control experience information for specific DNN and/or S-NSSAI.

 ContextType:

 anyOf:

 - type: string

 enum:

 - PENDING\_ANALYTICS

 - HISTORICAL\_ANALYTICS

 - AGGR\_SUBS

 - DATA

 - AGGR\_INFO

 - ML\_MODELS

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - PENDING\_ANALYTICS: Represents context information that relates to pending output analytics.

 - HISTORICAL\_ANALYTICS: Represents context information that relates to historical output analytics.

 - AGGR\_SUBS: Represents context information about the analytics subscriptions that an NWDAF has with other NWDAFs that collectively serve an analytics subscription.

 - DATA: Represents context information about historical data that is available.

 - AGGR\_INFO: Represents context information that is related to aggregation of analytics from multiple NWDAF subscriptions.

 - ML\_MODELS: Represents context information about used ML models.

 AdrfDataType:

 anyOf:

 - type: string

 enum:

 - HISTORICAL\_ANALYTICS

 - HISTORICAL\_DATA

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - HISTORICAL\_ANALYTICS: Indicates that historical analytics are stored in the ARDF.

 - HISTORICAL\_DATA: Indicates that historical data are stored in the ARDF.

\*\*\* 3rd Change \*\*\*

# A.5 Nnwdaf\_MLModelProvision API

openapi: 3.0.0

info:

 title: Nnwdaf\_MLModelProvision

 version: 1.0.0-alpha.2

 description: |

 Nnwdaf\_MLModelProvision API Service.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.520 V17.6.0; 5G System; Network Data Analytics Services.

 url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.520/

servers:

 - url: '{apiRoot}/nnwdaf-mlmodelprovision/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

security:

 - {}

 - oAuth2ClientCredentials:

 - nnwdaf-mlmodelprovision

paths:

 /subscriptions:

 post:

 summary: Create a new Individual NWDAF ML Model Provision Subscription resource.

 operationId: CreateNWDAFMLModelProvisionSubcription

 tags:

 - Subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NwdafMLModelProvSubsc'

 responses:

 '201':

 description: Create a new Individual NWDAF ML Model Provision Subscription resource.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NwdafMLModelProvSubsc'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nnwdaf-mlmodelprovision/v1/subscriptions/{subscriptionId}.'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 myNotification:

 '{$request.body#/notifUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/NwdafMLModelProvNotif'

 minItems: 1

 responses:

 '204':

 description: No Content, Notification was succesfull

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /subscriptions/{subscriptionId}:

 put:

 summary: update an existing Individual NWDAF ML Model Provision Subscription

 operationId: UpdateNWDAFMLModelProvisionSubcription

 tags:

 - Individual NWDAF ML Model Provision Subscription (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NwdafMLModelProvSubsc'

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying a subscription to the Nnwdaf\_MLModelProvision Service.

 required: true

 schema:

 type: string

 responses:

 '200':

 description: The Individual NWDAF ML Model Provision Subscription resource was modified successfully and a representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NwdafMLModelProvSubsc'

 '204':

 description: The Individual NWDAF ML Model Provision Subscription resource was modified successfully.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Delete an existing Individual NWDAF ML Model Provision Subscription.

 operationId: DeleteNWDAFMLModelProvisionSubcription

 tags:

 - Individual NWDAF ML Model Provision Subscription (Document)

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying a subscription to the Nnwdaf\_MLModelProvision Service.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. The Individual NWDAF ML Model Provision Subscription matching the subscriptionId was deleted.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 nnwdaf-mlmodelprovision: Access to the Nnwdaf\_MLModelProvision API

 schemas:

 NwdafMLModelProvSubsc:

 description: Represents NWDAF Event Subscription resources.

 type: object

 properties:

 mLEventSubscs:

 type: array

 items:

 $ref: '#/components/schemas/MLEventSubscription'

 minItems: 1

 description: Subscribed events

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 mLEventNotifs:

 type: array

 items:

 $ref: '#/components/schemas/MLEventNotif'

 minItems: 1

 suppFeats:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 notifCorreId:

 type: string

 eventReq:

 $ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

 required:

 - mLEventSubscs

 - notifUri

 MLEventSubscription:

 description: Represents a subscription to a single event.

 type: object

 properties:

 mLEvent:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NwdafEvent'

 mLEventFilter:

 $ref: 'TS29520\_Nnwdaf\_AnalyticsInfo.yaml#/components/schemas/EventFilter'

 tgtUe:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/TargetUeInformation'

 mLTargetPeriod:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 expiryTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 required:

 - mLEvent

 - mLEventFilter

 NwdafMLModelProvNotif:

 description: Represents notifications on events that occurred.

 type: object

 properties:

 eventNotifs:

 type: array

 items:

 $ref: '#/components/schemas/MLEventNotif'

 minItems: 1

 description: Notifications about Individual Events.

 subscriptionId:

 type: string

 description: String identifying a subscription to the Nnwdaf\_MLModelProvision Service.

 required:

 - eventNotifs

 - subscriptionId

 MLEventNotif:

 description: Represents a notification related to a single event that occurred.

 type: object

 properties:

 event:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NwdafEvent'

 notifCorreId:

 type: string

 mLFileAddr:

 type: string

 description: Indicates the address (e.g. a URL or an FQDN) of the ML model file.

 adrfId:

 type: string

 description: Identifies the ADRF where the ML model is stored.

 validityPeriod:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 spatialValidity:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 required:

 - event

 oneOf:

 - required: [mLFileAddr]

 - required: [adrfId]

\*\*\* End of Changes \*\*\*