**3GPP TSG-CT3 Meeting #120e C3-221677**

**E-Meeting, 17th – 25th February 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.554** | **CR** | **0075** | **rev** | **-** | **Current version:** | **17.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Update of info and externalDocs fields |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | TEI17 |  | ***Date:*** | 2022-02-25 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | CR modifying Npcf\_BDTPolicyControl API has been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in TS 29.501, subclause 4.3.1.The following agreed CR updates the Npcf\_BDTPolicyControl API for the present release:- TS 29.554 CR #0073 is a backward compatible correction in Rel-17.As the present release is not yet frozen, a draft version number should be assigned. As the first backward compatible changes without prior backward incompatible changes to the existing API were agreed in for present non-frozen release, the minor version number needs to be incremented.Since a new Rel-17 TS version will be provided with changes to the OpenAPI specification file, the TS version number included in the "description" field of the "externalDocs" object also needs to be updated.Furthermore, in the "description" field of the "info" object, at the end of the first and second line two white spaces should be added to make a "hard line break" mark, and in the "description" field of the "externalDocs" object the url part needs to be updated to:'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.554/'. |
|  |  |
| ***Summary of change:*** | The Npcf\_BDTPolicyControl Service API version value changed to "1.2.0-alpha.1".The TS version number included in the "description" field of the "externalDocs" object changed to "17.3.0".The "description" field of the "info" object, two white spaces added at the end of the first and second line.The url part in the "description" field of the "externalDocs" object updated to:'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.554/'. |
|  |  |
| ***Consequences if not approved:*** | Incorrect API version number and incorrect TS version number in the "description" field of the "externalDocs" object. |
|  |  |
| ***Clauses affected:*** | A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* First Change \*\*\*

# A.2 Npcf\_BDTPolicyControl API

openapi: 3.0.0

info:

 title: Npcf\_BDTPolicyControl Service API

 version: 1.2.0-alpha.1

 description: |

 PCF BDT Policy Control Service.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

#

externalDocs:

 description: >

 3GPP TS 29.554 V17.3.0; 5G System; Background Data Transfer Policy Control Service.

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.554/'

#

servers:

 - url: '{apiRoot}/npcf-bdtpolicycontrol/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

security:

 - {}

 - oAuth2ClientCredentials:

 - npcf-bdtpolicycontrol

paths:

 /bdtpolicies:

 post:

 summary: Create a new Individual BDT policy

 operationId: CreateBDTPolicy

 tags:

 - BDT policies (Collection)

 requestBody:

 description: Contains information for the creation of a new Individual BDT policy resource.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/BdtReqData'

 responses:

 '201':

 description: Background data transfer policies offered to an ASP.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/BdtPolicy'

 headers:

 Location:

 description: 'Contains the URI of the created individual BDT policy resource, according to the structure: {apiRoot}/npcf-bdtpolicycontrol/v1/bdtpolicies/{bdtPolicyId}'

 required: true

 schema:

 type: string

#

# Error scenarios POST

#

 '303':

 description: See Other. The result of the POST request would be equivalent to the existing Individual BDT policy resource.

 headers:

 Location:

 description: 'Contains the URI of the existing individual BDT policy resource.'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

# End error scenarios POST

#

 callbacks:

 BdtNotification:

 '{$request.body#/notifUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/Notification'

 responses:

 '204':

 description: No Content, a reception of the BDT notification was successful.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

 /bdtpolicies/{bdtPolicyId}:

 get:

 summary: Read an Individual BDT policy

 operationId: GetBDTPolicy

 tags:

 - Individual BDT policy (Document)

 parameters:

 - name: bdtPolicyId

 description: String identifying the individual BDT policy resource in the PCF.

 in: path

 required: true

 schema:

 type: string

 responses:

 '200':

 description: Background data transfer policies offered to and selected by an ASP.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/BdtPolicy'

#

# Redirection scenarios GET

#

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

#

# Error scenarios GET

#

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

# End error scenarios GET

#

 patch:

 summary: Update an Individual BDT policy

 operationId: UpdateBDTPolicy

 tags:

 - Individual BDT policy (Document)

 parameters:

 - name: bdtPolicyId

 description: String identifying the individual BDT policy resource in the PCF.

 in: path

 required: true

 schema:

 type: string

 requestBody:

 description: Contains modification instruction to be performed on the BdtPolicy data structure to select a transfer policy and in addition, may indicate whether the BDT warning notification is enabled or disabled.

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: '#/components/schemas/PatchBdtPolicy'

 responses:

 '200':

 description: The Individual BDT Policy resource is modified and a representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/BdtPolicy'

 '204':

 description: The Individual BDT Policy resource is modified.

#

# Redirection scenarios PATCH

#

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

#

# Error scenarios PATCH

#

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

# End error scenarios PATCH

#

#

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 npcf-bdtpolicycontrol: Access to the Npcf\_BDTPolicyControl API

 schemas:

#

# Structured data types

#

 BdtPolicy:

 description: Represents an Individual BDT policy resource.

 type: object

 properties:

 bdtPolData:

 $ref: '#/components/schemas/BdtPolicyData'

 bdtReqData:

 $ref: '#/components/schemas/BdtReqData'

#

 BdtReqData:

 description: Contains service requirements for creation a new Individual BDT policy resource.

 type: object

 required:

 - aspId

 - desTimeInt

 - numOfUes

 - volPerUe

 properties:

 aspId:

 $ref: '#/components/schemas/AspId'

 desTimeInt:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 interGroupId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 nwAreaInfo:

 $ref: '#/components/schemas/NetworkAreaInfo'

 numOfUes:

 description: Indicates a number of UEs.

 type: integer

 volPerUe:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 trafficDes:

 $ref: 'TS29122\_ResourceManagementOfBdt.yaml#/components/schemas/TrafficDescriptor'

 warnNotifReq:

 description: Indicates whether the BDT warning notification is enabled or disabled.

 type: boolean

 default: false

#

 BdtPolicyData:

 description: Describes the authorization data of an Individual BDT policy resource.

 type: object

 required:

 - bdtRefId

 - transfPolicies

 properties:

 bdtRefId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

 transfPolicies:

 description: Contains transfer policies.

 type: array

 items:

 $ref: '#/components/schemas/TransferPolicy'

 minItems: 1

 selTransPolicyId:

 description: Contains an identity of the selected transfer policy.

 type: integer

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

#

 PatchBdtPolicy:

 description: Describes the updates in authorization data of an Individual BDT Policy created by the PCF.

 type: object

 properties:

 bdtPolData:

 $ref: '#/components/schemas/BdtPolicyDataPatch'

 bdtReqData:

 $ref: '#/components/schemas/BdtReqDataPatch'

#

 BdtPolicyDataPatch:

 description: A JSON Merge Patch body schema containing modification instruction to be performed on the bdtPolData attribute of the BdtPolicy data structure to select a transfer policy. Adds selTransPolicyId to BdtPolicyData data structure.

 type: object

 required:

 - selTransPolicyId

 properties:

 selTransPolicyId:

 description: Contains an identity (i.e. transPolicyId value) of the selected transfer policy. If the BdtNotification\_5G feature is supported value 0 indicates that no transfer policy is selected.

 type: integer

#

 BdtReqDataPatch:

 description: A JSON Merge Patch body schema containing modification instruction to be performed on the bdtReqData attribute of the BdtPolicy data structure to indicate whether the BDT warning notification is enabled or disabled. Modifies warnNotifReq from BdtReqData data structure.

 type: object

 properties:

 warnNotifReq:

 description: Indicates whether the BDT warning notification is enabled or disabled.

 type: boolean

#

 TransferPolicy:

 description: Describes a transfer policy.

 type: object

 required:

 - ratingGroup

 - recTimeInt

 - transPolicyId

 properties:

 maxBitRateDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 maxBitRateUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 ratingGroup:

 description: Indicates a rating group for the recommended time window.

 type: integer

 recTimeInt:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 transPolicyId:

 description: Contains an identity of a transfer policy.

 type: integer

 NetworkAreaInfo:

 description: Describes a network area information in which the NF service consumer requests the number of UEs.

 type: object

 properties:

 ecgis:

 description: Contains a list of E-UTRA cell identities.

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ecgi'

 minItems: 1

 ncgis:

 description: Contains a list of NR cell identities.

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ncgi'

 minItems: 1

 gRanNodeIds:

 description: Contains a list of NG RAN nodes.

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GlobalRanNodeId'

 minItems: 1

 tais:

 description: Contains a list of tracking area identities.

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

 minItems: 1

#

 Notification:

 description: Describes a BDT notification.

 type: object

 required:

 - bdtRefId

 properties:

 bdtRefId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

 candPolicies:

 description: Contains a list of the candidate transfer policies from which the AF may select a new transfer policy due to a network performance is below the criteria set by the operator.

 type: array

 items:

 $ref: '#/components/schemas/TransferPolicy'

 minItems: 1

 nwAreaInfo:

 $ref: '#/components/schemas/NetworkAreaInfo'

 timeWindow:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

#

# Simple data types

#

 AspId:

 description: Contains an identity of an application service provider.

 type: string

#

#

\*\*\* End of Changes \*\*\*