**3GPP TSG-CT3 Meeting #121e C3-222156**

**E-Meeting, 6th – 12th April 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.514** | **CR** | **0405** | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | DNN and S-NSSAI notification | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | IIoT | | | | |  | ***Date:*** | | | 2022-04-12 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | As agreed in clause 4.15.9.2 of TS 23.502, the PCF includes the UE address of the PDU Session and DNN/S-NSSAI within Npcf\_PolicyAuthorization\_Notify service operation. In the case of private IPv4 address being used for the UE, the DNN and S-NSSAI are required for session binding in the PCF. We aslo propose to include the domain identity within the notification in stage 3. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Include the DNN, S-NSSAI and domain identity in the notification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Not aligned with stage 2. The TSCTSF can’t find the correct PCF. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.2.5.16, 5.6.2.40, A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduce a backward compatible correction to the OpenAPI file. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* \* Start of Changes \* \* \* \*

#### 4.2.5.16 Notification about TSC user plane node Information, no Individual Application Session Context exists

If the "TimeSensitiveNetworking" or "TimeSensitiveCommunication" feature is supported and if the PCF becomes aware that TSC user plane node information for an external network (e.g. TSN) is available, but there is no "Individual Application Session Context" resource bound to the SM Policy Association updated with TSC user plane node related information, the PCF shall inform the NF service consumer (i.e. TSN AF or TSCTSF) about the detection of a TSC user plane node information in the context of a PDU session by sending a notification request:

* to the request URI locally configured in the PCF for the NF service consumer; or

- if the request URI for the TSCTSF is not locally configured in the PCF, to the notification URI retrieved from NRFusing the discovery service, as specified in 3GPP TS 29.510[27] for the PDU session DNN/S-NSSAI.

NOTE 1: PCF configuration of TSN AF needs to ensure that the notification is addressed to a TSN AF that connects to the same external network the UPF/NW-TT connects to. How it is achieved is implementation specific. It can be based e.g. on dedicated DNN/S-NSSAI combinations or on the received TSC user plane node information.

NOTE 2: It is assumed that there is only one TSCTSF for a given DNN/S-NSSAI in this release of the specification.

Figure 4.2.5.16-1 illustrates the notification about TSC user plane node information when there is no Individual Application Session Context bound to the SM Policy Association.



Figure 4.2.5.16-1: Notification about TSC user plane node Information, no AF session context exists

When the PCF determines that the AF application session context does not exist for the SM Policy Association that detected new port information and a notification URI for the NF service consumer can be determined, the PCF shall invoke the Npcf\_PolicyAuthorization\_Notify service operation by sending the HTTP POST request (as shown in figure 4.2.5.16-1, step 1) using the notification URI locally configured in the PCF or, retrieved from NRF, and appending the "new-bridge" segment path at the end of the URI, to trigger the NF service consumer (i.e. TSN AF or TSCTSF) to request the creation of an Invidual Application Session Context resource to handle the TSC user plane node detected in the context of a PDU session, configuring ports and TSC user plane node management information, and providing the corresponding TSCAI input containers and TSC traffic QoS related data (see subclauses 4.2.2.2, 4.2.2.24, 4.2.2.25 and 4.2.2.31).

The PCF shall provide in the body of the HTTP POST request the "PduSessionTsnBridge" data type including TSC user plane node information as follows:

- the "tsnBridgeInfo" attribute as received from the SMF;

- the "tsnBridgeManCont" attribute as received from the SMF, if available;

- the "tsnPortManContDstt" attribute and/or "tsnPortManContNwtts" attribute as received from the SMF, if available; and

- when the "TimeSensitiveCommunication" feature is supported and for a PDU session of IP type, the UE IPv4 address within the "ueIpv4Addr" attribute or the UE IPv6 prefix within the "ueIpv6AddrPrefix", the DNN within the "dnn" attribute, the S-NSSAI within the "snssai" attribute and, if available, the domain identifier within the "ipDomain" attribute if UE IPv4 address is provided.

NOTE x1: In the case of private IPv4 address being used for the UE, the DNN, S-NSSAI and domain identifier if available are required for session binding in the PCF. Domain identfier is only applicable to the AF session with required QoS as defined in subclause 4.2.2.24.

Upon the reception of the HTTP POST request from the PCF, the NF service consumer shall acknowledge that request.

With the received information, the NF service consumer (i.e. TSN AF or TSCTSF) shall immediately trigger the creation of an Individual Application Session Context resource to handle in this association the configuration of the new TSC user plane node in the context of this PDU session, as described in subclauses 4.2.2.2, 4.2.2.24, 4.2.2.25 and 4.2.2.31.

NOTE x3: For the time synchronization service, the subscription to UE availability for time-synchronization service can occur after the PDU Session establishment has been completed in 5GS. Similarly, for the AF session with required QoS, the indication of the required QoS and TSC Assistance Container information can occur after the completion of the PDU session establishment. In such cases, the PCF sends the notification to the TSCTSF about the detection of a TSC user plane node information during PDU session establishment, and the TSCTSF defers the creation of the related "Individual Application Session Context" till the reception of the subscription to UE availability for time synchronization or the AF session with required QoS occurs, as specified in 3GPP TS 29.513[7].

The NF service consumer (i.e. TSN AF or TSCTSF) may use the received TSC user plane node information and/or the received DS-TT port management information container and/or NW-TT port management information containers and the local configuration to construct the DS-TT port and or NW-TT port management information required to interwork with the external network.

\* \* \* \* Next Change \* \* \* \*

#### 5.6.2.40 Type PduSessionTsnBridge

Table 5.6.2.40-1: Definition of type PduSessionTsnBridge

| Attribute name | Data type | P | Cardinality | Description | Applicability |
| --- | --- | --- | --- | --- | --- |
| tsnBridgeInfo | TsnBridgeInfo | M | 1 | Reports the TSC user plane node information. |  |
| tsnBridgeManCont | BridgeManagementContainer | O | 0..1 | Transports TSC user plane node management information. |  |
| tsnPortManContDstt | PortManagementContainer | O | 0..1 | Transports port management information for the DS-TT port. |  |
| tsnPortManContNwtts | array(PortManagementContainer) | O | 1..N | Transports port management information for one or more NW-TT ports. |  |
| ueIpv4Addr | Ipv4Addr | O | 0..1 | It represents the identifier of the PDU session related to the reported UP node information, and contains the UE IPv4 address.  It might be present for PDU sessions of IP type.  (NOTE) | TimeSensitiveCommunication |
| dnn | Dnn | O | 0..1 | The DNN of the PDU session, a full DNN with both the Network Identifier and Operator Identifier, or a DNN with the Network Identifier only. | TimeSensitiveCommunication |
| snssai | Snssai | O | 0..1 | Identifies the S-NSSAI. | TimeSensitiveCommunication |
| ipDomain | string | O | 0..1 | IPv4 address domain identifier. | TimeSensitiveCommunication |
| ueIpv6AddrPrefix | Ipv6Prefix | O | 0..1 | It represents the identifier of the PDU session related to the reported UP node information, and contains the UE IPv6 address prefix. It might be present for PDU sessions of IP type.  (NOTE) | TimeSensitiveCommunication |
| NOTE: For PDU sessions of IP type, either the ueIpv4Addr or the ueIpv6AddrPrefix shall be present in this release of the specification. | | | | | |

\* \* \* \* Next Change \* \* \* \*

# A.2 Npcf\_PolicyAuthorization API

openapi: 3.0.0

info:

title: Npcf\_PolicyAuthorization Service API

version: 1.2.0-alpha.5

description: |

PCF Policy Authorization Service.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.514 V17.4.0; 5G System; Policy Authorization Service; Stage 3.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.514/'

#

servers:

- url: '{apiRoot}/npcf-policyauthorization/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501

security:

- {}

- oAuth2ClientCredentials:

- npcf-policyauthorization

paths:

/app-sessions:

post:

summary: Creates a new Individual Application Session Context resource

operationId: PostAppSessions

tags:

- Application Sessions (Collection)

requestBody:

description: Contains the information for the creation the resource.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AppSessionContext'

responses:

'201':

description: Successful creation of the resource

content:

application/json:

schema:

$ref: '#/components/schemas/AppSessionContext'

headers:

Location:

description: >

Contains the URI of the created individual application session context resource,

according to the structure

{apiRoot}/npcf-policyauthorization/v1/app-sessions/{appSessionId}

or the URI of the created events subscription sub-resource,

according to the structure

{apiRoot}/npcf-policyauthorization/v1/app-sessions/{appSessionId}/events-subscription}

required: true

schema:

type: string

'303':

description: See Other. The result of the HTTP POST request would be equivalent to the existing Application Session Context.

headers:

Location:

description: Contains the URI of the existing individual Application Session Context resource.

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ExtendedProblemDetails'

headers:

Retry-After:

description: >

Indicates the time the AF has to wait before making a new request. It can be a

non-negative integer (decimal number) indicating the number of seconds the AF

has to wait before making a new request or an HTTP-date after which the AF can

retry a new request.

schema:

anyOf:

- type: integer

- type: string

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

terminationRequest:

'{$request.body#/ascReqData/notifUri}/terminate':

post:

requestBody:

description: Request of the termination of the Individual Application Session Context.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TerminationInfo'

responses:

'204':

description: The receipt of the notification is acknowledged.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

eventNotification:

'{$request.body#/ascReqData/evSubsc/notifUri}/notify':

post:

requestBody:

description: Notification of an event occurrence in the PCF.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/EventsNotification'

responses:

'204':

description: The receipt of the notification is acknowledged.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

detected5GsBridgeForPduSession:

'{$request.body#/ascReqData/evSubsc/notifUri}/new-bridge':

post:

requestBody:

description: Notification of a new TSC user plane node detected in the PCF.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PduSessionTsnBridge'

responses:

'204':

description: The receipt of the notification is acknowledged.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

eventNotificationPduSession:

'{$request.body#/ascReqData/evSubsc/notifUri}/pdu-session':

post:

requestBody:

description: Notification of PDU session established or terminated.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PduSessionEventNotification'

responses:

'204':

description: The receipt of the notification is acknowledged.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/app-sessions/pcscf-restoration:

post:

summary: "Indicates P-CSCF restoration and does not create an Individual Application Session Context"

operationId: PcscfRestoration

tags:

- PCSCF Restoration Indication

requestBody:

description: PCSCF Restoration Indication.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PcscfRestorationRequestData'

responses:

'204':

description: The deletion is confirmed without returning additional data.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

/app-sessions/{appSessionId}:

get:

summary: "Reads an existing Individual Application Session Context"

operationId: GetAppSession

tags:

- Individual Application Session Context (Document)

parameters:

- name: appSessionId

description: String identifying the resource.

in: path

required: true

schema:

type: string

responses:

'200':

description: A representation of the resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/AppSessionContext'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: "Modifies an existing Individual Application Session Context"

operationId: ModAppSession

tags:

- Individual Application Session Context (Document)

parameters:

- name: appSessionId

description: String identifying the resource.

in: path

required: true

schema:

type: string

requestBody:

description: Modification of the resource.

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/AppSessionContextUpdateDataPatch'

responses:

'200':

description: Successful modification of the resource and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/AppSessionContext'

'204':

description: The successful modification.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden

content:

application/problem+json:

schema:

$ref: '#/components/schemas/ExtendedProblemDetails'

headers:

Retry-After:

description: >

Indicates the time the AF has to wait before making a new request. It can be a

non-negative integer (decimal number) indicating the number of seconds the AF has

to wait before making a new request or an HTTP-date after which the AF can retry

a new request.

schema:

anyOf:

- type: integer

- type: string

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

eventNotification:

'{$request.body#/ascReqData/evSubsc/notifUri}/notify':

post:

requestBody:

description: Notification of an event occurrence in the PCF.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/EventsNotification'

responses:

'204':

description: The receipt of the notification is acknowledged

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

#

/app-sessions/{appSessionId}/delete:

post:

summary: "Deletes an existing Individual Application Session Context"

operationId: DeleteAppSession

tags:

- Individual Application Session Context (Document)

parameters:

- name: appSessionId

description: String identifying the Individual Application Session Context resource.

in: path

required: true

schema:

type: string

requestBody:

description: Deletion of the Individual Application Session Context resource, req notification.

required: false

content:

application/json:

schema:

$ref: '#/components/schemas/EventsSubscReqData'

responses:

'200':

description: The deletion of the resource is confirmed and a resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/AppSessionContext'

'204':

description: The deletion is confirmed without returning additional data.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

/app-sessions/{appSessionId}/events-subscription:

put:

summary: "creates or modifies an Events Subscription subresource"

operationId: updateEventsSubsc

tags:

- Events Subscription (Document)

parameters:

- name: appSessionId

description: String identifying the Events Subscription resource.

in: path

required: true

schema:

type: string

requestBody:

description: Creation or modification of an Events Subscription resource.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/EventsSubscReqData'

responses:

'201':

description: The creation of the Events Subscription resource is confirmed and its representation is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/EventsSubscPutData'

headers:

Location:

description: >

Contains the URI of the created Events Subscription resource,

according to the structure

{apiRoot}/npcf-policyauthorization/v1/app-sessions/{appSessionId}/events-subscription}

required: true

schema:

type: string

'200':

description: The modification of the Events Subscription resource is confirmed its representation is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/EventsSubscPutData'

'204':

description: The modification of the Events Subscription subresource is confirmed without returning additional data.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

eventNotification:

'{$request.body#/notifUri}/notify':

post:

requestBody:

description: Contains the information for the notification of an event occurrence in the PCF.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/EventsNotification'

responses:

'204':

description: The receipt of the notification is acknowledged.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: deletes the Events Subscription subresource

operationId: DeleteEventsSubsc

tags:

- Events Subscription (Document)

parameters:

- name: appSessionId

description: String identifying the Individual Application Session Context resource.

in: path

required: true

schema:

type: string

responses:

'204':

description: The deletion of the of the Events Subscription sub-resource is confirmed without returning additional data.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

npcf-policyauthorization: Access to the Npcf\_PolicyAuthorization API

schemas:

AppSessionContext:

description: Represents an Individual Application Session Context resource.

type: object

properties:

ascReqData:

$ref: '#/components/schemas/AppSessionContextReqData'

ascRespData:

$ref: '#/components/schemas/AppSessionContextRespData'

evsNotif:

$ref: '#/components/schemas/EventsNotification'

AppSessionContextReqData:

description: Identifies the service requirements of an Individual Application Session Context.

type: object

required:

- notifUri

- suppFeat

oneOf:

- required: [ueIpv4]

- required: [ueIpv6]

- required: [ueMac]

properties:

afAppId:

$ref: '#/components/schemas/AfAppId'

afChargId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationChargingId'

afReqData:

$ref: '#/components/schemas/AfRequestedData'

afRoutReq:

$ref: '#/components/schemas/AfRoutingRequirement'

aspId:

$ref: '#/components/schemas/AspId'

bdtRefId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

evSubsc:

$ref: '#/components/schemas/EventsSubscReqData'

mcpttId:

description: Indication of MCPTT service request.

type: string

mcVideoId:

description: Indication of MCVideo service request.

type: string

medComponents:

type: object

additionalProperties:

$ref: '#/components/schemas/MediaComponent'

minProperties: 1

description: Contains media component information. The key of the map is the medCompN attribute.

ipDomain:

type: string

mpsAction:

$ref: '#/components/schemas/MpsAction'

mpsId:

description: Indication of MPS service request.

type: string

mcsId:

description: Indication of MCS service request.

type: string

preemptControlInfo:

$ref: '#/components/schemas/PreemptionControlInformation'

resPrio:

$ref: '#/components/schemas/ReservPriority'

servInfStatus:

$ref: '#/components/schemas/ServiceInfoStatus'

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

servUrn:

$ref: '#/components/schemas/ServiceUrn'

sliceInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

sponId:

$ref: '#/components/schemas/SponId'

sponStatus:

$ref: '#/components/schemas/SponsoringStatus'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

ueIpv4:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ueIpv6:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

ueMac:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

tsnBridgeManCont:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/BridgeManagementContainer'

tsnPortManContDstt:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

tsnPortManContNwtts:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

minItems: 1

AppSessionContextRespData:

description: Describes the authorization data of an Individual Application Session Context created by the PCF.

type: object

properties:

servAuthInfo:

$ref: '#/components/schemas/ServAuthInfo'

ueIds:

type: array

items:

$ref: '#/components/schemas/UeIdentityInfo'

minItems: 1

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

AppSessionContextUpdateDataPatch:

description: Identifies the modifications to an Individual Application Session Context and/or the modifications to the sub-resource Events Subscription.

type: object

properties:

ascReqData:

$ref: '#/components/schemas/AppSessionContextUpdateData'

AppSessionContextUpdateData:

description: >

Identifies the modifications to the "ascReqData" property of an Individual Application

Session Context which may include the modifications to the sub-resource Events Subscription.

type: object

properties:

afAppId:

$ref: '#/components/schemas/AfAppId'

afRoutReq:

$ref: '#/components/schemas/AfRoutingRequirementRm'

aspId:

$ref: '#/components/schemas/AspId'

bdtRefId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

evSubsc:

$ref: '#/components/schemas/EventsSubscReqDataRm'

mcpttId:

description: Indication of MCPTT service request.

type: string

mcVideoId:

description: Indication of modification of MCVideo service.

type: string

medComponents:

type: object

additionalProperties:

$ref: '#/components/schemas/MediaComponentRm'

minProperties: 1

description: Contains media component information. The key of the map is the medCompN attribute.

mpsAction:

$ref: '#/components/schemas/MpsAction'

mpsId:

description: Indication of MPS service request.

type: string

mcsId:

description: Indication of MCS service request.

type: string

preemptControlInfo:

$ref: '#/components/schemas/PreemptionControlInformationRm'

resPrio:

$ref: '#/components/schemas/ReservPriority'

servInfStatus:

$ref: '#/components/schemas/ServiceInfoStatus'

sipForkInd:

$ref: '#/components/schemas/SipForkingIndication'

sponId:

$ref: '#/components/schemas/SponId'

sponStatus:

$ref: '#/components/schemas/SponsoringStatus'

tsnBridgeManCont:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/BridgeManagementContainer'

tsnPortManContDstt:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

tsnPortManContNwtts:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

minItems: 1

EventsSubscReqData:

description: Identifies the events the application subscribes to.

type: object

required:

- events

properties:

events:

type: array

items:

$ref: '#/components/schemas/AfEventSubscription'

minItems: 1

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

reqQosMonParams:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RequestedQosMonitoringParameter'

minItems: 1

qosMon:

$ref: '#/components/schemas/QosMonitoringInformation'

reqAnis:

type: array

items:

$ref: '#/components/schemas/RequiredAccessInfo'

minItems: 1

usgThres:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

notifCorreId:

type: string

afAppIds:

type: array

items:

$ref: '#/components/schemas/AfAppId'

minItems: 1

directNotifInd:

type: boolean

EventsSubscReqDataRm:

description: This data type is defined in the same way as the EventsSubscReqData data type, but with the OpenAPI nullable property set to true.

type: object

required:

- events

properties:

events:

type: array

items:

$ref: '#/components/schemas/AfEventSubscription'

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

reqQosMonParams:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RequestedQosMonitoringParameter'

minItems: 1

qosMon:

$ref: '#/components/schemas/QosMonitoringInformationRm'

reqAnis:

type: array

items:

$ref: '#/components/schemas/RequiredAccessInfo'

minItems: 1

usgThres:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThresholdRm'

notifCorreId:

type: string

directNotifInd:

type: boolean

nullable: true

MediaComponent:

description: Identifies a media component.

type: object

required:

- medCompN

properties:

afAppId:

$ref: '#/components/schemas/AfAppId'

afRoutReq:

$ref: '#/components/schemas/AfRoutingRequirement'

qosReference:

type: string

disUeNotif:

type: boolean

altSerReqs:

type: array

items:

type: string

minItems: 1

altSerReqsData:

type: array

items:

$ref: '#/components/schemas/AlternativeServiceRequirementsData'

minItems: 1

description: Contains alternative service requirements that include individual QoS parameter sets.

contVer:

$ref: '#/components/schemas/ContentVersion'

codecs:

type: array

items:

$ref: '#/components/schemas/CodecData'

minItems: 1

maxItems: 2

desMaxLatency:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

desMaxLoss:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

flusId:

type: string

fStatus:

$ref: '#/components/schemas/FlowStatus'

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

maxPacketLossRateDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

maxPacketLossRateUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

maxSuppBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

maxSuppBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

medCompN:

type: integer

medSubComps:

type: object

additionalProperties:

$ref: '#/components/schemas/MediaSubComponent'

minProperties: 1

description: Contains the requested bitrate and filters for the set of service data flows identified by their common flow identifier. The key of the map is the fNum attribute.

medType:

$ref: '#/components/schemas/MediaType'

minDesBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

minDesBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

mirBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

mirBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

preemptCap:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PreemptionCapability'

preemptVuln:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PreemptionVulnerability'

prioSharingInd:

$ref: '#/components/schemas/PrioritySharingIndicator'

resPrio:

$ref: '#/components/schemas/ReservPriority'

rrBw:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

rsBw:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

sharingKeyDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

sharingKeyUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

tsnQos:

$ref: '#/components/schemas/TsnQosContainer'

tscaiInputDl:

$ref: '#/components/schemas/TscaiInputContainer'

tscaiInputUl:

$ref: '#/components/schemas/TscaiInputContainer'

tscaiTimeDom:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

MediaComponentRm:

description: This data type is defined in the same way as the MediaComponent data type, but with the OpenAPI nullable property set to true.

type: object

required:

- medCompN

properties:

afAppId:

$ref: '#/components/schemas/AfAppId'

afRoutReq:

$ref: '#/components/schemas/AfRoutingRequirementRm'

qosReference:

type: string

nullable: true

altSerReqs:

type: array

items:

type: string

minItems: 1

nullable: true

altSerReqsData:

type: array

items:

$ref: '#/components/schemas/AlternativeServiceRequirementsData'

minItems: 1

description: Contains removable alternative service requirements that include individual QoS parameter sets.

nullable: true

disUeNotif:

type: boolean

contVer:

$ref: '#/components/schemas/ContentVersion'

codecs:

type: array

items:

$ref: '#/components/schemas/CodecData'

minItems: 1

maxItems: 2

desMaxLatency:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/FloatRm'

desMaxLoss:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/FloatRm'

flusId:

type: string

nullable: true

fStatus:

$ref: '#/components/schemas/FlowStatus'

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

maxPacketLossRateDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

maxPacketLossRateUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

maxSuppBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

maxSuppBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

medCompN:

type: integer

medSubComps:

type: object

additionalProperties:

$ref: '#/components/schemas/MediaSubComponentRm'

minProperties: 1

description: Contains the requested bitrate and filters for the set of service data flows identified by their common flow identifier. The key of the map is the fNum attribute.

medType:

$ref: '#/components/schemas/MediaType'

minDesBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

minDesBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

mirBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

mirBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

preemptCap:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PreemptionCapabilityRm'

preemptVuln:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PreemptionVulnerabilityRm'

prioSharingInd:

$ref: '#/components/schemas/PrioritySharingIndicator'

resPrio:

$ref: '#/components/schemas/ReservPriority'

rrBw:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

rsBw:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

sharingKeyDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32Rm'

sharingKeyUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32Rm'

tsnQos:

$ref: '#/components/schemas/TsnQosContainerRm'

tscaiInputDl:

$ref: '#/components/schemas/TscaiInputContainer'

tscaiInputUl:

$ref: '#/components/schemas/TscaiInputContainer'

tscaiTimeDom:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

nullable: true

MediaSubComponent:

description: Identifies a media subcomponent.

type: object

required:

- fNum

properties:

afSigProtocol:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AfSigProtocol'

ethfDescs:

type: array

items:

$ref: '#/components/schemas/EthFlowDescription'

minItems: 1

maxItems: 2

fNum:

type: integer

fDescs:

type: array

items:

$ref: '#/components/schemas/FlowDescription'

minItems: 1

maxItems: 2

fStatus:

$ref: '#/components/schemas/FlowStatus'

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

tosTrCl:

$ref: '#/components/schemas/TosTrafficClass'

flowUsage:

$ref: '#/components/schemas/FlowUsage'

MediaSubComponentRm:

description: >

This data type is defined in the same way as the MediaSubComponent data type, but with the

OpenAPI nullable property set to true. Removable attributes marBwDl and marBwUl are defined

with the corresponding removable data type.

type: object

required:

- fNum

properties:

afSigProtocol:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AfSigProtocol'

ethfDescs:

type: array

items:

$ref: '#/components/schemas/EthFlowDescription'

minItems: 1

maxItems: 2

nullable: true

fNum:

type: integer

fDescs:

type: array

items:

$ref: '#/components/schemas/FlowDescription'

minItems: 1

maxItems: 2

nullable: true

fStatus:

$ref: '#/components/schemas/FlowStatus'

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

tosTrCl:

$ref: '#/components/schemas/TosTrafficClassRm'

flowUsage:

$ref: '#/components/schemas/FlowUsage'

nullable: true

EventsNotification:

description: Describes the notification of a matched event.

type: object

required:

- evSubsUri

- evNotifs

properties:

adReports:

type: array

items:

$ref: '#/components/schemas/AppDetectionReport'

minItems: 1

description: Includes the detected application report.

accessType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

addAccessInfo:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AdditionalAccessInfo'

relAccessInfo:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AdditionalAccessInfo'

anChargAddr:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AccNetChargingAddress'

anChargIds:

type: array

items:

$ref: '#/components/schemas/AccessNetChargingIdentifier'

minItems: 1

anGwAddr:

$ref: '#/components/schemas/AnGwAddress'

evSubsUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

evNotifs:

type: array

items:

$ref: '#/components/schemas/AfEventNotification'

minItems: 1

failedResourcAllocReports:

type: array

items:

$ref: '#/components/schemas/ResourcesAllocationInfo'

minItems: 1

succResourcAllocReports:

type: array

items:

$ref: '#/components/schemas/ResourcesAllocationInfo'

minItems: 1

noNetLocSupp:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/NetLocAccessSupport'

outOfCredReports:

type: array

items:

$ref: '#/components/schemas/OutOfCreditInformation'

minItems: 1

plmnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

qncReports:

type: array

items:

$ref: '#/components/schemas/QosNotificationControlInfo'

minItems: 1

qosMonReports:

type: array

items:

$ref: '#/components/schemas/QosMonitoringReport'

minItems: 1

ranNasRelCauses:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RanNasRelCause'

minItems: 1

description: Contains the RAN and/or NAS release cause.

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

satBackhaulCategory:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SatelliteBackhaulCategory'

ueLoc:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ueLocTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

ueTimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

usgRep:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/AccumulatedUsage'

tsnBridgeManCont:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/BridgeManagementContainer'

tsnPortManContDstt:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

tsnPortManContNwtts:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

minItems: 1

AfEventSubscription:

description: Describes the event information delivered in the subscription.

type: object

required:

- event

properties:

event:

$ref: '#/components/schemas/AfEvent'

notifMethod:

$ref: '#/components/schemas/AfNotifMethod'

repPeriod:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

waitTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

AfEventNotification:

description: Describes the event information delivered in the notification.

type: object

required:

- event

properties:

event:

$ref: '#/components/schemas/AfEvent'

flows:

type: array

items:

$ref: '#/components/schemas/Flows'

minItems: 1

TerminationInfo:

description: Indicates the cause for requesting the deletion of the Individual Application Session Context resource.

type: object

required:

- termCause

- resUri

properties:

termCause:

$ref: '#/components/schemas/TerminationCause'

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

AfRoutingRequirement:

description: Describes the event information delivered in the subscription.

type: object

properties:

appReloc:

type: boolean

routeToLocs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

minItems: 1

spVal:

$ref: '#/components/schemas/SpatialValidity'

tempVals:

type: array

items:

$ref: '#/components/schemas/TemporalValidity'

minItems: 1

upPathChgSub:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/UpPathChgEvent'

addrPreserInd:

type: boolean

simConnInd:

type: boolean

description: Indicates whether simultaneous connectivity should be temporarily maintained for the source and target PSA.

simConnTerm:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

easIpReplaceInfos:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/EasIpReplacementInfo'

minItems: 1

description: Contains EAS IP replacement information.

easRedisInd:

type: boolean

description: Indicates the EAS rediscovery is required.

SpatialValidity:

description: Describes explicitly the route to an Application location.

type: object

required:

- presenceInfoList

properties:

presenceInfoList:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 1

description: Defines the presence information provisioned by the AF. The praId attribute within the PresenceInfo data type is the key of the map.

SpatialValidityRm:

description: This data type is defined in the same way as the SpatialValidity data type, but with the OpenAPI nullable property set to true.

type: object

required:

- presenceInfoList

properties:

presenceInfoList:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 1

description: Defines the presence information provisioned by the AF. The praId attribute within the PresenceInfo data type is the key of the map.

nullable: true

AfRoutingRequirementRm:

description: >

This data type is defined in the same way as the AfRoutingRequirement data type, but with

the OpenAPI nullable property set to true and the spVal and tempVals attributes defined as

removable.

type: object

properties:

appReloc:

type: boolean

routeToLocs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

minItems: 1

nullable: true

spVal:

$ref: '#/components/schemas/SpatialValidityRm'

tempVals:

type: array

items:

$ref: '#/components/schemas/TemporalValidity'

minItems: 1

nullable: true

upPathChgSub:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/UpPathChgEvent'

addrPreserInd:

type: boolean

nullable: true

simConnInd:

type: boolean

nullable: true

description: Indicates whether simultaneous connectivity should be temporarily maintained for the source and target PSA.

simConnTerm:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

easIpReplaceInfos:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/EasIpReplacementInfo'

minItems: 1

description: Contains EAS IP replacement information.

nullable: true

easRedisInd:

type: boolean

description: Indicates the EAS rediscovery is required.

nullable: true

AnGwAddress:

description: Describes the address of the access network gateway control node.

type: object

anyOf:

- required: [anGwIpv4Addr]

- required: [anGwIpv6Addr]

properties:

anGwIpv4Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

anGwIpv6Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

Flows:

description: Identifies the flows.

type: object

required:

- medCompN

properties:

contVers:

type: array

items:

$ref: '#/components/schemas/ContentVersion'

minItems: 1

fNums:

type: array

items:

type: integer

minItems: 1

medCompN:

type: integer

EthFlowDescription:

description: Identifies an Ethernet flow.

type: object

required:

- ethType

properties:

destMacAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

ethType:

type: string

fDesc:

$ref: '#/components/schemas/FlowDescription'

fDir:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/FlowDirection'

sourceMacAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

vlanTags:

type: array

items:

type: string

minItems: 1

maxItems: 2

srcMacAddrEnd:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

destMacAddrEnd:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

ResourcesAllocationInfo:

description: Describes the status of the PCC rule(s) related to certain media components.

type: object

properties:

mcResourcStatus:

$ref: '#/components/schemas/MediaComponentResourcesStatus'

flows:

type: array

items:

$ref: '#/components/schemas/Flows'

minItems: 1

altSerReq:

type: string

TemporalValidity:

description: Indicates the time interval(s) during which the AF request is to be applied.

type: object

properties:

startTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

stopTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

#

QosNotificationControlInfo:

description: Indicates whether the QoS targets for a GRB flow are not guaranteed or guaranteed again.

type: object

required:

- notifType

properties:

notifType:

$ref: '#/components/schemas/QosNotifType'

flows:

type: array

items:

$ref: '#/components/schemas/Flows'

minItems: 1

altSerReq:

type: string

#

AcceptableServiceInfo:

description: Indicates the maximum bandwidth that shall be authorized by the PCF.

type: object

properties:

accBwMedComps:

type: object

additionalProperties:

$ref: '#/components/schemas/MediaComponent'

description: Indicates the maximum bandwidth that shall be authorized by the PCF for each media component of the map. The key of the map is the media component number.

minProperties: 1

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

UeIdentityInfo:

description: Represents 5GS-Level UE identities.

type: object

anyOf:

- required: [gpsi]

- required: [pei]

- required: [supi]

properties:

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

pei:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

#

AccessNetChargingIdentifier:

description: Describes the access network charging identifier.

type: object

required:

- accNetChaIdValue

properties:

accNetChaIdValue:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

flows:

type: array

items:

$ref: '#/components/schemas/Flows'

minItems: 1

#

OutOfCreditInformation:

description: Indicates the SDFs without available credit and the corresponding termination action.

type: object

required:

- finUnitAct

properties:

finUnitAct:

$ref: 'TS32291\_Nchf\_ConvergedCharging.yaml#/components/schemas/FinalUnitAction'

flows:

type: array

items:

$ref: '#/components/schemas/Flows'

minItems: 1

#

QosMonitoringInformation:

description: Indicates the QoS Monitoring information to report, i.e. UL and/or DL and or round trip delay.

type: object

properties:

repThreshDl:

type: integer

repThreshUl:

type: integer

repThreshRp:

type: integer

#

#

PduSessionTsnBridge:

description: Contains the new TSC user plane node information and may contain the DS-TT port and/or NW-TT port management information.

type: object

required:

- tsnBridgeInfo

properties:

tsnBridgeInfo:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/TsnBridgeInfo'

tsnBridgeManCont:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/BridgeManagementContainer'

tsnPortManContDstt:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

tsnPortManContNwtts:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

minItems: 1

ueIpv4Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

ipDomain:

type: string

description: IPv4 address domain identifier.

ueIpv6AddrPrefix:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

#

QosMonitoringInformationRm:

description: This data type is defined in the same way as the QosMonitoringInformation data type, but with the OpenAPI nullable property set to true.

type: object

properties:

repThreshDl:

type: integer

repThreshUl:

type: integer

repThreshRp:

type: integer

nullable: true

#

PcscfRestorationRequestData:

description: Indicates P-CSCF restoration.

type: object

oneOf:

- required: [ueIpv4]

- required: [ueIpv6]

properties:

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

ipDomain:

type: string

sliceInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

ueIpv4:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ueIpv6:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

#

#

QosMonitoringReport:

description: QoS Monitoring reporting information.

type: object

properties:

flows:

type: array

items:

$ref: '#/components/schemas/Flows'

minItems: 1

ulDelays:

type: array

items:

type: integer

minItems: 1

dlDelays:

type: array

items:

type: integer

minItems: 1

rtDelays:

type: array

items:

type: integer

minItems: 1

#

TsnQosContainer:

description: Indicates TSC Traffic QoS.

type: object

properties:

maxTscBurstSize:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVol'

tscPackDelay:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

tscPrioLevel:

$ref: '#/components/schemas/TscPriorityLevel'

#

#

TsnQosContainerRm:

description: Indicates removable TSC Traffic QoS.

type: object

properties:

maxTscBurstSize:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVolRm'

tscPackDelay:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudgetRm'

tscPrioLevel:

$ref: '#/components/schemas/TscPriorityLevelRm'

nullable: true

#

TscaiInputContainer:

description: Indicates TSC Traffic pattern.

type: object

properties:

periodicity:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

burstArrivalTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

surTimeInNumMsg:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

surTimeInTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

nullable: true

#

#

AppDetectionReport:

description: Indicates the start or stop of the detected application traffic and the application identifier of the detected application traffic.

type: object

required:

- adNotifType

- afAppId

properties:

adNotifType:

$ref: '#/components/schemas/AppDetectionNotifType'

afAppId:

$ref: '#/components/schemas/AfAppId'

#

#

PduSessionEventNotification:

description: Indicates PDU session information for the concerned established/terminated PDU session.

type: object

required:

- evNotif

properties:

evNotif:

$ref: '#/components/schemas/AfEventNotification'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

ueIpv4:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ueIpv6:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

ueMac:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

status:

$ref: '#/components/schemas/PduSessionStatus'

pcfInfo:

$ref: '#/components/schemas/PcfAddressingInfo'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

#

#

PcfAddressingInfo:

description: Contains PCF address information.

type: object

properties:

pcfFqdn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Fqdn'

pcfIpEndPoints:

type: array

items:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/IpEndPoint'

minItems: 1

description: IP end points of the PCF hosting the Npcf\_PolicyAuthorization service.

bindingInfo:

type: string

description: contains the binding indications of the PCF.

#

AlternativeServiceRequirementsData:

description: Contains an alternative QoS related parameter set.

type: object

required:

- altQosParamSetRef

properties:

altQosParamSetRef:

type: string

description: Reference to this alternative QoS related parameter set.

gbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

gbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

pdb:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

#

EventsSubscPutData:

description: >

Identifies the events the application subscribes to within an Events Subscription

sub-resource data. It may contain the notification of the already met events.

anyOf:

- $ref: '#/components/schemas/EventsSubscReqData'

- $ref: '#/components/schemas/EventsNotification'

#

# EXTENDED PROBLEMDETAILS

#

ExtendedProblemDetails:

description: Extends ProblemDetails to also include the acceptable service info.

allOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- type: object

properties:

acceptableServInfo:

$ref: '#/components/schemas/AcceptableServiceInfo'

#

# SIMPLE DATA TYPES

#

AfAppId:

description: Contains an AF application identifier.

type: string

AspId:

description: Contains an identity of an application service provider.

type: string

CodecData:

description: Contains codec related information.

type: string

ContentVersion:

description: Represents the content version of some content.

type: integer

FlowDescription:

description: Defines a packet filter of an IP flow.

type: string

SponId:

description: Contains an identity of a sponsor.

type: string

ServiceUrn:

description: Contains values of the service URN and may include subservices.

type: string

TosTrafficClass:

description: >

2-octet string, where each octet is encoded in hexadecimal representation. The first octet

contains the IPv4 Type-of-Service or the IPv6 Traffic-Class field and the second octet

contains the ToS/Traffic Class mask field.

type: string

TosTrafficClassRm:

description: This data type is defined in the same way as the TosTrafficClass data type, but with the OpenAPI nullable property set to true.

type: string

nullable: true

TscPriorityLevel:

description: Represents the priority level of TSC Flows.

type: integer

minimum: 1

maximum: 8

TscPriorityLevelRm:

description: This data type is defined in the same way as the TscPriorityLevel data type, but with the OpenAPI nullable property set to true.

type: integer

minimum: 1

maximum: 8

nullable: true

#

# ENUMERATIONS DATA TYPES

#

MediaType:

description: Indicates the media type of a media component.

anyOf:

- type: string

enum:

- AUDIO

- VIDEO

- DATA

- APPLICATION

- CONTROL

- TEXT

- MESSAGE

- OTHER

- type: string

#

MpsAction:

description: Indicates whether it is an invocation, a revocation or an invocation with authorization of the MPS for DTS service.

anyOf:

- type: string

enum:

- DISABLE\_MPS\_FOR\_DTS

- ENABLE\_MPS\_FOR\_DTS

- AUTHORIZE\_AND\_ENABLE\_MPS\_FOR\_DTS

- type: string

#

ReservPriority:

description: Indicates the reservation priority.

anyOf:

- type: string

enum:

- PRIO\_1

- PRIO\_2

- PRIO\_3

- PRIO\_4

- PRIO\_5

- PRIO\_6

- PRIO\_7

- PRIO\_8

- PRIO\_9

- PRIO\_10

- PRIO\_11

- PRIO\_12

- PRIO\_13

- PRIO\_14

- PRIO\_15

- PRIO\_16

- type: string

#

ServAuthInfo:

description: Indicates the result of the Policy Authorization service request from the AF.

anyOf:

- type: string

enum:

- TP\_NOT\_KNOWN

- TP\_EXPIRED

- TP\_NOT\_YET\_OCURRED

- ROUT\_REQ\_NOT\_AUTHORIZED

- type: string

#

SponsoringStatus:

description: Indicates whether sponsored data connectivity is enabled or disabled/not enabled.

anyOf:

- type: string

enum:

- SPONSOR\_DISABLED

- SPONSOR\_ENABLED

- type: string

#

AfEvent:

description: Represents an event to notify to the AF.

anyOf:

- type: string

enum:

- ACCESS\_TYPE\_CHANGE

- ANI\_REPORT

- APP\_DETECTION

- CHARGING\_CORRELATION

- EPS\_FALLBACK

- FAILED\_QOS\_UPDATE

- FAILED\_RESOURCES\_ALLOCATION

- OUT\_OF\_CREDIT

- PDU\_SESSION\_STATUS

- PLMN\_CHG

- QOS\_MONITORING

- QOS\_NOTIF

- RAN\_NAS\_CAUSE

- REALLOCATION\_OF\_CREDIT

- SAT\_CATEGORY\_CHG

- SUCCESSFUL\_QOS\_UPDATE

- SUCCESSFUL\_RESOURCES\_ALLOCATION

- TSN\_BRIDGE\_INFO

- UP\_PATH\_CHG\_FAILURE

- USAGE\_REPORT

- type: string

#

AfNotifMethod:

description: Represents the notification methods that can be subscribed for an event.

anyOf:

- type: string

enum:

- EVENT\_DETECTION

- ONE\_TIME

- PERIODIC

- PDU\_SESSION\_RELEASE

- type: string

#

QosNotifType:

description: Indicates the notification type for QoS Notification Control.

anyOf:

- type: string

enum:

- GUARANTEED

- NOT\_GUARANTEED

- type: string

#

TerminationCause:

description: Indicates the cause behind requesting the deletion of the Individual Application Session Context resource.

anyOf:

- type: string

enum:

- ALL\_SDF\_DEACTIVATION

- PDU\_SESSION\_TERMINATION

- PS\_TO\_CS\_HO

- INSUFFICIENT\_SERVER\_RESOURCES

- INSUFFICIENT\_QOS\_FLOW\_RESOURCES

- SPONSORED\_DATA\_CONNECTIVITY\_DISALLOWED

- type: string

#

MediaComponentResourcesStatus:

description: Indicates whether the media component is active or inactive.

anyOf:

- type: string

enum:

- ACTIVE

- INACTIVE

- type: string

#

#

FlowUsage:

description: Describes the flow usage of the flows described by a media subcomponent.

anyOf:

- type: string

enum:

- NO\_INFO

- RTCP

- AF\_SIGNALLING

- type: string

FlowStatus:

description: Describes whether the IP flow(s) are enabled or disabled.

anyOf:

- type: string

enum:

- ENABLED-UPLINK

- ENABLED-DOWNLINK

- ENABLED

- DISABLED

- REMOVED

- type: string

#

RequiredAccessInfo:

description: Indicates the access network information required for an AF session.

anyOf:

- type: string

enum:

- USER\_LOCATION

- UE\_TIME\_ZONE

- type: string

#

SipForkingIndication:

description: Indicates whether several SIP dialogues are related to an "Individual Application Session Context" resource.

anyOf:

- type: string

enum:

- SINGLE\_DIALOGUE

- SEVERAL\_DIALOGUES

- type: string

#

AfRequestedData:

description: Represents the information that the AF requested to be exposed.

anyOf:

- type: string

enum:

- UE\_IDENTITY

- type: string

#

ServiceInfoStatus:

description: Represents the preliminary or final service information status.

anyOf:

- type: string

enum:

- FINAL

- PRELIMINARY

- type: string

#

PreemptionControlInformation:

description: Represents Pre-emption control information.

anyOf:

- type: string

enum:

- MOST\_RECENT

- LEAST\_RECENT

- HIGHEST\_BW

- type: string

#

PrioritySharingIndicator:

description: Represents the Priority sharing indicator.

anyOf:

- type: string

enum:

- ENABLED

- DISABLED

- type: string

#

PreemptionControlInformationRm:

description: This data type is defined in the same way as the PreemptionControlInformation data type, but with the OpenAPI nullable property set to true.

anyOf:

- $ref: '#/components/schemas/PreemptionControlInformation'

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/NullValue'

#

AppDetectionNotifType:

description: Indicates the notification type for Application Detection Control.

anyOf:

- type: string

enum:

- APP\_START

- APP\_STOP

- type: string

#

PduSessionStatus:

description: Indicates whether the PDU session is established or terminated.

anyOf:

- type: string

enum:

- ESTABLISHED

- TERMINATED

- type: string

\* \* \* \* End of change \* \* \* \*