**3GPP TSG-CT WG3 Meeting #122-eC3-223459r1**

**E-Meeting, 12th – 20th May 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.122** | **CR** | **0590** | **rev** | **-** | **Current version:** | **17.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Defining the default logical relationship between query parameters |
|  |  |
| ***Source to WG:*** | Huawei, Ericsson |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | NBI17 |  | ***Date:*** | 2022-05-05 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The default relationship between query parameters needs to be defined for northbound and application layer APIs, with some specific description on multiple query parameters e.g. on how to handle the logical relationship for the multiple individual UE identifiers. |
|  |  |
| ***Summary of change:*** | This CR proposes to:* Define default relationship between query parameters for northbound and application layer APIs to align with 5GC APIs, refer to TS 29.501 clause 4.6.1.1.5.1.
* Adding descriptions on multiple query parameters default logical relationship.
 |
|  |  |
| ***Consequences if not approved:*** | * Undefined default relationship between query parameters for northbound and application layer APIs.
 |
|  |  |
| ***Clauses affected:*** | 5.2.x (new subclause) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact the OpenAPI descriptions defined in this specification. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* \* Start of Changes \* \* \* \*

### 5.2.x Query parameters

The query parameters general handling described in subclause 4.6.1.1.5.1 of 3GPP TS 29.501 [49] shall be applicable for the APIs defined in the present specification.

When multiple query parameters are defined for a method on the resource, the logical 'AND' is the default logical relationship between the query parameters for this resource, except for the multiple query individual UE identifiers (e.g. GPSI, UE IP address or UE MAC address) with the logical 'OR' as the default logical relationship between the individual UE query parameters. If a logical relationship between multiple query parameters is specified in an API, then this overrides the default relationship. If multiple query parameters are defined for a method on the resource in an API, but there is no need to specify any logical relationship between these query parameters, the concerned API shall explicitly state it.

\* \* \* \* End of Changes \* \* \* \*