**3GPP TSG-CT WG3 Meeting #122-eC3-223abc**

**E-Meeting, 12th – 20th May 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.522** | **CR** | **-** | **rev** | **-** | **Current version:** | **17.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Updates to multiple query parameters in ServiceParameter API |
|  |  |
| ***Source to WG:*** | Ericsson, Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | NBI17 |  | ***Date:*** | 2022-05-17 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The specific handling on multiple query parameters and/or parameter of type array for the applicable API need to be specified in this specification. |
|  |  |
| ***Summary of change:*** | This CR proposes to:* Adding specific handling descriptions for the special multiple query parameters and/or type array parameter in the applicable clauses.
 |
|  |  |
| ***Consequences if not approved:*** | * Undefined specific handling for multiple query parameters and/or type array parameter in the applicable clause.
 |
|  |  |
| ***Clauses affected:*** | 5.11.1.2.3.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact the OpenAPI file.**To MCC/Rapporteur**: Need to implement CR 0583 which update the query parameters’ name before this CR. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* \* 1st Change \* \* \* \*

5.11.1.2.3.2 GET

The GET method allows to read all active subscriptions for a given AF. The AF shall initiate the HTTP GET request message and the NEF shall respond to the message.

This method shall support the URI query parameters specified in table 5.11.1.2.3.2-1.

**Table 5.11.1.2.3.2-1: URI query parameters supported by the GET****method on this resource**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Data type** | **P** | **Cardinality** | **Description** | **Applicability** |
| gpsi | array(Gpsi) | O | 0..N | The GPSI of the requested UE(s). | EnNB |
| Ip-addrs | array(IpAddr) | O | 0..N | The IP address(es) of the requested UE(s). | EnNB |
| Ip-domain | string | O | 0..1 | The IPv4 address domain identifier.The attribute may only be provided if IPv4 address is included in the ip-addrs query parameter. | EnNB |
| mac-addrs | array(MacAddr48) | O | 0..N | The MAC address(es) of the requested UE(s). | EnNB |
| NOTE: One of the "gpsis" parameter, the "ip-addrs" parameter or the "mac-addrs" parameter may be provided in the same request. If multiple elements are provided in the array data structure, then each element shall be taken as a separate query parameter. |

This method shall support the request data structures specified in table 5.11.1.2.3.2-2 and the response data structures and response codes specified in table 5.11.1.2.3.2-3.

**Table 5.11.1.2.3.2-2: Data structures supported by the GET****Request Body on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **P** | **Cardinality** | **Description** |
| N/A |  |  |  |

**Table 5.11.1.2.3.2-3: Data structures supported by the****GET Response Body on this resource**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Data type** | **P** | **Cardinality** | **Response codes** | **Description** |
| array(ServiceParameterData) | M | 0..N | 200 OK | All the subscription information for the AF in the request URI are returned. |
| N/A |  |  | 307 Temporary Redirect | Temporary redirection, during subscription retrieval. The response shall include a Location header field containing an alternative URI of the resource located in an alternative NEF.Redirection handling is described in subclause 5.2.10 of 3GPP TS 29.122 [4]. |
| N/A |  |  | 308 Permanent Redirect | Permanent redirection, during subscription retrieval. The response shall include a Location header field containing an alternative URI of the resource located in an alternative NEF.Redirection handling is described in subclause 5.2.10 of 3GPP TS 29.122 [4]. |
| NOTE: The mandatory HTTP error status codes for the GET method listed in table 5.2.6-1 of 3GPP TS 29.122 [4] also apply. |

**Table 5.11.1.2.3.2-4: Headers supported by the 307 Response Code on this resource**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Name** | **Data type** | **P** | **Cardinality** | **Description** |
| Location | string | M | 1 | An alternative URI of the resource located in an alternative NEF. |

**Table 5.11.1.2.3.2-5: Headers supported by the 308 Response Code on this resource**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Name** | **Data type** | **P** | **Cardinality** | **Description** |
| Location | string | M | 1 | An alternative URI of the resource located in an alternative NEF. |

\* \* \* \* End of Changes \* \* \* \*