**3GPP TSG-CT3 Meeting #122e C3-223720**

**E-Meeting, 12th – 20th May 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.523** | **CR** | **0073** | **rev** | **-** | **Current version:** | **17.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Update of info and externalDocs fields |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | TEI17 |  | ***Date:*** | 2022-05-20 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | CR modifying Npcf\_EventExposure API has been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in TS 29.501, clause 4.3.1.The following agreed CR update the Npcf\_EventExposure API for the present release:- TS 29.571 CR #0354 is a backward compatible correction in Rel-17.As the present release will be frozen for OpenAPI, and a draft version number was already assigned, only the additional Pre-Release version field field needs to be removed.Since a new TS version will be provided with changes to the OpenAPI specification file, the TS version number included in the "description" field of the "externalDocs" object also needs to be updated. |
|  |  |
| ***Summary of change:*** | The Npcf\_EventExposure API version number set to value "1.2.0".The TS version number in the "description" field of the "externalDocs" object is changed to "17.7.0". |
|  |  |
| ***Consequences if not approved:*** | Incorrect API version number and incorrect TS version number in the "description" field of the "externalDocs" object. |
|  |  |
| ***Clauses affected:*** | A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* First Change \*\*\*

# A.2 Npcf\_EventExposure API

openapi: 3.0.0

info:

 version: 1.2.0

 title: Npcf\_EventExposure

 description: |

 PCF Event Exposure Service.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.523 V17.7.0; 5G System; Policy Control Event Exposure Service; Stage 3.

 url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.523/

servers:

 - url: '{apiRoot}/npcf-eventexposure/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501

security:

 - {}

 - oAuth2ClientCredentials:

 - npcf-eventexposure

paths:

 /subscriptions:

 post:

 summary: Creates a new Individual Policy Control Events Subscription resource

 operationId: PostPcEventExposureSubsc

 tags:

 - Policy Control Events Subscription (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PcEventExposureSubsc'

 responses:

 '201':

 description: Success

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PcEventExposureSubsc'

 headers:

 Location:

 description: >

 Contains the URI of the created individual policy control events subscription

 resource, according to the structure

 {apiRoot}/npcf-eventexposure/v1/subscriptions/{subscriptionId}

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 PcEventNotification:

 '{$request.body#/notifUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PcEventExposureNotif'

 responses:

 '204':

 description: No Content, Notification was succesfull.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /subscriptions/{subscriptionId}:

 get:

 summary: "Reads an existing Individual Policy Control Events Subscription"

 operationId: GetPcEventExposureSubsc

 tags:

 - Individual Policy Control Events Subscription (Document)

 parameters:

 - name: subscriptionId

 in: path

 description: Policy Control Event Subscription ID.

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource representation is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PcEventExposureSubsc'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 summary: "Modifies an existing Individual Policy Control Events Subscription "

 operationId: PutPcEventExposureSubsc

 tags:

 - Individual Policy Control Events Subscription (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PcEventExposureSubsc'

 parameters:

 - name: subscriptionId

 in: path

 description: Policy Control Event Subscription ID.

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource was succesfully modified and representation is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PcEventExposureSubsc'

 '204':

 description: No Content. Resource was succesfully modified.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 summary: "Cancels an existing Individual Policy Control Events Subscription "

 operationId: DeletePcEventExposureSubsc

 tags:

 - Individual Policy Control Events Subscription (Document)

 parameters:

 - name: subscriptionId

 in: path

 description: Policy Control Event Subscription ID.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. Resource was succesfully deleted.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 npcf-eventexposure: Access to the Npcf\_EventExposure API.

 schemas:

 PcEventExposureNotif:

 description: >

 Represents notifications about Policy Control events related to an Individual

 Policy Events Subscription resource.

 type: object

 properties:

 notifId:

 type: string

 eventNotifs:

 type: array

 items:

 $ref: '#/components/schemas/PcEventNotification'

 minItems: 1

 required:

 - notifId

 - eventNotifs

 PcEventExposureSubsc:

 description: Represents an Individual Policy Events Subscription resource.

 type: object

 properties:

 eventSubs:

 type: array

 items:

 $ref: '#/components/schemas/PcEvent'

 minItems: 1

 eventsRepInfo:

 $ref: '#/components/schemas/ReportingInformation'

 groupId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 filterDnns:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 minItems: 1

 filterSnssais:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 snssaiDnns:

 type: array

 items:

 $ref: '#/components/schemas/SnssaiDnnCombination'

 minItems: 1

 filterServices:

 type: array

 items:

 $ref: '#/components/schemas/ServiceIdentification'

 minItems: 1

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 notifId:

 type: string

 eventNotifs:

 type: array

 items:

 $ref: '#/components/schemas/PcEventNotification'

 minItems: 1

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - eventSubs

 - notifId

 - notifUri

 ReportingInformation:

 description: Represents the type of reporting that the subscription requires.

 type: object

 properties:

 immRep:

 type: boolean

 notifMethod:

 $ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/NotificationMethod'

 maxReportNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 monDur:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 repPeriod:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 sampRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 partitionCriteria:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PartitioningCriteria'

 minItems: 1

 description: Criteria for partitioning the UEs before applying the sampling ratio.

 grpRepTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 notifFlag:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NotificationFlag'

 ServiceIdentification:

 description: Identifies the service to which the subscription applies.

 type: object

 properties:

 servEthFlows:

 type: array

 items:

 $ref: '#/components/schemas/EthernetFlowInfo'

 minItems: 1

 servIpFlows:

 type: array

 items:

 $ref: '#/components/schemas/IpFlowInfo'

 minItems: 1

 afAppId:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AfAppId'

 # All conditions in allOf must be met

 allOf:

 # First condition is that servEthFlows and servIpFlows are mutually exclusive

 - not:

 required: [servEthFlows, servIpFlows]

 # Second condition is that at least one the servEthFlows, servIpFlows and afAppId shall be present

 - anyOf:

 - required: [servEthFlows]

 - required: [servIpFlows]

 - required: [afAppId]

 EthernetFlowInfo:

 description: Identifies an UL/DL ethernet flow.

 type: object

 properties:

 ethFlows:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

 minItems: 1

 maxItems: 2

 flowNumber:

 type: integer

 required:

 - flowNumber

 IpFlowInfo:

 description: Identifies an UL/DL IP flow.

 type: object

 properties:

 ipFlows:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/FlowDescription'

 minItems: 1

 maxItems: 2

 flowNumber:

 type: integer

 required:

 - flowNumber

 PcEventNotification:

 description: Represents the information reported for a Policy Control event.

 type: object

 properties:

 event:

 $ref: '#/components/schemas/PcEvent'

 accType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 addAccessInfo:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AdditionalAccessInfo'

 relAccessInfo:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AdditionalAccessInfo'

 anGwAddr:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AnGwAddress'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 plmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

 satBackhaulCategory:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SatelliteBackhaulCategory'

 appliedCov:

 $ref: 'TS29534\_Npcf\_AMPolicyAuthorization.yaml#/components/schemas/ServiceAreaCoverageInfo'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 timeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 pduSessionInfo:

 $ref: '#/components/schemas/PduSessionInformation'

 repServices:

 $ref: '#/components/schemas/ServiceIdentification'

 delivFailure:

 $ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/Failure'

 required:

 - event

 - timeStamp

 PduSessionInformation:

 description: Represents PDU session identification information.

 type: object

 properties:

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 ueIpv4:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ueIpv6:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 ipDomain:

 type: string

 ueMac:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 required:

 - snssai

 - dnn

 oneOf:

 - required: [ueMac]

 - anyOf:

 - required: [ueIpv4]

 - required: [ueIpv6]

 SnssaiDnnCombination:

 description: Represents a combination of S-NSSAI and DNN(s).

 type: object

 properties:

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 dnns:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 minItems: 1

# Simple data types and Enumerations

 PcEvent:

 description: Represents the policy control events that can be subscribed.

 anyOf:

 - type: string

 enum:

 - AC\_TY\_CH

 - PLMN\_CH

 - SAC\_CH

 - SAT\_CATEGORY\_CH

 - SUCCESS\_UE\_POL\_DEL\_SP

 - UNSUCCESS\_UE\_POL\_DEL\_SP

 - type: string

\*\*\* End of Changes \*\*\*