**3GPP TSG-CT3 Meeting #122e C3-223727**

**E-Meeting, 12th – 20th May 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.554** | **CR** | **0077** | **rev** | **-** | **Current version:** | **17.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Update of info and externalDocs fields | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI17 | | | | |  | ***Date:*** | | | 2022-05-20 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | CRs modifying Npcf\_BDTPolicyControl API have been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in TS 29.501, clause 4.3.1.  The following agreed CRs update the Npcf\_BDTPolicyControl API for the present release:  - TS 29.554 CR #0076 is a backward compatible correction in Rel-17.  - TS 29.571 CR #0354 is a backward compatible correction in Rel-17.  As the present release will be frozen for OpenAPI, and a draft version number was already assigned, only the additional Pre-Release version field field needs to be removed.  Since a new TS version will be provided with changes to the OpenAPI specification file, the TS version number included in the "description" field of the "externalDocs" object also needs to be updated. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The Npcf\_BDTPolicyControl API version number set to value "1.2.0".  The TS version number in the "description" field of the "externalDocs" object is changed to "17.4.0". | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incorrect API version number and incorrect TS version number in the "description" field of the "externalDocs" object. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\*\*\* First Change \*\*\*

# A.2 Npcf\_BDTPolicyControl API

openapi: 3.0.0

info:

title: Npcf\_BDTPolicyControl Service API

version: 1.2.0

description: |

PCF BDT Policy Control Service.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

#

externalDocs:

description: >

3GPP TS 29.554 V17.4.0; 5G System; Background Data Transfer Policy Control Service.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.554/'

#

servers:

- url: '{apiRoot}/npcf-bdtpolicycontrol/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

security:

- {}

- oAuth2ClientCredentials:

- npcf-bdtpolicycontrol

paths:

/bdtpolicies:

post:

summary: Create a new Individual BDT policy

operationId: CreateBDTPolicy

tags:

- BDT policies (Collection)

requestBody:

description: >

Contains information for the creation of a new Individual BDT policy resource.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/BdtReqData'

responses:

'201':

description: Background data transfer policies offered to an ASP.

content:

application/json:

schema:

$ref: '#/components/schemas/BdtPolicy'

headers:

Location:

description: >

Contains the URI of the created individual BDT policy resource,

according to the structure

{apiRoot}/npcf-bdtpolicycontrol/v1/bdtpolicies/{bdtPolicyId}

required: true

schema:

type: string

#

# Error scenarios POST

#

'303':

description: >

See Other. The result of the POST request would be equivalent to the

existing Individual BDT policy resource.

headers:

Location:

description: Contains the URI of the existing individual BDT policy resource.

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

# End error scenarios POST

#

callbacks:

BdtNotification:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/Notification'

responses:

'204':

description: No Content, a reception of the BDT notification was successful.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

/bdtpolicies/{bdtPolicyId}:

get:

summary: Read an Individual BDT policy

operationId: GetBDTPolicy

tags:

- Individual BDT policy (Document)

parameters:

- name: bdtPolicyId

description: String identifying the individual BDT policy resource in the PCF.

in: path

required: true

schema:

type: string

responses:

'200':

description: Background data transfer policies offered to and selected by an ASP.

content:

application/json:

schema:

$ref: '#/components/schemas/BdtPolicy'

#

# Redirection scenarios GET

#

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

#

# Error scenarios GET

#

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

# End error scenarios GET

#

patch:

summary: Update an Individual BDT policy

operationId: UpdateBDTPolicy

tags:

- Individual BDT policy (Document)

parameters:

- name: bdtPolicyId

description: String identifying the individual BDT policy resource in the PCF.

in: path

required: true

schema:

type: string

requestBody:

description: >

Contains modification instruction to be performed on the BdtPolicy data

structure to select a transfer policy and in addition, may indicate whether

the BDT warning notification is enabled or disabled.

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/PatchBdtPolicy'

responses:

'200':

description: >

The Individual BDT Policy resource is modified and a representation of that

resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/BdtPolicy'

'204':

description: The Individual BDT Policy resource is modified.

#

# Redirection scenarios PATCH

#

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

#

# Error scenarios PATCH

#

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

# End error scenarios PATCH

#

#

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

npcf-bdtpolicycontrol: Access to the Npcf\_BDTPolicyControl API

schemas:

#

# Structured data types

#

BdtPolicy:

description: Represents an Individual BDT policy resource.

type: object

properties:

bdtPolData:

$ref: '#/components/schemas/BdtPolicyData'

bdtReqData:

$ref: '#/components/schemas/BdtReqData'

#

BdtReqData:

description: >

Contains service requirements for creation a new Individual BDT policy resource.

type: object

required:

- aspId

- desTimeInt

- numOfUes

- volPerUe

properties:

aspId:

$ref: '#/components/schemas/AspId'

desTimeInt:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

interGroupId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

nwAreaInfo:

$ref: '#/components/schemas/NetworkAreaInfo'

numOfUes:

description: Indicates a number of UEs.

type: integer

volPerUe:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

trafficDes:

$ref: 'TS29122\_ResourceManagementOfBdt.yaml#/components/schemas/TrafficDescriptor'

warnNotifReq:

description: Indicates whether the BDT warning notification is enabled or disabled.

type: boolean

default: false

#

BdtPolicyData:

description: Describes the authorization data of an Individual BDT policy resource.

type: object

required:

- bdtRefId

- transfPolicies

properties:

bdtRefId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

transfPolicies:

description: Contains transfer policies.

type: array

items:

$ref: '#/components/schemas/TransferPolicy'

minItems: 1

selTransPolicyId:

description: Contains an identity of the selected transfer policy.

type: integer

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

#

PatchBdtPolicy:

description: >

Describes the updates in authorization data of an Individual BDT Policy created

by the PCF.

type: object

properties:

bdtPolData:

$ref: '#/components/schemas/BdtPolicyDataPatch'

bdtReqData:

$ref: '#/components/schemas/BdtReqDataPatch'

#

BdtPolicyDataPatch:

description: >

A JSON Merge Patch body schema containing modification instruction to be performed

on the bdtPolData attribute of the BdtPolicy data structure to select a transfer

policy. Adds selTransPolicyId to BdtPolicyData data structure.

type: object

required:

- selTransPolicyId

properties:

selTransPolicyId:

description: >

Contains an identity (i.e. transPolicyId value) of the selected transfer

policy. If the BdtNotification\_5G feature is supported value 0 indicates that

no transfer policy is selected.

type: integer

#

BdtReqDataPatch:

description: >

A JSON Merge Patch body schema containing modification instruction to be performed

on the bdtReqData attribute of the BdtPolicy data structure to indicate whether

the BDT warning notification is enabled or disabled. Modifies warnNotifReq from

BdtReqData data structure.

type: object

properties:

warnNotifReq:

description: Indicates whether the BDT warning notification is enabled or disabled.

type: boolean

#

TransferPolicy:

description: Describes a transfer policy.

type: object

required:

- ratingGroup

- recTimeInt

- transPolicyId

properties:

maxBitRateDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

maxBitRateUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

ratingGroup:

description: Indicates a rating group for the recommended time window.

type: integer

recTimeInt:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

transPolicyId:

description: Contains an identity of a transfer policy.

type: integer

NetworkAreaInfo:

description: >

Describes a network area information in which the NF service consumer requests

the number of UEs.

type: object

properties:

ecgis:

description: Contains a list of E-UTRA cell identities.

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ecgi'

minItems: 1

ncgis:

description: Contains a list of NR cell identities.

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ncgi'

minItems: 1

gRanNodeIds:

description: Contains a list of NG RAN nodes.

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GlobalRanNodeId'

minItems: 1

tais:

description: Contains a list of tracking area identities.

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

minItems: 1

#

Notification:

description: Describes a BDT notification.

type: object

required:

- bdtRefId

properties:

bdtRefId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

candPolicies:

description: >

Contains a list of the candidate transfer policies from which the AF may

select a new transfer policy due to a network performance is below the criteria

set by the operator.

type: array

items:

$ref: '#/components/schemas/TransferPolicy'

minItems: 1

nwAreaInfo:

$ref: '#/components/schemas/NetworkAreaInfo'

timeWindow:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

#

# Simple data types

#

AspId:

description: Contains an identity of an application service provider.

type: string

#

#

\*\*\* End of Changes \*\*\*