**3GPP TSG-CT WG3 Meeting #123e *C3-224106***

**E-meeting, 18th - 26th, August, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.525** | **CR** | **0217** | **rev** | **-** | **Current version:** | **17.7.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Alignment with the SBI template |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | CT3  |
|  |  |
| ***Work item code:*** | SBIProtoc17 |  | ***Date:*** | 2022-07-22 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | According to [C4-222295](https://www.3gpp.org/ftp/tsg_ct/WG4_protocollars_ex-CN4/TSGCT4_109e_meeting/Docs/C4-222295.zip), CT4 updated SBI template to remove the "apiVersion" placeholder from the "Resource URI variables" table since the "apiVersion" placeholder is not a resource URI variable and added introduction part in the clause showing the resource overview.In this specification the "Resource URI variables" tables are aligned with the SBI template, but the introduction part in the clause showing the resource overview needs to be added. |
|  |  |
| ***Summary of change:*** | Clause 5.3.1:As per the updated SBI template, added that the clause describes the structure for the Resource URIs, the resources and methods used for the service; and that figure 5.3.1-1 depicts the resource URIs structure for the Npcf\_UEPolicyControl API. |
|  |  |
| ***Consequences if not approved:*** | This specification will not be inline with the updated SBI template |
|  |  |
| ***Clauses affected:*** | 5.3.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact the OpenAPI file  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* First Change \*\*\*

### 5.3.1 Resource Structure

This clause describes the structure for the Resource URIs and the resources and methods used for the service.

Figure 5.3.1-1 depicts the resource URIs structure for the Npcf\_UEPolicyControl API.



Figure 5.3.1-1: Resource URI structure of the Npcf\_UEPolicyControl API

Table 5.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 5.3.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method or custom operation | Description |
| UE Policy Associations | /policies | POST | Create a new Individual UE policy association resource. |
| Individual UE Policy Association | /policies/{polAssoId} | GET | Read an Individual UE Policy Association resource. |
| DELETE | Delete an Individual UE Policy Association resource. |
| /policies/{polAssoId}/update | update (POST) | Report observed event trigger and obtain updated UE policies. |

\*\*\* End of Changes \*\*\*