**3GPP TSG-CT WG3 Meeting #****125 C3-225746**

**Toulouse, France, 14th - 18th, November, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.525** | **CR** | **0233** | **rev** | **-** | **Current version:** | **17.8.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Update of info and externalDocs fields |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | TEI18 |  | ***Date:*** | 2022-11-23 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | CR modifying Npcf\_UEPolicyControl API has been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in TS 29.501, subclause 4.3.1.The following agreed CR updates the Npcf\_UEPolicyControl API for the present release:+ TS 29.525 CR #0225 is a backward compatible correction in Rel-18. + TS 29.525 CR #0227 is a backward compatible correction in Rel-18. + TS 29.571 CR #0383 is a backward compatible correction in Rel-18.As the present release is not yet frozen, a draft version number should be assigned. As the first backward compatible changes without prior backward incompatible changes to the existing API were agreed in for present non-frozen release, the minor version number needs to be incremented.Since a new Rel-18 TS version will be provided with changes to the OpenAPI specification file, the TS version number included in the "description" field of the "externalDocs" object also needs to be updated. |
|  |  |
| ***Summary of change:*** | The Npcf\_UEPolicyControl API version value changed to:"1.3.0-alpha.1".The TS version number included in the "description" field of the "externalDocs" object changed to "18.0.0". |
|  |  |
| ***Consequences if not approved:*** | Incorrect API version number and incorrect TS version number in the "description" field of the "externalDocs" object. |
|  |  |
| ***Clauses affected:*** | A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* First Change \*\*\*

# A.2 Npcf\_UEPolicyControl API

openapi: 3.0.0

info:

 version: 1.3.0-alpha.1

 title: Npcf\_UEPolicyControl

 description: |

 UE Policy Control Service.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.525 V18.0.0; 5G System; UE Policy Control Service.

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.525/'

servers:

 - url: '{apiRoot}/npcf-ue-policy-control/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

security:

 - {}

 - oAuth2ClientCredentials:

 - npcf-ue-policy-control

paths:

 /policies:

 post:

 operationId: CreateIndividualUEPolicyAssociation

 summary: Create individual UE policy association.

 tags:

 - UE Policy Associations (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PolicyAssociationRequest'

 responses:

 '201':

 description: Created

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PolicyAssociation'

 headers:

 Location:

 description: >

 Contains the URI of the newly created resource, according to the structure

 {apiRoot}/npcf-ue-policy-control/v1/policies/{polAssoId}'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 policyUpdateNotification:

 '{$request.body#/notificationUri}/update':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PolicyUpdate'

 responses:

 '200':

 description: >

 OK. The current applicable values corresponding to the policy control request

 trigger is reported

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/UeRequestedValueRep'

 '204':

 description: No Content, Notification was successful

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 policyAssocitionTerminationRequestNotification:

 '{$request.body#/notificationUri}/terminate':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TerminationNotification'

 responses:

 '204':

 description: No Content, Notification was successful

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /policies/{polAssoId}:

 get:

 operationId: ReadIndividualUEPolicyAssociation

 summary: Read individual UE policy association.

 tags:

 - Individual UE Policy Association (Document)

 parameters:

 - name: polAssoId

 in: path

 description: Identifier of a policy association

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource representation is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PolicyAssociation'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 operationId: DeleteIndividualUEPolicyAssociation

 summary: Delete individual UE policy association.

 tags:

 - Individual UE Policy Association (Document)

 parameters:

 - name: polAssoId

 in: path

 description: Identifier of a policy association

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. Resource was successfully deleted

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /policies/{polAssoId}/update:

 post:

 operationId: ReportObservedEventTriggersForIndividualUEPolicyAssociation

 summary: >

 Report observed event triggers and possibly obtain updated policies for an individual UE

 policy association.

 tags:

 - Individual UE Policy Association (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PolicyAssociationUpdateRequest'

 parameters:

 - name: polAssoId

 in: path

 description: Identifier of a policy association

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Updated policies are returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PolicyUpdate'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 npcf-ue-policy-control: Access to the Npcf\_UEPolicyControl API

 schemas:

 PolicyAssociation:

 description: >

 Contains the description of a policy association that is returned by the PCF when a policy

 Association is created, updated, or read.

 type: object

 properties:

 request:

 $ref: '#/components/schemas/PolicyAssociationRequest'

 uePolicy:

 $ref: '#/components/schemas/UePolicy'

 n2Pc5Pol:

 $ref: 'TS29518\_Namf\_Communication.yaml#/components/schemas/N2InfoContent'

 n2Pc5ProSePol:

 $ref: 'TS29518\_Namf\_Communication.yaml#/components/schemas/N2InfoContent'

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/RequestTrigger'

 minItems: 1

 description: >

 Request Triggers that the PCF subscribes. Only values "LOC\_CH" and "PRA\_CH" are permitted.

 pras:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 1

 description: >

 Contains the presence reporting area(s) for which reporting was requested.

 The praId attribute within the PresenceInfo data type is the key of the map.

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - suppFeat

 PolicyAssociationRequest:

 description: >

 Represents information that the NF service consumer provides when requesting the creation of

 a policy association.

 type: object

 properties:

 notificationUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 altNotifIpv4Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 minItems: 1

 description: Alternate or backup IPv4 Address(es) where to send Notifications.

 altNotifIpv6Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 minItems: 1

 description: Alternate or backup IPv6 Address(es) where to send Notifications.

 altNotifFqdns:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Fqdn'

 minItems: 1

 description: Alternate or backup FQDN(s) where to send Notifications.

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 accessType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 pei:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 userLoc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 timeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 servingPlmn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 groupIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 hPcfId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 uePolReq:

 $ref: '#/components/schemas/UePolicyRequest'

 guami:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

 serviceName:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/ServiceName'

 servingNfId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 pc5Capab:

 $ref: '#/components/schemas/Pc5Capability'

 proSeCapab:

 type: array

 items:

 $ref: '#/components/schemas/ProSeCapability'

 minItems: 1

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - notificationUri

 - suppFeat

 - supi

 PolicyAssociationUpdateRequest:

 description: >

 Represents Information that the NF service consumer provides when requesting the update of

 a policy association.

 type: object

 properties:

 notificationUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 altNotifIpv4Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 minItems: 1

 description: Alternate or backup IPv4 Address(es) where to send Notifications.

 altNotifIpv6Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 minItems: 1

 description: Alternate or backup IPv6 Address(es) where to send Notifications.

 altNotifFqdns:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Fqdn'

 minItems: 1

 description: Alternate or backup FQDN(s) where to send Notifications.

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/RequestTrigger'

 minItems: 1

 description: Request Triggers that the NF service consumer observes.

 praStatuses:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 description: >

 Contains the UE presence status for tracking area for which changes of the UE presence

 occurred. The praId attribute within the PresenceInfo data type is the key of the map.

 minProperties: 1

 userLoc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uePolDelResult:

 $ref: '#/components/schemas/UePolicyDeliveryResult'

 uePolTransFailNotif:

 $ref: '#/components/schemas/UePolicyTransferFailureNotification'

 uePolReq:

 $ref: '#/components/schemas/UePolicyRequest'

 guami:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

 servingNfId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 plmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 connectState:

 $ref: 'TS29518\_Namf\_EventExposure.yaml#/components/schemas/CmState'

 groupIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 proSeCapab:

 type: array

 items:

 $ref: '#/components/schemas/ProSeCapability'

 minItems: 1

 PolicyUpdate:

 description: >

 Represents updated policies that the PCF provides in a notification or in the reply to an

 Update Request.

 type: object

 properties:

 resourceUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 uePolicy:

 $ref: '#/components/schemas/UePolicy'

 n2Pc5Pol:

 $ref: 'TS29518\_Namf\_Communication.yaml#/components/schemas/N2InfoContent'

 n2Pc5ProSePol:

 $ref: 'TS29518\_Namf\_Communication.yaml#/components/schemas/N2InfoContent'

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/RequestTrigger'

 minItems: 1

 nullable: true

 description: >

 Request Triggers that the PCF subscribes. Only values "LOC\_CH" and "PRA\_CH" are permitted.

 pras:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 description: >

 Contains the presence reporting area(s) for which reporting was requested.

 The praId attribute within the PresenceInfo data type is the key of the map.

 minProperties: 1

 nullable: true

 required:

 - resourceUri

 TerminationNotification:

 description: >

 Represents a request to terminate a policy association that the PCF provides in a

 notification.

 type: object

 properties:

 resourceUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 cause:

 $ref: '#/components/schemas/PolicyAssociationReleaseCause'

 required:

 - resourceUri

 - cause

 UePolicyTransferFailureNotification:

 description: >

 Represents information on the failure of a UE policy transfer to the UE because the UE is not

 reachable.

 type: object

 properties:

 cause:

 $ref: 'TS29518\_Namf\_Communication.yaml#/components/schemas/N1N2MessageTransferCause'

 ptis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 minItems: 1

 required:

 - cause

 - ptis

 UeRequestedValueRep:

 description: >

 Contains the current applicable values corresponding to the policy control request triggers.

 type: object

 properties:

 userLoc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 praStatuses:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 1

 description: >

 Contains the UE presence statuses for tracking areas. The praId attribute within the

 PresenceInfo data type is the key of the map.

 plmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 connectState:

 $ref: 'TS29518\_Namf\_EventExposure.yaml#/components/schemas/CmState'

 UePolicy:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

 UePolicyDeliveryResult:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

 UePolicyRequest:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

 RequestTrigger:

 anyOf:

 - type: string

 enum:

 - LOC\_CH

 - PRA\_CH

 - UE\_POLICY

 - PLMN\_CH

 - CON\_STATE\_CH

 - GROUP\_ID\_LIST\_CHG

 - UE\_CAP\_CH

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are:

 - LOC\_CH: Location change (tracking area). The tracking area of the UE has changed.

 - PRA\_CH: Change of UE presence in PRA. The AMF reports the current presence status of the UE

 in a Presence Reporting Area, and notifies that the UE enters/leaves the Presence Reporting

 Area.

 - UE\_POLICY: A MANAGE UE POLICY COMPLETE message or a MANAGE UE POLICY COMMAND REJECT

 message, as defined in Annex D.5 of 3GPP TS 24.501 or a "UE POLICY PROVISIONING REQUEST"

 message, as defined in clause 7.2.1.1 of 3GPP TS 24.587 , has been received by the AMF

 and is being forwarded.

 - PLMN\_CH: PLMN change. the serving PLMN of UE has changed.

 - CON\_STATE\_CH: Connectivity state change: the connectivity state of UE has changed.

 - GROUP\_ID\_LIST\_CHG: UE Internal Group Identifier(s) has changed. This policy control request

 trigger does not require a subscription

 - UE\_CAP\_CH: UE Capabilities change: the UE provided 5G ProSe capabilities have changed.

 This policy control request trigger does not require subscription.

 PolicyAssociationReleaseCause:

 anyOf:

 - type: string

 enum:

 - UNSPECIFIED

 - UE\_SUBSCRIPTION

 - INSUFFICIENT\_RES

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are:

 - UNSPECIFIED: This value is used for unspecified reasons.

 - UE\_SUBSCRIPTION: This value is used to indicate that the policy association needs to be

 terminated because the subscription of UE has changed (e.g. was removed).

 - INSUFFICIENT\_RES: This value is used to indicate that the server is overloaded and needs

 to abort the policy association.

 Pc5Capability:

 anyOf:

 - type: string

 enum:

 - LTE\_PC5

 - NR\_PC5

 - LTE\_NR\_PC5

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Possible values are:

 - LTE\_PC5: This value is used to indicate that UE supports PC5 LTE RAT for V2X communications

 over the PC5 reference point.

 - NR\_PC5: This value is used to indicate that UE supports PC5 NR RAT for V2X communications

 over the PC5 reference point.

 - LTE\_NR\_PC5: This value is used to indicate that UE supports both PC5 LTE and NR RAT for

 V2X communications over the PC5 reference point.

 ProSeCapability:

 anyOf:

 - type: string

 enum:

 - PROSE\_DD

 - PROSE\_DC

 - PROSE\_L2\_U2N\_RELAY

 - PROSE\_L3\_U2N\_RELAY

 - PROSE\_L2\_REMOTE\_UE

 - PROSE\_L3\_REMOTE\_UE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 the content defined in the present version of this API.

 description: |

 Possible values are:

 - PROSE\_DD: This value is used to indicate that 5G ProSe Direct Discovery is supported

 by the UE.

 - PROSE\_DC: This value is used to indicate that 5G ProSe Direct Communication is supported

 by the UE.

 - PROSE\_L2\_U2N\_RELAY: This value is used to indicate that Layer-2 5G ProSe UE-to-Network

 Relay is supported by the UE.

 - PROSE\_L3\_U2N\_RELAY: This value is used to indicate that Layer-3 5G ProSe UE-to-Network

 Relay is supported by the UE.

 - PROSE\_L2\_REMOTE\_UE: This value is used to indicate that Layer-2 5G ProSe Remote UE is

 supported by the UE.

 - PROSE\_L3\_REMOTE\_UE: This value is used to indicate that Layer-3 5G ProSe Remote UE is

 supported by the UE.

\*\*\* End of Changes \*\*\*