**3GPP TSG-CT WG3 Meeting #****125 C3-225761**

**Toulouse, France, 14th - 18th, November, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.565** | **CR** | **0035** | **rev** | **-** | **Current version:** | **17.1.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Update of info and externalDocs fields |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | TEI18 |  | ***Date:*** | 2022-11-18 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | CRs modifying the Ntsctsf\_TimeSynchronization, Ntsctsf\_QoSandTSCAssistance and Ntsctsf\_ASTI APIs have been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in TS 29.501, subclause 4.3.1.The following agreed CRs update theOpenAPI file for **Ntsctsf\_TimeSynchronization** **API** for the present release:+ TS 29.565 CR#0031 introduces a backward compatible correctionThe following agreed CRs update theOpenAPI file for **Ntsctsf\_QoSandTSCAssistance** **API** for the present release:+ TS 29.565 CR#0031 introduces a backward compatible correction+ TS 29.565 CR#0032 introduces a backward compatible correctionThe following agreed CRs update theOpenAPI file for **Ntsctsf\_ASTI** **API** for the present release:+ TS 29.565 CR#0031 introduces a backward compatible correctionAs the present release is not yet frozen, a draft version number should be assigned. As the first backward compatible changes without prior backward incompatible changes to the existing API were agreed in for present non-frozen release, the minor version number needs to be incremented.Since a new Rel-18 TS version will be provided with changes to the OpenAPI specification file, the TS version number included in the "description" field of the "externalDocs" object also needs to be updated. |
|  |  |
| ***Summary of change:*** | Update the API version number and TS version in externalDocs field for above the API. |
|  |  |
| ***Consequences if not approved:*** | Incorrect API version number and TS version in externalDocs field. |
|  |  |
| ***Clauses affected:*** | A.2, A.3, A.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* First Change \*\*\*

# A.2 Ntsctsf\_TimeSynchronization API

openapi: 3.0.0

info:

 title: Ntsctsf\_TimeSynchronization Service API

 version: 1.1.0-alpha.1

 description: |

 TSCTSF Time Synchronization Service.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 29.565 V18.0.0; 5G System; Time Sensitive Communication and Time Synchronization Function

 Services; Stage 3.

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.565/'

servers:

 - url: '{apiRoot}/ntsctsf-time-sync/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

security:

 - {}

 - oAuth2ClientCredentials:

 - ntsctsf-time-sync

paths:

 /subscriptions:

 post:

 summary: Creates a new subscription to notification of capability of time synchronization service resource

 operationId: TimeSynchronizationExposureSubscriptions

 tags:

 - Time Synchronization Exposure Subscriptions (Collection)

 requestBody:

 description: Contains the information for the creation the resource.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureSubsc'

 responses:

 '201':

 description: Successful creation of the resource.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureSubsc'

 headers:

 Location:

 description: >

 Contains the URI of the created individual time synchronization exposure

 subscription resource, according to the structure

 {apiRoot}/ntsctsf-time-sync/{apiVersion}/subscriptions/{subscriptionId}

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 subsEventNotification:

 '{$request.body#/subsNotifUri':

 post:

 requestBody:

 description: Notification of an event occurrence in the TSCTSF.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureSubsNotif'

 responses:

 '204':

 description: The receipt of the notification is acknowledged.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /subscriptions/{subscriptionId}:

 get:

 summary: "Reads an existing Individual Time Synchronization Exposure Subscription"

 operationId: GetIndividualTimeSynchronizationExposureSubscription

 tags:

 - Individual Time Synchronization Exposure Subscription (Document)

 parameters:

 - name: subscriptionId

 description: String identifying an Individual Time Synchronization Exposure Subscription

 in: path

 required: true

 schema:

 type: string

 responses:

 '200':

 description: A representation of the resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureSubsc'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 operationId: ReplaceIndividualTimeSynchronizationExposureSubscription

 summary: Replace an individual Time Synchronization Exposure Subscription

 tags:

 - IndividualTimeSynchronizationExposureSubscription (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/TimeSyncExposureSubsc'

 parameters:

 - name: subscriptionId

 description: String identifying an Individual Time Synchronization Exposure Subscription.

 in: path

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource was successfully modified and representation is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureSubsc'

 '204':

 description: No Content. Resource was successfully modified.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 operationId: DeleteIndividualTimeSynchronizationExposureSubscription

 summary: Delete an Individual TimeSynchronization Exposure Subscription

 tags:

 - Individual Time Synchronization Exposure Subscription (Document)

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying an Individual Time Synchronization Exposure Subscription.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. Resource was successfully deleted.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /subscriptions/{subscriptionId}/configurations:

 post:

 summary: "Craete a new Individual Time Synchronization Exposure Configuration"

 operationId: CreateIndividualTimeSynchronizationExposureConfiguration

 tags:

 - Individual Time Synchronization Exposure Configuration (Document)

 parameters:

 - name: subscriptionId

 description: String identifying an Individual Time Synchronization Exposure Subscription.

 in: path

 required: true

 schema:

 type: string

 requestBody:

 description: Contains the information for the creation the resource.

 required: true

 content:

 application/json:

 schema:

 $ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/TimeSyncExposureConfig'

 responses:

 '201':

 description: Successful creation of the resource.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureConfig'

 headers:

 Location:

 description: >

 Contains the URI of the created individual time synchronization exposure

 configuration resource, according to the structure

 {apiRoot}/ntsctsf-time-sync/{apiVersion}/subscriptions/{subscriptionId}

 /configurations/{configurationId}

 required: true

 schema:

 type: string

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 configEventNotification:

 '{$request.body#/configNotifUri':

 post:

 requestBody:

 description: Notification of an event occurrence in the TSCTSF.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureConfigNotif'

 responses:

 '204':

 description: The receipt of the notification is acknowledged.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /subscriptions/{subscriptionId}/configurations/{configurationId}:

 get:

 summary: "Reads an existing Individual Time Synchronization Exposure Configuration"

 operationId: GetIndividualTimeSynchronizationExposureConfiguration

 tags:

 - Individual Time Synchronization Exposure Configuration (Document)

 parameters:

 - name: subscriptionId

 description: String identifying an Individual Time Synchronization Exposure Subscription.

 in: path

 required: true

 schema:

 type: string

 - name: configurationId

 description: String identifying an Individual Time Synchronization Exposure Configuration.

 in: path

 required: true

 schema:

 type: string

 responses:

 '200':

 description: A representation of the resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureConfig'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 operationId: ReplaceIndividualTimeSynchronizationExposureConfiguration

 summary: Replace an individual Time Synchronization Exposure Configuration

 tags:

 - IndividualTimeSynchronizationExposureConfiguration (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/TimeSyncExposureConfig'

 parameters:

 - name: subscriptionId

 description: String identifying an Individual Time Synchronization Exposure Subscription.

 in: path

 required: true

 schema:

 type: string

 - name: configurationId

 description: String identifying an Individual Time Synchronization Exposure Configuration.

 in: path

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource was successfully modified and representation is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureConfig'

 '204':

 description: No Content. Resource was successfully modified.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 operationId: DeleteIndividualTimeSynchronizationExposureConfiguration

 summary: Delete an Individual TimeSynchronization Exposure Configuration

 tags:

 - Individual Time Synchronization Exposure Configuration (Document)

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying an Individual Time Synchronization Exposure Subscription.

 required: true

 schema:

 type: string

 - name: configurationId

 description: String identifying an Individual Time Synchronization Exposure Configuration.

 in: path

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. Resource was successfully deleted

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 ntsctsf-timesynchronization: Access to the Ntsctsf\_TimeSynchronization API

 schemas:

 TimeSyncExposureSubsc:

 description: >

 Contains the parameters for the subscription to notification of capability of time

 synchronization service.

 type: object

 properties:

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 gpsis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 minItems: 1

 interGrpId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 exterGrpId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ExternalGroupId'

 anyUeInd:

 type: boolean

 description: >

 Identifies whether the request applies to any UE. This attribute shall set to "true" if

 applicable for any UE, otherwise, set to "false".

 notifMethod:

 $ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/NotificationMethod'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 subscribedEvents:

 type: array

 items:

 $ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/SubscribedEvent'

 minItems: 1

 eventFilters:

 type: array

 items:

 $ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/EventFilter'

 minItems: 1

 subsNotifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 subsNotifId:

 type: string

 description: Notification Correlation ID assigned by the NF service consumer.

 maxReportNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 expiry:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 repPeriod:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - subsNotifUri

 - subsNotifId

 - dnn

 - snssai

 - subscribedEvents

 oneOf:

 - required: [supis]

 - required: [interGrpId]

 - required: [gpsis]

 - required: [exterGrpId]

 - required: [anyUeInd]

 TimeSyncExposureSubsNotif:

 description: Contains the notification of time synchronization service.

 type: object

 properties:

 subsNotifId:

 type: string

 description: Notification Correlation ID assigned by the NF service consumer.

 eventNotifs:

 type: array

 items:

 $ref: '#/components/schemas/SubsEventNotification'

 minItems: 1

 SubsEventNotification:

 description: >

 Contains the notification of capability of time synchronization for a list of UEs.

 type: object

 properties:

 event:

 $ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/SubscribedEvent'

 timeSyncCapas:

 type: array

 items:

 $ref: '#/components/schemas/TimeSyncCapability'

 minItems: 1

 required:

 - event

 TimeSyncCapability:

 description: Contains the capability of time synchronization service.

 type: object

 properties:

 upNodeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 gmCapables:

 type: array

 items:

 $ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/GmCapable'

 minItems: 1

 asTimeRes:

 $ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/AsTimeResource'

 ptpCapForUes:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/PtpCapabilitiesPerUe'

 minProperties: 1

 description: >

 Contains the PTP capabilities supported by each of the SUPI(s). The key of the map is the

 SUPI.

 ptpCapForGpsis:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/PtpCapabilitiesPerUe'

 minProperties: 1

 description: >

 Contains the PTP capabilities supported by each of the GPSI(s). The key of the map is

 the GPSI.

 required:

 - upNodeId

 anyOf:

 - required: [gmCapables]

 - required: [asTimeRes]

 PtpCapabilitiesPerUe:

 description: Contains the supported PTP capabilities per UE.

 type: object

 properties:

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 ptpCaps:

 type: array

 items:

 $ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/EventFilter'

 minItems: 1

 required:

 - ptpCaps

 oneOf:

 - required: [supi]

 - required: [gpsi]

 TimeSyncExposureConfigNotif:

 description: Contains the notification of time synchronization service state.

 type: object

 properties:

 configNotifId:

 type: string

 description: Notification Correlation ID assigned by the NF service consumer.

 stateOfConfig:

 $ref: '#/components/schemas/StateOfConfiguration'

 required:

 - configNotifId

 - stateOfConfig

 StateOfConfiguration:

 description: Contains the state of the time synchronization configuration.

 type: object

 properties:

 stateNwtt:

 type: boolean

 description: >

 When the PTP port state is Leader, Follower or Passive, it is included and set to true

 to indicate the state of configuration for NW-TT port is active; when PTP port state is

 in any other case, it is included and set to false to indicate the state of

 configuration for NW-TT port is inactive. Default value is false.

 stateOfDstts:

 description: Contains the PTP port states of the DS-TT(s).

 type: array

 items:

 $ref: '#/components/schemas/StateOfDstt'

 minItems: 1

 StateOfDstt:

 description: Contains the PTP port state of a DS-TT.

 type: object

 properties:

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 state:

 type: boolean

 description: >

 When the PTP port state is Leader, Follower or Passive, it is included and set to true

 to indicate the state of configuration for DS-TT port is active; when PTP port state is

 in any other case, it is included and set to false to indicate the state of

 configuration for DS-TT port is inactive. Default value is false.

 required:

 - state

 oneOf:

 - required: [supi]

 - required: [gpsi]

 TimeSyncExposureConfig:

 description: Contains the Time Synchronization Configuration parameters.

 type: object

 properties:

 upNodeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 reqPtpIns:

 $ref: '#/components/schemas/PtpInstance'

 gmEnable:

 type: boolean

 description: >

 Indicates that the AF requests 5GS to act as a grandmaster for PTP or gPTP if it is

 included and set to true.

 gmPrio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 timeDom:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 timeSyncErrBdgt:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 configNotifId:

 type: string

 description: Notification Correlation ID assigned by the NF service consumer.

 configNotifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 tempValidity:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TemporalValidity'

 required:

 - upNodeId

 - reqPtpIns

 - timeDom

 - configNotifId

 - configNotifUri

 PtpInstance:

 description: Contains PTP instance configuration and activation requested by the AF.

 type: object

 properties:

 instanceType:

 $ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/InstanceType'

 protocol:

 $ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/Protocol'

 ptpProfile:

 type: string

 portConfigs:

 type: array

 items:

 $ref: '#/components/schemas/ConfigForPort'

 minItems: 1

 required:

 - instanceType

 - protocol

 - ptpProfile

 ConfigForPort:

 description: Contains configuration for each port.

 type: object

 properties:

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 n6Ind:

 type: boolean

 ptpEnable:

 type: boolean

 logSyncInter:

 type: integer

 logSyncInterInd:

 type: boolean

 logAnnouInter:

 type: integer

 logAnnouInterInd:

 type: boolean

 oneOf:

 - required: [supi]

 - required: [gpsi]

 - required: [n6Ind]

\*\*\* Next Change \*\*\*

# A.3 Ntsctsf\_QoSandTSCAssistance API

openapi: 3.0.0

info:

 title: Ntsctsf\_QoSandTSCAssistance Service API

 version: 1.1.0-alpha.1

 description: |

 TSCTSF QoS and TSC Assistance Service.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 29.565 V18.0.0; 5G System; Time Sensitive Communication and Time Synchronization function

 Services; Stage 3.

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.565/'

servers:

 - url: '{apiRoot}/ntsctsf-qos-tscai/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

security:

 - {}

 - oAuth2ClientCredentials:

 - ntsctsf-qos-tscai

paths:

 /tsc-app-sessions:

 post:

 summary: Creates a new Individual TSC Application Session Context resource

 operationId: PostTSCAppSessions

 tags:

 - TSC Application Sessions (Collection)

 requestBody:

 description: Contains the information for the creation the resource.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TscAppSessionContextData'

 responses:

 '201':

 description: Successful creation of the resource.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TscAppSessionContextData'

 headers:

 Location:

 description: >

 Contains the URI of the created individual TSC application session context resource,

 according to the structure

 {apiRoot}/ntsctsf-qos-tscai/v1/tsc-app-sessions/{appSessionId} or the URI of the

 created events subscription sub-resource, according to the structure

 {apiRoot}/ntsctsf-qos-tscai/v1/tsc-app-sessions/{appSessionId}/events-subscription}

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 terminationRequest:

 '{$request.body#/notifUri}/terminate':

 post:

 requestBody:

 description: >

 Request of the termination of the Individual TSC Application Session Context

 required: true

 content:

 application/json:

 schema:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TerminationInfo'

 responses:

 '204':

 description: The receipt of the notification is acknowledged.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 eventNotification:

 '{$request.body#/evSubsc/notifUri}/notify':

 post:

 requestBody:

 description: Notification of an event occurrence in the TSCTSF.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsNotification'

 responses:

 '204':

 description: The receipt of the notification is acknowledged.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /tsc-app-sessions/{appSessionId}:

 get:

 summary: Reads an existing Individual TSC Application Session Context

 operationId: GetTSCAppSession

 tags:

 - Individual TSC Application Session Context (Document)

 parameters:

 - name: appSessionId

 description: String identifying the resource.

 in: path

 required: true

 schema:

 type: string

 responses:

 '200':

 description: A representation of the resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TscAppSessionContextData'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 patch:

 summary: Modifies an existing Individual TSC Application Session Context

 operationId: ModAppSession

 tags:

 - Individual TSC Application Session Context (Document)

 parameters:

 - name: appSessionId

 description: String identifying the resource.

 in: path

 required: true

 schema:

 type: string

 requestBody:

 description: Modification of the resource.

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: '#/components/schemas/TscAppSessionContextUpdateData'

 responses:

 '200':

 description: >

 successful modification of the resource and a representation of that resource is

 returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TscAppSessionContextData'

 '204':

 description: The successful modification.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 eventNotification:

 '{$request.body#/evSubsc/notifUri}/notify':

 post:

 requestBody:

 description: Notification of an event occurrence in the TSCTSF.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsNotification'

 responses:

 '204':

 description: The receipt of the notification is acknowledged.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /tsc-app-sessions/{appSessionId}/delete:

 post:

 summary: Deletes an existing Individual TSC Application Session Context

 operationId: DeleteTSCAppSession

 tags:

 - Individual TSC Application Session Context (Document)

 parameters:

 - name: appSessionId

 description: String identifying the Individual TSC Application Session Context resource.

 in: path

 required: true

 schema:

 type: string

 requestBody:

 description: >

 Deletion of the Individual TSC Application Session Context resource, request notification.

 required: false

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsSubscReqData'

 responses:

 '200':

 description: The deletion of the resource is confirmed and a resource is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsNotification'

 '204':

 description: The deletion is confirmed without returning additional data.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /tsc-app-sessions/{appSessionId}/events-subscription:

 put:

 summary: Creates or modifies an Events Subscription subresource

 operationId: putEventsSubsc

 tags:

 - Events Subscription (Document)

 parameters:

 - name: appSessionId

 description: String identifying the Events Subscription resource

 in: path

 required: true

 schema:

 type: string

 requestBody:

 description: Creation or modification of an Events Subscription resource.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsSubscReqData'

 responses:

 '201':

 description: >

 The creation of the Events Subscription resource is confirmed and its representation is

 returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsSubscReqData'

 headers:

 Location:

 description: >

 Contains the URI of the created Events Subscription resource,

 according to the structure

 {apiRoot}/ntsctsf-qos-tscai/v1/tsc-app-sessions/{appSessionId}/events-subscription}

 required: true

 schema:

 type: string

 '200':

 description: >

 The modification of the Events Subscription resource is confirmed and its representation

 is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsSubscReqData'

 '204':

 description: >

 The modification of the Events Subscription subresource is confirmed without returning

 additional data.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 eventNotification:

 '{$request.body#/notifUri}/notify':

 post:

 requestBody:

 description: >

 Contains the information for the notification of an event occurrence in the TSCTSF.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsNotification'

 responses:

 '204':

 description: The receipt of the notification is acknowledged.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Deletes the Events Subscription subresource.

 operationId: DeleteEventsSubsc

 tags:

 - Events Subscription (Document)

 parameters:

 - name: appSessionId

 description: String identifying the Individual TSC Application Session Context resource

 in: path

 required: true

 schema:

 type: string

 responses:

 '204':

 description: >

 The deletion of the of the Events Subscription sub-resource is confirmed without returning

 additional data.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 ntsctsf-qos-tscai: Access to the Ntsctsf\_QoSandTSCAssistance API

 schemas:

 TscAppSessionContextData:

 description: Represents an Individual TSC Application Session Context resource.

 type: object

 required:

 - notifUri

 - afId

 - qosReference

 oneOf:

 - required: [ueIpAddr]

 - required: [ueMac]

 properties:

 ueIpAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

 ipDomain:

 type: string

 description: The IPv4 address domain identifier.

 ueMac:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 appId:

 type: string

 description: Identifies the Application Identifier.

 ethFlowInfo:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

 minItems: 1

 enEthFlowInfo:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/EthFlowInfo'

 minItems: 1

 description: >

 Identifies the Ethernet flows which require QoS. Each Ethernet flow consists of a flow

 identifer and the corresponding UL and/or DL flows.

 flowInfo:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

 minItems: 1

 afId:

 type: string

 description: Identifies the AF identifier.

 tscQosReq:

 $ref: 'TS29122\_AsSessionWithQoS.yaml#/components/schemas/TscQosRequirement'

 qosReference:

 type: string

 description: Identifies a pre-defined QoS information.

 altQosReferences:

 type: array

 items:

 type: string

 minItems: 1

 description: Identifies an ordered list of pre-defined QoS information.

 altQosReqs:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AlternativeServiceRequirementsData'

 minItems: 1

 description: >

 Identifies an ordered list of alternative service requirements that include individual

 QoS parameter sets. The lower the index of the array for a given entry, the higher the

 priority.

 aspId:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AspId'

 sponId:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/SponId'

 sponStatus:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/SponsoringStatus'

 evSubsc:

 $ref: '#/components/schemas/EventsSubscReqData'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 TscAppSessionContextUpdateData:

 description: >

 Describes the authorization data of an Individual TSC Application Session Context created by

 the PCF.

 type: object

 properties:

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 appId:

 type: string

 description: Identifies the Application Identifier.

 ethFlowInfo:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

 minItems: 1

 enEthFlowInfo:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/EthFlowInfo'

 minItems: 1

 description: >

 Identifies the Ethernet flows which require QoS. Each Ethernet flow consists of a flow

 identifer and the corresponding UL and/or DL flows.

 flowInfo:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

 minItems: 1

 tscQosReq:

 $ref: 'TS29122\_AsSessionWithQoS.yaml#/components/schemas/TscQosRequirementRm'

 qosReference:

 type: string

 description: Identifies a pre-defined QoS information.

 altQosReferences:

 type: array

 items:

 type: string

 minItems: 1

 description: Identifies an ordered list of pre-defined QoS information.

 altQosReqs:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AlternativeServiceRequirementsData'

 minItems: 1

 description: >

 Identifies an ordered list of alternative service requirements that include individual

 QoS parameter sets. The lower the index of the array for a given entry, the higher the

 priority.

 aspId:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AspId'

 sponId:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/SponId'

 sponStatus:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/SponsoringStatus'

 evSubsc:

 $ref: '#/components/schemas/EventsSubscReqDataRm'

 EventsSubscReqData:

 description: Identifies the events the application subscribes to.

 type: object

 required:

 - events

 - notifUri

 - notifCorreId

 properties:

 events:

 type: array

 items:

 $ref: '#/components/schemas/TscEvent'

 minItems: 1

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 qosMon:

 $ref: 'TS29122\_AsSessionWithQoS.yaml#/components/schemas/QosMonitoringInformation'

 usgThres:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

 notifCorreId:

 type: string

 EventsSubscReqDataRm:

 description: >

 This data type is defined in the same way as the EventsSubscReqData data type, but with the

 OpenAPI nullable property set to true.

 type: object

 required:

 - events

 properties:

 events:

 type: array

 items:

 $ref: '#/components/schemas/TscEvent'

 minItems: 1

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 qosMon:

 $ref: 'TS29122\_AsSessionWithQoS.yaml#/components/schemas/QosMonitoringInformationRm'

 usgThres:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThresholdRm'

 notifCorreId:

 type: string

 nullable: true

 EventsNotification:

 description: Describes the notification of matched events.

 type: object

 required:

 - notifCorreId

 - events

 properties:

 notifCorreId:

 type: string

 events:

 type: array

 items:

 $ref: '#/components/schemas/EventNotification'

 minItems: 1

 EventNotification:

 description: Describes a notification of an matched event.

 type: object

 required:

 - event

 properties:

 event:

 $ref: '#/components/schemas/TscEvent'

 flowIds:

 type: array

 items:

 type: integer

 minItems: 1

 description: Identifies the IP flows that were sent during event subscription.

 qosMonReports:

 type: array

 items:

 $ref: 'TS29122\_AsSessionWithQoS.yaml#/components/schemas/QosMonitoringReport'

 minItems: 1

 usgRep:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/AccumulatedUsage'

 appliedQosRef:

 type: string

 description: >

 The currently applied alternative QoS requirement referring to an alternative QoS

 reference or a requested alternative QoS parameter set. Applicable for

 event QOS\_NOT\_GUARANTEED or SUCCESSFUL\_RESOURCES\_ALLOCATION.

#

# ENUMERATIONS DATA TYPES

#

 TscEvent:

 description: Represents an event to notify to the AF.

 anyOf:

 - type: string

 enum:

 - FAILED\_RESOURCES\_ALLOCATION

 - QOS\_MONITORING

 - QOS\_GUARANTEED

 - QOS\_NOT\_GUARANTEED

 - SUCCESSFUL\_RESOURCES\_ALLOCATION

 - USAGE\_REPORT

 - type: string

\*\*\* Next change \*\*\*

# A.4 Ntsctsf\_ASTI API

openapi: 3.0.0

info:

 title: Ntsctsf\_ASTI Service API

 version: 1.1.0-alpha.1

 description: |

 TSCTSF Access Stratum time distribution configuration Service.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 29.565 V18.0.0; 5G System; Time Sensitive Communication and

 Time Synchronization Function Services; Stage 3.

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.565/'

servers:

 - url: '{apiRoot}/ntsctsf-asti/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

security:

 - {}

 - oAuth2ClientCredentials:

 - ntsctsf-asti

paths:

 /configurations:

 post:

 summary: Creates a new Individual ASTI Configuration resource.

 operationId: ASTIConfiguration

 tags:

 - ASTI Configurations (Collection)

 requestBody:

 description: Contains the information for the creation the resource.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AccessTimeDistributionData'

 responses:

 '201':

 description: Successful creation of the resource.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AccessTimeDistributionData'

 headers:

 Location:

 description: >

 Contains the URI of the created individual ASTI Configuration resource,

 according to the structure

 {apiRoot}/ntsctsf-asti/{apiVersion}/configurations/{configId}

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /configurations/retrieve:

 post:

 summary: Request the status of the 5G access stratum time distribution for a list of UEs.

 operationId: RequestStatusof5GAccessStratumTimeDistribution

 tags:

 - ASTI Configurations

 requestBody:

 description: >

 Contains the information for the status of the 5G access stratum time distribution.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/StatusRequestData'

 responses:

 '200':

 description: >

 Successful retrieval of the status of the 5G access stratum time distribution.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/StatusResponseData'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /configurations/{configId}:

 put:

 summary: Modifies an existing Individual ASTI Configuration resource.

 operationId: ModifyIndividualASTIConfiguration

 tags:

 - Individual ASTI Configuration (Document)

 parameters:

 - name: configId

 description: String identifying an Individual ASTI Configuration.

 in: path

 required: true

 schema:

 type: string

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AccessTimeDistributionData'

 responses:

 '200':

 description: OK. Resource was succesfully modified and representation is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AccessTimeDistributionData'

 '204':

 description: No Content. Resource was succesfully modified.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 operationId: DeleteIndividualASTIConfiguration

 summary: Delete an Individual ASTI Configuration

 tags:

 - Individual ASTI Configuration (Document)

 parameters:

 - name: configId

 in: path

 description: String identifying an Individual ASTI Configuration.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. Resource was successfully deleted.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 ntsctsf-asti: Access to the Ntsctsf\_ASTI API

 schemas:

 AccessTimeDistributionData:

 description: >

 Contains the parameters for the creation of 5G access stratum time distribution

 configuration.

 type: object

 properties:

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 gpsis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 minItems: 1

 interGrpId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 exterGrpId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ExternalGroupId'

 asTimeDisParam:

 $ref: '#/components/schemas/AsTimeDistributionParam'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - asTimeDisParam

 oneOf:

 - required: [supis]

 - required: [interGrpId]

 - required: [gpsis]

 - required: [exterGrpId]

 AsTimeDistributionParam:

 description: Contains the 5G access stratum time distribution parameters.

 type: object

 properties:

 asTimeDisEnabled:

 type: boolean

 description: >

 When this attribute is included and set to true, it indicates that the access stratum

 time distribution via Uu reference point is activated.

 timeSyncErrBdgt:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 tempValidity:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TemporalValidity'

 StatusRequestData:

 description: >

 Contains the parameters for retrieval of the status of the access stratum time distribution

 for a list of UEs.

 type: object

 properties:

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 gpsis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 minItems: 1

 oneOf:

 - required: [supis]

 - required: [gpsis]

 StatusResponseData:

 description: >

 Contains the parameters for the status of the access stratum time distribution for a list of

 UEs.

 type: object

 properties:

 inactiveUes:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 inactiveGpsis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 minItems: 1

 activeUes:

 type: array

 items:

 $ref: '#/components/schemas/ActiveUe'

 minItems: 1

 ActiveUe:

 description: >

 Contains the UE identifier whose status of the access stratum time distribution is active

 and the optional requested time synchronization error budget.

 type: object

 properties:

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 timeSyncErrBdgt:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 oneOf:

 - required: [supi]

 - required: [gpsi]

\*\*\* End of Changes \*\*\*