**3GPP TSG-CT WG3 Meeting #127eC3-231271**

**E-meeting, 17th – 21st, April, 2023 (revision of C3-231xxx)**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.522** | **CR** | 0880 | **rev** | **-** | **Current version:** | **18.1.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Correction to AF influence on Service Function Chaining |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | SFC |  | ***Date:*** | 2023-03-15 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | The attrubte name of SDF Id is not correct in table 5.4.3.3.2. |
|  |  |
| ***Summary of change:*** | Corect the errors above. |
|  |  |
| ***Consequences if not approved:*** | SFC is not fully supported. |
|  |  |
| ***Clauses affected:*** | 5.4.3.3.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | The CR does not impact the OpenAPI file of TrafficInfluence.  |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

##### 5.4.3.3.2 Type: TrafficInfluSub

This type represents a traffic influence subscription. The same structure is used in the subscription request and subscription response.

Table 5.4.3.3.2-1: Definition of type TrafficInfluSub

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability(NOTE 1) |
| afServiceId | string | O | 0..1 | Identifies a service on behalf of which the AF is issuing the request. |  |
| afAppId | string | O | 0..1 | Identifies an application.(NOTE 3) |  |
| afTransId | string | O | 0..1 | Identifies an NEF Northbound interface transaction, generated by the AF. |  |
| appReloInd | boolean | O | 0..1 | Identifies whether an application can be relocated once a location of the application has been selected. Set to "true" if it can be relocated; otherwise set to "false". Default value is "false" if omitted. |  |
| dnn | Dnn | O | 0..1 | Identifies a DNN, a full DNN with both the Network Identifier and Operator Identifier, or a DNN with the Network Identifier only. |  |
| snssai | Snssai | O | 0..1 | Identifies an S-NSSAI. |  |
| externalGroupId | ExternalGroupId | O | 0..1 | Identifies a group of users.(NOTE 2) (NOTE 6) |  |
| externalGroupIds | array(ExternalGroupId) | O | 2..N | List of external group identifiers associated with the subscriber.(NOTE 2) (NOTE 6) (NOTE 7) | FinerGranUEs |
| extSubscCats | array(string) | O | 1..N | List of external categories associated with the subscriber.(NOTE 8) | FinerGranUEs |
| anyUeInd | boolean | O | 0..1 | Identifies whether the AF request applies to any UE (i.e. all UEs). This attribute shall set to "true" if applicable for any UE, otherwise, set to "false".(NOTE 2) |  |
| subscribedEvents | array(SubscribedEvent) | O | 1..N | Identifies the requirement to be notified of the event(s). |  |
| gpsi | Gpsi | O | 0..1 | Identifies a user. (NOTE 2) |  |
| ipv4Addr | Ipv4Addr | O | 0..1 | Identifies the IPv4 address. (NOTE 2) |  |
| ipDomain | string | O | 0..1 | The IPv4 address domain identifier.The attribute may only be provided if the ipv4Addr attribute is present. |  |
| ipv6Addr | Ipv6Addr | O | 0..1 | Identifies the IPv6 address. (NOTE 2) |  |
| macAddr | MacAddr48 | O | 0..1 | Identifies the MAC address. (NOTE 2) |  |
| dnaiChgType | DnaiChangeType | O | 0..1 | Identifies a type of notification regarding UP path management event. |  |
| notificationDestination | Link | C | 0..1 | Contains the Callback URL to receive the notification from the NEF.It shall be present if the "subscribedEvents" is present. |  |
| requestTestNotification | boolean | O | 0..1 | Set to true by the AF to request the NEF to send a test notification as defined in clause 5.2.5.3 of 3GPP TS 29.122 [4]. Set to false or omitted otherwise. | Notification\_test\_event |
| websockNotifConfig | WebsockNotifConfig | O | 0..1 | Configuration parameters to set up notification delivery over Websocket protocol. | Notification\_websocket |
| self | Link | C | 0..1 | Link to the created resource. This parameter shall be supplied by the NEF in HTTP responses that include an object of TrafficInfluSub type |  |
| trafficFilters | array(FlowInfo) | O | 1..N | Identifies IP packet filters.(NOTE 3) |  |
| ethTrafficFilters | array(EthFlowDescription) | O | 1..N | Identifies Ethernet packet filters.(NOTE 3) |  |
| trafficRoutes | array(RouteToLocation) | O | 1..N | Identifies the N6 traffic routing requirement. (NOTE 9) |  |
| sfcIdDl(NOTE 5) | string | O | 0..1 | Reference to a pre-configured steering of user traffic to service function chain in downlink. | SFC |
| sfcIdUl(NOTE 5) | string | O | 0..1 | Reference to a pre-configured steering of user traffic to service function chain in uplink.  | SFC |
| metadata | Metadata | C | 0..1 | Contains opaque information for the service functions in the N6-LAN that is provided by AF and transparently sent to UPF. May only provided when "sfcIdDl" and/or "sfcIdUl" are provided. | SFC |
| tfcCorrInd | boolean | O | 0..1 | Indication of traffic correlation.May only be included when "externalGroupId" attribute was included within the TrafficInfluSub data type previously.It is used to indicate that for the group of UEs, the targeted PDU sessions should be correlated by a common DNAI.Set to "true" if it should be correlated; otherwise set to "false". Default value is "false" if omitted. (NOTE 4) (NOTE 10) |  |
| tfcCorreInfo | TraficCorrelationInfo | O | 0..1 | Contains the information for traffic correlation. (NOTE 10) | CommonEASDNAI |
| tempValidities | array(TemporalValidity) | O | 1..N | Indicates the time interval(s) during which the AF request is to be applied. |  |
| validGeoZoneIds | array(string) | O | 1..N | Identifies a geographic zone that the AF request applies only to the traffic of UE(s) located in this specific zone.This attribute is deprecated; the attribute "geoAreas" should be used instead. |  |
| geoAreas | array(GeographicalArea) | O | 1..N | Identifies geographical areas within which the AF request applies.This attribute deprecates validGeoZoneIds attribute. |  |
| afAckInd | boolean | O | 0..1 | Identifies whether the AF acknowledgement of UP path event notification is expected.Set to "true" if the AF acknowledge is expected; otherwise set to "false". Default value is "false" if omitted. | URLLC |
| addrPreserInd | boolean | O | 0..1 | Indicates whether UE IP address should be preserved.This attribute shall set to "true" if preserved, otherwise, set to "false".Defalult value is "false" if omitted. | URLLC |
| simConnInd | boolean | O | 0..1 | Indication of simultaneous connectivity temporarily maintained for the source and target PSA. If it is included and set to "true", temporary simultaneous connectivity should be kept. The default value "false" applies, if the attribute is not present and has not been supplied previously. | SimultConnectivity |
| simConnTerm | DurationSec | O | 0..1 | Indication of the minimum time interval to be considered for inactivity of the traffic routed via the source PSA during the edge re-location procedure. It may be included when the "simConnInd" attribute is set to true.  | SimultConnectivity |
| maxAllowedUpLat | Uinteger | O | 0..1 | Indicates the target user plane latency in units of milliseconds. The SMF may use this value to decide whether edge relocation is needed to ensure that the user plane latency does not exceed the value. | AF\_lantency |
| easIpReplaceInfos | array(EasIpReplacementInfo) | O | 1..N | Contains EAS IP replacement information. | EASIPreplacement |
| easRedisInd | boolean | O | 0..1 | Indicates the EAS rediscovery is required for the application if it is included and set to "true". Defalult value is "false" if omitted.The indication shall be invalid after it was applied unless it is provided again. | EASDiscovery |
| eventReq | ReportingInformation | O | 0..1 | Indicates the event reporting requirements.This attribute may be provided if the "EDGEAPP" feature is supported and the "subscribedEvents" attribute is present. | EDGEAPP |
| eventReports | array(EventNotification) | C | 1..N | Represents user plane path management event report(s).This attribute shall be present in an HTTP POST response if the immediate reporting indication in the "immRep" attribute within the "eventReq" attribute is set to true and the "subscribedEvents" was present in the corresponding HTTP POST request and the report(s) are available.This attribute may also be present in an HTTP PUT or PATCH response when the report(s) are available. | EDGEAPP |
| candDnaiInd | boolean | O | 0..1 | Indication of reporting candidate DNAI(s). If it is included and set to "true", the candidate DNAI(s) for the PDU session need to be reported. Otherwise set to "false" or omitted. | CommonEASDNAI |
| suppFeat | SupportedFeatures | C | 0..1 | Indicates the list of Supported features used as described in clause 5.4.4.This attribute shall be provided in the POST request and in the response of successful resource creation. |  |
| NOTE 1: Properties marked with a feature as defined in clause 5.4.4 are applicable as described in clause 5.2.7 of 3GPP TS 29.122 [4]. If no feature is indicated, the related property applies for all the features.NOTE 2: One of individual UE identifier (i.e. "gpsi", "macAddr", "ipv4Addr" or "ipv6Addr"), External Group Identifier (i.e. "externalGroupId" or "externalGroupIds" (is included when FinerGranUEs feature is supported)) or any UE indication "anyUeInd" shall be included.NOTE 3: One of "afAppId", "trafficFilters" or "ethTrafficFilters" shall be included.NOTE 4: The indication of traffic correlation shall be provided only when the AF requires that all the PDU sessions related to the 5G VN group member UEs should be correlated by a common DNAI in the user plane for the traffic as described in 3GPP TS 23.501 [3], clause 5.6.7.1 and clause 5.29.NOTE 5: When the SFC feature is supported, for the purpose of influencing service function chaining, at least one attribute shall be present.NOTE 6: The attributes "externalGroupId" and "externalGroupIds" are mutually exclusive attributes.NOTE 7: The AF request applies to the UE(s) that belong to all the External Group Identifiers indicated by the attribute " externalGroupIds", when included.NOTE 8: The AF request applies to the UE(s) that belong to all the External Subscriber Categories indicated by the attribute " extSubscCats", which is included only if either "externalGroupIds" attribute is included or "externalGroupId" is included or "anyUeInd" attribute is included.NOTE 9: When only one DNAI is included, and the Indication of traffic correlation within the "tfcCorrInd" attribute is available or the "correType" attribute of the "tfcCorreInfo" includes the value "COMMON\_DNAI", the DNAI is used as common DNAI for UEs identified by AF request.NOTE 10: The "tfcCorrInd" attribute and the "tfcCorreInfo" attribute are mutually exclusive. |

\*\*\* End of Changes \*\*\*