**3GPP TSG CT WG3 Meeting #134 *C3-242115***

**Changsha, China, 15 - 19 April, 2024 (Revision of C3-242xyz)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.122** | **CR** | **0821** | **rev** | **-** | **Current version:** | **18.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Application Specific Expected UE Behaviour parameters update | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Nokia | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | AIMLsys | | | | |  | ***Date:*** | | | 2024-04-08 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In TS 23.502 clause 5.2.6.4.3 (as per S2-2313620), Application Specific Expected UE Behaviour parameters are updated as follows:  **Inputs, Optional:** GPSI or UE addressing information, **one or multiple Expected UE Behaviour parameters (optionally with associated confidence and/or accuracy levels) or one or multiple Application-Specific Expected UE Behaviour parameters (optionally with associated confidence and/or accuracy levels),** External Group ID for 5G VN group creation or for multicast MBS group creation, External Group ID, 5G VN group related information (e.g. 5G VN group data, 5G VN membership management), MTC Provider Information, Multicast MBS related information, DNN and S-NSSAI specific Group Parameters, DNN, S-NSSAI.  The corresponding update has to be reflected in the stage 3 data model and openAPI.  The application specific expected UE behavior as the multiple instance is achieved by CpInfo instead of CpParameterSet. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Application Specific Expected UE Behaviour parameters is defined as single instance in CpParameterSet The openAPI is updated correspondingly. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | There is a misalignment between stage 2 and stage 3 specfications.. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.10.2.2.2, A.10 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces new backward compatible features to the OpenAPI definition of the CpProvisioning API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* \* First Change \* \* \* \*

##### 5.10.2.2.2 Type: CpParameterSet

This data type represents an offered communication pattern parameter set sent from the SCC/AS to the SCEF.

Table 5.10.2.2.2-1: Definition of type CpParameterSet

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | Cardinality | Description | Applicability (NOTE 1) |
| setId | string | 1 | SCS/AS-chosen correlator provided by the SCS/AS in the request to create a resource fo CP parameter set(s).  (NOTE 4) |  |
| self | Link | 0..1 | Link to the resource "Individual CP set Provisioning". This parameter shall be supplied by the SCEF in HTTP responses. |  |
| validityTime | DateTime | 0..1 | Identifies when the CP parameter set expires and shall be deleted. If absent, it indicates that there is no expiration time for this CP parameter set. |  |
| periodicCommunicationIndicator | CommunicationIndicator | 0..1 | Identifies whether UE communicates periodically or on demand. |  |
| communicationDurationTime | DurationSec | 0..1 | Identifies duration time of periodic communication. |  |
| periodicTime | DurationSec | 0..1 | Identifies interval time of periodic communication. |  |
| scheduledCommunicationTime | ScheduledCommunicationTime | 0..1 | Identifies time zone and day of the week when the UE is available for communication. |  |
| scheduledCommunicationType | ScheduledCommunicationType | 0..1 | Indicates the Scheduled Communication Type.  May only be present if the "scheduledCommunicationTime" attribute is provided. | ScheduledCommType\_5G |
| stationaryIndication | StationaryIndication | 0..1 | Identifies whether the UE is stationary or mobile. |  |
| batteryInds | array(BatteryIndication) | 0..N | Indicates the power consumption type(s) of the UE.  (NOTE 3) |  |
| trafficProfile | TrafficProfile | 0..1 | Identifies the type of data transmission. |  |
| expectedUmts | array(UmtLocationArea5G) | 0..N | Identifies the UE's expected geographical movement. The attribute is only applicable in 5G.  (NOTE 2) | ExpectedUMT\_5G  ExpectedUmtTime\_5G |
| expectedUmtDays | DayOfWeek | 0..6 | Identifies the day of the week. If absent, it indicates every day of the week. | ExpectedUmtTime\_5G |
| expectedUmtDaysAdd | array(DayOfWeek) | 0..5 | Identifies the additional day(s) of the week.  (NOTE 5) | ExpectedUmtTime\_Add |
| appExpUeBehv | AppExpUeBehaviour | 0..1 | Contains the Application Specific Expected UE Behaviour parameters. | AppExpUeBehaviour |
| confidenceLevel | string | 0..1 | When present, this IE indicates the Confidence level for the associated Expected UE Behaviour parameter.  The value shall be between 0.01 and 1.00 with a step size of 0.01, represented as string.  If not present, confidence level 1.00 applies.  Pattern: '^[0]\.[0-9]{2}|[1.00]$' | ConfAccuLevels |
| accuracyLevel | string | 0..1 | When present, this IE indicates the accuracy level for the associated Expected UE Behaviour parameter.  The value shall be between 0.01 and 1.00 with a step size of 0.01, represented as string.  If not present, accuracy level 1.00 applies.  Pattern: '^[0]\.[0-9]{2}|[1.00]$' | ConfAccuLevels |
| NOTE 1: Properties marked with a feature as defined in clause 5.10.4 are applicable as described in clause 5.2.7. If no features are indicated, the related property applies for all the features.  NOTE 2: The first instance of the attribute represents the start of the location, and the last one represents the stop of the location.  NOTE 3: If "BATTERY\_RECHARGE" is provided, "BATTERY\_NO\_RECHARGE" shall not be provided simultaneously, vice versa; If "BATTERY\_REPLACE" is provided, "BATTERY\_NO\_REPLACE" shall not be provided simultaneously, vice versa; If "NO\_BATTERY" is provided, any value indicating UE powered with battery shall not be provided simultaneously, vice versa.  NOTE 4: A setId can only belong to one "Individual CP Provisioning Subscription" resource.  NOTE 5: The "expectedUmtDaysAdd" attribute may only be provided to indicate the additional day(s) if the "expectedUmtDays" attribute is also provided. | | | | |

\* \* \* \* Next changes \* \* \* \*

# A.10 CpProvisioning API

openapi: 3.0.0

info:

title: 3gpp-cp-parameter-provisioning

version: 1.3.0-alpha.4

description: |

API for provisioning communication pattern parameters.

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V18.4.0 T8 reference point for Northbound APIs

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-cp-parameter-provisioning/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

/{scsAsId}/subscriptions:

get:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in clause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

summary: Read all active CP parameter provisioning subscription resources for a given SCS/AS.

operationId: FetchAllCPProvisioningSubscriptions

tags:

- CP provisioning Subscriptions

responses:

'200':

description: OK. The subscription information related to the request URI is returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/CpInfo'

minItems: 0

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in clause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

summary: Create a new subscription resource of provisioning CP parameter set(s).

operationId: CreateCPProvisioningSubscription

tags:

- CP provisioning Subscriptions

requestBody:

description: >

Create new subscriptions for a given SCS/AS and the provisioning CP parameter sets.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/CpInfo'

responses:

'201':

description: >

Created. The subscription was created successfully. The SCEF shall return the created

subscription in the response content.

content:

application/json:

schema:

$ref: '#/components/schemas/CpInfo'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: >

The CP parameters for all sets were not created successfully. CpReport may be included

with detailed information.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/CpReport'

minItems: 1

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/subscriptions/{subscriptionId}:

get:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in clause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Subscription ID

required: true

schema:

type: string

summary: Read a CP parameter provisioning subscription resource.

operationId: FetchIndCPProvisioningSubscription

tags:

- Individual CP Provisioning Subscription

responses:

'200':

description: OK. The subscription information related to the request URI is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/CpInfo'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Modify a CP parameter provisioning subscription resource.

operationId: UpdateIndCPProvisioningSubscription

tags:

- Individual CP Provisioning Subscription

requestBody:

description: Modify a CP parameter provisioning subscription resource.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/CpInfo'

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in clause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Subscription ID

required: true

schema:

type: string

responses:

'200':

description: >

OK. The subscription was modified successfully. The SCEF shall return an updated

subscription in the response content.

content:

application/json:

schema:

$ref: '#/components/schemas/CpInfo'

'204':

description: >

No Content. The subscription was modified successfully and no content is to be sent

in the response message body.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: >

The CP parameters for all sets were not updated successfully. CpReport may be included

with detailed information.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/CpReport'

minItems: 1

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in clause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Subscription ID

required: true

schema:

type: string

summary: Delete a CP parameter provisioning subscription resource.

operationId: DeleteIndCPProvisioningSubscription

tags:

- Individual CP Provisioning Subscription

responses:

'204':

description: >

No Content. The subscription was deleted successfully. The content shall be empty.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/subscriptions/{subscriptionId}/cpSets/{setId}:

get:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in clause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Subscription ID

required: true

schema:

type: string

- name: setId

in: path

description: Identifier of the CP parameter set

required: true

schema:

type: string

summary: Read CP at individual CP set(s) level associated with a CP parameter set Id.

operationId: FetchIndCPSetProvisioning

tags:

- Individual CP set Provisioning

responses:

'200':

description: OK. The subscription information related to the request URI is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/CpParameterSet'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Update CP at individual CP set(s) level associated with a CP parameter set Id.

operationId: UpdateIndCPSetProvisioning

tags:

- Individual CP set Provisioning

requestBody:

description: Change information for a CP parameter set.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/CpParameterSet'

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in clause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Subscription ID

required: true

schema:

type: string

- name: setId

in: path

description: Identifier of the CP parameter set

required: true

schema:

type: string

responses:

'200':

description: >

OK. The CP parameter set resource was modified successfully. The SCEF shall return an

updated CP parameter set resource in the response content.

content:

application/json:

schema:

$ref: '#/components/schemas/CpParameterSet'

'204':

description: >

No Content. The CP parameter set resource was modified successfully and no content

is to be sent in the response message body.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'409':

description: The CP parameters for the CP set were not updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/CpReport'

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: The CP parameters for the CP set were not updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/CpReport'

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in clause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Subscription ID

required: true

schema:

type: string

- name: setId

in: path

description: Identifier of the CP parameter set

required: true

schema:

type: string

summary: Delete CP at individual CP set(s) level associated with a CP parameter set Id.

operationId: DeleteIndCPSetProvisioning

tags:

- Individual CP set Provisioning

responses:

'204':

description: >

No Content. The subscription was deleted successfully. The content shall be empty.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

CpInfo:

description: Represents the resources for communication pattern parameter provisioning.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

mtcProviderId:

type: string

description: Identifies the MTC Service Provider and/or MTC Application.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

externalGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

cpParameterSets:

type: object

additionalProperties:

$ref: '#/components/schemas/CpParameterSet'

minProperties: 1

description: >

Identifies a set of CP parameter information that may be part of this CpInfo structure.

Any string value can be used as a key of the map.

cpReports:

type: object

additionalProperties:

$ref: '#/components/schemas/CpReport'

minProperties: 1

description: >

Supplied by the SCEF and contains the CP set identifiers for which CP parameter(s) are

not added or modified successfully. The failure reason is also included. Each element

provides the related information for one or more CP set identifier(s) and is identified

in the map via the failure identifier as key.

readOnly: true

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

ueIpAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

ueMacAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

required:

- cpParameterSets

oneOf:

- required: [externalId]

- required: [msisdn]

- required: [externalGroupId]

CpParameterSet:

description: Represents an offered communication pattern parameter set.

type: object

properties:

setId:

type: string

description: >

SCS/AS-chosen correlator provided by the SCS/AS in the request to create a resource

for CP parameter set(s).

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

validityTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

periodicCommunicationIndicator:

$ref: '#/components/schemas/CommunicationIndicator'

communicationDurationTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

periodicTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

scheduledCommunicationTime:

$ref: '#/components/schemas/ScheduledCommunicationTime'

scheduledCommunicationType:

$ref: '#/components/schemas/ScheduledCommunicationType'

stationaryIndication:

$ref: '#/components/schemas/StationaryIndication'

batteryInds:

type: array

items:

$ref: '#/components/schemas/BatteryIndication'

minItems: 1

trafficProfile:

$ref: '#/components/schemas/TrafficProfile'

expectedUmts:

type: array

items:

$ref: '#/components/schemas/UmtLocationArea5G'

minItems: 1

description: >

Identifies the UE's expected geographical movement. The attribute is only applicable

in 5G.

expectedUmtDays:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DayOfWeek'

expectedUmtDaysAdd:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DayOfWeek'

minItems: 1

maxItems: 5

description: Identifies the additional day(s) of the week.

appExpUeBehv:

$ref: '#/components/schemas/AppExpUeBehaviour'

confidenceLevel:

type: string

pattern: '^[0]\.[0-9]{2}|[1.00]$'

accuracyLevel:

type: string

pattern: '^[0]\.[0-9]{2}|[1.00]$'

required:

- setId

ScheduledCommunicationTime:

description: Represents an offered scheduled communication time.

type: object

properties:

daysOfWeek:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DayOfWeek'

minItems: 1

maxItems: 6

description: >

Identifies the day(s) of the week. If absent, it indicates every day of the week.

timeOfDayStart:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeOfDay'

timeOfDayEnd:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeOfDay'

CpReport:

description: >

Represents a CP report indicating the CP set identifier(s) which CP parameter(s) are not

added or modified successfully and the corresponding failure cause(s).

type: object

properties:

setIds:

type: array

items:

type: string

minItems: 1

description: >

Identifies the CP set identifier(s) which CP parameter(s) are not added or modified

successfully

failureCode:

$ref: '#/components/schemas/CpFailureCode'

required:

- failureCode

UmtLocationArea5G:

description: Represents the user location area describing the UE moving trajectory.

allOf:

- $ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea5G'

- type: object

properties:

umtTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeOfDay'

umtDuration:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

AppExpUeBehaviour:

description: Contains the Application Specificf Expected UE Behaviour parameters.

type: object

properties:

appId:

type: string

description: Indicates the Application Identifier.

expPduSesInacTm:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

flowDescriptions:

type: array

items:

type: string

minItems: 1

description: >

Represents a 3-tuple with protocol, server ip and server port for UL/DL application

traffic. The content of the string has the same encoding as the IPFilterRule AVP

value as defined in IETF RFC 6733.

confidenceLevel:

type: string

pattern: '^[0]\.[0-9]{2}|[1.00]$'

accuracyLevel:

type: string

pattern: '^[0]\.[0-9]{2}|[1.00]$'

failureCode:

$ref: '#/components/schemas/CpFailureCode'

validityTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

oneOf:

- required: [appId]

- required: [flowDescriptions]

CommunicationIndicator:

anyOf:

- type: string

enum:

- PERIODICALLY

- ON\_DEMAND

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents the type of the communication.

Possible values are:

- PERIODICALLY: Identifies the UE communicates periodically

- ON\_DEMAND: Identifies the UE communicates on demand

StationaryIndication:

anyOf:

- type: string

enum:

- STATIONARY

- MOBILE

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents the stationarity of the UE.

Possible values are:

- STATIONARY: Identifies the UE is stationary

- MOBILE: Identifies the UE is mobile

CpFailureCode:

anyOf:

- type: string

enum:

- MALFUNCTION

- SET\_ID\_DUPLICATED

- OTHER\_REASON

- CONFIDENCE\_LEVEL\_NOT\_SUFFICIENT

- ACCURACY\_LEVEL\_NOT\_SUFFICIENT

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents the failure reason of the CP parameter provisioning.

Possible values are

- MALFUNCTION: This value indicates that something functions wrongly in CP parameter

provisioning or the CP parameter provisioning does not function at all.

- SET\_ID\_DUPLICATED: The received CP set identifier(s) are already provisioned.

- OTHER\_REASON: Other reason unspecified.

- CONFIDENCE\_LEVEL\_NOT\_SUFFICIENT: The received confidence level for the expected UE

parameter is not sufficient.

- ACCURACY\_LEVEL\_NOT\_SUFFICIENT: The received accuracy level for the expected UE parameter

is not sufficient.

BatteryIndication:

anyOf:

- type: string

enum:

- BATTERY\_RECHARGE

- BATTERY\_REPLACE

- BATTERY\_NO\_RECHARGE

- BATTERY\_NO\_REPLACE

- NO\_BATTERY

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents the type of power consumption.

Possible values are:

- BATTERY\_RECHARGE: UE powered with rechargeable battery.

- BATTERY\_REPLACE: UE powered with replaceable battery.

- BATTERY\_NO\_RECHARGE: UE powered with no rechargeable battery.

- BATTERY\_NO\_REPLACE: UE powered with no replaceable battery.

- NO\_BATTERY: UE not battery powered.

TrafficProfile:

anyOf:

- type: string

enum:

- SINGLE\_TRANS\_UL

- SINGLE\_TRANS\_DL

- DUAL\_TRANS\_UL\_FIRST

- DUAL\_TRANS\_DL\_FIRST

- MULTI\_TRANS

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents the type of data transmission.

Possible values are:

- SINGLE\_TRANS\_UL: Uplink single packet transmission.

- SINGLE\_TRANS\_DL: Downlink single packet transmission.

- DUAL\_TRANS\_UL\_FIRST: Dual packet transmission, firstly uplink packet transmission with

subsequent downlink packet transmission.

- DUAL\_TRANS\_DL\_FIRST: Dual packet transmission, firstly downlink packet transmission with

subsequent uplink packet transmission.

- MULTI\_TRANS: Multiple packet transmission.

ScheduledCommunicationType:

anyOf:

- type: string

enum:

- DOWNLINK

- UPLINK

- BIDIRECTIONAL

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents the type of scheduled communication.

Possible values are:

- DOWNLINK: Downlink only.

- UPLINK: Uplink only.

- BIDIRECTIONAL: Bi-directional.

\* \* \* \* End of Changes \* \* \* \*