**3GPP TSG-CT WG4 Meeting #107-eC4-216**

**E-Meeting, 15th – 23rd November 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.504** | **CR** | **0165** | **rev** | **1** | **Current version:** | **16.9.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Naming Conventions |
|  |  |
| ***Source to WG:*** | China Mobile |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | SBIProtoc16 |  | ***Date:*** | 2021-11-15 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | As per the discussion on naming conventions on CT4#106e, see discussion paper in C4-215364, the deviations from naming conventions in the normative text and YAML should be addressed. |
|  |  |
| ***Summary of change:*** | To address the deviations from naming conventions accordingly. |
|  |  |
| ***Consequences if not approved:*** | Risk of interoperability issue. |
|  |  |
| ***Clauses affected:*** | A.2, A.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces backward compatible corrections to the Nudr\_dr and Nudr\_GroupIDmap APIs. |
|  |  |
| ***This CR's revision history:*** |  |

**\*\*\*\*\*\*\***

\* \* \* First Change \* \* \* \*

## A.2 Nudr\_DataRepository API

This Annex specifies the formal definition of the Nudr\_DataRepository service. It consists of OpenAPI 3.0.0 specifications, in YAML format.

The OpenAPI 3.0.0 definition related to SubscriptionData shall comply with the definition in 3GPP TS 29.505 [2].

The OpenAPI 3.0.0 definition related to PolicyData, StructuredDataForExposure and ApplicationData shall comply with the definition in 3GPP TS 29.519 [3].

The OpenAPI file for the Nudr\_DataRepository API is defined as follows:

openapi: 3.0.0

**\*\*\*\*\*\*\*\*\*\* skipped for clarity \*\*\*\*\*\*\*\*\*\***

 /application-data/influenceData:

 $ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1influenceData'

# The path segment is left not following the naming convention as defined in 3GPP TS 29.501 due to backward compatibility consideration.

 /application-data/influenceData/{influenceId}:

 $ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1influenceData~1%7BinfluenceId%7D'

# The path segment is left not following the naming convention as defined in 3GPP TS 29.501 due to backward compatibility consideration.

**\*\*\*\*\*\*\*\*\*\* skipped for clarity \*\*\*\*\*\*\*\*\*\***

 /application-data/influenceData/subs-to-notify:

 $ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1influenceData~1subs-to-notify'

# The path segment is left not following the naming convention as defined in 3GPP TS 29.501 due to backward compatibility consideration.

 /application-data/influenceData/subs-to-notify/{subscriptionId}:

 $ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1influenceData~1subs-to-notify~1%7BsubscriptionId%7D'

# The path segment is left not following the naming convention as defined in 3GPP TS 29.501 due to backward compatibility consideration.

**\*\*\*\*\*\*\*\*\*\* skipped for clarity \*\*\*\*\*\*\*\*\*\***

 /application-data/bdtPolicyData:

 $ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1bdtPolicyData'

# The path segment is left not following the naming convention as defined in 3GPP TS 29.501 due to backward compatibility consideration.

 /application-data/bdtPolicyData/{bdtPolicyId}:

 $ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1bdtPolicyData~1%7BbdtPolicyId%7D'

# The path segment is left not following the naming convention as defined in 3GPP TS 29.501 due to backward compatibility consideration.

**\*\*\*\*\*\*\*\*\*\* skipped for clarity \*\*\*\*\*\*\*\*\*\***

 /application-data/iptvConfigData:

 $ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1iptvConfigData'

# The path segment is left not following the naming convention as defined in 3GPP TS 29.501 due to backward compatibility consideration.

 /application-data/iptvConfigData/{configurationId}:

 $ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1iptvConfigData~1%7BconfigurationId%7D'

# The path segment is left not following the naming convention as defined in 3GPP TS 29.501 due to backward compatibility consideration.

**\*\*\*\*\*\*\*\*\*\* skipped for clarity \*\*\*\*\*\*\*\*\*\***

 /application-data/serviceParamData:

 $ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1serviceParamData'

# The path segment is left not following the naming convention as defined in 3GPP TS 29.501 due to backward compatibility consideration.

 /application-data/serviceParamData/{serviceParamId}:

 $ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1serviceParamData~1%7BserviceParamId%7D'

# The path segment is left not following the naming convention as defined in 3GPP TS 29.501 due to backward compatibility consideration.

**\*\*\*\*\*\*\*\*\*\* skipped for clarity \*\*\*\*\*\*\*\*\*\***

\* \* \* Next Change \* \* \* \*

## A.3 Nudr\_GroupIDmap API

openapi: 3.0.0

**\*\*\*\*\*\*\*\*\*\* skipped for clarity \*\*\*\*\*\*\*\*\*\***

paths:

 /nf-group-ids:

 get:

 summary: Retrieves NF-Group IDs for provided Subscriber and NF types

 operationId: GetNfGroupIDs

 tags:

 - NF Group IDs (Document)

 parameters:

 - name: nf-type

 in: query

 description: Type of NF

 required: true

 style: form

 explode: false

 schema:

 type: array

 items:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/NFType'

 minItems: 1

 - name: subscriberId

# The name of this query parameter is left not following the naming convention as defined in 3GPP TS 29.501 due to backward compatibility consideration.

 in: query

 description: Identifier of the subscriber

 required: true

 schema:

 $ref: '#/components/schemas/SubscriberId'

 responses:

 '200':

 description: Expected response to a valid request

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NfGroupIdMapResult'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 default:

 description: Unexpected error

**\*\*\*\*\*\*\*\*\*\* skipped for clarity \*\*\*\*\*\*\*\*\*\***

\* \* \* End of Changes \* \* \* \*