**3GPP TSG-CT WG4 Meeting #108-eC4-221087**

**E-Meeting, 17th – 25th February 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.503** | **CR** | **0811** | **rev** | **-** | **Current version:** | **16.10.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Nssaa feature description |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | eNS |  | ***Date:*** | 2022-02-08 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Description of the Nssaa feature in table 6.1.8-1 does not address Subscribe response messages containing an immediate report and does not address notification messages. |
|  |  |
| ***Summary of change:*** | Clarify that UDM behaviour for subscribe response messages and notification messages when the NF consumer does not support the Nssaa feature |
|  |  |
| ***Consequences if not approved:*** | Incomplete feature description |
|  |  |
| ***Clauses affected:*** | 6.1.6.2.2, 6.1.8 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | No impact to OpenAPI |
|  |  |
| ***This CR's revision history:*** |  |

**\*\*\*\*\*\*\***

\* \* \* First Change \* \* \* \*

##### 6.1.6.2.2 Type: Nssai

Table 6.1.6.2.2-1: Definition of type Nssai

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| supportedFeatures | SupportedFeatures | O | 0..1 | See clause 6.1.8 |  |
| defaultSingleNssais | array(Snssai) | M | 1..N | A list of Single Nssais used as default. (NOTE) |  |
| singleNssais | array(Snssai) | O | 1..N | List of non default Single Nssais. (NOTE) |  |
| provisioningTime | DateTime | C | 0..1 | This attribute shall be present if the Nssai is sent to the AMF while reception has not yet been acknowledged from the UE; otherwise shall be absent.This attribute serves as Network Slicing Subscription Change Indication. |  |
| additionalSnssaiData | map(AdditionalSnssaiData) | O | 1..N | A map (list of key-value pairs where singleNssai converted to string serves as key) of additional information related to this single Nssai. | Nssaa |
| NOTE: If the NF consumer does not support Nssaa optional feature, the UDM shall not include S-NSSAI(s) subject to Network Slice-Specific Authentication and Authorization in Get response messages, immediate reports within Subscribe response messages, or data change notifications where the data change is limited to S-NSSAI(s) subject to Network Slice-Specific Authentication and Authorization |

\* \* \* Next Change \* \* \* \*

### 6.1.8 Feature Negotiation

The optional features in table 6.1.8-1 are defined for the Nudm\_SDM API. They shall be negotiated using the extensibility mechanism defined in clause 6.6 of 3GPP TS 29.500 [4].

Table 6.1.8-1: Supported Features

|  |  |  |
| --- | --- | --- |
| Feature number | Feature Name | Description |
| 1 | SharedData | When receiving a Nudm\_SDM\_Get service operation request to retrieve a UE's individual subscription data, and the request does not contain a supported-features query parameter indicating support of this feature, the UDM shall not include Shared Data Ids in the response. Instead the UDM may – based on operator policy – take no further action (i.e. allow the UE to get services based on only the UE's individual subscription data), or send the shared data as individual data (this may result in notifications of individual subscription data change – if so subscribed – when shared data, which are sent as individual data, are modified, and/or when the UE's Shared Data IDs are modified). |
| 2 | ImmediateReport | When a NF consumer detects the UDM support ImmediateReport feature, it can indicate an immediateReport flag when invoking Nudm\_SDM\_Subscribe service operation. If UDM supports ImmediateReport received Nudm\_SDM\_Subscribe service operation request, it shall return the resource representation(s) of the monitored resource(s) in the service operation response body. |
| 3 | PatchReport | If some of the modifications included in the PATCH request are not successfully implemented, the UDM reports the result of PATCH request execution to the consumer. See clause 5.2.7.2 of 3GPP TS 29.500 [4]. |
| 4 | Nssaa | If the NF consumer does not support this feature, the UDM shall not include information of S-NSSAI(s) subject to Network Slice-Specific Authentication and Authorization in Get response messages, immediate reports within Subscribe response messages, or data change notifications where the data change is limited to S-NSSAI(s) subject to Network Slice-Specific Authentication and Authorization |
| 5 | CAGFeature | If the NF consumer does not support this feature, the UDM shall not include CAG information list in the message body with "200 OK" response (clause 5.2.2.2.3). The UDM performs action as executes step 2c of clause 5.3.2.2.2 and 5.3.2.2.3 if UE is allowed to access 5GS via CAG cell(s) only. |

\* \* \* End Of Change \* \* \* \*