**3GPP TSG-RAN WG1 Meeting # 100bis-e *R1-200xxxx***

**e-Meeting, April 20th – 30th, 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.213** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **15.9.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | NR\_newRAT-Core |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | For NR-DC, according to LS R1-1907956 in RAN1#97, RAN1 agreed that *pdcch-BlindDetectionMCG-UE* + *pdcch-BlindDetectionSCG-UE* >= the maximum number of DL serving cells over CGs that UE can support if the UE does not report *pdcch-BlindDetectionCA*.The maximum number of DL serving cells over CGs that UE can support is determined by the UE capability *UE-MRDC-Capability*, which is specified in TS38.306. However, the corresponding spec in TS38.213 refers the maximum number of DL serving cells over CGs that UE can support to TS38.133. TS38.133 specifies the maximum number of serving carriers for NR-DC from the perspective of applicability of requirements (as shown below).**3.6.2.4 Number of serving carriers for NR-DC**Requirements for NR-DC are applicable for the UE configured with the following number of serving NR CCs:- up to 2 NR DL CCs in total in FR1, up to 8 NR DL CCs in total in FR2, with 1 in PCell, 1 UL in PSCell, and up to 1 UL in each SCell.Referring the maximum number of DL serving cells over CGs that UE can support to TS38.133 is ambiguous. |
|  |  |
| ***Summary of change:*** | Following the similar description for NR CA in Section 10 of TS38.213, this CR is to refer the maximum number of DL serving cells over CGs that UE can support to UE capability *UE-MRDC-Capability*. |
|  |  |
| ***Consequences if not approved:*** | The definition of the maximum number of DL serving cells over CGs that UE can support is not clear. |
|  |  |
| ***Clauses affected:*** | 10 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | **Isolated impact analysis:**This CR is based on RAN1’s common understanding, which has no impact on UE behavior.  |
|  |  |
| ***This CR's revision history:*** | This is the second version for this CR, the first version is in R1-2001610. |

# 10 UE procedure for receiving control information

If the UE is configured with a SCG, the UE shall apply the procedures described in this clause for both MCG and SCG except for PDCCH monitoring in Type0/0A/2-PDCCH CSS sets where the UE is not required to apply the procedures in this clause for the SCG

- When the procedures are applied for MCG, the terms 'secondary cell', 'secondary cells' , 'serving cell', 'serving cells' in this clause refer to secondary cell, secondary cells, serving cell, serving cells belonging to the MCG respectively.

- When the procedures are applied for SCG, the terms 'secondary cell', 'secondary cells', 'serving cell', 'serving cells' in this clause refer to secondary cell, secondary cells (not including PSCell), serving cell, serving cells belonging to the SCG respectively. The term 'primary cell' in this clause refers to the PSCell of the SCG.

A UE monitors a set of PDCCH candidates in one or more CORESETs on the active DL BWP on each activated serving cell configured with PDCCH monitoring according to corresponding search space sets where monitoring implies decoding each PDCCH candidate according to the monitored DCI formats.

For monitoring of a PDCCH candidate in a slot

- If the UE has received *ssb-PositionsInBurst* in *SIB1* and has not received *ssb-PositionsInBurst* in *ServingCellConfigCommon* for a serving cell and if the UE does not monitor PDCCH candidates in a Type0-PDCCH CSS set and at least one RE for a PDCCH candidate overlaps with at least one RE corresponding to a SS/PBCH block index provided by *ssb-PositionsInBurst* in *SIB1*, the UE is not required to monitor the PDCCH candidate.

- If a UE has received *ssb-PositionsInBurst* in *ServingCellConfigCommon* for a serving cell and if the UE does not monitor PDCCH candidates in a Type0-PDCCH CSS set and at least one RE for a PDCCH candidate overlaps with at least one RE corresponding to a SS/PBCH block index provided by *ssb-PositionsInBurst* in *ServingCellConfigCommon*, the UE is not required to monitor the PDCCH candidate.

- If the UE monitors the PDCCH candidate for a Type0-PDCCH CSS set on the serving cell according to the procedure described in Subclause 13, the UE may assume that no SS/PBCH block is transmitted in REs used for monitoring the PDCCH candidate on the serving cell.

- If at least one RE of a PDCCH candidate on the serving cell overlaps with at least one RE of *lte-CRS-ToMatchAround*, the UE is not required to monitor the PDCCH candidate.

If a UE indicates in *UE-NR-Capability* a carrier aggregation capability larger than 4 serving cells, the UE includes in *UE-NR-Capability* an indication for a maximum number of PDCCH candidates the UE can monitor per slot when the UE is configured for carrier aggregation operation over more than 4 cells. When a UE is not configured for NR-DC operation, the UE determines a capability to monitor a maximum number of PDCCH candidates per slot that corresponds to  downlink cells, where

-  is the number of configured downlink cells if the UE does not provide *pdcch-BlindDetectionCA*

- otherwise,  is the value of *pdcch-BlindDetectionCA*

When a UE is configured for NR-DC operation, the UE determines a capability to monitor a maximum number of PDCCH candidates per slot that corresponds to  downlink cells for the MCG where  is provided by *pdcch-BlindDetection* for the MCG and determines a capability to monitor a maximum number of PDCCH candidates per slot that corresponds to  downlink cells for the SCG where  is provided by *pdcch-BlindDetection* for the SCG. When the UE is configured for carrier aggregation operation over more than 4 cells, or for a cell group when the UE is configured for NR-DC operation, the UE does not expect to monitor per slot a number of PDCCH candidates that is larger than the maximum number as derived from the corresponding value of .

When a UE is configured for NR-DC operation with a total of downlink cells on both the MCG and the SCG, the UE expects to be provided *pdcch-BlindDetection* for the MCG and *pdcch-BlindDetection* for the SCG with values that satisfy

- *pdcch-BlindDetection* for the MCG + *pdcch-BlindDetection* for the SCG <= *pdcch-BlindDetectionCA*, if the UE reports *pdcch-BlindDetectionCA*, or

- *pdcch-BlindDetection* for the MCG + *pdcch-BlindDetection* for the SCG <= , if the UE does not report *pdcch-BlindDetectionCA*.

For NR-DC operation, the UE may indicate, through *pdcch-BlindDetectionMCG-UE* and *pdcch-BlindDetectionSCG-UE*, respective maximum values for *pdcch-BlindDetection* for the MCG and *pdcch-BlindDetection* for the SCG.

If the UE reports *pdcch-BlindDetectionCA*,

- the value range of *pdcch-BlindDetectionMCG-UE* or of *pdcch-BlindDetectionSCG-UE* is [1, …, *pdcch-BlindDetectionCA*-1], and

- *pdcch-BlindDetectionMCG-UE* + *pdcch-BlindDetectionSCG-UE* >= *pdcch-BlindDetectionCA*.

Otherwise, if  is a maximum total number of downlink cells that the UE can be configured on both the MCG and the SCG for NR-DC as indicated in *UE-MRDC-Capability*,

- the value range of *pdcch-BlindDetectionMCG-UE* or of *pdcch-BlindDetectionSCG-UE* is [1, 2, 3], and

- *pdcch-BlindDetectionMCG-UE* + *pdcch-BlindDetectionSCG-UE* >= .