**3GPP TSG-RAN WG1 #100bis-e R1-20xxxxx**

**e-Meeting, April 20th – 30th, 2020**

**Source: Ericsson**

**Title: Summary of email discussion [100b-e-NR- LTE\_NR\_DC\_CA-ScellDormancy-01]**

**Agenda item:** **7.2.10.3**

**Document for:** **Discussion and Decision**

# 1 Introduction

This document provides summary of email discussion [100b-e-NR- LTE\_NR\_DC\_CA-ScellDormancy-01] on following TPs discussed during preparation phase of RAN1#100bis-eMeeting

Below are the TPs identified in [R1-2002739](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_100b_e/Inbox/R1-2002739.zip) [1]

* TP (from R1-2001542) to 38.212 on FDRA for Case2 dormancy indication for dynamic RA type indication
* TP (from R1-2002149) to 38.213 on DCI indication for configured SCells with dormant BWP
* TP (from R1-2002228) to 38.213 on aligning with RAN2 agreements on UL dormancy handling
* TP (from R1-2001542) to 38.213 on wording for SCell dormancy “without scheduling PDSCH”

# 2. Discussion

### 2.1 TP1

--------------------------------- Start TP1 for TS 38.212 sub-clause 7.3.1.2.2 ---------------------------------------

**7.3.1.2.2 Format 1\_1**

<Unchanged parts omitted>

- SCell dormancy indication – 0 bit if higher layer parameter *Scell-groups-for-dormancy-within-active-time* is not configured; otherwise 1, 2, 3, 4 or 5 bits bitmap determined according to higher layer parameter *Scell-groups-for-dormancy-within-active-time,* where each bit corresponds to one of the SCell group(s) configured by higher layers parameter *Scell-groups-for-dormancy-within-active-time,* with MSB to LSB of the bitmap corresponding to the first to last configured SCell group. The field is only present when this format is carried by PDCCH on the primary cell within DRX Active Time and the UE is configured with at least two DL BWPs for an SCell.

If all bits of frequency domain resource assignment are set to 0 for resource allocation type 0 or set to 1 for resource allocation type 1 or set to 0 or 1 for dynamic switch resource allocation type, this field is reserved and the following fields among the fields above are used for SCell dormancy indication, where each bit corresponds to one of the configured SCell(s), with MSB to LSB of the following fields concatenated in the order below corresponding to the SCell with lowest to highest SCell index

- Modulation and coding scheme of transport block 1

- New data indicator of transport block 1

- Redundancy version of transport block 1

- HARQ process number

- Antenna port(s)

<Unchanged parts omitted>

--------------------------------- End TP1 for TS 38.212 sub-clause 7.3.1.2.2 ----------------------------------------

Q: Is it OK to agree to above TP1 for 38.212 sub-clause 7.3.1.2.2?

*Note: For background related to the TP, please see [2]*

Please provide your input preferably by 04/21 (evening PST).

|  |  |  |
| --- | --- | --- |
| **Company Name** | **Yes/No** | **Comments (TP1)** |
| vivo | Partially Yes | DMRS sequence initialization should not be removed, it has been present in 38.213 section 10.3. So we should just remove the bracket to be consistent with 38.213.  |
|  |  |  |

### 2.2 TP2

--------------------------------- Start TP2 for TS 38.213 sub-clause 10.3 ---------------------------------------

If a UE is provided search space sets to monitor PDCCH for detection of DCI format 1\_1, and if

- the CRC of DCI format 1\_1 is scrambled by a C-RNTI or a MCS-C-RNTI, and if

- *resourceAllocation* = *resourceAllocationType0* and all bits of the frequency domain resource assignment field in DCI format 1\_1 are equal to 0, or

- *resourceAllocation* = *resourceAllocationType1* and all bits of the frequency domain resource assignment field in DCI format 1\_1 are equal to 1

- *resourceAllocation = dynamicSwitch* and all bits of the frequency domain resource assignment field in DCI format 1\_1 are equal to 0 or 1

the UE considers the DCI format 1\_1 as indicating SCell dormancy, not scheduling a PDSCH reception or indicating a SPS PDSCH release, and for transport block 1 interprets the sequence of fields of

- modulation and coding scheme

- new data indicator

- redundancy version

and of

- HARQ process number

- antenna port(s)

- DMRS sequence initialization

as providing a bitmap to each configured SCell with a DL BWP provided by *dormant-BWP*, in an ascending order of the SCell index, where

- a '0' value for a bit of the bitmap indicates an active DL BWP, provided by *dormant-BWP*, for the UE for a corresponding activated SCell

- a '1' value for a bit of the bitmap indicates

- an active DL BWP, provided by *first-non-dormant-BWP-ID-for-DCI-inside-active-time*, for the UE for a corresponding activated SCell, if a current active DL BWP is the dormant DL BWP

- a current active DL BWP, for the UE for a corresponding activated SCell, if the current active DL BWP is not the dormant DL BWP

- the UE sets the active DL BWP to the indicated active DL BWP

<Unchanged parts omitted>

--------------------------------- end TP2 for TS 38.213 sub-clause 10.3 ---------------------------------------

Q: Is it OK to agree to above TP2 for 38.213 sub-clause 10.3?

*Note: For background related to the TP, please see [3]*

Please provide your input preferably by 04/21 (evening PST).

|  |  |  |
| --- | --- | --- |
| **Company Name** | **Yes/No** | **Comments (TP2)** |
| vivo  | Yes |  |
|  |  |  |

### 2.2 TP3

--------------------------------- Start TP3 for TS 38.213 sub-clause 12 ---------------------------------------

12 Bandwidth part operation

<Unchanged parts omitted>

For unpaired spectrum operation, a non-dormant DL BWP from the set of configured DL BWPs with index provided by BWP-Id is linked with an UL BWP from the set of configured UL BWPs, with index provided by BWP-Id when the DL BWP index and the UL BWP index are same. For unpaired spectrum operation, a UE does not expect to receive a configuration where the center frequency for a DL BWP is different than the center frequency for an UL BWP when the BWP-Id of the DL BWP is same as the BWP-Id of the UL BWP.

<Unchanged parts omitted>

--------------------------------- end TP3 for TS 38.213 sub-clause 12 ---------------------------------------

Q: Is it OK to agree to above TP3 for 38.213 sub-clause 12?

*Note: For background related to the TP, please see [4]*

Please provide your input preferably by 04/21 (evening PST).

|  |  |  |
| --- | --- | --- |
| **Company Name** | **Yes/No** | **Comments (TP3)** |
| vivo | Yes |  |
|  |  |  |

### 2.2 TP4

--------------------------------- Start TP4 for TS 38.213 sub-clause 9.1---------------------------------------

**9.1 HARQ-ACK codebook determination**

<Unchanged parts omitted>

In the remaining of this Clause, reference is to one HARQ-ACK codebook.

If a UE detects a DCI format 1\_1 indicating

- SCell dormancy without scheduling PDSCH, as described in Clause 10.3, and

- is provided *pdsch-HARQ-ACK-Codebook = dynamic*

the UE generates a HARQ-ACK information bit as described in Clause 9.1.3 for a DCI format 1\_1 indicating SCell dormancy and the HARQ-ACK information bit value is ACK.

If a UE is not provided *PDSCH-CodeBlockGroupTransmission*, the UE generates one HARQ-ACK information bit per transport block.

<Unchanged parts omitted>

--------------------------------- Start TP4 for TS 38.213 sub-clause 9.1---------------------------------------

Q: Is it OK to agree to above TP4 for 38.213 sub-clause 9.1?

*Note: For background related to the TP, please see [2]*

Please provide your input preferably by 04/21 (evening PST).

|  |  |  |
| --- | --- | --- |
| **Company Name** | **Yes/No** | **Comments (TP4)** |
| vivo | Yes |  |
|  |  |  |

# 3 Conclusions

To be updated later

# References

1. [R1-2002739](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_100b_e/Inbox/R1-2002739.zip) Summary of efficient and low latency serving cell configuration/activation/setup, Moderator (Ericsson), RAN1#100bis-e, April 2020.
2. [R1-2001542](http://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_100b_e/Docs/R1-2001542.zip) Remaining issues on SCell dormancy indication Huawei, HiSilicon
3. [R1-2002149](http://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_100b_e/Docs/R1-2002149.zip) Remaining issues on dormancy Scell Samsung
4. [R1-2002228](http://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_100b_e/Docs/R1-2002228.zip) Remaining issues on Efficient CA design Nokia, Nokia Shanghai Bell