**3GPP TSG RAN WG1 #100bis-e R1-2002458**

e-Meeting, April 20th – 30th, 2020

Source: NTT DOCOMO, INC.

Title: Summary on UE features for NR-U

Agenda Item: 7.2.11.2

**Document for:** **Discussion and Decision**

# **Introduction**

This contribution summarizes the discussions and proposals in AI 7.2.11.2 regarding UE features for NR-U.

In R1-2001484 [1] which is the version after [100e-NR-Rel-16-UEFeatures] email discussion, there are following feature groups for NR-U.

* 10-1 UE stand-alone (DL and UL) operation in shared spectrum under dynamic channel access mode
* 10-1a UE DL only operation in shared spectrum under dynamic channel access mode
* 10-2 UE stand-alone (DL and UL) operation in shared spectrum under semi-static channel access mode
* 10-2a UE DL only operation in shared spectrum under semi-static channel access mode
* 10-2b UE stand-alone (DL and UL) operation in shared spectrum under semi-static channel access mode (Support fixed frame periods shorter than 5ms)
* 10-3 PRB interlace mapping for PUSCH
* 10-3a PRB interlace mapping for PUCCH format 0 and format 1
* 10-3b PRB interlace mapping for PUCCH format 2
* 10-3c PRB interlace mapping for PUCCH format 3
* 10-7 LBT bandwidth size of 10MHz
* 10-8 Type B PDSCH length
* 10-9 Search space set group switching with explicit DCI 2\_0 bit field trigger
* 10-9a Search space set group switching with implicit PDCCH decoding with DCI 2\_0 monitoring
* 10-9b Search space set group switching with implicit PDCCH decoding without DCI 2\_0 monitoring
* 10-9c Joint search space group switching across multiple cells
* 10-10 RSSI and channel occupancy measurement and reporting
* 10-11 SRS starting position at any OFDM symbol in a slot
* [10-12] OCC for PRB interlace mapping for PF2 and PF3
* [10-13a] Extended CP range of more than one symbol for CG-PUSCH
* 10-14 Non-numerical PDSCH to HARQ-ACK timing
* 10-15 Enhanced dynamic HARQ codebook
* 10-16 One-shot HARQ ACK feedback
* 10-16a One-shot HARQ ACK feedback trigger with empty DCI 1\_1
* 10-17 Multi-PUSCH UL grant
* 10-18 Configured grant with retransmission in CG resources
* [10-19] Number of LBT bandwidth
* 10-19a Support DL reception with subset of RB sets
* 10-19b Support UL transmission with subset of RB sets passing LBT
* [10-19c] Support intra-cell guard band(s) for DL carrier BW > 20MHz
* 10-20 Support search space set configuration with freqMonitorLocation-r16
* 10-20a Support coreset configuration with rb-Offset
* 10-21 Support using ED threshold for UL to DL COT sharing
* 10-22 No gap 2-step RACH msgA transmission
* 10-23 CGI reading based on off-sync raster SSB for ANR functionality
* 10-24 CG-UCI multiplexing with HARQ ACK
* 10-25 Enable configured UL transmission out of COT
* 10-26 CSI-RS based RLM outside of discovery burst transmission window
* 10-27 Wideband PRACH
* 10-28 Configured grant with Rel-16 enhanced resource configuration
* 10-29 Support available RB set indicator field in DCI 2\_0
* 10-30 Support channel occupancy duration indicator field in DCI 2\_0
* [10-31] Support of CSI-RS measurements for CSI reporting and tracking without COT duration from DCI 2\_0

Based on the discussions summarized in Section 2-21, following is the suggested list of issues to be discussed and priority order considering RAN2 impact especially for capability signaling design.

**FL proposal of list of issues/proposals and priority:**

**1st priority issues (basic FGs definition):**

* **10-1 to 10-2b**
	+ **How to define basic FGs which support all deployment scenarios**
		- **Options 1 or 2 stated below can be the starting point to discuss**
			* **Option 1: define new basic FGs in addition to current basic FGs to support all deployment scenarios (e.g., [3] and [5])**
			* **Option 2: define new basic FGs with components that have tightly related functionality to replace current basic FGs (e.g., [8])**

**2nd priority issues (such as a certain FG is necessary or not):**

* **10-1 to 10-2b**
	+ **Whether or not following FGs can be included in basic FGs**
		- **10-3, 10-11, 10-14, 10-15, 10-16, 10-16a, 10-17, 10-18, 10-19, 10-20, 10-20a, 10-24, 10-25, 10-28, 10-29, 10-30**
	+ **Whether or not “Support fixed frame period of 5ms and 10ms” and “Support fixed frame periods shorter than 5ms” can be separate capabilities.**
	+ **Whether or not “Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_0” can be separate capability from basic FGs**
	+ **Whether or not “Type 2B channel access” can be separate capability from basic FGs**
* **10-3 to 10-3b and [10-12]**
	+ **Whether or not 10-3/10-3a/10-3b/10-3c can be combined into a single FG**
	+ **Whether or not 10-12 can be combined into 10-3b/10-3c**
		- **If not, whether or not 10-12 can be split for PF2 and PF3 separately**
* **10-8**
	+ **Whether or not the capability are separate for each length or some groups are formed to signal the capability together**
* **10-9 to 10-9c**
	+ **Whether or not 10-9/9a/9b/9c can be combined into a single FG**
* **[10-13a]**
	+ **Whether or not 10-13a is needed as a FG**
* **10-14 to 10-17**
	+ **Whether or not 10-14/10-15/10-16/10-16a/10-17 can be combined into a single FG**
		- **If no, whether or not 10-15 can be further split under other group DAI/NFI configured or not**
* **10-18, 10-24 and 10-28**
	+ **Whether or not 10-18/10-24/10-28 can be combined into a single FG**
* **[10-19] to [10-19c]**
	+ **Whether or not 10-19/10-19a/10-19b/10-19c are needed**
* **10-21**
	+ **Whether or not following update can be applied**

|  |  |  |
| --- | --- | --- |
| 10-21a | Support using ED threshold for UL to DL COT sharing | 1. Use ULtoDL-CO-SharingED-Threshold-r16 for cat 4 LBT for scheduled UL to share COT with gNB for DL2. Use ULtoDL-CO-SharingED-Threshold-r16 for cat 4 LBT for CG-PUSCH to share COT with gNB for DL3. Indicate in CG-UCI the COT sharing information |
| 10-21b | Support UL to DL COT sharing | 1. Support cat 4 LBT for scheduled UL to share COT with gNB for DL without ULtoDL-CO-SharingED-Threshold-r162. Support cat 4 LBT for CG-PUSCH to share COT with gNB for DL without ULtoDL-CO-SharingED-Threshold-r163. Indicate in CG-UCI the COT sharing information |

* **10-22**
	+ **Whether or not 10-22 is needed**
* **10-26**
	+ **Whether or not 10-26 is needed**
* **[10-31]**
	+ **Whether or not 10-31 is needed**
* **Confirm following updates that seem acceptable**
	+ **10-3 to 10-3b**
		- **10-3/10-3a/10-3b/10-3c are used only for unlicensed band**
	+ **10-14 to 10-16a**

|  |  |  |
| --- | --- | --- |
| 10-14 | Non-numerical PDSCH to HARQ-ACK timing | 1. Support configuration of a value for dl-DataToUL-ACK indicating an i~~m~~napplicable time to report HARQ ACK |
| 10-15 | Enhanced dynamic HARQ codebook | 1. Support of bit fields signalling PDSCH HARQ group index and NFI in DCI 1\_12. Support of bit field in DCI 0\_1 and DCI 1\_1 for other group total DAI if configured. 3. Support the retransmission of HARQ ACKFFS if need to further split under other group DAI/NFI configured or not |
| 10-16 | One-shot HARQ ACK feedback | 1. Support feedback of type 3 HARQ-ACK codebook, triggered by a DCI 1\_1 scheduling a PDSCH |
| 10-16a | One-shot HARQ ACK feedback trigger with empty DCI 1\_1 | 1. Support feedback of type 3 HARQ-ACK codebook triggered by a DCI 1\_1 without scheduling a PDSCH using a reserved FDRA value |

* + **10-18, 10-24 and 10-28**
		- **10-18/10-24/10-28 are used for unlicensed band only.**
	+ **10-20**
		- **10-20 is used for unlicensed band only**

**3rd priority issues (such as components and type that have capability signaling impacts):**

* **10-7**
	+ **Whether or not 10-7 can be updated as follows**

|  |  |  |
| --- | --- | --- |
| 10-7 | ~~LBT bandwidth size of 10MHz~~UL channel access for 10 MHz SCell  | ~~FFS the components~~1. 10 MHz LBT bandwidth |

* **10-8**
	+ **Whether or not 10-8 can be extended to licensed use**
* **10-9 to 10-9c**
	+ **Whether or not 10-9/9a/9b/9c can be extended to licensed use**
* **10-10**
	+ **Whether or not 10-10 can be per UE**
* **10-11**
	+ **Whether or not 10-11 can be extended to licensed use**
* **[10-13a]**
	+ **Whether or not 10-2 can be added as prerequisite FG for 10-13a if 10-13a is needed**
* **10-14 to 10-17**
	+ **Whether or not 10-14/10-15/10-16/10-16a/10-17 can be extended to licensed use**
* **10-18**
	+ **Whether or not 10-18 can be removed from prerequisite of 10-28 if 10-18 and 10-28 are not combined into a single FG**
* **10-20 and 10-20a**
	+ **Whether or not the component of 10-20 can be changed to “Maximum number of frequency domain locations for a search space set configuration with *freqMonitorLocations-r16*”**
	+ **Whether or not 10-20a can be extended to licensed use**
		- **If no, whether or not 10-20a can be prerequisites for 10-20**
* **10-23**
	+ **Whether or not following update can be applied**

|  |  |  |
| --- | --- | --- |
| 10-23 | CGI reading ~~based on off-sync raster SSB~~of an unlicensed cell for ANR functionality | 1. Support acquisition of relevant information from a neighbouring NR unlicensed cell in an unlicensed carrier by reading the RMSI of the neighbouring unlicensed cell and reporting the acquired information to the network |

* **10-25**
	+ **Whether or not following update can be applied**

|  |  |  |
| --- | --- | --- |
| 10-25 | Enable configured UL transmissions when SFI is configured but not detected ~~out of COT~~ | 1. Support configuration of enableConfiguredUL-r16 and enable ~~Cat 4 LBT based~~ transmission of ~~RRC~~higher-layer configured UL \*SRS, PUCCH, CG-PUSCH etc) ~~out of COT~~ when SFI~~DCI 2\_0~~ is configured but not detected |

* **10-29 and 10-30**
	+ **Whether or not 10-30 or 3-6 can be prerequisite FGs for 10-29**

Companies are encouraged to check above FL proposals and to provide feedback if any in below.

|  |  |
| --- | --- |
| Company | Comment |
| vivo | Regarding the NRU feature discussion priority, we think the 2nd set (i.e. definition of each FG) is actually more important as it has direct impact to the capability signaling design. The 1st set (i.e. the basic FGs for each deployment scenario) can be either discussed in parallel or after the definition of each FG is completed as it is possible to be achieved without signaling impact, e.g. by adding some note to each of the basic FG for each deployment scenario. Therefore we propose to reverse the priority order or at least make them as equal priority. |
| Ericsson | We agree with the FL’s recommendation that it is important to decide on the approach used to define the basic FGs; this will affect much of the remaining discussion. We also agree that it is important to define what goes inside those basic FGs, and which FGs should remain separate. Hence, some of the 2nd priority issues listed by the FL are related to the 1st priority issue. We think these can be discussed in parallel. Making some progress in those areas will help RAN2 with the signaling design. |
|  |  |

# **10-1 to 10-2b: Possible basic feature groups for operating in unlicensed band and their related feature group**

In [1], FGs 10-1 to 10-2b are captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-1 | UE stand-alone (DL and UL) operation in shared spectrum under dynamic channel access mode  | 1. Type 1 channel access2. Type 2A channel access3. Type 2B channel access (FFS if move this to separate feature)4. Type 2C channel access5. 20MHz LBT bandwidth6. Contention window adjustment7. CP extension up to 1 symbol for PUSCH/PUCCH transmission8. SSB/MIB/RMSI reception with Q9. SSB RRM with Q in DMTC10. SSB-RLM with Q in DMTC window11. Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_0 |  |  | N/A |  | Per band | N/A | N/A |  | This can be a basic feature group for operating in unlicensed band with both DL and UL transmission support under dynamic channel access | Optional with capability signalling |
| 10-1a | UE DL only operation in shared spectrum under dynamic channel access mode | 1. SSB RRM with Q in DMTC | 6-5 |  | N/A |  | Per band | N/A | N/A |  | This can be a basic feature group for operating in unlicensed band with DL only operation | Optional with capability signalling |
| 10-2 | UE stand-alone (DL and UL) operation in shared spectrum under semi-static channel access mode  | 1. Type 2C channel access2. Single sensing slot of 9us channel access3. 20MHz LBT bandwidth4. SSB/MIB/RMSI reception with Q5. SSB RRM with Q in DMTC6. SSB-RLM with Q in DMTC window7. Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_08. Support fixed frame period of 5ms and 10ms |  |  | N/A |  | Per band | N/A | N/A |  | This can be a basic feature group for operating in unlicensed band.Support of channel access mechanism for FBE operation, including fixed frame period, Cat 2 LBT, Cat 1 LBT | Optional with capability signalling |
| 10-2a | UE DL only operation in shared spectrum under semi-static channel access mode | 1. SSB RRM with Q in DMTC2. Support fixed frame period of 5ms and 10ms | 6-5 |  | N/A |  | Per band | N/A | N/A |  | This can be a basic feature group for operating in unlicensed band with DL only operation | Optional with capability signalling |
| 10-2b | UE stand-alone (DL and UL) operation in shared spectrum under semi-static channel access mode  | 1. Support fixed frame periods shorter than 5ms | 10-2 or 10-2a |  | N/A |  | Per band | N/A | N/A |  |  | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [2] | ZTE, Sanechips | For NR-U, depending on different use scenarios, there could be multiple basic feature groups defined for UE to support LBE mode (DL+UL), FBE mode (DL+UL), LBE mode (DL only) and FBE mode (DL only), respectively. The different operation modes can be regarded as different sub-features for the NR-U feature.Each basic feature group includes multiple components that are essential for the UE to support the sub-feature. Other optional feature groups can use one or multiple of the above basic feature groups as prerequisite. One thing could be further discussed is that whether or not to include more components to the basic feature group, for example the supported enhancements on HARQ, configured grant, SRS and CORESET/SS. Those enhancements are used to compensate the potential loss of LBT failure in terms of efficiency and reliability, it may be useful to make these function as mandatory, at least for LBE mode.***Proposal 1:*** * ***Multiple basic feature groups can be defined for NR-U, corresponding to different operation modes.***
	+ ***Further discuss whether the enhancements on CORESET/SS, SRS, HARQ, CG can be merged into the basic feature group(s).***
 |
| [3] | vivo | In current table, different basic feature groups (i.e. 10-1, 10-1a, 10-2, 10-2a) are defined to support standalone and CA DL only scenario for LBE and FBE respectively. However, the scenario regarding CA DL+UL operation in unlicensed band is missing. Under this scenario, initial access related features are not needed as components in this basic feature group compared to standalone scenario. Therefore, the following should be added as separate basic feature groups: a) UE DL and UL operation in shared spectrum under dynamic channel access mode; b) UE DL and UL operation in shared spectrum under semi-static channel access mode.Proposal 3: Add the following two basic feature groups to NRU UE feature table.

|  |  |  |  |
| --- | --- | --- | --- |
| **Index** | **Feature group** | **Components** | **Prerequisite feature groups** |
| 10-1b | UE DL and UL operation in shared spectrum under dynamic channel access mode  | 1. Type 1 channel access2. Type 2A channel access3. Type 2B channel access (FFS if move this to separate feature)4. Type 2C channel access5. 20MHz LBT bandwidth6. Contention window adjustment7. CP extension up to 1 symbol for PUSCH/PUCCH transmission8. SSB RRM with Q in DMTC | 6-5 |
| 10-2c | UE DL and UL operation in shared spectrum under semi-static channel access mode | 1. Type 2C channel access2. Single sensing slot of 9us channel access3. 20MHz LBT bandwidth4. SSB RRM with Q in DMTC5. Support fixed frame period of 5ms and 10ms | 6-5 |

On **10-2a** (*UE DL only operation in shared spectrum under semi-static channel access mode*), we don’t see much difference with different FFP period for LAA DL only scenario. In LAA DL only case, UE only performed reception in shared spectrum and shorter FFP period doesn’t bring more complexity. Therefore, the component “Support fixed frame period of 5ms and 10ms” is not needed.Proposal 4: Remove component “Support fixed frame period of 5ms and 10ms” from 10-2a. |
| [4] | OPPO | **FG 10-1, 10-1a, 10-2, 10-2a**: SSB RRM with Q in DMTC, in NRU we should replace DMTC with SMTC. Moreover, SSB RLM with Q in DMTC, in NRU we should replace DMTC with discovery burst transmission window. Another point is that Type 2B channel access should not be a basic component. NRU can perfectly runs its function without having to implement Type 2B channel access.

|  |  |  |
| --- | --- | --- |
| 10-1 | UE stand-alone (DL and UL) operation in shared spectrum under dynamic channel access mode  | 1. Type 1 channel access2. Type 2A channel access3. ~~Type 2B channel access (FFS if move this to separate feature)~~4. Type 2C channel access5. 20MHz LBT bandwidth6. Contention window adjustment7. CP extension up to 1 symbol for PUSCH/PUCCH transmission8. SSB/MIB/RMSI reception with Q9. SSB RRM with Q in ~~DMTC~~ SMTC10. SSB-RLM with Q in ~~DMTC~~ discovery burst transmission window11. Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_0 |
| 10-1a | UE DL only operation in shared spectrum under dynamic channel access mode | 1. SSB RRM with Q in ~~DMTC~~ SMTC |
| 10-2 | UE stand-alone (DL and UL) operation in shared spectrum under semi-static channel access mode  | 1. Type 2C channel access2. Single sensing slot of 9us channel access3. 20MHz LBT bandwidth4. SSB/MIB/RMSI reception with Q5. SSB RRM with Q in ~~DMTC~~ SMTC6. SSB-RLM with Q in ~~DMTC~~ discovery burst transmission window7. Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_08. Support fixed frame period of 5ms and 10ms |
| 10-2a | UE DL only operation in shared spectrum under semi-static channel access mode | 1. SSB RRM with Q in ~~DMTC~~ SMTC2. Support fixed frame period of 5ms and 10ms |

**Proposal 1: Remove Type 2B channel access from basic feature group 10-1.**  |
| [5] | MediaTek Inc. | According to NR-U WID, Rel-16 NR-U aims to support the following deployment scenarios. However, with the current UE feature structure, it may not be feasible for UE to indicate its support for the deployments highlighted in yellow without excessive support of NR-U features. Scenario A specifies the carrier aggregation where NR-U serves as a secondary cell (SCell). In this scenario, UE should not be mandated to support procedures such as MIB/RMSI acquisition, RACH, and RLM in an unlicensed cell. In Scenario D where NR-R stand-alone operation is targeted but only DL is in unlicensed and UL is in licensed band. In this case, UE should support initial access procedures but does not have to support uplink features such as channel access procedures or interlaced resource mapping. Therefore, the corresponding basic feature groups should be defined for it. Alternatively, we can discuss whether this scenario should be supported. * Scenario A: Carrier aggregation between licensed band NR (PCell) and NR-U (SCell).
	+ NR-U SCell may have both DL and UL, or DL-only.
	+ In this scenario, NR PCell is connected to 5G-CN.
* Scenario B: Dual connectivity between licensed band LTE (PCell) and NR-U (PSCell)
	+ In this scenario, LTE PCell connected to EPC as higher priority than PCell connected to 5G-CN.
* Scenario C: Stand-alone NR-U
	+ In this scenario, NR-U is connected to 5G-CN.
* Scenario D: A stand-alone NR cell in unlicensed band and UL in licensed band (single cell architecture).
	+ In this scenario, NR-U is connected to 5G-CN.
* Scenario E: Dual connectivity between licensed band NR and NR-U.
	+ In this scenario, PCell is connected to 5G-CN.

**Proposal 2: The NR-U UE feature list should make it possible that UE can indicate which NR-U deployment scenarios it is capable of supporting without excessive support of other NR-U features.** **Proposal 3: UE should not be mandated to support MIB/RMSI acquisition, RACH, and RLM when it only plans to support Scenario A specified in NR-U WID.** **Proposal 4: Add basic feature groups (10-1c and 10-2d added to the table below) for carrier aggregation between NR licensed (PCell) and NR-U (SCell) where the NR-U SCell have both DL and UL.** **Proposal 5: Add basic feature groups (10-1b and 10-2c added to the table below) for Scenario D or discuss whether Scenario D should be supported.**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 10-1b | UE stand-alone (DL only) operation in shared spectrum under dynamic channel access mode | 1. SSB/MIB/RMSI reception with *SSB-PositionQCL-Relationship*2. SSB RRM with *SSB-PositionQCL-Relationship* in DMTC3. SSB-RLM with *SSB-PositionQCL-Relationship* in DMTC window4. Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_05. Support monitoring DCI 2\_0 to read availableRB-Sets-r166. Support monitoring DCI 2\_0 to read CO duration |  |  | N/A |  | Per band | N/A | N/A |  | This can be a basic feature group for the Scenario D in NR-U WID | Optional with capability signalling  |
| 10-1c | UE DL and UL operation in shared spectrum under dynamic channel access mode | 1. Type 1 channel access2. Type 2A channel access3. Type 2B channel access (FFS if move this to separate feature)4. Type 2C channel access5. 20MHz LBT bandwidth6. Contention window adjustment7. CP extension up to 1 symbol for PUSCH/PUCCH transmission8. SSB RRM with *SSB-PositionQCL-Relationship* in DMTC9. Support monitoring DCI 2\_0 to read availableRB-Sets-r1610. Support monitoring DCI 2\_0 to read CO duration | 6-5 and 6-6 |  | N/A |  | Per band | N/A | N/A |  | This can be a basic feature group for operating in an unlicensed SCell with both DL and UL | Optional with capability signalling |
| 10-2c | UE stand-alone (DL only) operation in shared spectrum under semi-static channel access mode | 1. Type 2C channel access2. Single sensing slot of 9us channel access3. 20MHz LBT bandwidth4. SSB/MIB/RMSI reception with Q5. SSB RRM with Q in DMTC6. SSB-RLM with Q in DMTC window7. Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_08. FFS: Support fixed frame period of 5ms and 10ms9. Support monitoring DCI 2\_0 to read availableRB-Sets-r1610. Support monitoring DCI 2\_0 to read CO duration11. Invalidate RACH occasions that partially or fully fall within the idle period of a fixed frame period  |  |  |  |  |  |  |  |  | This can be a basic feature group for the Scenario D in NR-U WID | Optional with capability signalling  |
| 10-2d | UE DL and UL operation in shared spectrum under semi-static channel access mode | 1. Type 2C channel access2. Single sensing slot of 9us channel access3. 20MHz LBT bandwidth4. SSB RRM with Q =8 in DMTC5. UL transmission conditioned on the detection of DL transmission in the same fixed frame period6. FFS: Support fixed frame period of 5ms and 10ms | 6-5 and 6-6 |  |  |  |  |  |  |  | This can be a basic feature group for operating in an unlicensed SCell with both DL and UL | Optional with capability signalling  |

With the introduction of discovery burst transmission windows, the number of SSB positions that UE has to monitor for measurements and PBCH reading is increased dramatically especially for small Q values. In addition, PCI collision is no new issue in NR-U. LTE-LAA has the same issue. However, it is resolved by eNB without mandating UE to read and report CGI. **Proposal 6: For a UE that only supports NR-U as SCell (i.e. CA deployments in unlicensed operation), the UE is not required to read PBCH of an unlicensed cell.** HARQ procedures are essential for stand-alone operation. However, they are missing from the basic feature groups for stand-alone. **Proposal 10: Add the following HARQ components to the basic feature groups for stand-alone operation 10-1 and 10-2.** * **Non-numerical PDSCH to HARQ-ACK timing**
* **Enhanced dynamic HARQ-ACK codebook**

For FBE feature group 10-2b, it is not clear why FFP smaller than 5ms needs to be single out. So far we only have an agreement saying no SSB and corresponding PDSCH rate matching is required when an SSB falls within an idle period. But this does not evoke us that much difference between handling an FFP smaller than 5ms and handling an FFP not smaller than 5ms. **Proposal 11: Discuss whether we need 10-2b.** |
| [7] | Intel Corporation | It is proposed to clarify that the basic feature groups including 10-1, 10-1a, 10-2, and 10-2a are targeting unlicensed band in the FR1 regime in order to avoid unnecessary capability signaling to licensed band or FR2. Therefore, it is proposed to put the restriction of FR1 unlicensed band in the note of the basic feature groups as shown below:**Proposal 1: Put the restriction of FR1 unlicensed band in the note of 10-1, 10-1a, 10-2, and 10-2a.**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Index** | **Feature group** | **Components** | **Prerequisite feature groups** | **Type** | **Note** | **Mandatory/Optional** |
| 10-1 | UE stand-alone (DL and UL) operation in shared spectrum under dynamic channel access mode  | 1. Type 1 channel access2. Type 2A channel access3. Type 2B channel access (FFS if move this to separate feature)4. Type 2C channel access5. 20MHz LBT bandwidth6. Contention window adjustment7. CP extension up to 1 symbol for PUSCH/PUCCH transmission8. SSB/MIB/RMSI reception with Q9. SSB RRM with Q in DMTC10. SSB-RLM with Q in DMTC window11. Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_0 |  | Per band | This can be a basic feature group for operating only in FR1 unlicensed band with both DL and UL transmission support under dynamic channel access | Optional with capability signalling |
| 10-1a | UE DL only operation in shared spectrum under dynamic channel access mode | 1. SSB RRM with Q in DMTC | 6-5 | Per band | This can be a basic feature group for operating only in FR1 unlicensed band with DL only operation | Optional with capability signalling |
| 10-2 | UE stand-alone (DL and UL) operation in shared spectrum under semi-static channel access mode  | 1. Type 2C channel access2. Single sensing slot of 9us channel access3. 20MHz LBT bandwidth4. SSB/MIB/RMSI reception with Q5. SSB RRM with Q in DMTC6. SSB-RLM with Q in DMTC window7. Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_08. Support fixed frame period of 5ms and 10ms |  | Per band | This can be a basic feature group for operating only in FR1 unlicensed band with DL only operation | Optional with capability signalling |
| 10-2a | UE DL only operation in shared spectrum under semi-static channel access mode | 1. SSB RRM with Q in DMTC2. Support fixed frame period of 5ms and 10ms | 6-5 | Per band | This can be a basic feature group for operating only in FR1 unlicensed band with DL only operation | Optional with capability signalling |

It is OK to have 10-2 and 10-2a for both stand-alone operation and DL only operation. However, current table has different feature groups for stand-alone operation depending on the fixed frame period length. We do not have clear motivation to define additional feature groups for supporting small fixed frame period length. And this differentiation is only applied for stand-alone operation and not applied for DL only operation, which does not look desirable either.**Proposal 2: Remove 10-2b and change the 8th bullet of 10-2.**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Index | Feature group | Components | Prerequisite feature groups | **Type** | Note | Mandatory/Optional |
| 10-2 | UE stand-alone (DL and UL) operation in shared spectrum under semi-static channel access mode  | 1. Type 2C channel access2. Single sensing slot of 9us channel access3. 20MHz LBT bandwidth4. SSB/MIB/RMSI reception with Q5. SSB RRM with Q in DMTC6. SSB-RLM with Q in DMTC window7. Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_0 |  | Per band | This can be a basic feature group for operating in unlicensed band.Support of channel access mechanism for FBE operation, including fixed frame period, Cat 2 LBT, Cat 1 LBT | Optional with capability signalling |
| 10-2a | UE DL only operation in shared spectrum under semi-static channel access mode | 1. SSB RRM with Q in DMTC2. Support fixed frame period of 5ms and 10ms | 6-5 | Per band | This can be a basic feature group for operating in unlicensed band with DL only operation | Optional with capability signalling |
|  |  |  |  |  |  |  |

 |
| [8] | Ericsson | We observe that in the most recent UE features list [R1-2001484] there has been an attempt to define feature groups based on some (but not all) deployment scenarios for both LBE and FBE with some components repeated in multiple feature groups. We refer to this as “deployment based grouping.” For example, 10-1 is currently defined for standalone (Scenario C) for LBE, and 10-1a is for DL only LAA operation (one of the 2 possible deployments in Scenario A). There are several problems with deployment based grouping, namely:* It is not consistent with the grouping approach used in Rel-15. As NR evolves, a consistent approach should be used across releases.
	+ In Rel-15, the Notes column in TR38.822 was used to provide information on which deployment scenarios a particular feature group is applicable to when needed, and this same approach can be used in Rel-16 if needed.
* Not all deployment scenarios are covered, e.g., dual connectivity is missing
	+ It becomes unmanageable to define basic feature groups for all possible deployment scenarios
	+ The structure will unnecessarily restrict the ability to signal support for a different deployment scenario in the future that may need a different combination of components
* The basic feature groups have overlapping functionality
	+ This can complicate IODT testing in that there would likely need to be a partitioning of components different from the defined feature groups which is undesirable
* It becomes very hard to define prerequisites in a logical way
	+ If basic FGs are defined only for a subset of scenarios (as in [R1-2001484] currently), what pre-requisite should be defined for a FG-x if the UE implementation is targeted for a deployment for which a basic FG is not defined?
	+ IODT testing becomes complicated if multiple pre-requisites corresponding to different deployments are needed to capture the pre-requisite components

To alleviate these problems, it is better to define basic feature groups with components that have tightly related functionality. The goal of this grouping is that for any given deployment scenario, the pre-requisites can be defined as a subset of the basic feature groups, and those feature groups by design should have non-overlapping functionality. This is the approach that was used in Rel-15 and is closer to the approach that was used in the prior version of the UE feature list [R1-2000390] in contrast to the deployment-based grouping approach in the current version [R1-2001484]. The Notes column in TR 38.822 can be used to indicate which functionality is necessary for a particular deployment scenario if needed.Based on this we make the following proposals that should be used as general principles:1. Define basic feature groups with components that have tightly related functionality
2. Define basic feature groups that have non-overlapping functionality as much as possible

Based on these general principles, we propose to replace the 5 basic FGs 10-1, 10-1a, 10-2, 10-2a, and 10-2c in [R1-2001484] by the following 5 basic feature groups. We note that FGs 10-2, 10-3, and 10-4 in this proposal very much follow the structure used in Rel-15 for FGs 1-1 and 1-3 related to initial access, RRM, RLM, and RMSI reception (see Appendix of [R1-2001484]).1. Replace FGs 10-1, 10-1a, 10-2, 10-2a, and 10-2c in by the 5 basic feature groups shown in the table below

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-1 | UL channel access for dynamic channel access mode  | 1. Type 1 channel access2. Type 2A channel access3. Type 2B channel access (FFS whether or not this should be defined as a separate FG)4. Type 2C channel access5. 20MHz LBT bandwidth6. Contention window adjustment7. CP extension up to 1 symbol for PUSCH/PUCCH transmission |  |  | N/A |  | Per band | N/A | N/A |  | Basic feature group | Optional with capability signaling |
| 10-1a | UL channel access for semi-static channel access mode | 1. Type 2C channel access2. Single sensing slot of 9us channel access3. 20MHz LBT bandwidth |  |  | N/A |  | Per band | N/A | N/A |  | Basic feature group | Optional with capability signaling |
| 10-2 | SSB reception (including reading MIB) and SSB-based RRM | 1. SSB reception with Q2. SSB RRM with Q |  |  | N/A |  | Per band | N/A | N/A |  | Basic feature group | Optional with capability signaling |
| 10-3 | SSB-based RLM | 1. SSB RLM with Q |  |  | N/A |  | Per band | N/A | N/A |  | Basic feature group | Optional with capability signaling |
| 10-4 | SIB1 reception | 1. SIB1 reception with Q |  |  | N/A |  | Per band | N/A | N/A |  | Basic feature groupNote: SIB1 reception for ANR (FG 10-23) remains as a separate FG with 10-4 as a pre-requisite | Optional with capability signaling |

With the basic feature groups defined as above, all of the deployment scenarios captured in the WID are covered with combinations of the basic feature groups. The deployment scenarios can be summarized as follows:1. SCell (DL only) in unlicensed band
	1. Maps to Scenario A with DL only, i.e., LAA – DL Only
	2. Required Basic FGs: 10-2
2. SCell (DL + UL) in unlicensed band
	1. Maps to Scenario A with DL + UL, i.e., LAA – DL + UL
	2. Required Basic FGs:
		1. LBE: 10-1 + 10-2
		2. FBE: 10-1a + 10-2
3. PSCell in unlicensed band
	1. Maps to Scenario B and E, i.e., ENDC and NR-NR DC
	2. Required Basic FGs: 10-1 + 10-2 + 10-3
4. PCell in unlicensed band
	1. Maps to Scenario C and D, i.e., Standalone and Standalone + SUL
	2. Required Basic FGs:
		1. LBE: 10-1 + 10-2 + 10-3 + 10-4
		2. FBE: 10-1a + 10-2 + 10-3 + 10-4

In this way, the deployment scenarios are described based on different combinations of the basic feature groups. Moreover, the basic feature groups have non-overlapping functionality as much as possible, thus simplifying IODT testing.As a general principle, feature group A should be listed as a pre-requisite for feature group B only if feature group B cannot *functionally* operate without feature group A.For operation in shared spectrum, a UE should indeed support UL LBT. However, the **functionality** of feature groups, for example one-shot-HARQ (10-16), that have nothing to do with UL LBT operation should not have the feature group with UL LBT as a prerequisite. This means that it is technically incorrect to include 10-1 or 10-2 as a pre-requisite for 10-16 (numbering as per the latest draft in [R1-2001484]). It should be noted that feature group 10-16 being listed as part of feature “10. NR-unlicensed” in TR 38.822 makes it amply clear that this feature was developed for operation in unlicensed spectrum. There is no further need to artificially link functionally unrelated feature groups together to attempt to indicate the intended scenario for a feature. This type of pre-requisite definition has the same issues as the deployment based grouping discussed in the previous section.We have previously commented that adding pre-requisite features for a feature group should have technical justifications with respect to the functionality being tested for the feature group. Hence, we reiterate the following proposal.1. We propose the following:
* A feature group A should be listed as a pre-requisite for another feature group, B, only if feature group B cannot functionally operate without feature group A.
* The basic feature groups related to UL channel access should be removed as pre-requisites from the following feature groups (as per the latest draft in [R1-2001484]) since these feature groups do not require UL LBT to operate:
	+ 10-3, -3a, -3b, -3c, -9, -9a, -9b, -9c, -10, -11, -14, -15, -16, -16a, -17, -18a, -19a, -19c, -20, -20a, -23, -24, -26, -27, -28, -29, -30, -31

For supporting the semi-static channel access mode, the main additional functionalities that are useful to be implemented in the UE are1. RACH validation to take into account idle periods in the fixed frame period
2. Sensing in a single slot of 9 us

It should be noted that the system can operate in FBE even without these two functionalities with appropriate configuration of RACH occasions and with the use of a short LBT over 25 μs that also meets the requirements of sensing in a single slot of 9 μs. Therefore, there is no necessity to define multiple feature groups individually for dynamic and semi-static channel access modes. Only a basic feature group for dynamic channel access and one for semi-static channel access as in Proposal 3 are needed. Furthermore, for semi-static channel access mode, support of fixed frame period of 5 and 10 ms is listed. It is not clear why a limitation to a fixed frame period of 5 and 10 ms needs to be included in the feature group definition considering the functionalities listed above for which there isn’t any significant complexity difference between for the different fixed frame periods. Finally, the current structure doesn’t allow signaling of support for fixed frame periods that are less than 5 and 10 ms unless the UE also supports UL which seems like a very strange restriction.1. Remove values for fixed frame period from the definition of feature groups related to semi-static channel access

Component 11 is “Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_0” in our view, it is not critical if NR-U capable UEs do not support the extended RAR window. Collisions do not happen frequently, and if there is a collision, a UE can retry to access the channel again. It is true that the gNB does not know the UE’s capability if the RACH procedure is initiated by the IDLE/INACTIVE UE. However, if support of extended RAR is a separate FG with its own an capability bit, this can be used to collect statistics on UE capabilities, and the gNB may decide based on the penetration and use case whether to configure the extended RAR window or not. If considered useful, this can be implemented in the initial phase. Otherwise, UEs may also be upgraded with this capability if enhancements are considered needed.1. Introduce a separate FG for support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_0
 |
| [12] | Nokia, Nokia Shanghai Bell | * 10-1/10-1a/10-2/10-2a: Missing clear relationship with 10-30 (COT duration). It should be a pre-requisite at least for 10-1/10-1a.
* 10-1, components 8, 9, 10: remove “with Q” or clarify the text so that it becomes self-contained.
* 10-1a: remove “with Q” or clarify the text so that it becomes self-contained.
* 10-2:
	+ Components 4, 5, 6: remove “with Q” or clarify the text so that it becomes self-contained.
	+ Component 8: add 2ms support
* 10-2a:
	+ Component 1: remove “with Q” or clarify the text so that it becomes self-contained.
	+ Component 2: add 2ms support
* 10-2b: it is unclear why this component would be needed.
 |
| [13] | Qualcomm Incorporated |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 10-1 | UE stand-alone (DL and UL) operation in shared spectrum under dynamic channel access mode  | 1. Type 1 channel access2. Type 2A channel access3. Type 2B channel access (FFS if move this to separate feature)4. Type 2C channel access5. 20MHz LBT bandwidth6. Contention window adjustment7. CP extension up to 1 symbol for PUSCH/PUCCH transmission8. SSB/MIB/RMSI reception with Q9. SSB RRM with Q in DMTC10. SSB-RLM with Q in DMTC window11. Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_0 |  |  | N/A |  | Per band | N/A | N/A |  | This is a basic feature group for operating in unlicensed band with both DL and UL transmission support under dynamic channel access | Optional with capability signalling |
| 10-1a | UE DL only operation in shared spectrum under dynamic channel access mode | 1. SSB RRM with Q in DMTC | 6-5 |  | N/A |  | Per band | N/A | N/A |  | This is a basic feature group for operating in unlicensed band with DL only operation under CA mode | Optional with capability signalling |
| 10-2 | UE stand-alone (DL and UL) operation in shared spectrum under semi-static channel access mode  | 1. Type 2C channel access2. Single sensing slot of 9us channel access3. 20MHz LBT bandwidth4. SSB/MIB/RMSI reception with Q5. SSB RRM with Q in DMTC6. SSB-RLM with Q in DMTC window7. Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_08. Support fixed frame period of 5ms and 10ms |  |  | N/A |  | Per band | N/A | N/A |  | This is a basic feature group for operating in unlicensed band. | Optional with capability signalling |
| 10-2a | UE DL only operation in shared spectrum under semi-static channel access mode | 1. SSB RRM with Q in DMTC2. Support fixed frame period of 5ms and 10ms | 6-5 |  | N/A |  | Per band | N/A | N/A |  | This is a basic feature group for operating in unlicensed band with DL only operation | Optional with capability signalling |
| 10-2b | UE operation in shared spectrum under semi-static channel access mode with shorter fixed frame periods | 1. Support fixed frame periods shorter than 5ms | 10-2 or 10-2a |  | N/A |  | Per band | N/A | N/A |  |  | Optional with capability signalling |

10-2b: An alternative solution is to merge this back to 10-2 and 10-2a where introducing a component on supported fixed frame period lengths with {5ms, 10ms} as one value and {1ms, 2ms, 2.5ms, 4ms, 5ms, 10ms} as another value |
| [14] | Huawei, HiSilicon | It cannot be excluded that certain UEs may only support one of the above scenarios, e.g. Scenario A (licensed-assisted access) with DL-only. Therefore some UEs may not support uplink on unlicensed band. So any FG that only contains UL components should not be a basic feature group according to approach 1.The discussion on UE feature groups for NR-U is considering defining basic feature groups for the following FGs associated with NR-U operation scenarios: 10-1, 10-1a, 10-2, 10-2a, 10-2b (see Table 1 below). Previously FGs 10-1 and 10-2 were only about UL capabilities, but in the latest version [R1-2001484] DL components were added and certain DL components are repeated in several of those FGs, i.e. SSB RRM with Q in DMTC. This means approach 2 is taken as basis for the proposed definition of basic FGs in [R1-2001484], as this is not consistent with approach 1. However it is unclear if there would be separate capability signaling for the components within FG 10-1 and 10-2, or if all components of FG 10-1 and 10-2 would also need to be individual FGs of their own.Alternatively FG10-1a could be considered a prerequisite of FG10-1, and FG10-2a a prerequisite of FG10-2. The earlier version clearly separating the UL and DL components into different FGs allowed a UE to clearly report those capabilities separately for signaling support for various operation scenarios. With the latest grouping in [R1-2001484], how would a UE signal support for scenario B with dual-connectivity? Would the UE have to support standalone DL and UL in order to support scenario B? If so, why should such constraint be introduced?For DL only operation with SCell in unlicensed band, there are now 2 FGs: one for LBE and one for FBE. If those 2 FGs (10-1a and 10-2a) are considered as basic FGs, then it is clear that it should not be expected that a UE has to report support for both FGs if the UE signals support for band n46. So again, FGs 10-1a and 10-2a as defined in [R1-2001484] can only be considered as basic FGs according to approach 2 in [RP-200502]. If the minimum required for operation on band n46 is considered, according to the current list, it should be SSB RRM with Q in DMTC, and support for FBE comes with one additional capability (support fixed frame period of 5ms and 10ms).***Observation 1:**** ***According to the definition of basic feature group of approach 1 in RP-200502, only a FG10-1a with SSB RRM with Q in DMTC as a single component may qualify as a basic FG for NR-U.***
* ***FGs 10-1, 10-1a, 10-2, 10-2a, 10-2b in R1-2001484 are defined according to the definition of basic feature group of approach 2 in RP-200502.***

***Proposal 1:**** ***RAN1 needs to clearly indicate whether separate capability signaling for each component is expected for FGs 10-1 and 10-2 in R1-2001484.***
* ***RAN1 needs to clarify why certain components are included in multiple NR-U FGs in R1-2001484.***

**Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_0**FG10-27 is kept as a separate FG for wideband PRACH (same as RB-interlaced PUSCH and PUCCH), so it is unclear why “*Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_0*” was included as a component of FG10-1 and FG10-2. This functionality is for 2-step RACH, so it should be a separate FG because support of 2-step RACH is not a prerequisite for FG10-1 or FG10-2. |
| [15] | TCL Communication | We believe that for NR-Unlicensed, similar to V2X, for the UEs able to interoperate with the network over the shared spectrum using NR-U as standardized in 3GPP Rel-16, the 3GPP should define a set of features which are mandatory for the NR-U capable UEs. This base group of features defines the minimum functionalities which 3GPP deems necessary for unlicensed operation.Without such baseline future interoperability testing will prove difficult and the market will require another level of alignment between vendors.**Proposal 1:**There is a base group of UE features defined among the NR-Unlicensed capabilities which are defined to be mandatory if a UE indicates its capability to operate over shared spectrum. These features shall be group in UE feature 10-1 or 10-2.We believe that NR-U Rel-16 provides for shared spectrum usage what NR Rel-15 provides for Uu opeatrion. For this reason, we believe that it will be useful to define the basic features which may provide certain quality of communication. For this reason, we believe that 10-3 (PRB interlace mapping for PUSCH) should be part of basic feature set which are mandatory for UEs indicating being capable of Rel-16 NR-U operation. For feature 10-25 (Enable configured UL transmission out of COT), we understand the description of this feature as to support CG UL transmissions where UE initiates the COT. If this understanding is correct, and when this feature is not supported, UE will not initiate channel access to make a CG UL transmission. From our perspective, this is very performance inefficient for configured grant operation and this behaviour should be supported as mandatory or among the basic feature groups.Feature 10-16 (One-shot HARQ ACK feedback) is a very important feature. Without this feature, system efficiency is very low due to loss of feedback for many DL packets. For this reason, this should be added as one of the mandatory features to UEs capable of Rel-16 NR-U operation.Similarly, 10-19 (number of LBT bandwidths), this is more of a fundamental feature compared to carrier aggregation. One aspect is related to per band nature, and one other aspect is related to UE processing capability. Independent of the representation, from our perspective, given NR supports upto 100 MHz BW, the basic feature set for NR-U should be the support of BW larger than 20 MHz. This also means that feature 10-29 (support available RB set indicator field in DCI 2\_0) should be supported as mandatory NR-U Rel-16 feature as this signaling in the DCI largely facilitates the effective usage of wideband carrier over the shared spectrum. The feature 10-30 (Support channel occupancy duration indicator field in DCI 2\_0) also provides very basic functionliaty about the channel occupancy representation and utilization over the shared spectrum and thus should be mandatory.From our understanding, following the strategy of making the basic features as components in 10-1 and 10-2, we believe that the best way to ensure meaningful NR-U operation is to add 10-3, 10-25, 10-19, 10-29 and 10-30 as components in the basic features groups of 10-1 and 1-2.**Proposal 2:**Add 10-3, 10-25, 10-19, 10-29, 10-30 and 10-16 as components in 10-1 and 10-2. |

**As pointed out by multiple companies, current basic FGs do not support all deployment scenarios listed in NR-U WID as below:**

* **Scenario A: Carrier aggregation between licensed band NR (PCell) and NR-U (SCell).**
	+ **NR-U SCell may have both DL and UL, or DL-only.**
	+ **In this scenario, NR PCell is connected to 5G-CN.**
* **Scenario B: Dual connectivity between licensed band LTE (PCell) and NR-U (PSCell)**
	+ **In this scenario, LTE PCell connected to EPC as higher priority than PCell connected to 5G-CN.**
* **Scenario C: Stand-alone NR-U**
	+ **In this scenario, NR-U is connected to 5G-CN.**
* **Scenario D: A stand-alone NR cell in unlicensed band and UL in licensed band (single cell architecture).**
	+ **In this scenario, NR-U is connected to 5G-CN.**
* **Scenario E: Dual connectivity between licensed band NR and NR-U.**
	+ **In this scenario, PCell is connected to 5G-CN.**

**However, the way to modify current basic FGs seems still divergent, e.g.**

* **Option 1: define new basic FGs in addition to current basic FGs to support all deployment scenarios (e.g., [3] and [5])**
* **Option 2: define new basic FGs with components that have tightly related functionality to replace current basic FGs (e.g., [8])**

**Based on above, following should be discussed at first.**

* **How to define basic FGs which support all deployment scenarios**
	+ **Options 1 or 2 stated above can be the starting point to discuss**

**In addition, following points should be discussed for FGs 10-1 to 10-2b.**

* **Whether or not following FGs can be included in basic FGs**
	+ **10-3, 10-11, 10-14, 10-15, 10-16, 10-16a, 10-17, 10-18, 10-19, 10-20, 10-20a, 10-24, 10-25, 10-28, 10-29, 10-30**
* **Whether or not “Support fixed frame period of 5ms and 10ms” and “Support fixed frame periods shorter than 5ms” can be separate capabilities.**
* **Whether or not “Support of RAR extension from 10ms to [40ms] by decoding of the 2-bit SFN indication in DCI 1\_0” can be separate capability from basic FGs**
* **Whether or not “Type 2B channel access” can be separate capability from basic FGs**

# **10-3 to 10-3c and [10-12]: PRB interlace mapping for PUSCH and PUCCH**

In [1], FGs 10-3 to 10-3c are captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-3 | PRB interlace mapping for PUSCH | 1. PRB interlace frequency domain resource allocation for PUSCH | 10-1 or 10-2Need discussion for licensed use | Yes | N/A |  | Per band | N/A | N/A |  | Support of PRB interlace PUSCH | Optional with capability signalling |
| 10-3a | PRB interlace mapping for PUCCH format 0 and format 1 | 1. PRB interlace frequency domain resource allocation for PUCCH format 0 and format 1 | 10-1 or 10-2Need discussion for licensed use | Yes | N/A |  | Per band | N/A | N/A |  | Support of PRB interlace PUCCH format 0/1 | Optional with capability signalling |
| 10-3b | PRB interlace mapping for PUCCH format 2 | 1. PRB interlace frequency domain resource allocation for PUCCH format 2 | 10-1 or 10-2Need discussion for licensed use | Yes | N/A |  | Per band | N/A | N/A |  | Support of PRB interlace PUCCH format 2 | Optional with capability signalling |
| 10-3c | PRB interlace mapping for PUCCH format 3 | 1. PRB interlace frequency domain resource allocation for PUCCH format 3 | 10-1 or 10-2Need discussion for licensed use | Yes | N/A |  | Per band | N/A | N/A |  | Support of PRB interlace PUCCH format 3 | Optional with capability signalling |
|  | 10-12 | OCC for PRB interlace mapping for PF2 and PF3 FFS if need this capability, or if we split this for PF2 and PF3 separately | 1. OCC22. OCC4 | 10-3b or 10-3c | Yes | N/A |  | Per band | N/A | N/A |  | UE OCC capability for EPF2/EFP3 | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [2] | ZTE, Sanechips | There has been various enhancements made in NR-U WI on different aspects based on Rel-15 NR design. For the enhancements on the same aspect, it may not be a good way to split the features into too many small pieces and make all of them as optional. It would be hard for network to implement and utilize a meaningful Rel-16 functionality if different UEs support drastically different combinations of feature groups for one aspect. For example for the interlace structure, currently there are 4 optional feature groups defined for PUSCH and each of the PUCCH formats respectively, which implies one UE may support interlaced PUSCH but not support interlaced PUCCH, or vice versa. This is not necessary, as in the RRC signalling there is only one parameter to just indicate whether the interlaced structure is enabled or not. Therefore, it would be better to merge them into one feature group. Similar principle can be applied to the enhancements on HARQ and configured grant.***Proposal 2:*** * ***To avoid implementation complexity, the enhancements on the same aspect should be combined into one feature group, including the following:***
	+ ***Interlaced structure: combine 10-3, 10-3a, 10-3b, and 10-3c***
	+ ***HARQ enhancement: combine 10-14, 10-15, 10-16, 10-16a, and 10-17***
	+ ***Configured grant: combine 10-18 and 10-28***
* Interlaced mapping including FG 10-3/3a/3b/3c.

The interlaced mapping is proposed to simplify the signalling of the FDRA of interlace in order to satisfy the OCB requirement from ESTI. There is no such OCB requirement for NR licensed spectrum, so we do not think there is a need to extend the application range for this feature.  |
| [3] | vivo | For interlace UL related features (10-3, 10-3a, 10-3b, 10-3c), we do not see the need of extension to licensed band since interlace is introduced due to regulatory requirement on unlicensed band which doesn’t exist in licensed band.Proposal 1: Interlace UL related features (10-3, 10-3a, 10-3b, 10-3c) should be limited to unlicensed band only and SS group switching related features (10-9, 10-9a, 10-9b) could be extended to licensed use.  |
| [4] | OPPO | **FG 10-3b/12**: In Rel-15, UE capability of supporting PUCCH format 2, 3, 4 are separately reported. To analog with Rel-15, in NRU, enhanced PF2 and PF3 should also be separated in two FGs. Moreover, we should further discuss if OCC is an additional add-on capability. To our understanding, the OCC is not mandatory for supporting PF2 or PF3. Thus, it should be allowed that a UE supports PF2/PF3 without supporting OCC.

|  |  |  |
| --- | --- | --- |
| 10-3b | PRB interlace mapping for PUCCH format 2 | 1. PRB interlace frequency domain resource allocation for PUCCH format 2 |
| 10-3~~b~~c | PRB interlace mapping for PUCCH format 3 | 1. PRB interlace frequency domain resource allocation for PUCCH format 3 |
| ~~10-12~~ | ~~OCC for PRB interlace mapping for PF2 and PF3~~ ~~FFS if need this capability, or if we split this for PF2 and PF3 separately~~ | ~~1. OCC2~~~~2. OCC4~~ |
| 10-12 | OCC for PRB interlace mapping for EPF2 FFS if need this capability | 1. OCC22. OCC4 |
| 10-12a | OCC for PRB interlace mapping for EPF3 FFS if need this capability | 1. OCC22. OCC4 |

**Proposal 2: Separate OCC capability from PUCCH format 2 or format 3 with interlace mapping.** |
| [5] | MediaTek Inc. | Proposal 1: NR-U features can only be extended to licensed operation when uses cases and benefits are well justified.  |
| [7] | Intel Corporation | Interlace design is a fundamental feature for uplink transmission in order to be complaint with the unlicensed band regulation. Also based on the agreement below (first two agreements), a gNB can configure the interlaced mapping for the whole cell both for PUCCH and PUSCH. From this perspective, it is proposed to merge the “PRB interlace frequency domain resource allocation” into 10-1 and 10-2. Even though it is separately defined, it is proposed to combine 10-3/10-3a/10-3b/10-3c into a single feature group. This is because if interlace mapping is used for one PUCCH format, then other PUCCH formats also have to use interlace mapping based on the 3rd agreement below. However, we do not need to use the interlace mapping for licensed use since there is no reason for it.

|  |
| --- |
| Agreement:In Rel-16, for a cell, the UE can expect that cell-specifically configured PUCCH resources and UE-specifically configured PUCCH resources either all have interlaced mapping or all have non-interlaced mapping as per Rel-15.* Note: RRC parameters that are made redundant due to this agreement can be eliminated

Agreement:In Rel-16, for a cell, the UE can expect that cell-specifically configured PUSCH resources and UE-specifically configured PUSCH resources either all have interlaced mapping or all have non-interlaced mapping as per Rel-15.* Note: RRC parameters that are made redundant due to this agreement can be eliminated

Agreement:In Rel-16, for a cell, the UE can expect that UE-specifically configured PUCCH resources and all PUSCH transmissions (scheduled and configured) after dedicated configurations either all have interlaced mapping or all have non-interlaced mapping as per Rel-15. |

**Proposal 3:** * **Merge 10-3/10-3a/10-3b/10-3c into 10-1 and 10-2.**
* **If not merged, combine 10-3/10-3a/10-3b/10-3c into a single feature group and remove “Need discussion for licensed use”.**
 |
| [8] | Ericsson | We understand that for DL only LAA deployments it is not necessary for the UE to support interlaced PUCCH, hence it makes sense to split the UE capability for interlacing into separate FGs, one for PUSCH and one for PUCCH. However, it is undesirable to further split the capability for interlaced PUCCH into 3 separate FGs for PF0/1, PF2, and PF3. This results in too fine grained capability signaling.1. Merge FG 10-3a/b/c for PUCCH into a single FG. Keep FG 10-3 for PUSCH as a separate FG.

Regarding the FFS, in our view this capability should be kept, but it is not necessary to split into separate capabilities for PF2 and PF31. Keep FG-12; do not split into separate capabilities for PUCCH Format 2 and PUCCH Format 3
 |
| [9] | Samsung | NR-U functions have been introduced to handle inherit problem of unlicensed band such as LBT failure and regulation. Hence, in our view, except FG-8 and FG-11 which are general function for licensed band, applicability of NR-U feature groups should be restricted to unlicensed band. If some of NR-U feature groups are identified to be beneficial for licensed band operation, we will be able to make an agreement for each.Proposal 2: UE features for NR-U should be used only for unlicensed band. |
| [12] | Nokia, Nokia Shanghai Bell | * 10-3a/3b/3c: to be merged as a single feature group as originally proposed. If interlace is required it is required for all formats.
* 10-12: It should be combined with 10-3a/b/c (PUCCH component).
 |
| [13] | Qualcomm Incorporated |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 10-12 | OCC for PRB interlace mapping for PF2 and PF3  | 1. OCC22. OCC4 | 10-3b or 10-3c | Yes | N/A |  | Per band | N/A | N/A |  | UE OCC capability for EPF2/EFP3 | Optional with capability signalling |

 |
| [14] | Huawei, HiSilicon |

|  |  |  |
| --- | --- | --- |
| Functionality | FGs | Need for licensed band operation |
| PRB interlace mapping for PUSCH and PUCCH | 10-3 PRB interlace mapping for PUSCH10-3a PRB interlace mapping for PUCCH format 0 and format 110-3b PRB interlace mapping for PUCCH format 2 10-3c PRB interlace mapping for PUCCH format 3 | Per bandThere is no clear benefit for a UE to support those features for licensed bands at the cost of extra complexity at the UE and with increased complexity for multiplexing UEs with different uplink capabilities |

 |

**Based on above, following conclusion would be acceptable.**

* **10-3/10-3a/10-3b/10-3c are used only for unlicensed band**

**In addition, following points should be discussed.**

* **Whether or not 10-3/10-3a/10-3b/10-3c can be combined into a single FG**
* **Whether or not 10-12 can be combined into 10-3b/10-3c**
	+ **If not, whether or not 10-12 can be split for PF2 and PF3 separately**

# **10-7: LBT bandwidth size of 10MHz**

In [1], FG 10-7 is captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-7 | LBT bandwidth size of 10MHz | FFS the components | 10-1 or 10-2 | Yes | N/A |  | Per band | N/A | N/A |  |  | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| [8] | Ericsson | 10 MHz LBT bandwidth is only needed for the special case of configuring an SCell only on one of two specific ARFCNs in one specific geographic region in the world (India), and only if UL is enabled. Hence the capability should be restructured as shown below. This FG can have FG 10-1 in our Proposal 3 as a pre-requisite.1. Rename FG 10-7 as follows. This FG can have FG 10-1 in our Proposal 3 as a pre-requisite.

|  |  |  |
| --- | --- | --- |
| 10-7 | ~~LBT bandwidth size of 10MHz~~UL channel access for 10 MHz SCell  | ~~FFS the components~~1. 10 MHz LBT bandwidth |

 |

**Based on above, following point should be discussed.**

* **Whether or not 10-7 can be updated as follows**

|  |  |  |
| --- | --- | --- |
| 10-7 | ~~LBT bandwidth size of 10MHz~~UL channel access for 10 MHz SCell  | ~~FFS the components~~1. 10 MHz LBT bandwidth |

# **10-8: Type B PDSCH length**

In [1], FG 10-8 is captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-8 | Type B PDSCH length | Length 3, 5, 6, 8, 11, 12, 13FFS the capability are separate for each length or some groups are formed to signal the capability together |  | Yes | N/A |  | FFS: Per UE or per band | N/A | N/A |  | Support of additional length (other than 2/4/7) for type B PDSCH.Note length 9/10 are already covered by 14-3 | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [2] | ZTE, Sanechips | * TypeB PDSCH length: including FG 10-8

In general, the above enhancements on PDSCH could be beneficial to licensed spectrum in terms of enhanced flexibility and reliability. On the other hand, it may introduce implementation complexity for NR UEs. Probably they can be considered as optional features to be applied to NR licensed spectrum. |
| [5] | MediaTek Inc. | Proposal 1: NR-U features can only be extended to licensed operation when uses cases and benefits are well justified.  |
| [7] | Intel Corporation | We support that some of feature groups are used for licensed use, including 10-8 and 10-11. And also some of HARQ features seem beneficial for licensed use as well including enhanced dynamic HARQ codebook, one-shot HARQ ACK, and multi-PUSCH UL grant. **Proposal 5:** * **Let 10-8/10-11/10-14/10-15/10-16/10-16a/10-17 be used for licensed band**
 |
| [8] | Ericsson | Regarding the FFS, it is beneficial (and simpler) that if any new Type B mapping lengths are supported, then all are supported. Having separate capabilities for each new length results in too fine grained capability signalling and is hard to manage in the network. Since the PDSCH mapping lengths are generally useful, regardless of the band, in our view this feature should be per UE.1. Support only single capability bit for all new PDSCH mapping lengths (3,5,6,8,11,12,13). FG 10-8 should be per UE.
 |
| [9] | Samsung | NR-U functions have been introduced to handle inherit problem of unlicensed band such as LBT failure and regulation. Hence, in our view, except FG-8 and FG-11 which are general function for licensed band, applicability of NR-U feature groups should be restricted to unlicensed band. If some of NR-U feature groups are identified to be beneficial for licensed band operation, we will be able to make an agreement for each.**Proposal 2: UE features for NR-U should be used only for unlicensed band.** |
| [12] | Nokia, Nokia Shanghai Bell | * 10-8: Preference to have length 9/10 included in this feature for clarity. However, if length 9/10 is assumed to be covered by 14-3 then it needs to be added as a pre-requisite.
 |
| [13] | Qualcomm Incorporated | For supported type B PDSCH lengths, we propose to have two components: {3, 5, 6, 8, 11} supported and {12, 13} supported |
| [14] | Huawei, HiSilicon |

|  |  |  |
| --- | --- | --- |
| Functionality | FGs | Need for licensed band operation |
| Type B PDSCH length | 10-8 Type B PDSCH length14-2 PDSCH Type B mapping of length 9 and 10 OFDM symbols | Per UEFG10-8 and FG14-2 could be “per UE”. At least FG14-2 is applicable to licensed and unlicensed bands in FR1. |

***Proposal 2: The following FGs could be extended to licensed bands, i.e. reported “per UE”:**** ***10-8 Type B PDSCH length***
 |

**Based on above, following points should be discussed for FG 10-8.**

* **Whether or not the capability are separate for each length or some groups are formed to signal the capability together**
* **Whether or not 10-8 can be extended to licensed use**

# **10-9 to 10-9c: Search space set group switching**

In [1], FGs 10-9 to 10-9c are captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-9 | Search space set group switching with explicit DCI 2\_0 bit field trigger | 1. Two groups of search space sets2. Monitor DCI 2\_0 with a search space set switching field 3. Support a timer to switch back to original search space set group4. Monitor DCI 2\_0 for channel occupancy time and use the end of channel occupancy time to switch back to the original search space set group | 10-1, 10-1a, 10-2, or 10-2aNeed discussion for licensed use | Yes | N/A |  | FFS: Per UE or per band or per BC | N/A | N/A |  | Being configured with two groups of search spaces, and switch between them. Some search space sets can be configured in both groups. | Optional with capability signalling |
| 10-9a | Search space set group switching with implicit PDCCH decoding with DCI 2\_0 monitoring | 1. Two groups of search space sets2. Support switching the search space set group with PDCCH decoding in group 1 3. Support a timer to switch back to original search space set group4. Monitor DCI 2\_0 for channel occupancy time and use the end of channel occupancy time to switch back to the original search space set group | 10-1, 10-1a, 10-2, or 10-2aNeed discussion for licensed use | Yes | N/A |  | FFS: Per UE or per band | N/A | N/A |  | Being configured with two groups of search spaces, and switch between them. Some search space sets can be configured in both groups. | Optional with capability signalling |
| 10-9b | Search space set group switching with implicit PDCCH decoding without DCI 2\_0 monitoring | 1. Two groups of search space sets2. Support switching the search space set group with PDCCH decoding in group 1 3. Support a timer to switch back to original search space set group | 10-1, 10-1a, 10-2, or 10-2aNeed discussion for licensed use | Yes | N/A |  | FFS: Per UE or per band | N/A | N/A |  | Being configured with two groups of search spaces, and switch between them. Some search space sets can be configured in both groups. | Optional with capability signalling |
| 10-9c | Joint search space group switching across multiple cells | 1. Configured with a group of cells and switch search space set group jointly over these cells | 10-9, 10-9a, or 10-9b | Yes | N/A |  | FFS: Per UE or per band | N/A | N/A |  | Without this capability, the UE will switch search space set groups for different cells independently | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [2] | ZTE, Sanechips | * CORESET/SS: including FG 10-9/9a/9b/9c, 10-20/20a.

In general, the above enhancements on CORESET/SS could be beneficial to licensed spectrum in terms of enhanced flexibility and reliability. On the other hand, it may introduce implementation complexity for NR UEs. Probably they can be considered as optional features to be applied to NR licensed spectrum. |
| [3] | Vivo | For search space set (SS) group switching related features (10-9, 10-9a, 10-9b), it is beneficial for power saving purpose in licensed band, i.e. one SS with sparse PDCCH monitoring in power saving mode and switch to another SS with frequent PDCCH monitoring when traffic arrives. Thus, these UE features could be extended to licensed use.Proposal 1: Interlace UL related features (10-3, 10-3a, 10-3b, 10-3c) should be limited to unlicensed band only and SS group switching related features (10-9, 10-9a, 10-9b) could be extended to licensed use.  |
| [5] | MediaTek Inc. | Proposal 1: NR-U features can only be extended to licensed operation when uses cases and benefits are well justified.  |
| [6] | LG Electronics | On the type for this feature group (and including FG 10-9a), one FFS point is between per UE and per band. In our view, per band (i.e., unlicensed band only) would be more desirable since switching behaviour based on channel occupancy time indicated by DCI format 2\_0 (which corresponds to 4th component in FG 10-9 and FG 10-9a) is only applicable to unlicensed band.**Proposal #1: Per band (i.e., unlicensed band only) as type for FG 10-9 and FG 10-9a.** |
| [7] | Intel Corporation | However, do not see any motivation to let the features for search space set group switching and search space/CORESET configuration in wideband to be used for licensed band. Those features were introduced to overcome the limitation of unlicensed band and we do not see any benefits when used for licensed operation.**Proposal 6:** * **Do not open 10-9/10-9a/10-9b/10-20/10-20a for licensed use.**
 |
| [8] | Ericsson | There is no need to split the search space switching capability into 4 separate feature groups. This complicates managing of different UEs with different capabilities in the network due to too fine grained capability signalling. In our view, this feature is useful for UE power saving, regardless of the operating band. Hence this feature should be per UE.1. Merge FG 10-9, 10-9a, 10-9b, and 10-9c into a single FG. The merged FG should be per UE.
 |
| [9] | Samsung | NR-U functions have been introduced to handle inherit problem of unlicensed band such as LBT failure and regulation. Hence, in our view, except FG-8 and FG-11 which are general function for licensed band, applicability of NR-U feature groups should be restricted to unlicensed band. If some of NR-U feature groups are identified to be beneficial for licensed band operation, we will be able to make an agreement for each.**Proposal 2: UE features for NR-U should be used only for unlicensed band.** |
| [12] | Nokia, Nokia Shanghai Bell | * 10-9/10-9a/9b 10-9b should be baseline and required for UEs implementing 10-9 or 10-9a.
 |
| [14] | Huawei, HiSilicon |

|  |  |  |
| --- | --- | --- |
| Functionality | FGs | Need for licensed band operation |
| Search space set group switching | 10-9 Search space set group switching with explicit DCI 2\_0 bit field trigger10-9a Search space set group switching with implicit PDCCH decoding with DCI 2\_0 monitoring10-9 b Search space set group switching with implicit PDCCH decoding without DCI 2\_0 monitoring10-9 c Joint search space group switching across multiple cells | Per bandIt is unclear what benefit could be obtained for operation on a licensed carrier since the monitoring periodicity of PDCCH search spaces would generally not need to change frequently nor depend on implicit rules.  |

 |
| [14] | Huawei, HiSilicon | **FG 10-9/9a/9b/9c (Search space set group switching)**FG10-9b (implicit switching without DCI 2\_0 decoding) should be a prerequisite of 10-9/9a/9c. |

**Based on above, following points should be discussed for FGs 10-9/9a/9b/9c.**

* **Whether or not 10-9/9a/9b/9c can be combined into a single FG**
* **Whether or not 10-9/9a/9b/9c can be extended to licensed use**

# **10-10: RSSI and channel occupancy measurement and reporting**

In [1], FG 10-10 is captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-10 | RSSI and channel occupancy measurement and reporting | 1. RSSI measurement2. Channel occupancy reporting | 10-1, 10-1a, 10-2, or 10-2a | Yes | N/A |  | per band | N/A | N/A |  | RSSI measurement for channel occupancy. | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [8] | Ericsson | It is not clear why RSSI channel occupancy measurement and reporting needs to be per band instead of being per UE as it was in the case of LTE-LAA. It is simpler to make this per UE, especially considering there are at least two bands already (5 and 6 GHz) and there may potentially also be other unlicensed bands that may open up in the future.1. FG 10-10 should be per UE
 |

**Based on above, following point should be discussed for FG10-10.**

* **Whether or not 10-10 can be per UE**

# **10-11: SRS starting position at any OFDM symbol in a slot**

In [1], FG 10-11 is captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-11 | SRS starting position at any OFDM symbol in a slot |  |  | Yes | N/A |  | Per band or per UE | N/A | N/A |  | Support transmitting SRS starting in all symbols (0,…,13) of a slot | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [2] | ZTE, Sanechips | * SRS starting position: including FG 10-11

In general, the above enhancements on SRS could be beneficial to licensed spectrum in terms of enhanced flexibility and reliability. On the other hand, it may introduce implementation complexity for NR UEs. Probably they can be considered as optional features to be applied to NR licensed spectrum. |
| [5] | MediaTek Inc. | Proposal 1: NR-U features can only be extended to licensed operation when uses cases and benefits are well justified.  |
| [7] | Intel Corporation | We support that some of feature groups are used for licensed use, including 10-8 and 10-11. And also some of HARQ features seem beneficial for licensed use as well including enhanced dynamic HARQ codebook, one-shot HARQ ACK, and multi-PUSCH UL grant. **Proposal 5:** **Let 10-8/10-11/10-14/10-15/10-16/10-16a/10-17 be used for licensed band** |
| [8] | Ericsson | The ability to configure an SRS resource to start at any OFDM symbol in a slot is generally useful, regardless of the band. For example, it can enable 1T4R antenna switching in the same slot (currently 2-slots are needed), it can be useful for positioning, and also URLLC. Hence this FG should be per UE.1. FG 10-11 should be per UE
 |
| [9] | Samsung | NR-U functions have been introduced to handle inherit problem of unlicensed band such as LBT failure and regulation. Hence, in our view, except FG-8 and FG-11 which are general function for licensed band, applicability of NR-U feature groups should be restricted to unlicensed band. If some of NR-U feature groups are identified to be beneficial for licensed band operation, we will be able to make an agreement for each.**Proposal 2: UE features for NR-U should be used only for unlicensed band.** |
| [13] | Qualcomm Incorporated |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 10-11 | SRS starting position at any OFDM symbol in a slot | 1. Support transmitting SRS starting in all symbols (0,…,13) of a slot |  | Yes | N/A |  | Per band or per UE | N/A | N/A |  |  | Optional with capability signalling |

 |
| [14] | Huawei, HiSilicon |

|  |  |  |
| --- | --- | --- |
| Functionality | FGs | Need for licensed band operation |
| SRS starting position at any OFDM symbol in a slot | 10-11 SRS starting position at any OFDM symbol in a slot | Per UE |

***Proposal 2: The following FGs could be extended to licensed bands, i.e. reported “per UE”:**** ***10-11 SRS starting position at any OFDM symbol in a slot***
 |

**Based on above, following point should be discussed for FG 10-11.**

* **Whether or not 10-11 can be extended to licensed use**

# **[10-13a]: Extended CP range of more than one symbol for CG-PUSCH**

In [1], FG 10-13a is captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-13a | Extended CP range of more than one symbol for CG-PUSCHFFS if need this capability |  | 10-1,Do we need this for 10-2?5-19 or 5-20 | Yes | N/A |  | Per band | N/A | N/A |  | How long a UE can generate the CP extension beyond 1 symbol for CG-PUSCH | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [4] | OPPO | **FG 10-13a**: during RAN1 discussion, there is no agreement that the CP extension for CG transmission could be more than one symbol. It is also unclear to us that which case needs to transmit CP extension with more than one symbol instead of transmitting the effective data. Our view is to remove this UE feature group.**Proposal 3: Remove 10-13a from the NRU UE feature lists due to lack of agreement and motivation.** |
| [6] | LG Electronics | While we have discussed CG-PUSCH so far, any behaviour for CG-PUSCH is not differentiated between FBE and LBE cases. Therefore, if FG 10-13a is kept as a feature group, the prerequisite feature groups for this should be 10-2 in addition to 10-1.**Proposal #2: Add 10-2 as prerequisite feature group for FG 10-13a, if FG 10-13a is needed as a feature group.** |
| [13] | Qualcomm Incorporated |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 10-13a | Extended CP range of more than one symbol for CG-PUSCH | 1. UE supports generating a CP extension of length longer than 1 symbol for Configured Grant PUSCH transmission | 10-1,5-19 or 5-20 | Yes | N/A |  | Per band | N/A | N/A |  | How long a UE can generate the CP extension beyond 1 symbol for CG-PUSCH | Optional with capability signalling |

 |

**Based on above, following points should be discussed for FG 10-13a.**

* **Whether or not 10-13a is needed as a FG**
	+ **If yes, whether or not 10-2 can be added as prerequisite FG for 10-13a**

# **10-14 to 10-17: HARQ enhancements**

In [1], FGs 10-14 to 10-17 are captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-14 | Non-numerical PDSCH to HARQ-ACK timing | 1. Support configuration of a value for dl-DataToUL-ACK indicating an imapplicable time to report HARQ ACK | 10-1 or 10-2Need discussion for licensed use | Yes | N/A |  | Per band or per UE | N/A | N/A |  | If non-numerical K1 value is supported | Optional with capability signalling |
| 10-15 | Enhanced dynamic HARQ codebook | 1. Support of bit fields signalling PDSCH HARQ group index and NFI in DCI 1\_12. Support of bit field in DCI 0\_1 for other group total DAI if configured. 3. Support the retransmission of HARQ ACKFFS if need to further split under other group DAI/NFI configured or not | 10-1 or 10-2Need discussion for licensed use | Yes | N/A |  | Per band or per UE | N/A | N/A |  | Enhanced dynamic HARQ codebook supporting grouping of HARQ ACK and triggering the retransmission of HARQ ACK in each groups | Optional with capability signalling |
| 10-16 | One-shot HARQ ACK feedback | 1. Support feedback of HARQ-ACK codebook containing all configured HARQ processes for all configured CCs, triggered by a DCI 1\_1 scheduling a PDSCH | 10-1 or 10-2Need discussion for licensed use | Yes | N/A |  | Per band or per UE | N/A | N/A |  | Upon triggering, UE reports A/N for all HARQ processes and all CCs in a PUCCH group.  | Optional with capability signalling |
| 10-16a | One-shot HARQ ACK feedback trigger with empty DCI 1\_1 | 1. Support feedback of HARQ-ACK codebook containing all configured HARQ processes for all configured CCs with a DCI 1\_1 without scheduling a PDSCH using a reserved FDRA value | 10-16Need discussion for licensed use | Yes | N/a |  | Per band or per UE | N/A | N/A |  |  | Optional with capability signalling |
| 10-17 | Multi-PUSCH UL grant | 1. Support of scheduling up to 8 PUSCH with a single DCI 0\_1  | 10-1 or 10-2 Need discussion for licensed use | Yes | N/A |  | Per band or per UE | N/A | N/A |  |  | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [2] | ZTE, Sanechips | There has been various enhancements made in NR-U WI on different aspects based on Rel-15 NR design. For the enhancements on the same aspect, it may not be a good way to split the features into too many small pieces and make all of them as optional. It would be hard for network to implement and utilize a meaningful Rel-16 functionality if different UEs support drastically different combinations of feature groups for one aspect. For example for the interlace structure, currently there are 4 optional feature groups defined for PUSCH and each of the PUCCH formats respectively, which implies one UE may support interlaced PUSCH but not support interlaced PUCCH, or vice versa. This is not necessary, as in the RRC signalling there is only one parameter to just indicate whether the interlaced structure is enabled or not. Therefore, it would be better to merge them into one feature group. Similar principle can be applied to the enhancements on HARQ and configured grant.***Proposal 2:*** * ***To avoid implementation complexity, the enhancements on the same aspect should be combined into one feature group, including the following:***
	+ ***Interlaced structure: combine 10-3, 10-3a, 10-3b, and 10-3c***
	+ ***HARQ enhancement: combine 10-14, 10-15, 10-16, 10-16a, and 10-17***
	+ ***Configured grant: combine 10-18 and 10-28***
* HARQ enhancements: including FG 10-14 ~ 10-17.

In general, the above enhancements on HARQ could be beneficial to licensed spectrum in terms of enhanced flexibility and reliability. On the other hand, it may introduce implementation complexity for NR UEs. Probably they can be considered as optional features to be applied to NR licensed spectrum. |
| [3] | vivo | For other UE features, the extension to licensed band could be considered if the benefit is identified in certain licensed scenario.Proposal 2: For UE features that are not agreed to be extended to licensed use, update “per band” to “per unlicensed band”.  |
| [4] | OPPO | **FG 10-15**: In NRU the enhanced dynamic HARQ-ACK codebook may be realized by DCI 1\_1 that contains NFI for two groups or 1 group. Moreover, the DAI in DCI 0\_1 can indicate for two groups or one group. All these can be configurable at the network side, if the UE supports each of these individual features. Thus, one FG that aggregates multiple sub-FGs seems too restricted, it should be allowed that a UE only implements one configuration, which does not refrain the UE from supporting enhanced dynamic HARQ-ACK codebook. For this reason, two FGs are indeed needed for the UE to report if it can support enhanced dynamic HARQ-ACK codebook with UL-TotalDAI-Included-r16 or without UL-TotalDAI-Included-r16.

|  |  |  |
| --- | --- | --- |
| ~~10-15~~ | ~~Enhanced dynamic HARQ codebook~~ | ~~1. Support of bit fields signalling PDSCH HARQ group index and NFI in DCI 1\_1~~~~2. Support of bit field in DCI 0\_1 for other group total DAI if configured.~~ ~~3. Support the retransmission of HARQ ACK~~~~FFS if need to further split under other group DAI/NFI configured or not~~ |
| 10-15 | Enhanced dynamic HARQ codebook  | 1. Support of bit fields signalling PDSCH HARQ group index and NFI in DCI 1\_1 for scheduled group2. Support of bit field in DCI 0\_1 for total DAI of scheduled group 3. Support the retransmission of HARQ ACK  |
| 10-15a | Enhanced dynamic HARQ codebook with DAI/NFI for the other group | 1. Support of bit fields signalling PDSCH HARQ group index and NFI in DCI 1\_1 for non-scheduled group2. Support of bit field in DCI 0\_1 for total DAI of non-scheduled group  |

**Proposal 4: Split feature group 10-15 enhanced dynamic HARQ codebook into two cases: enhanced dynamic HARQ codebook with or without reading DAI/NFI for non-scheduled group.**  |
| [5] | MediaTek Inc. | Proposal 1: NR-U features can only be extended to licensed operation when uses cases and benefits are well justified.  |
| [6] | LG Electronics | One correction is necessary for 2nd component since total DAI field for other PDSCH group can be configured to DCI format 1\_1 in addition to DCI format 0\_1.**Proposal #3: Modify 2nd component of FG 10-15 as follows.**

|  |  |  |
| --- | --- | --- |
| 10-15 | Enhanced dynamic HARQ codebook | 1. Support of bit fields signalling PDSCH HARQ group index and NFI in DCI 1\_12. Support of bit field in DCI 0\_1 and DCI 1\_1 for other group total DAI if configured. 3. Support the retransmission of HARQ ACKFFS if need to further split under other group DAI/NFI configured or not |

 |
| [7] | Intel Corporation | We support that some of feature groups are used for licensed use, including 10-8 and 10-11. And also some of HARQ features seem beneficial for licensed use as well including enhanced dynamic HARQ codebook, one-shot HARQ ACK, and multi-PUSCH UL grant. **Proposal 5:** **Let 10-8/10-11/10-14/10-15/10-16/10-16a/10-17 be used for licensed band** |
| [8] | Ericsson | The word “inapplicable” is misspelled in the description of the component.Multi-PUSCH UL grants should be per UE instead of per band. Firstly, the functionality will be very useful in any band where PDCCH capacity can be constrained. Secondly, it is functionality that once implemented is fundamentally not related to the band of operation.1. FG 10-17 should be per UE
 |
| [9] | Samsung | NR-U functions have been introduced to handle inherit problem of unlicensed band such as LBT failure and regulation. Hence, in our view, except FG-8 and FG-11 which are general function for licensed band, applicability of NR-U feature groups should be restricted to unlicensed band. If some of NR-U feature groups are identified to be beneficial for licensed band operation, we will be able to make an agreement for each.**Proposal 2: UE features for NR-U should be used only for unlicensed band.** |
| [12] | Nokia, Nokia Shanghai Bell | * 10-14: fix typo “imapplicable time -> inapplicable time”. It is OK to support it for licensed use as well.
* 10-15: Remove “FFS if need to further split under other group DAI/NFI configured or not”
* 10-16 and 10-16a: to be merged into a single feature
* 10-17: It is OK to support it for licensed use as well.
 |
| [13] | Qualcomm Incorporated |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 10-14 | Non-numerical PDSCH to HARQ-ACK timing | 1. Support configuration of a value for dl-DataToUL-ACK indicating an imapplicable time to report HARQ ACK | 10-1 or 10-2Need discussion for licensed use | Yes | N/A |  | Per band  | N/A | N/A |  | If non-numerical K1 value is supported | Optional with capability signalling |
| 10-15 | Enhanced dynamic HARQ codebook | 1. Support of bit fields signalling PDSCH HARQ group index and NFI in DCI 1\_12. Support of bit field in DCI 0\_1 for other group total DAI if configured. 3. Support the retransmission of HARQ ACKFFS if need to further split under other group DAI/NFI configured or not | 10-1 or 10-2Need discussion for licensed use | Yes | N/A |  | Per band  | N/A | N/A |  | Enhanced dynamic HARQ codebook supporting grouping of HARQ ACK and triggering the retransmission of HARQ ACK in each groups | Optional with capability signalling |
| 10-16 | One-shot HARQ ACK feedback | 1. Support feedback of type 3 HARQ-ACK codebook, triggered by a DCI 1\_1 scheduling a PDSCH | 10-1 or 10-2Need discussion for licensed use | Yes | N/A |  | Per band  | N/A | N/A |  | Upon triggering, UE reports A/N for all HARQ processes and all CCs in a PUCCH group.  | Optional with capability signalling |
| 10-16a | One-shot HARQ ACK feedback trigger with empty DCI 1\_1 | 1. Support feedback of type 3 HARQ-ACK codebook triggered by a DCI 1\_1 without scheduling a PDSCH using a reserved FDRA value | 10-16Need discussion for licensed use | Yes | N/a |  | Per band  | N/A | N/A |  |  | Optional with capability signalling |
| 10-17 | Multi-PUSCH UL grant | 1. Support of scheduling up to 8 PUSCH with a single DCI 0\_1  | 10-1 or 10-2 Need discussion for licensed use | Yes | N/A |  | Per band | N/A | N/A |  |  | Optional with capability signalling |

 |
| [14] | Huawei, HiSilicon |

|  |  |  |
| --- | --- | --- |
| Functionality | FGs | Need for licensed band operation |
| HARQ enhancements | 10-14 Non-numerical PDSCH to HARQ-ACK timing10-15 Enhanced dynamic HARQ codebook10-16 One-shot HARQ ACK feedback10-16a One-shot HARQ ACK feedback trigger with empty DCI 1\_1 | TBD Per band or Per UEFGs 10-14/15/16/16a each offer their own trade-offs between overhead, latency and scheduling flexibility, so they should all be considered together to either be allowed for both licensed and unlicensed bands, or just for unlicensed bands. |
| Multi-PUSCH UL grant | 10-17 Multi-PUSCH UL grant | Per UEThis feature is beneficial for reducing control overhead on licensed bands. To avoid additional complexity, we suggest no further optimization for this feature in Rel-16, so it should be limited to time-consecutive PUSCHs even on licensed bands.. |

***Proposal 2: The following FGs could be extended to licensed bands, i.e. reported “per UE”:**** ***10-17 Multi-PUSCH UL grant***

**FG 10-16a (One-shot HARQ ACK feedback trigger with empty DCI 1\_1)**FG10-16 does not need to be a prerequisite for FG10-16a. Otherwise it would make more sense to merge the two FGs into a single FG. |

**Based on above, following update for FGs 10-14/10-15/10-16/10-16a would be acceptable.**

|  |  |  |
| --- | --- | --- |
| 10-14 | Non-numerical PDSCH to HARQ-ACK timing | 1. Support configuration of a value for dl-DataToUL-ACK indicating an i~~m~~napplicable time to report HARQ ACK |
| 10-15 | Enhanced dynamic HARQ codebook | 1. Support of bit fields signalling PDSCH HARQ group index and NFI in DCI 1\_12. Support of bit field in DCI 0\_1 and DCI 1\_1 for other group total DAI if configured. 3. Support the retransmission of HARQ ACKFFS if need to further split under other group DAI/NFI configured or not |
| 10-16 | One-shot HARQ ACK feedback | 1. Support feedback of type 3 HARQ-ACK codebook, triggered by a DCI 1\_1 scheduling a PDSCH |
| 10-16a | One-shot HARQ ACK feedback trigger with empty DCI 1\_1 | 1. Support feedback of type 3 HARQ-ACK codebook triggered by a DCI 1\_1 without scheduling a PDSCH using a reserved FDRA value |

**In addition, following points should be discussed for FGs 10-14/10-15/10-16/10-16a/10-17.**

* **Whether or not 10-14/10-15/10-16/10-16a/10-17 can be extended to licensed use**
* **Whether or not 10-14/10-15/10-16/10-16a/10-17 can be combined into a single FG**
	+ **If no, whether or not 10-15 can be further split under other group DAI/NFI configured or not**

# **10-18, 10-24 and 10-28: Configured grant enhancements**

In [1], FGs 10-18, 10-24 and 10-28 are captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-18 | Configured grant with retransmission in CG resources  | 1. Support retransmission in CG resources2. Support configured grant retransmission timer3. Support DFI monitoring4. Support CG-UCI in CG-PUSCH | 10-1 or 10-2,5-19 or 5-20Need discussion for licensed use | Yes | N/A |  | Per band | N/A | N/A |  | Support configured grant with retransmission in configured grant resource | Optional with capability signalling |
|  | 10-24 | CG-UCI multiplexing with HARQ ACK | 1. Support multiplexing CG-UCI with HARQ ACK | 10-18,5-19 or 5-20Need discussion for licensed use | Yes | N/A |  | Per band | N/A | N/A |  |  | Optional with capability signalling |
|  | 10-28 | Configured grant with Rel-16 enhanced resource configuration | 1. Support configuration of resources with cg-nrofSlots-r16 and cg-nrofPUSCH-InSlot-r16, | 10-185-19 or 5-20 | Yes | N/A |  | FFS Per band or Per UE | N/A | N/A |  |  | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [2] | ZTE, Sanechips | There has been various enhancements made in NR-U WI on different aspects based on Rel-15 NR design. For the enhancements on the same aspect, it may not be a good way to split the features into too many small pieces and make all of them as optional. It would be hard for network to implement and utilize a meaningful Rel-16 functionality if different UEs support drastically different combinations of feature groups for one aspect. For example for the interlace structure, currently there are 4 optional feature groups defined for PUSCH and each of the PUCCH formats respectively, which implies one UE may support interlaced PUSCH but not support interlaced PUCCH, or vice versa. This is not necessary, as in the RRC signalling there is only one parameter to just indicate whether the interlaced structure is enabled or not. Therefore, it would be better to merge them into one feature group. Similar principle can be applied to the enhancements on HARQ and configured grant.***Proposal 2:*** * ***To avoid implementation complexity, the enhancements on the same aspect should be combined into one feature group, including the following:***
	+ ***Interlaced structure: combine 10-3, 10-3a, 10-3b, and 10-3c***
	+ ***HARQ enhancement: combine 10-14, 10-15, 10-16, 10-16a, and 10-17***
	+ ***Configured grant: combine 10-18 and 10-28***
* CG enhancement: FG 10-18 and 10-24.

The enhancement on the configured grant, for example the CG-UCI and retransmission on CG resources have been discussed in Rel-15, but not agreed at that moment. And then in Rel-16 URLLC WI, the configured grant has been enhanced with different approaches. If the enhancements in NR-U are applied to licensed spectrum, there will be two ways to do configured grant which are not compatible. It is not clear on the configurations and UE behavior for the operation of configured grant. So we think the CG enhancement shall not be applied to licensed spectrum at least in Rel-16. We can further discuss how to optimize the URLLC for NR-U in Rel-17. |
| [3] | vivo | For other UE features, the extension to licensed band could be considered if the benefit is identified in certain licensed scenario.**Proposal 2: For UE features that are not agreed to be extended to licensed use, update “per band” to “per unlicensed band”.** On **10-24/28 (***CG-UCI multiplexing with HARQ ACK* and *Configured grant with Rel-16 enhanced resource configuration*), we propose to remove the prerequisite 10-18 (*retransmission on CG resource*) as 10-18 is not essentially needed in all the cases for enhanced configured grant in NRU.**Proposal 8: Remove the prerequisite 10-18 for 10-24/28.** |
| [4] | OPPO | **FG 10-28**: this FG is about the UE capability of supporting CG resource configuration. Moreover, there is a chicken-egg problem with FG 10-18. In our view, FG 10-28 is the pre-requisite FG for FG 10-18. Regarding repetition, in the rapporteur’s note, the CG repetition capability is already covered in Rel-15, but this should be clarified that the Rel-15 CG repetition is different from NRU CG repetition, for example, UE may select the first transmission occasion according to the CG resources and RV by itself in NRU. In this case, the CG dedicated feature should be additionally implemented, which is difficultly bundled with Rel-15 FG. It would be naturally possible that a UE supports Rel-15 CG repetition but not support NRU CG repetition. We would suggest that dedicated FG should be added to reflect this particular capability.

|  |  |  |
| --- | --- | --- |
| 10-18 | Configured grant with retransmission in CG resources  | 1. Support retransmission in CG resources2. Support configured grant retransmission timer~~3. Support DFI monitoring~~~~4. Support CG-UCI in CG-PUSCH~~ |
| 10-28 | Configured grant with Rel-16 enhanced resource configuration | 1. Support configuration of resources with cg-nrofSlots-r16 and cg-nrofPUSCH-InSlot-r16~~,~~2. Support DFI monitoring3. Support CG-UCI in CG-PUSCH |
| 10-28a | Configured grant repetition | 1. Support CG repetition2. Support UE selected first transmission occasion and RV |

**Proposal 7: Move DFI monitoring and CG-UCI transmission from feature group 10-18 to 10-28.****Proposal 8: Introduce a feature group to support configured grant repetition in NRU.**  |
| [5] | MediaTek Inc. | Proposal 1: NR-U features can only be extended to licensed operation when uses cases and benefits are well justified.  |
| [8] | Ericsson | This feature should not have feature group 10-18 as a pre-requisite since the enhancement of resource configuration is also applicable to CG without the functionalities in 10-18.1. For FG 10-28 remove the pre-requisite 10-18
 |
| [9] | Samsung | NR-U functions have been introduced to handle inherit problem of unlicensed band such as LBT failure and regulation. Hence, in our view, except FG-8 and FG-11 which are general function for licensed band, applicability of NR-U feature groups should be restricted to unlicensed band. If some of NR-U feature groups are identified to be beneficial for licensed band operation, we will be able to make an agreement for each.**Proposal 2: UE features for NR-U should be used only for unlicensed band.** |
| [13] | Qualcomm Incorporated | 10-28: Need discussion on if 10-18 is a prerequisite |
| [14] | Huawei, HiSilicon |

|  |  |  |
| --- | --- | --- |
| Functionality | FGs | Need for licensed band operation |
| CG with retransmission in CG resources | 10-18 Configured grant with retransmission in CG resources10-24 CG-UCI multiplexing with HARQ ACK10-28 Configured grant with Rel-16 enhanced resource configuration | Per bandThe flexibility was introduced considering potential LBT failure in unlicensed band. No strong motivation to have it in licensed band. CG in licensed band is usually for URLLC and multiplexing of CG-UCI in CG-PUSCH might cause reliability issue. It might not be compatible with CG in Rel-15/16 in licensed band because UE will assume ACK when no NDI toggle is detected.  |

 |

**Based on above, following conclusion would be acceptable.**

* **10-18/10-24/10-28 are used for unlicensed band only.**

**In addition, following points should be discussed for FGs 10-18/10-24/10-28.**

* **Whether or not 10-18/10-24/10-28 can be combined into a single FG**
	+ **If no, whether or not 10-18 can be removed from prerequisite of 10-28**

# **[10-19] to [10-19c]: Number of LBT bandwidth and its related feature groups**

In [1], FGs 10-19 to 10-19c are captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-19 | Number of LBT bandwidthFFS if this is needed | Number of ED measurements the UE is able to perform simultaneously[Whether the UE in WB operating mode can support nx20MHz measurement | 10-1 or 10-2 | Yes | N/A |  | Per band | N/A | N/A |  | This is the number of LBT bandwidth a UE can perform separate ED check on simultaneously | Optional with capability signalling |
| 10-19a | Support DL reception with subset of RB sets | 1. When DL BWP has multiple RB sets, support using the available RB set bitmap in DCI 2\_0 to validate the periodic CSI-RS transmission if the CSI-RS is over multiple RB-sets | 10-1 or 10-2 | Yes | N/A |  | Per band | N/A | N/A |  | Without this capability, UE will assume all RB sets in the DL BWP are all transmitted or none of them are transmitted | Optional with capability signalling |
| 10-19b | Support UL transmission with subset of RB sets passing LBT | 1. When UL BWP has multiple RB sets, support transmission of UL signal or channels when LBT passes for only the RB sets the UL signals or channels are located | 10-1 or 10-2 | Yes | N/A |  | Per band | N/A | N/A |  | Without this capability, UE will transmit UL when all RB sets in the UL BWP pass LBT | Optional with capability signalling |
| [10-19c] | Support intra-cell guard band(s) for DL carrier BW > 20MHz | Support DL frequency domain resource allocation type 0 with PRG partially overlapped with Type-2 intra-cell gard band between two adjacent LBT RB sets where CCA is clear on only one of RB sets as defined by RAN4, and rate matching around the guard bands either at RB level (in case of wideband precoding) or at PRG level (in case of precoding granularity of 2 or 4 RBs) according to the information provided by DCI Format 2\_0 available RB set bitmap and RRC intra-cell guard band configurations | 10-1a | Yes | N/A |  | [Per band] | N/A | N/A |  |  | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [3] | vivo | On **10-19a** (*Support DL reception with subset of RB sets*), it seems only related with CSI-RS from component description but not aligned with the feature name or description part. It should be clarified what’s the intention for this UE feature.**Proposal 5: Clarify the intention of 10-19a.** |
| [4] | OPPO | **FG 10-19**: Our initial understanding of this FG is the capability of simultaneously performing multiple LBT within the same CC. A typical use case is that an active UL BWP contains more than one LBT subbands. When the scheduled resources are spreading over multiple LBT subbands, the UE needs the capability of performing simultaneous LBT. Therefore, this feature is not tightly related to CA.**Proposal 5: Keep feature group 10-19 to support nx20MHz measurement simultaneously.**  |
| [5] | MediaTek Inc. | For 10-19c, the description of the component is lack of the support of agreements. It is not clear what the use cases and benefits of this proposal while it require to specify new UE behaviour. We should discuss it first under the NR-U agenda item before we can agree to this feature. **Proposal 12: FG 10-19c, discuss it under the NR-U agenda item.**  |
| [6] | LG Electronics | In our view, FG 10-19 is not needed, with the following understandings.* This feature group is related to UE capability on how many 20 MHz LBT bandwidths UE can perform energy detection based channel access procedure at the same time.
* The number of LBT bandwidths supported by a UE would be determined based on the UE’s capability on supported carrier BW. In other words, if a UE indicates the support of 80 MHz carrier BW, then the UE should support up to 4 LBT bandwidths.

**Proposal #4: Remove FG 10-19 from NR-U UE feature list.**The necessity of this feature group should be first discussed in RAN1. To be specific, our opinion is that this is not needed since rate-matching pattern supported in Rel-15 seems to work also for the case of type-1/2 intra-cell guard band.**Proposal #5: Remove FG 10-19c from NR-U UE feature list.** |
| [7] | Intel Corporation | In the context of 10-19b, in previous meetings RAN1 has made the agreements listed below on the UL wideband operation. From them, it is straightforward that a UE will transmit UL channels using the RB sets that overlap with the resource allocation for the UL transmission. From this perspective, the UE only perform the transmission based on the LBT outcomes of the RB sets of interest. Since LBT operation is performed per RB set (LBT BW), we do not see any motivation to define the feature group of 10-19b.

|  |
| --- |
| Agreement:* For UL transmissions in a serving cell with carrier bandwidth greater than the LBT bandwidth, for the case where UE performs CCA before UL transmission, UE transmits on the UL only if CCA is successful at UE in all LBT bandwidths that overlap with the resource allocation for the UL transmission
* The UE is not expected to receive resource allocations in discontiguous LBT bandwidths within a wideband carrier
	+ This does not preclude such resource allocation in discontiguous LBT bandwidths being supported by specifications managed by RAN1 in Rel-16.
 |

As for 0-19c, we do not have enough justification to support it due to the lack of discussion. Therefore, there is need to discuss further whether this is really needed. Also, it is not clear on the reason that the prerequisite is only 10-1a (only for DL-only operation under dynamic channel access mode). **Proposal 4:** * **Remove 10-19b.**
* **Discuss more on the necessity of 10-19c.**
 |
| [8] | Ericsson | Regarding the FFS, this feature group is needed, as it is important for the network to know the UE capability to enable proper UL scheduling.1. Keep FG 10-19; FFS can be deleted

It seems that this capability is more general and applies not only to CSI-RS but also PDSCH. We suggest to add a second component to this feature group. It can be further discussed if this is a separate capability, or whether it should be merged with 10-19c1. Add a component to FG 10-19a for reception of PDSCH over a subset of RB sets as follows

|  |  |  |  |
| --- | --- | --- | --- |
| 10-19a | Support DL reception with subset of RB sets | 1. When DL BWP has multiple RB sets, support using the available RB set bitmap in DCI 2\_0 to validate the periodic CSI-RS transmission if the CSI-RS is over multiple RB-sets2. When DL BWP has multiple RB sets, support PDSCH reception on a subset of RB sets | Without this capability, UE will assume all RB sets in the DL BWP are all transmitted or none of them are transmitted |

It should be clarified which signals/channels to which this FG applies. It is already specified that PUSCH is only transmitted if LBT is successful on all scheduled RB sets. Hence it seems that this capability is related to SRS only.1. Clarify to which signals/channels to which FG-19b applies, e.g., SRS only.

In principle we agree that FG 10-19c is needed, either as a separate FG or merged with 10-19a; however, several aspects need to be clarified. It is not clear what Type-2 intra-cell guard bands are. Also, our understanding of the available RB-set bitmap is that it indicates to the UE which RB sets for which the UE can skip PDCCH monitoring. PDSCH reception is controlled by the scheduling DCI, so there is not a dependence on decoding DCI 2\_0. It should also be clarified what is the gNB/UE assumption if the capability is not supported. Shall the UE be scheduled only if LBT is successful in all RB sets as mentioned in FG 10-19a?1. FG 10-19c is needed (or can be merged with 10-19a); clarify FG description.
 |
| [9] | Samsung | During the email discussion, following feature groups (10-19c, 10-22, and 10-31) have been added without discussion in NR-U WI. These features would affect not only UE behaviour but also gNB implementation so that sufficient discussion should be proceeded before the introduction. Hence, we propose to remove above feature groups in UE feature list for NR-U at this stage.**Proposal 1: Remove FG 10-19c, 10-22, and 10-31 in UE feature list for NR-U.** |
| [10] | Apple | As detailed in our companion paper [2], we believe the FG 10-19c should be added for Type 0 resource allocation to provide flexibility at the UE to avoid processing increased number of PRG(s) due to puncturing by Type-2 CC guard band. More specifically, UE behavior can be different depending on the precoding granularity configurations. If PRG size is one of two values {2,4}, the overlapped PRG should be not used. On the other hand, for wideband configuration, RB-level rate-matching is still possible without increasing complexity. **Proposal 1:** * *For DL wideband operation and Type-0 RA, UE feature FG 10-19c should be introduced as optional feature to allow rate-matching around the overlapped PRG level with Type-2 intra-CC guard band in case of PRG = 2/4 or overlapped RB(s) with Type-2 intra-CC guard band for the case of wideband precoding.*
 |
| [11] | Sharp | FG 10-19 specifies the number of ED measurements the UE is able to perform simultaneously. We see that it is not necessary since the number of ED measurements should be implicitly determined by the supported channel bandwidth. If the UE supports 80 MHz channel bandwidth, the UE is required to support 4 ED measurements.**Proposal 1: FG 10-19 is not necessary since the number of ED measurements is determined by the supported channel bandwidth.**The functionality of FG 10-19a coincides with FG 10-29. Both FG indicates RB-set indicator interpretation in DCI format 2\_0. Thus, we propose to delete FG 10-19a from the list.**Proposal 2: FG 10-19a is deleted from the list since the functionality coincides with FG 10-29.** |
| [12] | Nokia, Nokia Shanghai Bell | * 10-19: Numbers need to be more clear, otherwise we need to assume maximum is supported always. Is this applicable for all LBT types with ED measurement equally?
* 10-19b: Feature is not needed as it is not fundamentally different single-RB set operation.
* 10-19c: Feature is under discussion in R16 NR-U maintenance.
 |
| [13] | Qualcomm Incorporated |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
| 10-19a | Support DL reception with subset of RB sets | 1. When DL BWP has multiple RB sets, support using the available RB set bitmap in DCI 2\_0 to validate the periodic CSI-RS transmission if the CSI-RS is over multiple RB-sets | 10-1 or 10-2 | Yes | N/A |  | Per band | N/A | N/A |  | Without this capability, UE will assume all RB sets in the DL BWP are all transmitted or none of them are transmitted | Optional with capability signalling |
| 10-19b | Support UL transmission with subset of RB sets passing LBT | 1. When UL BWP has multiple RB sets, support transmission of UL signal or channels when LBT passes for only the RB sets the UL signals or channels are located | 10-1 or 10-2 | Yes | N/A |  | Per band | N/A | N/A |  | Without this capability, UE will transmit UL when all RB sets in the UL BWP pass LBT | Optional with capability signalling |
| [10-19c] | Suppport intra-cell guard band(s) for DL carrier BW > 20MHz | Support DL frequency domain resource allocation type 0 with PRG partially overlapped with Type-2 intra-cell gard band between two adjacent LBT RB sets where CCA is clear on only one of RB sets as defined by RAN4, and rate matching around the guard bands either at RB level (in case of wideband precoding) or at PRG level (in case of precoding granularity of 2 or 4 RBs) according to the information provided by DCI Format 2\_0 available RB set bitmap and RRC intra-cell guard band configurations | 10-19a | Yes | N/A |  | [Per band] | N/A | N/A |  |  | Optional with capability signalling |

10-19: We propose to remove this as the functionality is included in band combination capability, and 10-19a and 10-19b are introduced10-19c: We are fine introducing this. However, should the prerequisite be 10-19a? Also the title may need some clarification. Might be better to describe this as “support partial PRG reception on the intra-cell guard band boundary |
| [14] | Huawei, HiSilicon | **FG 10-19 (Number of LBT bandwidth)**There is no need to have a separate L1 feature group of 10-19. It can be derived implicitly from the supported channel combinations. If the carrier bandwidth is larger than 20 MHz, the UE should be capable to perform LBT on all LBT bandwidths in the carrier. It is proposed to delete FG10-19.**FG10-19a (Support DL reception with subset of RB sets)**The component should be clarified, it should be about the basic behavior in support of the configuration of intra-cell guard band where the UE assumes there is no data mapped to the intra-cell guard (which may happen with a PDSCH scheduled by DCI format 1\_0). Another component should be added to FG10-19a.**FG10-19b (Support UL transmission with subset of RB sets passing LBT)**Change “only” to “at least”, or delete “only” from the component description: *When UL BWP has multiple RB sets, support transmission of UL signal or channels when LBT passes for ~~only~~ the RB sets the UL signals or channels are located.***FG10-19c (Support DL reception with subset of RB sets and support intra-cell guard bands)**We support removing the brackets of FG10-19c.  |

**Based on above, following point should be discussed for FGs 10-19/10-19a/10-19/b/10-19c.**

* **Whether or not 10-19/10-19a/10-19b/10-19c are needed**

# **10-20 and 10-20a: Search space set and CORESET configurations for wide-band operation**

In [1], FGs 10-20 and 10-20a are captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-20 | Support search space set configuration with freqMonitorLocation-r16 | 1. Support search space set configuration with freqMonitorLocations-r16 | 10-1, 10-1a, 10-2, or 10-2aNeed discussion for licensed use | Yes | N/A |  | Per band | N/A | N/A |  |  | Optional with capability signalling |
| 10-20a | Support coreset configuration with rb-Offset | 1. Support coreset configuration with rb-Offset  | 10-1, 10-1a, 10-2, or 10-2aNeed discussion for licensed use | Yes | N/A |  | Per band | N/A | N/A |  |  | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [2] | ZTE, Sanechips | * CORESET/SS: including FG 10-9/9a/9b/9c, 10-20/20a.

In general, the above enhancements on CORESET/SS could be beneficial to licensed spectrum in terms of enhanced flexibility and reliability. On the other hand, it may introduce implementation complexity for NR UEs. Probably they can be considered as optional features to be applied to NR licensed spectrum. |
| [3] | vivo | For other UE features, the extension to licensed band could be considered if the benefit is identified in certain licensed scenario.**Proposal 2: For UE features that are not agreed to be extended to licensed use, update “per band” to “per unlicensed band”.**  |
| [5] | MediaTek Inc. | Proposal 1: NR-U features can only be extended to licensed operation when uses cases and benefits are well justified. For 10-20, the number of PDCCH search space sets/CORESETs/candidates that UE can monitor is highly related to UE’s complexity. The more cost a UE is willing to pay, the more candidates/search spaces sets/CORESETs the UE is able to process. Therefore, 10-20 should not be just a “whether or not” indication. Instead, it should be a “how many” indication. **Proposal 13: For 10-20, change the component to “Maximum number of frequency domain locations for a search space set configuration with *freqMonitorLocations-r16*”** |
| [7] | Intel Corporation | However, do not see any motivation to let the features for search space set group switching and search space/CORESET configuration in wideband to be used for licensed band. Those features were introduced to overcome the limitation of unlicensed band and we do not see any benefits when used for licensed operation.**Proposal 6:** **Do not open 10-9/10-9a/10-9b/10-20/10-20a for licensed use.** |
| [9] | Samsung | NR-U functions have been introduced to handle inherit problem of unlicensed band such as LBT failure and regulation. Hence, in our view, except FG-8 and FG-11 which are general function for licensed band, applicability of NR-U feature groups should be restricted to unlicensed band. If some of NR-U feature groups are identified to be beneficial for licensed band operation, we will be able to make an agreement for each.**Proposal 2: UE features for NR-U should be used only for unlicensed band.** |
| [12] | Nokia, Nokia Shanghai Bell | * 10-20a: It is OK to support it for licensed use as well.
 |
| [14] | Huawei, HiSilicon |

|  |  |  |
| --- | --- | --- |
| Functionality | FGs | Need for licensed band operation |
| Support search space set configuration with freqMonitorLocation-r16 | 10-20 Support search space set configuration with freqMonitorLocation-r16 | Per bandThe motivation of this feature is to save RRC signaling overhead and complexity to configure too many CORESETs when UE is expect to monitor PDCCH on multiple RB sets in case gNB may fail to transmit PDCCH on RB set where LBT fail. In licensed band, there is no LBT failure and UE can be configured with exact CORESET location in the BWP. |
| Support coreset configuration with rb-Offset | 10-20a Support coreset configuration with rb-Offset | Per bandThe motivation of this feature is to increase usable CCE in a CORESET confined in fixed LBT bandwidth. In licensed band, there is no such restriction from LBT bandwidth.  |

**FG 10-20 (Support search space set configuration with freqMonitorLocation-r16**FG10-20a and 10-19a should be prerequisites for FG10-20. |

**Based on above, following conclusion would be acceptable.**

* **10-20 is used for unlicensed band only.**

**In addition, following points should be discussed for FGs 10-20/10-20a.**

* **Whether or not the component of 10-20 can be changed to “Maximum number of frequency domain locations for a search space set configuration with *freqMonitorLocations-r16*”**
* **Whether or not 10-20a can be extended to licensed use**
	+ **If no, whether or not 10-20a can be prerequisites for 10-20**

# **10-21: Support using ED threshold for UL to DL COT sharing**

In [1], FG 10-21 is captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-21 | Support using ED threshold for UL to DL COT sharing | 1. Use ULtoDL-CO-SharingED-Threshold-r16 for cat 4 LBT for scheduled UL to share COT with gNB for DL2. Use ULtoDL-CO-SharingED-Threshold-r16 for cat 4 LBT for CG-PUSCH to share COT with gNB for DL3. Indicate in CG-UCI the COT sharing information as configured in cg-COT-Sharing-r16 | 10-1 | Yes | N/A |  | Per band | N/A | N/A |  |  | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| [4] | OPPO | **FG 10-21**: In our view whether or not the ULtoDL-CO-SharingED-Threshold-r16 is provided, the CG-UCI indication fields will be implemented differently. And either way can support the COT sharing function. In this case, the UE should be allowed to report which one is supported.

|  |  |  |
| --- | --- | --- |
| 10-21a | Support using ED threshold for UL to DL COT sharing | 1. Use ULtoDL-CO-SharingED-Threshold-r16 for cat 4 LBT for scheduled UL to share COT with gNB for DL2. Use ULtoDL-CO-SharingED-Threshold-r16 for cat 4 LBT for CG-PUSCH to share COT with gNB for DL3. Indicate in CG-UCI the COT sharing information |
| 10-21b | Support UL to DL COT sharing | 1. Support cat 4 LBT for scheduled UL to share COT with gNB for DL without ULtoDL-CO-SharingED-Threshold-r162. Support cat 4 LBT for CG-PUSCH to share COT with gNB for DL without ULtoDL-CO-SharingED-Threshold-r163. Indicate in CG-UCI the COT sharing information |

**Proposal 6: Introduce a feature group to support UL to DL COT sharing without using ED.**  |

**Based on above, following point should be discussed for FG 10-21.**

* **Whether or not following update can be applied**

|  |  |  |
| --- | --- | --- |
| 10-21a | Support using ED threshold for UL to DL COT sharing | 1. Use ULtoDL-CO-SharingED-Threshold-r16 for cat 4 LBT for scheduled UL to share COT with gNB for DL2. Use ULtoDL-CO-SharingED-Threshold-r16 for cat 4 LBT for CG-PUSCH to share COT with gNB for DL3. Indicate in CG-UCI the COT sharing information |
| 10-21b | Support UL to DL COT sharing | 1. Support cat 4 LBT for scheduled UL to share COT with gNB for DL without ULtoDL-CO-SharingED-Threshold-r162. Support cat 4 LBT for CG-PUSCH to share COT with gNB for DL without ULtoDL-CO-SharingED-Threshold-r163. Indicate in CG-UCI the COT sharing information |

# **10-22: No gap 2-step RACH msgA transmission**

In [1], FG 10-22 is captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-22 | No gap 2-step RACH msgA transmission | 1. Support transmitting PRACH and PUSCH of msgA without gap in betweenFFS if RAN1 can disallow this in NR-U. | 10-1 or 10-2 and 9-1 | Yes | N/A |  | Per band | N/A | N/A |  | For licensed case, a minimum gap between PRACH and PUSCH of msgA is introduced, but is not applicable to NR-U | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [5] | MediaTek Inc. | As to 10-22, in Rel-16, msgA PRACH and msgA PUSCH are only allowed to be transmitted in different slots. Looking at the R15 PRACH configuration for TDD in FR1 (Table 6.3.3.2-3 in 38.211), there would be always gaps between msgA PRACH and msgA PUSH for formats A1/A2/A3. While for formats B1, C0, A1/B1, A2/B2, A3/B3, there would be always a gap in between the associated RACH occasion and PUSCH occasion expect for the last RACH occasion in a slot. Now, it only leaves formats B4 and C2 on the table which in total have 46 out of the 256 preambles. If not all the UEs in the cell can support no gap in between its msgA PRACH and msgA PUSCH transmissions, it means there should be gaps in the cell-specifically configured PRACH resources and PUSCH resources. The “no-gap msgA” is only applicable to CFRA.**Observation 1: The cases that UE can take advantage from supporting no gap in between msgA PRACH and msgA PUSCH are not many.****Proposal 14: Apply the same gap defined in the R15 to msgA PRACH for NR-U.****Proposal 15: Remove 10-22 from the UE feature list.**  |
| [6] | LG Electronics | In general, it seems beneficial to allow continuous transmission (with no gap) between PRACH and PUSCH for a same msgA especially for NR-U, in terms of reducing the channel access procedure to be performed by the UE. Regarding this issue, the method to support no gap between RACH and PUSCH is discussed in our companion paper [2] (e.g., by using extended CP of PUSCH).**Proposal #6: Further discuss how to support no gap between RACH and msgA PUSCH for 2-step RACH procedure, under corresponding NR-U agenda item.** |
| [8] | Ericsson | As indicated in our contribution in the Initial Access Enhancements agenda item, we support no gap (N = 0) for unlicensed operation since it enables MsgA configuration using some PRACH formats with a gap of less than 16us between PRACH and PUSCH thus avoiding an extra LBT operation. This is one of the primary benefits of 2-step RACH in unlicensed.1. FG 10-22 is needed so that UEs can indicate support for no gap (N = 0) between the PRACH and PUSCH parts of MsgA for 2-step RACH
 |
| [9] | Samsung | During the email discussion, following feature groups (10-19c, 10-22, and 10-31) have been added without discussion in NR-U WI. These features would affect not only UE behaviour but also gNB implementation so that sufficient discussion should be proceeded before the introduction. Hence, we propose to remove above feature groups in UE feature list for NR-U at this stage.**Proposal 1: Remove FG 10-19c, 10-22, and 10-31 in UE feature list for NR-U.** |
| [10] | Apple | FG 10-22 proposed to introduce UE capability to indicate support 2-step RACH procedure without gap between PRACH and PUSCH of MsgA. We acknowledge the comment that there is no agreement made in NR-U session to support this. On the other hand, we understand the benefits without gap for unlicensed operation and can be fine to support it in case of same numerology between PRACH and PUSCH. However, if different numerologies between PRACH and PUSCH are configured, the gap agreed under 2-step WI should be used. The FG 10-22 is modified correspondingly to implement the suggestion.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 10-22 | No gap 2-step RACH msgA transmission | 1. Support transmitting PRACH and PUSCH of msgA without gap in between if a same numerology is configured;
2. With Gap between PRACH and msgA if different numerologies are configured.

FFS if RAN1 can disallow this in NR-U. | 10-1 or 10-2 and 9-1 | Per-band | Optional with capability signalling |

**Proposal 3:** * *Modify the FG 10-22 to support no gap between PRACH and PUSCH Msg-A in case of same numerology; Otherwise, support the gap if different numerologies are configured.*
 |
| [14] | Huawei, HiSilicon | **FG 10-22 (No gap 2-step RACH msgA transmission)**In 2-step RACH agenda item, a minimum gap is defined between msgA PRACH and msgA PUSCH for licensed operation, and no such decision is made for unlicensed operation.Agreements**:*** The minimum transmission gap between the end of msgA PRACH and the beginning of msgA PUSCH (guard time excluded) is no less than Ngap symbols, as specified in TS 38.213, i.e., 2 or 4 symbols depending on the SCS
	+ This is not applied for NR-U
	+ Note: This is aligned with Rel-15

This means that there is no agreement for NR-U of what should be the minimum gap between the end of msgA PRACH and the beginning of msgA PUSCH (guard time excluded), including no agreement to support no gap in NR-U. What values of gap can a UE be allowed to signal as a capability for NR-U? The default, as clarified in the agreement copied above, should be aligned with Rel-15.In the moderator’s proposal, “*FFS if RAN1 can disallow this in NR-U*” in FG10-22 is incorrect and should be changed to “*FFS if RAN1 can allow this in NR-U*”.

|  |  |  |
| --- | --- | --- |
| 10-22 | No gap 2-step RACH msgA transmission | Support transmitting PRACH and PUSCH of msgA without gap in betweenFFS if RAN1 can disallow this in NR-U. |

We think that the licensed band design is sufficient for 2-step RACH with NR-U, and allows reusing the same BS receiver implementation, which is the Rel-15 implementation. If a UE has to perform LBT between PRACH and PUSCH of msgA, then the UE will either pass LBT and be able to transmit msgA faster than by 4-step RACH even with a 2 or 4 symbols gap, or the UE will fail LBT which probably indicates that it would be better for the UE to choose another 20 MHz channel for initial access in unlicensed band because the current 20 MHz channel is already heavily congested since the UE would have passed on LBT and failed one LBT in a short interval. Therefore a NR-U UE can reuse the 2-step RACH FG to signal its capability and there is no need for a specified NR-U FG for 2-step RACH. Hence, “FFS if RAN1 can disallow this in NR-U” in FG10-22 is incorrect and should be changed to “FFS if RAN1 can allow this in NR-U”.***Proposal 3: No gap is not supported for NR-U and 10-22 (no gap 2-step RACH msgA transmission) should be deleted until further agreement.*** |

**Based on above, following point should be discussed for FG 10-22.**

* **Whether or not 10-22 is needed**

# **10-23: CGI reading based on off-sync raster SSB for ANR functionality**

In [1], FG 10-23 is captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-23 | CGI reading based on off-sync raster SSB for ANR functionality | 1. Support acquisition of relevant information from a neighbouring NR unlicensed cell in an unlicensed carrier by reading the RMSI of the neighbouring unlicensed cell and reporting the acquired information to the network | 10-1, 10-1a, 10-2, or 10-2a | Yes | N/A |  | Per band | N/A | N/A |  | Support reading RMSI from SCell from an off-sync raster SSB for ANR | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| [5] | MediaTek Inc. | In addition, PCI collision is no new issue in NR-U. LTE-LAA has the same issue. However, it is resolved by eNB without mandating UE to read and report CGI. **Proposal 7: CGI reading of an unlicensed cell for ANR functionality should be UE capability regardless whether its SSB is on or off sync rater.**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 10-23 | CGI reading ~~based on off-sync raster SSB~~of an unlicensed cell for ANR functionality | 1. Support acquisition of relevant information from a neighbouring NR unlicensed cell in an unlicensed carrier by reading the RMSI of the neighbouring unlicensed cell and reporting the acquired information to the network | 10-1, 10-1a, 10-2, or 10-2a | Yes | N/A |  | Per band | N/A | N/A |  | Support reading RMSI from SCell from an off-sync raster SSB for ANR | Optional with capability signalling |

 |

**Based on above, following point should be discussed for FG 10-23.**

* **Whether or not following update can be applied**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 10-23 | CGI reading ~~based on off-sync raster SSB~~of an unlicensed cell for ANR functionality | 1. Support acquisition of relevant information from a neighbouring NR unlicensed cell in an unlicensed carrier by reading the RMSI of the neighbouring unlicensed cell and reporting the acquired information to the network | 10-1, 10-1a, 10-2, or 10-2a | Yes | N/A |  | Per band | N/A | N/A |  | Support reading RMSI from SCell from an off-sync raster SSB for ANR | Optional with capability signalling |

# **10-25: Enable configured UL transmission out of COT**

In [1], FG 10-25 is captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-25 | Enable configured UL transmission out of COT | 1. Support configuration of enableConfiguredUL-r16 and enable Cat 4 LBT based transmission of RRC configured UL \*SRS, PUCCH, CG-PUSCH etc) out of COT when DCI 2\_0is configured but not detected | 10-1 | Yes | N/A |  | Per band | N/A | N/A |  |  | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [3] | vivo | On **10-25** (*Enable configured UL transmission out of COT*), to be more accurate, we suggest to change “DCI 2\_0” to “SFI” since DCI 2\_0 is not SFI only in NRU Rel-16.**Proposal 6: Change “DCI 2\_0” to “SFI” in the component of 10-25.**  |
| [5] | MediaTek Inc. | For 10-25, change “RRC configured UL” to “higher-layer configured UL” to be aligned with the specification. And remove Cat 4 LBT from the description. We did not make the agreement only for LBE. It is applicable to FBE as well.**Proposal 16: In 10-25, change “RRC configured UL” to “higher-layer configured UL” to be aligned with the specification.****Proposal 17: Remove Cat 4 LBT from the description of 10-25.**  |
| [8] | Ericsson | The description of the feature group and its components is erroneous. The ability to use the configuration of *enableConfiguredUL-r16* has nothing to do with whether the configured UL transmission happens inside or outside the COT. This parameter applies to both cases and the type of UL channel access method used is conditioned on whether the transmission happens within or outside the COT based on another parameter. Hence “Cat 4 LBT” and “out of COT” should be removed from the description of the feature group and its components.1. Modify the FG name and description as follows:

|  |  |  |
| --- | --- | --- |
| 10-25 | Enable configured UL transmissions when DCI 2\_0 is configured but not detected ~~out of COT~~ | 1. Support configuration of enableConfiguredUL-r16 and enable ~~Cat 4 LBT based~~ transmission of RRC configured UL \*SRS, PUCCH, CG-PUSCH etc) ~~out of COT~~ when DCI 2\_0 is configured but not detected |

 |
| [14] | Huawei, HiSilicon | **FG10-25 (enable configured UL transmission out of COT)**It is not clear whether it is gNB acquired COT or UE acquired COT.  |

**Based on above, following point should be discussed for FG 10-23.**

* **Whether or not following update can be applied**

|  |  |  |
| --- | --- | --- |
| 10-25 | Enable configured UL transmissions when SFI is configured but not detected ~~out of COT~~ | 1. Support configuration of enableConfiguredUL-r16 and enable ~~Cat 4 LBT based~~ transmission of ~~RRC~~higher-layer configured UL \*SRS, PUCCH, CG-PUSCH etc) ~~out of COT~~ when SFI~~DCI 2\_0~~ is configured but not detected |

# **10-26: CSI-RS based RLM outside of discovery burst transmission window**

In [1], FG 10-26 is captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-26 | CSI-RS based RLM outside of discovery burst transmission window | Support RLM measurements using CSI-RS resources that are outside of discovery burst transmission window | 10-1 or 10-2 | Yes | N/A |  | Per band | N/A | N/A |  |  | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [3] | vivo | On **10-26 (***CSI-RS based RLM outside of discovery burst transmission window*), we do not see the motivation for having this feature group as there is currently no new RLM behavior defined for unlicensed band. If new RAN1 agreement is made for RLM, this UE feature could be revisited.**Proposal 7: Remove 10-26 currently and revisit it when any RLM enhancement is agreed for NRU.** |
| [5] | MediaTek Inc. | Without any agreements on “the initial signal” design and any guaranteed DL transmissions (e.g. (GC-) PDCCH) in the beginning of a COT, it is challenging to UE to adjust AGC and conduct periodic/semi-persistent DL reception. We hence propose the following. **Proposal 9: Periodic/semi-persistent CSI-RS reception without SSB/PDCCH in the beginning of a COT should be UE capability. Support 10-26, 10-31 and 10-32.**  |
| [8] | Ericsson | It is not clear why this feature group is needed as Rel-15 already includes RLM measurements based on CSI-RS. There should be no dependency on inside or outside the discovery burst transmission window (formerly DRS window) as CSI-RS is not constrained to be either inside or outside the window, in contrast to SS/PBCH blocks.1. FG 10-26 should be removed; CSI-RS is not constrained to be either inside or outside the discovery burst transmission window.
 |

**Based on above, following point should be discussed for FG 10-26.**

* **Whether or not 10-26 is needed**

# **10-27: Wideband PRACH**

In [1], FG 10-27 is captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-27 | Wideband PRACH | Enhanced PRACH design for NR-U by adopting a single long ZC sequence, with ZC sequence = 1151 for 15kHz and ZC sequence = 571 for 30kHz | 10-1 or 10-2 | Yes | N/A |  | Per band | N/A | N/A |  |  | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| [10] | Apple |

|  |  |
| --- | --- |
| Question | Comments |
| Can we merge 10-27 to 10-1 and 10-2 as components, instead of separate feature? | No. legacy PRACH formats can still be used for RACH procedure and also meets regulatory requirement. The wideband operation was agreed as enhancement feature and unnecessary to merge into basic feature group.  |

 |

**Based on above, no update would be necessary for FG 10-27.**

# **10-29 and 10-30: Support available RB set indicator field and channel occupancy duration indicator field in DCI 2\_0**

In [1], FGs 10-29 and 10-30 are captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | 10-29 | Support available RB set indicator field in DCI 2\_0 | Support monitoring DCI 2\_0 to read availableRB-Sets-r16 | 10-1, 10-1a, 10-2, or 10-2a | Yes | N/A |  | Per band | N/A | N/A |  |  | Optional with capability signalling |
| 10-30 | Support channel occupancy duration indicator field in DCI 2\_0 | Support monitoring DCI 2\_0 to read COT duration | 10-1, 10-1a, 10-2, or 10-2a | Yes | N/A |  | Per band | N/A | N/A |  |  | Optional with capability signalling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |
| --- | --- | --- |
| [5] | MediaTek Inc. | Without any agreements on “the initial signal” design and any guaranteed DL transmissions (e.g. (GC-) PDCCH) in the beginning of a COT, it is challenging to UE to adjust AGC and conduct periodic/semi-persistent DL reception. We hence propose the following. **Proposal 8: Components 10-29 and 10-30 should be mandatory for UE. Merge 10-29 and 10-30 to 10-1, 10-2, 10-1x, and 10-2x.**  |
| [6] | LG Electronics | FG 10-29 and FG-30 seem to be essential for NR-U since they enable to* Increase UE’s channel access probability within channel occupancy by allowing to change LBT type
* Reduce UE’s power consumption by skipping PDCCH monitoring for unavailable RB set(s) and adapting PDCCH monitoring frequency

**Proposal #7: FG 10-29 and FG 10-30 are to be the component of basic feature groups such as 10-1, 10-1a, 10-2, and 10-2a.** |
| [10] | Apple |

|  |  |
| --- | --- |
| Question | Comments |
| Can we merge 10-29 to 10-1, 10-1a, and 10-2 as components, instead of separate feature? | Yes. We think it is beneficial and important to merge these two into basic feature group 10-1, 10-1a and 10-2. It should be noted that many NR-U functionalities, especially for wideband operation as well as periodic/SP-CSI-RS processing, are specified assuming DCI 2\_0 is available. As Qualcomm said, many UE behaviors are not defined if the UE cannot detect this DCI format to know the COT structure, we therefore prefer to merge these two features to basic feature groups.  |
| Can we merge 10-30 to 10-1 and 10-1a as components, instead of separate feature? For 10-2, I guess we will need further discussion separately on how necessary the COT duration needs to be indicated. | Yes. COT duration is essential and needed to support COT sharing information.  |

 |
| [11] | Sharp | FG 10-29 requires Support of COT indication since the availability of the RB-sets continues until the end of the COT. Thus, this feature requires COT indication reception or dynamic SFI in DCI format 2\_0. **Proposal 3: Set “10-30 or 3-6” as pre-requisite feature for FG 10-29.** |

**Based on above, following point should be discussed for FG 10-29/10-30.**

* **Whether or not 10-30 or 3-6 can be Prerequisite FGs for 10-29**

# **[10-31]: Support of CSI-RS measurements for CSI reporting and tracking without COT duration from DCI 2\_0**

In [1], FG 10-31 is captured as below.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Need for the gNB to know if the feature is supported | Applicable to the capability signalling exchange between UEs (V2X WI only)”. | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Capability interpretation for mixture of FDD/TDD and/or FR1/FR2 | Note | Mandatory/Optional |
| 10. NR-unlicensed | [10-31] | Support of CSI-RS measurements for CSI reporting and tracking without COT duration from DCI 2\_0 | · Perform CSI measurements for reporting and tracking using CSI-RS resources that are not within a COT duration indicated by DCI 2\_0· Note: This includes the cases when DCI 2\_0 is not configured and when DCI 2\_0 is configured but COT duration is not provided by either CO duration field or SFI. | 10-1a | Yes | N/A |  | [Per band] | N/A | N/A |  |  | Optional with capability signaling |

Following feedbacks are provided in contributions for the RAN1#100bis-e meeting.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| [5] | MediaTek Inc. | Without any agreements on “the initial signal” design and any guaranteed DL transmissions (e.g. (GC-) PDCCH) in the beginning of a COT, it is challenging to UE to adjust AGC and conduct periodic/semi-persistent DL reception. We hence propose the following. **Proposal 9: Periodic/semi-persistent CSI-RS reception without SSB/PDCCH in the beginning of a COT should be UE capability. Support 10-26, 10-31 and 10-32.**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 10. NR-unlicensed | [10-32] | CSI-RS based CBD outside discovery burst transmission windows | Support CBD (candidate beam detection) measurements using CSI-RS resources that are outside transmission windows | 10-1, 10-1a, 10-2, 10-2a, 10-1d, or 10-2e | Yes | N/A |  | [Per band] | N/A | N/A |  |  | Optional with capability signalling |

 |
| [6] | LG Electronics | We support this feature group to avoid significant burden of UE implementation to blindly detect CSI-RS for CSI reporting and tracking, as discussed in our companion paper [R1-2001933].**Proposal #8: Support FG 10-31 for NR-U UE feature list.** |
| [8] | Ericsson | We don’t believe that such a feature group is needed or useful. It is well understood that in unlicensed spectrum, quality cannot be ensured and is always dependent on the number of other devices trying to access the carrier. It is also well understood that CSI-RS measurements for reporting and tracking are highly implementation dependent and rely on the UE admitting measurements into its averaging processes and tracking loops when the UE is able to ascertain reliably that the measurement is legitimate.Consider the two extreme cases, the first where the gNB has excellent access to the channel, similar to licensed spectrum. It is clear that in these cases, the UE can rely on detecting the presence of other transmissions such as SSBs and PDCCHs in order to ensure that the CSI-RS measurements are reliable. In fact, this functionality is so fundamental to the UE that it does not make sense to define a capability for this. In the other extreme, if the gNB is unable to get access to the channel for long periods, it is well understood that not only do CSI-RS measurements get affected, but other core functions also will be affected. In this case, it is not expected that the UE is able to operate normally and would need some duration of transmissions from the gNB before it can measure CSI-RS reliably. In such a situation, a capability does not make sense since no UE would be able to report having the capability to measure CSI-RS under these conditions.So, in summary, the proposed capability is not something that the UE can credibly report unless it is tied to some very specific set of conditions, e.g., some signals such as SSB are received with at least some periodicity or within some vicinity in time from the CSI-RS transmission occasion. These conditions will not only be very difficult to define, but this is the exact task that RAN4 will anyway undertake when defining requirements. Therefore, it is best to just leave it to RAN4 to define a reasonable test case for the UE to be able to measure CSI-RS when DCI 2\_0 is not configured or no pertinent information is received in DCI 2\_0. We also note that there has not been any discussion that has taken place on this issue from a capability perspective thus far.1. FG 10-31 should be removed
 |
| [9] | Samsung | During the email discussion, following feature groups (10-19c, 10-22, and 10-31) have been added without discussion in NR-U WI. These features would affect not only UE behaviour but also gNB implementation so that sufficient discussion should be proceeded before the introduction. Hence, we propose to remove above feature groups in UE feature list for NR-U at this stage.**Proposal 1: Remove FG 10-19c, 10-22, and 10-31 in UE feature list for NR-U.** |
| [10] | Apple | As in Rel-15, NR-U supports DL transmissions that are semi-statically configuration by higher layers including periodic, semi-persistent CSI-RS transmission/reporting, CSI-IM and DL SPS transmission. However, it is possible that these semi-statically configured DL resources maybe actually not transmitted by gNB due to LBT failure. The monitoring and blind detection of P/SP-CSI-RS at each configured occasion causes unnecessary UE complexity and power consumption especially for the case of frequent detection and monitoring with a small period. Moreover, the uncertainty of CSI-IM resources makes it challenging for interference measurement. This motivates to introduce FG 10-31 to provides flexibility at UE side to implement CSI measurements based on periodic or semi-persistent CSI-RS/CSI-IM. The same analysis is also applicable for SPS PDSCH reception on unlicensed band and justify the need of FG 10-32.Further details can be found in our paper [R1- 2002320].

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| [10-31] | Support of CSI-RS measurements for CSI reporting and tracking without COT duration from DCI 2\_0 | Perform CSI measurements for reporting and tracking using CSI-RS/CSI-IM resources that are not within a COT duration indicated by DCI 2\_0 Note: This includes the cases when DCI 2\_0 is not configured and when DCI 2\_0 is configured but COT duration is not provided by either CO duration field or SFI. | 10-1a | Per-band | Optional with capability signalling |
| [10-32] | Support of SPS PDSCH reception without COT duration from DCI 2\_0 | Receiving SPS PDSCH that are not within a COT duration indicated by DCI 2\_0Note: This includes the cases when DCI 2\_0 is not configured and when DCI 2\_0 is configured but COT duration is not provided by either CO duration field or SFI. | 10-1a | Per-band | Optional with capability signalling |

**Proposal 2:** * *Add the FG 10-31 and FG 10-32 as optional UE features for CSI-RS measurement and SPS PDSCH reception without COT duration from DCI 2\_0.*
 |
| [12] | Nokia, Nokia Shanghai Bell | * 10-31: Feature is under discussion in R16 NR-U maintenance.
 |
| [14] | Huawei, HiSilicon | **FG10-31 (Support of CSI-RS measurements for CSI reporting and tracking without COT duration from DCI 2\_0)**There is no agreement in Rel-16 for this UE behavior, so this FG requires more discussion and clarification first. |

**Based on above, following point should be discussed for FG 10-31**

* **Whether or not 10-31 is needed**

# **References**

[1] R1-2001484 RAN1 UE features list for Rel-16 NR after RAN1#100-E Moderator (AT&T, NTT DOCOMO, INC.)

[2] R1-2001715 Discussion on the UE features for NR-U ZTE, Sanechips

[3] R1-2001720 Discussion on Rel-16 NRU UE features vivo

[4] R1-2001765 Discussion on UE feature for NRU OPPO

[5] R1-2001826 Views on Rel-16 UE features for NR-U MediaTek Inc.

[6] R1-2001941 Discussion on UE features for NR-U LG Electronics

[7] R1-2002016 UE features for NR-U Intel Corporation

[8] R1-2002037 UE features for NR-U Ericsson

[9] R1-2002151 UE features for NR-U Samsung

[10] R1-2002350 Discussions on NR-U UE features Apple

[11] R1-2002393 Discussion on UE feature for NR-U Sharp

[12] R1-2002480 On UE features NR Unlicensed Nokia, Nokia Shanghai Bell

[13] R1-2002563 Discussion on NR-U UE features Qualcomm Incorporated

[14] R1-2002589 Rel-16 UE features for NR-U Huawei, HiSilicon

[15] R1-2002683 UE Features for NR-U TCL Communications