[100b-e-NR-5G\_V2X\_NRSL-PHYstructure-02]

Email discussion/approval on resource pool configuration - subchannel size and resource pool size

[100b-e-NR-5G\_V2X\_NRSL-PHYstructure-02] Email discussion/approval on resource pool configuration - subchannel size and resource pool size

- A. Whether/how to introduce additional subchannel size and whether the number of PRBs configured for a resource pool should be integer multiple of sub-channel size

 till 4/24, with potential TP till 4/29 – Jeongho (SS)

This document has the following questions.

- A. Whether the number of PRBs configured for a resource pool should be integer multiple of sub-channel size?

- B. Whether/which new numbers is defined for a subchannel size?

# **A. Whether the number of PRBs configured for a resource pool should be integer multiple of sub-channel size?**

Based on the submitted contributions, there are the following alternatives and supporting companies.

* Alt A-1. All numbers of PRBs can be configured and a UE is not expected to use the last subchannel in Rel-16.
  + [vivo], [OPPO], [Sony], [MediaTek], [TCL], [Apple], [Panasonic], [Qualcomm]
* Alt A-2. All number of PRBs can be configured and a different size is used for the last subchannel.
  + [LGE], [Intel], [NTT DCM](assume the same PRBs for TBS determination)
* Alt A-3. Use only integer multiple of subchannel for the resource pool size.

Based on the contributions, the following proposal can be made.

*Proposal 1. For the size of resource pool, numbers of PRBs can be configured and a UE is not expected to use the last subchannel in Rel-16.*

Please share your views if Proposal 1 is agreeable or, if not, please share your views on the reason why it is not workable.

|  |  |
| --- | --- |
| **Company** | **Views** |
| NTT DOCOMO | We are supportive of Alt A-2 and Alt A-3, but Alt A-1 is unclear for us.  Let us ask question for Alt A-1: When all numbers of PRBs are (pre-)configured and the PRBs are not a multiple of sub-channel size, does UE need to do something on the remaining PRBs? Does not do anything? If UE does not anything, what is the motivation of Alt A-1? |
| Huawei, HiSilicon | The important point is to avoid PRB wastage in NR V2X, where the cost of doing so is not only in % spectral efficiency, but also in comparisons to other technologies. As we stated in the last meeting, we open to any reasonable solution. We are aware that various configuration options can be used so that not all cases have lost PRBs. But, the assumption we make is that any company wishing to include a configuration which would discard PRBs should have a way to explain how they will reclaim them for some other purpose, before proposal 1 can be considered.  PS. The proposal as written does not seem to operate. |
| Futurewei | We expect this problem to be largely solved by implementation with A-3 being the logical implementation/deployment being used. In that sense, not putting additional constraint is fine with us. If the group feels that some specification is needed to handle this error case, either A-1 or A-3 is fine. A-2 would make the implementation more complex and is not preferred |
| Intel | Our goal is to enable mechanism to efficiently use SL spectrum for different numerologies and avoid waist of spectrum resources. We disagree with current proposal and do not understand its value and motivation behind. In order to solve problem, we are open to consider Alt A-2. At the same time, we believe that more reasonable technical solution is to distribute reminder of PRBs across allocated subchannels.  We suggest the following proposal:  *Proposal 1. Arbitrary number of PRBs can be configured for the size of resource pool. UEs use all configured PRBs for communication, irrespective of sub-channel size configuration.* |
| Sharp | We think Alt A-3 is sufficient here. If there is any problem, it can be resolved by a solution for issue B below. |
| CATT | Our preference is Alt 3, the resource pool can be configured with suitable sub-channel size to lead no or small resource wastage. We can also accept alt 2 with the consideration of resource efficiency, in alt 2, PSCCH can’t be transmitted on the last sub-channel. |
| LG | We are supportive of that all numbers of PRBs can be configured and have a strong concern not to use remaining PRBs.  Currently, the NR sidelink is not a unique solution for V2X, and it competes with other techniques. In the future, it would be possible that the NR sidelink could be competed with brand new technique.  In this situation, it cannot be understood why companies allow some PRBs in a resource pool would not be used for the actual transmission despite of the inherent disadvantage in the spectral efficiency. |
| vivo | We prefer Alt A-1.  Our understanding is that Alt A-1 and Alt A-2 are basically the same, except that the last sub-channel is not used *in this release*. Our concern on Alt A-2 is simply on the efforts to resolve the remaining issues in this release within two e-meetings, given there are still lots of issues to be fixed. The TBS issue notified by DoCoMo is one of them, but probably not the only one. These issues can be resolved in later release.  We object to the Alt A-3, it may lead to wasting a large portion of PRBs in many cases. |

# **B. Whether/which new numbers is defined for a subchannel size?**

Based on the submitted contributions, there are the following alternatives and supporting companies.

* Alt B-1. Introduce 11, 12, 13, 17, 19, 27, 53 PRBs as new subchannel sizes
  + [Huawei, HiSilicon]
* Alt B-2. Introduce 4,5,6 as new subchannel size
  + ~~[LGE],~~ [Ericsson], [Spreadtrum], [NEC]
* Alt B-3. No need to define a new size for a subchannel.

Please share your views on this issue and the reason of your views.

|  |  |
| --- | --- |
| **Company** | **Views** |
| NTT DOCOMO | Support Alt B-3.  We would like to support Alt B-2, while we are not sure whether decoding performance of PSCCH/2nd-stage SCI is sufficient. In addition, when sufficient PSCCH/2nd-stage SCI could lead to quite small number of REs for SL-SCH. If multiple sub-channels are used in typical case, the motivation of Alt B-2 will be lost. |
| Huawei, HiSilicon | We are open to any reasonable solution: B-1, B-2, or something else. The purpose of our proposal was to show one simple (we hope) way that PRB loss can be avoided without impact on sensing procedures, UE complexity, etc. |
| Futurewei | In our view, with good implementation/deployment scenarios, there should not be needs for new subchannel, thus B-3 is preferred. That said, if a new subchannel size is shown to provide deployment benefits, we are willing to consider. |
| Intel | Alt B-3 is our first preference. We do not see motivation to introduce many options for subchannels sizes, since it does not solve issue of reminder of PRBs completely. We should not forget that it also increases UE complexity, since we may need new configurations for control channels (1st and 2nd stage SCI) and DMRS, as well as more challenges in PSSCH demodulations. |
| Sharp | Fine with Alt B-1. |
| CATT | We are open for this issue.  Regarding to Alt 2, since the sub-channel size is reduced, in order to maintain the PSCCH reliability, it may be need to enlarge the PSCCH symbols. |
| LG | Since the current version of B-1 does not serves all the problematic cases, we still prefer A-2.  In case of B-2, at this maintenance stage, it is not preferable to introduce new number of PSCCH PRB numbers.  Note that B-2 is not our preference, so we remove our company name on B-2. |
| vivo | We are fine with Alt B-3. We understand Huawei’s concern on the PRB loss issue. But if Alt A-1 or Alt A-1 is agreed, we don’t need to introduce additional number of sub-channel size. |