**3GPP TSG RAN WG1 Meeting #103-e R1-200xxxx**

**e-Meeting, October 26 – November 13, 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **DRAFT CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **36.213** | **CR** |  | **rev** | **-** | **Current version:** | **V16.3.0** |  |
|  | | | | | | | | |
| *For* ***[HE](http://www.3gpp.org/3G_Specs/CRs.htm" \l "_blank)******[LP](http://www.3gpp.org/3G_Specs/CRs.htm" \l "_blank)*** *on using this form: comprehensive instructions can be found at  <http://www.3gpp.org/Change-Requests>.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction on TPC command for multi-TB scheduling in LTE-MTC | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Moderator(Ericsson),ZTE,Ericsson | | | | | | | | | |
| ***Source to TSG:*** | R1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | LTE\_eMTC5 -Core | | | | |  | ***Date:*** | | | 2020-11-05 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In 5.1.1.1 of 36.213, current spec description about TPC command is used for single TB. It is not clear whether the same transmit power should be assumed for multiple TBs scheduled by one DCI. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Clarify that all the subframes in the PUSCH transmission, scheduled by one DCI, have the same transmit power. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The transmit power for multi-TB unicast scheduling is not clear. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.1.1.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | |  | | |
| ***affected:*** | |  | **X** | Test specifications | | | |  | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | |  | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

5.1.1.1 UE behaviour

**<Unchanged parts are omitted>**

For a BL/CE UE configured with CEModeA, if the PUSCH transmission, scheduled by one DCI, is transmitted in more than one subframe *i0*, *i1*, …, *iN-1* where *i0*< *i1*< …< *iN-1*, the PUSCH transmit power in subframe *ik* , *k*=0, 1, …, *N*-1, is determined by



For a BL/CE UE configured with CEModeB, the PUSCH transmit power in subframe *ik* is determined by



**<Unchanged parts are omitted>**