**3GPP TSG-RAN WG1 Meeting # 103-e *R1-200xxxx***

**e-Meeting, October 26th – November 13th, 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.213** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **16.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | 38.213 CR Correction on HARQ-ACK codebook for secondary PUCCH group |
|  |  |
| ***Source to WG:*** | Moderator (Nokia) |
| ***Source to TSG:*** | R1 |
|  |  |
| ***Work item code:*** | LTE\_NR\_DC\_CA\_enh-Core |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | According to the RAN1#97 agreements, new RRC parameters for HARQ-ACK codebook type and HARQ-ACK spatial bundling configuration were introduced in Rel-16 for the secondary PUCCH group, i.e. *pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup-r16*, *harq-ACK-SpatialBundlingPUCCH-secondaryPUCCHgroup* and *harq-ACK-SpatialBundlingPUSCH-secondaryPUCCHgroup.*The HARQ-ACK codebook type for the secondary PUCCH group is determined by *pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup-r16* if present and by *pdsch-HARQ-ACK-Codebook* otherwise according to the field descriptions in TS38.331.Similarly, the HARQ-ACK spatial bundling configuration for the secondary PUCCH group is determined by *harq-ACK-SpatialBundlingPUCCH-secondaryPUCCHgroup* and *harq-ACK-SpatialBundlingPUSCH-secondaryPUCCHgroup* if present and by *harq-ACK-SpatialBundlingPUCCH* and *harq-ACK-SpatialBundlingPUSCH* otherwise according to the field descriptions in TS38.331.These RRC parameters are not reflected in TS38.213 |
|  |  |
| ***Summary of change:*** | Introducing the RRC parameter *pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup-r16* to subclause 7.2Introducing RRC parameters *pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup-r16*,*harq-ACK-SpatialBundlingPUCCH-secondaryPUCCHgroup* and *harq-ACK-SpatialBundlingPUSCH-secondaryPUCCHgroup* to subclause 9 |
|  |  |
| ***Consequences if not approved:*** | UE behavior in relation to the mentioned three RRC parameters is not properly defined in TS38.213 |
|  |  |
| ***Clauses affected:*** | 7.2, 9 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |   |
|  |  |
| ***This CR's revision history:*** | This is the first version for this CR. |

## 7.2 Physical uplink control channel

If the UE is configured with a SCG, the UE shall apply the procedures described in this clause for both MCG and SCG.

- When the procedures are applied for MCG, the term 'serving cell' in this clause refers to serving cell belonging to the MCG.

- When the procedures are applied for SCG, the term 'serving cell' in this clause refers to serving cell belonging to the SCG. The term 'primary cell' in this clause refers to the PSCell of the SCG.

If the UE is configured with a PUCCH-SCell, the UE shall apply the procedures described in this clause for both primary PUCCH group and secondary PUCCH group.

- When the procedures are applied for the primary PUCCH group, the term 'serving cell' in this clause refers to serving cell belonging to the primary PUCCH group.

- When the procedures are applied for the secondary PUCCH group, the term 'serving cell' in this clause refers to serving cell belonging to the secondary PUCCH group. The term 'primary cell' in this clause refers to the PUCCH-SCell of the secondary PUCCH group. If *pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup-r16* is provided, *pdsch-HARQ-ACK-Codebook* is replaced by *pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup-r16*.

<unchanged text omitted>

# 9 UE procedure for reporting control information

If a UE is configured with a SCG, the UE shall apply the procedures described in this clause for both MCG and SCG.

- When the procedures are applied for MCG, the terms 'secondary cell', 'secondary cells' , 'serving cell', 'serving cells' in this clause refer to secondary cell, secondary cells, serving cell, serving cells belonging to the MCG respectively.

- When the procedures are applied for SCG, the terms 'secondary cell', 'secondary cells', 'serving cell', 'serving cells' in this clause refer to secondary cell, secondary cells (not including PSCell), serving cell, serving cells belonging to the SCG respectively. The term 'primary cell' in this clause refers to the PSCell of the SCG.

If a UE is configured with a PUCCH-SCell, the UE shall apply the procedures described in this clause for both primary PUCCH group and secondary PUCCH group

- When the procedures are applied for the primary PUCCH group, the terms 'secondary cell', 'secondary cells' , 'serving cell', 'serving cells' in this clause refer to secondary cell, secondary cells, serving cell, serving cells belonging to the primary PUCCH group respectively.

- When the procedures are applied for secondary PUCCH group, the terms 'secondary cell', 'secondary cells', 'serving cell', 'serving cells' in this clause refer to secondary cell, secondary cells (not including the PUCCH-SCell), serving cell, serving cells belonging to the secondary PUCCH group respectively. The term 'primary cell' in this clause refers to the PUCCH-SCell of the secondary PUCCH group. If *pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup-r16* is provided, *pdsch-HARQ-ACK-Codebook* is replaced by *pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup-r16*. If *harq-ACK-SpatialBundlingPUCCH-secondaryPUCCHgroup* is provided, *harq-ACK-SpatialBundlingPUCCH* is replaced by *harq-ACK-SpatialBundlingPUCCH-secondaryPUCCHgroup*. If *harq-ACK-SpatialBundlingPUSCH-secondaryPUCCHgroup* is provided, *harq-ACK-SpatialBundlingPUSCH* is replaced by *harq-ACK-SpatialBundlingPUSCH-secondaryPUCCHgroup*.

If a UE

- is not provided *CORESETPoolIndex* or is provided *CORESETPoolIndex* with a value of 0 for first CORESETs on active DL BWPs of serving cells, and

- is provided *CORESETPoolIndex* with a value of 1 for second CORESETs on active DL BWPs of the serving cells, and

- is provided *ackNACKFeedbackMode-r16* = *separate*

<unchanged text omitted>