**Proposal 3.A**: On Rel.17 DCI-based beam indication, the beam application time X or Y is configured by the gNB via higher-layer (RRC) signaling. The minimum value(s) X or Y are down-selected from the following:

* Alt1: Support a UE capability for the minimum value of X or Y
	+ FFS: the exact minimum values of X (e.g., 0.5ms, 2ms, 3ms) or Y supported by UE
	+ FFS: whether existing UE capability (e.g. beamSwitchTime, TimeDurationQCL) can be reused as this UE capability.
* Alt2: The minimum value of the beam application time X or Y is fixed, with value(s) defined in specification
	+ FFS: Whether to support more than one values of X/Y