3GPP TSG-RAN WG1 Meeting #103-e Tdoc R1-20xxxxx

e-Meeting, October 26th – November 13th, 2020

**Agenda Item: 8.6.1**

**Title: FL summary #5 for Potential UE complexity reduction features for RedCap**

**Source: Moderator (Ericsson)**

**Document for: Discussion, Decision**

# 1 Introduction

Contributions [1] – [28] submitted to RAN1#103e AI 8.6.1 plus relevant parts from a few contributions [29] – [34] that were submitted to other agenda items under AI 8.6, as well as initial evaluation results in [35], were summarized in FL summary #1 (FLS1) in [R1-2008869](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2008869.zip).

This document captures the following RAN1#103e RedCap email discussion.

|  |
| --- |
| [103-e-NR-RedCap-02] Email discussion for potential UE complexity reduction features – Johan (Ericsson)   * 1st check point: 10/29 * 2nd check point: 11/4 * 3rd check point: 11/10 * Last check point 11/12 |

The previous round of this email discussion is documented in FL summary #4 (FLS4) in [R1-2009394](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009394.zip).

In this round of the email discussion, please provide input on the following:

|  |
| --- |
| * By Wednesday 11th November Noon UTC:   + FL1 proposals for endorsement tagged ‘FL1: Phase 1:’ or ‘FL1: Phase 2:’ * By Wednesday 11th November 23:59 UTC:   + FL2 proposals for endorsement tagged ‘FL2: Phase 2:’ |

Follow the naming convention in this example:

* *RedCapComplexityFLS4-v000.docx*
* *RedCapComplexityFLS4-v001-CompanyA.docx*
* *RedCapComplexityFLS4-v002-CompanyA-CompanyB.docx*
* *RedCapComplexityFLS4-v003-CompanyB-CompanyC.docx*

If needed, you may “lock” a spreadsheet file for 30 minutes by creating a checkout file, as in this example:

* Assume CompanyC wants to update *RedCapComplexityFLS4-v002-CompanyA-CompanyB.docx*.
* CompanyC uploads an empty file named *RedCapComplexityFLS4-v003-CompanyB-CompanyC.checkout*
* CompanyC then has 30 minutes to upload *RedCapComplexityFLS4-v003-CompanyB-CompanyC.docx*
* If no update is uploaded in 30 minutes, other companies can ignore the checkout file.
* Note that the file timestamps on the server are in UTC time.

In file names, please use the hyphen character (not underline character) and include ‘v’ in front of the version number.

The structure of this document follows the structure in TR 38.875 V0.0.3 ([R1-2009490](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009490.zip)). The tables with device cost evaluation results in this contribution will be updated as needed with new evaluation results from the email discussion [103-e-NR-RedCap-EvaluationResults].

# 6 Evaluation methodology

## 6.1 Evaluation methodology for UE complexity reduction

Based on earlier agreements, submitted contributions and email discussion responses, the following TP can be considered.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| For cost/complexity evaluation of UE complexity reduction techniques, the methodology used in TR 36.888 was used as a starting point.  Reference NR devices were defined as follows for FR1 FDD, FR1 TDD and FR2, respectively.   * All mandatory Rel-15 features (with or without capability signaling) * Single RAT * Operation in a single band at a time * Maximum bandwidth:   + For FR1: 100 MHz for DL and UL   + For FR2: 200 MHz for DL and UL * Antennas:   + For FR1 FDD: 2Rx/1Tx   + For FR1 TDD: 4Rx/1Tx   + For FR2: 2Rx/1Tx * Power class: PC3 * Processing time: Capability 1 * Modulation:   + For FR1: support 256QAM for DL and 64QAM for UL   + For FR2: support 64QAM for DL and 64QAM for UL * Access: Direct DL/UL access between UE and gNB   Detailed cost breakdown for the reference NR devices according to Table 6.1-1 was assumed in the study. The RF-to-baseband cost ratio was assumed to be 40:60 for an FR1 UE and 50:50 for an FR2 UE.  The study considered impacts on cost/complexity reduction from the studied UE complexity reduction techniques for a UE that supports multiple RF bands through operation in a single band at a time, where it was assumed that support of multiple RF bands may affect the RF cost but not the baseband cost significantly.  NOTE: This study assesses, from a 3GPP standpoint, the technical feasibility of reduced-capability NR devices for industrial wireless sensors, video surveillance and wearables use cases. Given that factors outside 3GPP responsibility influence the cost of a modem/device, this study item (and this study report) cannot guarantee, or be used as a guarantee, that such modem/device will be low-cost in the market.  **Table 6.1-1: Detailed cost breakdown for the reference NR devices**   |  |  |  |  | | --- | --- | --- | --- | | **Functional block** | **FR1 FDD (2Rx)** | **FR1 TDD (4Rx)** | **FR2** | | **RF** | | | | | Antenna array for FR2 |  |  | ~33% | | Power amplifier | ~25% | ~25% | ~18% | | Filters | ~10% | ~15% | ~8% | | RF transceiver (including LNAs, mixer, and local oscillator) | ~45% | ~55% | ~41% | | Duplexer / Switch | ~20% | ~5% | ~0% | | **Baseband** | | | | | ADC / DAC | ~10% | ~9% | ~4% | | FFT/IFFT | ~4% | ~4% | ~4% | | Post-FFT data buffering | ~10% | ~10% | ~11% | | Receiver processing block | ~24% | ~29% | ~24% | | LDPC decoding | ~10% | ~9% | ~9% | | HARQ buffer | ~14% | ~12% | ~11% | | DL control processing & decoder | ~5% | ~4% | ~5% | | Synchronization / cell search block | ~9% | ~9% | ~7% | | UL processing block | ~5% | ~5% | ~7% | | MIMO specific processing blocks | ~9% | ~9% | ~18% | |

In FLS4, the responses regarding the TP for TR clause 6.1 concerned the sentence about multi-band support.

**Phase 1: Proposal 6.1-1d: Adopt the updated TP above for TR clause 6.1.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | N | It should be Ok to just remove “(single-carrier)”, or revise as “non-CA” or “single carrier/cell”. The reference UE has “single band at a time” so all these are applicable. SUL in our view does not increase UE cost as long as it is semi-statically configured for a band, thus it can be viewed included in our estimate. Whether it is recommended or not should be separate from the discussion. |
| CATT | Y | We think the current version is fine for us. No strong view. |
| CMCC | Y |  |
| LG | Y |  |
| ZTE | Y | The updated TP is aligned with the cost evaluation assumption.  SUL would increase RF cost. |
| vivo | Y |  |
| Nokia, NSB | Y |  |
| SONY5 | Y | This has been discussed at length over the past two weeks. The current text is OK. Our understanding is that the “multiple bands” text is not about whether more than one band is active at the same time, but rather it is about whether the hardware can operate in one band at one time and another band at another time.  Summary: current text is OK. |
| FUTUREWEI |  | We had this debate much earlier and ended up with the “single band at a time” so should stick with that language. |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y | The cost/complexity evaluation assumed single-carrier operation, so it is a good clarification to make. |
| Spreadtrum | Y |  |
| OPPO | Y |  |
| NEC | Y |  |
| Xiaomi | Y |  |
| FL | The TP above has been updated based on the received responses. While the formulation might not be perfect, hopefully it can be accepted by everyone, so that we can spend the very limited time left in this meeting on more critical sections.  **FL1: Phase 1: Proposal 6.1-1e: Adopt the updated TP above for TR clause 6.1.** | |
| FUTUREWEI2 | Y |  |
| MediaTek | Y |  |
| Ericsson | Y |  |
| Qualcomm | Y | Thanks for the efforts of FL. We can live with the updated proposal for the sake of progress. |
| Nokia, NSB | Y |  |
| DOCOMO | Y |  |
| LG | Y |  |
| CATT | Y |  |
| SONY6 | Y |  |
| NEC | Y |  |
| CMCC | Y |  |
| ZTE | Y |  |
| OPPO | Y |  |
| Samsung | Y |  |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | Y |  |

One response in Section 7.5.2 in FLS4 expressed the view that the averaging of cost estimates from different sources should be done by excluding outlier numbers. The following methods can be considered.

* Method A: Average of all values
* Method B: Average of all values except the smallest value and the largest value

**Phase 1: Question 6.1-3: Which method for averaging of cost estimates should be used?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Method (A or B)** | **Comments** |
| Huawei, HiSilicon | None or A with addressing individual questions raised by companies | We assume the question is applicable for all techniques, not only for section 7.5.2.  We also assume in the end all results should be captured, instead of only averaged values which cannot reflects different UE implementations.  Given the above, it should be the motivation for efforts to identify/resolve discussion points/typos/mis-calcuation for completing the cost estimate. Specifically,   * + Values with large difference are possible due to different implementations, thus may not change the relevant observations, e.g.     - For Rx reduction, whether the PA will be impacted     - Whether the cost saving of Transceiver can be more than 1/3 from the reference number (i.e. 45%-> around 30%) when 1T2R->1T1R in FDD.     - If they are understood so, we can live with those as different UE implementations.   + Values with large difference are based on potential mis-calculation and potentially can lead to different observations among results, e.g.     - For FDD HD-FDD vs reference UE, when replacing a duplexer (20% cost) integrated with T/R filter inside (10% cost, similar to the Filter block outside the duplexer) by a switch, the cost saving cannot be reduced down to less than 10% due to the remains of filters inside, in order to keep 1Tx&2Rx.     - This high proportion of cost saving exceed the theoretical value that is possible based on the template, thus shall be clarified before endorsement or being used for drawing observations.   So our suggestion is:  **Method C: All values should be captured and can be used for averaging, but companies are encouraged to address individual questions/discussion points that are relevant.** |
| CATT | A | We believe that there will not be large difference for Method A and B in the end. |
| LG | A | As we have quite a large number of evaluation results for the complexity reduction, either way is fine for us. We would like to just go for a majority view to make a progress. |
| ZTE | A |  |
| vivo | A | We think A is sufficient. |
| Nokia, NSB | A | Given the large number of results, we think A is sufficient. |
| SONY5 | A | There are results from nearly 20 companies. Any “outliers” get averaged out anyway due to this large number of results.  We need to respect that different companies have different views on some of the cost estimates.  The “addressing individual questions raised by companies” is a two way process. While we feel that we have answered questions directed at us, other companies might not have done so. In particular, we have answered the question about HD-FDD: we think that replacing a duplexer with a switch/filter does not have a significant impact on the “filter” cost. |
| FUTUREWEI | A | More concerned with results where companies included combinations into individual technique results, or reported the wrong combination such as half-duplex type B instead of type A. Please FL work with those companies for a resolution. |
| Qualcomm | A |  |
| DOCOMO | A |  |
| Sierra Wireless | A | Agree with Sony. The averaging of results from many companies averages out any outliers. |
| Samsung | A |  |
| Ericsson | A | The tables only need to contain averages of all values (but all values should be documented in some contribution for future reference). |
| Spreadtrum | A |  |
| OPPO | A | Method A would be enough. |
| Xiaomi | A |  |
| FL | RAN1#103e agreement:   * For averaging of cost estimates, take the average of all values. | |

# 7 UE complexity reduction features

## 7.1 Introduction to UE complexity reduction features

## 7.2 Reduced number of UE Rx/Tx antennas

### 7.2.1 Description of feature

RAN1#103e agreement:

* Adopt the TP in [R1-2009393](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009393.zip) for TR clause 7.2.1.

### 7.2.2 Analysis of UE complexity reduction

The tables with device cost evaluation results in this contribution are based on [RedCapCost-v048-FL-Samsung2.xlsx](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Inbox/drafts/8.6/EvaluationResults/RedCapCost/RedCapCost-v048-FL-Samsung2.xlsx). They will eventually be updated with new results from the email discussion [103-e-NR-RedCap-EvaluationResults].

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| The estimated cost for a device with reduced number of UE Rx branches without taking reduced number of downlink MIMO layers into consideration, relative to the reference NR device (see evaluation methodology described in clause 6.1) and averaged over the results provided by the sourcing companies, is summarized in Table 7.2.2-1. As can be seen in the last row for the total cost, the average estimated cost reduction achieved by reducing the number of UE Rx branches are as follows:   * FR1 FDD (2Rx 🡪 1Rx): ~26% * FR1 TDD (4Rx 🡪 2Rx): ~31% * FR1 TDD (4Rx 🡪 1Rx): ~46% * FR2 TDD (2Rx 🡪 1Rx): ~31%   By comparing Table 7.2.2-1 with the reference NR device cost breakdown in clause 6.1, it can be observed that the main contributors of the cost reduction are the following functional blocks:   * RF: Antenna array (only FR2) * RF: Filters * RF: Transceiver (including LNAs, mixer, and local oscillator) * Baseband: ADC/DAC * Baseband: FFT/IFFT * Baseband: Post-FFT data buffering * Baseband: Receiver processing block * Baseband: Synchronization/cell search block   Furthermore, all sourcing companies indicated that the RF cost savings (but not the baseband cost savings) from reducing the number of UE Rx branches accumulate across supported bands in both FR1 and FR2.  **Table 7.2.2-1: Estimated relative device cost for reduced number of UE Rx branches**   |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Reduced number of UE Rx branches** | **FR1 FDD**  **(2Rx 🡪 1Rx)** | **FR1 TDD**  **(4Rx 🡪** **2Rx)** | **FR1 TDD**  **(4Rx 🡪 1Rx)** | **FR2 TDD**  **(2Rx 🡪 1Rx)** | | RF: Antenna array | - | - | - | 18.2% | | RF: Power amplifier | 25.0% | 25.0% | 25.0% | 18.0% | | RF: Filters | 4.8% | 7.6% | 3.9% | 4.3% | | RF: Transceiver (including LNAs, mixer, and local oscillator) | 25.3% | 30.4% | 17.8% | 23.7% | | RF: Duplexer / Switch | 19.6% | 4.9% | 4.9% | 0.0% | | **RF: Total relative cost** | **74.7%** | **67.9%** | **51.6%** | **64.2%** | | BB: ADC / DAC | 6.4% | 5.2% | 3.4% | 2.4% | | BB: FFT/IFFT | 2.3% | 2.2% | 1.3% | 2.2% | | BB: Post-FFT data buffering | 5.6% | 5.3% | 3.0% | 6.0% | | BB: Receiver processing block | 13.7% | 15.7% | 9.0% | 13.3% | | BB: LDPC decoding | 9.7% | 8.7% | 8.6% | 8.6% | | BB: HARQ buffer | 13.6% | 11.6% | 11.4% | 10.5% | | BB: DL control processing & decoder | 4.9% | 4.0% | 3.9% | 4.9% | | BB: Synchronization / cell search block | 5.1% | 4.8% | 2.7% | 3.8% | | BB: UL processing block | 5.0% | 5.0% | 5.0% | 7.0% | | BB: MIMO specific processing blocks | 8.2% | 7.9% | 7.3% | 15.8% | | **BB: Total relative cost** | **74.4%** | **70.4%** | **55.7%** | **74.5%** | | **RF+BB: Total relative cost** | **74.5%** | **69.4%** | **54.0%** | **69.4%** |   The estimated cost for a device with reduced number of UE Rx branches and a corresponding reduction of the number of downlink MIMO layers, relative to the reference NR device (see evaluation methodology described in clause 6.1) and averaged over the results provided by the sourcing companies, is summarized in Table 7.2.2-2. As can be seen in the last row for the total cost, the average estimated cost reduction achieved by reducing the number of UE Rx branches and MIMO layers are as follows:   * FR1 FDD (2Rx 🡪 1Rx): ~37% * FR1 TDD (4Rx 🡪 2Rx): ~40% * FR1 TDD (4Rx 🡪 1Rx): ~60% * FR2 TDD (2Rx 🡪 1Rx): ~40%   By comparing Table 7.2.2-2 with the reference NR device cost breakdown in clause 6.1, it can be observed that the main contributors of the cost reduction are the following functional blocks:   * RF: Antenna array (only FR2) * RF: Filters * RF: Transceiver (including LNAs, mixer, and local oscillator) * Baseband: ADC/DAC * Baseband: FFT/IFFT * Baseband: Post-FFT data buffering * Baseband: Receiver processing block * Baseband: LDPC decoding * Baseband: HARQ buffer * Baseband: Synchronization/cell search block * Baseband: MIMO specific processing blocks   Furthermore, all sourcing companies indicated that the RF cost savings (but not the baseband cost savings) from reducing the number of UE Rx branches accumulate across supported bands in both FR1 and FR2, whereas the cost savings from reducing the number of downlink MIMO layers do not.  **Table 7.2.2-2: Estimated relative device cost for reduced number of UE Rx branches and a corresponding reduction of the supported maximum number of MIMO layers**   |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Reduced number of UE Rx branches and MIMO layers** | **FR1 FDD**  **(2Rx 🡪 1Rx)** | **FR1 TDD**  **(4Rx 🡪** **2Rx)** | **FR1 TDD**  **(4Rx 🡪 1Rx)** | **FR2 TDD**  **(2Rx 🡪 1Rx)** | | RF: Antenna array | - | - | - | 18.7% | | RF: Power amplifier | 25.0% | 25.0% | 25.0% | 18.0% | | RF: Filters | 5.2% | 7.6% | 4.0% | 4.4% | | RF: Transceiver (including LNAs, mixer, and local oscillator) | 24.6% | 30.4% | 17.4% | 23.8% | | RF: Duplexer / Switch | 19.5% | 4.9% | 4.8% | 0.0% | | **RF: Total relative cost** | **74.2%** | **68.0%** | **51.3%** | **64.9%** | | BB: ADC / DAC | 5.9% | 5.0% | 3.1% | 2.3% | | BB: FFT/IFFT | 2.1% | 2.1% | 1.1% | 2.1% | | BB: Post-FFT data buffering | 5.0% | 5.0% | 2.5% | 5.5% | | BB: Receiver processing block | 12.1% | 14.6% | 7.5% | 12.1% | | BB: LDPC decoding | 5.0% | 4.5% | 2.3% | 4.5% | | BB: HARQ buffer | 7.2% | 6.1% | 3.1% | 5.7% | | BB: DL control processing & decoder | 5.0% | 4.0% | 4.0% | 5.0% | | BB: Synchronization / cell search block | 4.5% | 4.5% | 2.3% | 3.5% | | BB: UL processing block | 5.0% | 5.0% | 5.0% | 7.0% | | BB: MIMO specific processing blocks | 4.1% | 4.5% | 2.0% | 8.0% | | **BB: Total relative cost** | **55.9%** | **55.4%** | **33.0%** | **55.7%** | | **RF+BB: Total relative cost** | **63.2%** | **60.4%** | **40.3%** | **60.3%** | |

Since RAN1#103e has agreed to collect cost estimates for reduced number of Rx branches including corresponding reduction of number of MIMO layers, the TP for TR clause 7.2.2 can be updated to capture these estimates.

**Phase 1: Proposal 7.2.2-1b: Adopt the TP above as baseline text for TR clause 7.2.2, where the tables will be updated according to [103-e-NR-RedCap-EvaluationResults].**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | Y | It is Ok to state that “a corresponding reduction of the supported maximum number of downlink MIMO layers”, while in our estimate we will not reduce the MIMO layers in baseband, as reduction of Rx results in reduced MIMO layers of the entire UE already. The cost increment by a specialized single Layer chipset for e.g. FDD plus a two-Layer chipset for e.g. TDD, is not cost-efficient compared to a two-Layer chipset used across multiple bands, and thus not our implementation. |
| CATT | Y |  |
| CMCC | Y |  |
| LG | Y |  |
| ZTE | Y |  |
| vivo | Y |  |
| Nokia, NSB | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | N | Suggest to delete table 7.2.2.-1 and corresponding descriptions. And added analysis on cost saving for main contributors for table 7.2.2-2  Suggested changes as below:  ~~Table 7.2.2-1 summarizes the estimated cost for a device with reduced number of Rx branches without taking reduced number of downlink MIMO layers into consideration, relative to the reference NR device (see evaluation methodology described in clause 6.1) and averaged over the results provided by the sourcing companies.~~  Table 7.2.2-2 summarizes the estimated cost for a device with reduced number of Rx branches and a corresponding reduction of the supported maximum number of downlink MIMO layers, relative to the reference NR device (see evaluation methodology described in clause 6.1) and averaged over the results provided by the sourcing companies.  By comparing Table 7.2.2-2~~1~~ with the reference NR device cost breakdown in clause 6.1, it can be observed that the main contributors of the cost reduction are the following functional blocks:   * RF: Antenna array (only FR2) * RF: Filters * RF: Transceiver (including LNAs, mixer, and local oscillator) * Baseband: ADC/DAC * Baseband: FFT/IFFT * Baseband: Post-FFT data buffering * Baseband: Receiver processing block * Baseband: LDPC decoding * Baseband: HARQ buffer * Baseband: Synchronization/cell search block * Baseband: MIMO specific processing blocks |
| Ericsson | Y |  |
| Intel | Y |  |
| Spreadtrum | Y |  |
| OPPO | Y |  |
| FL | The TP above has been updated based on the received responses.  **FL1: Phase 1: Proposal 7.2.2-1c: Adopt the TP above as baseline text for TR clause 7.2.2.** | |
| FUTUREWEI2 | Y |  |
| MediaTek | Y |  |
| Ericsson | Y |  |
| Qualcomm | Y |  |
| Intel | Y |  |
| Nokia, NSB | Y |  |
| DOCOMO | Y |  |
| LG | Y |  |
| CATT | Y |  |
| SONY6 | Y |  |
| CMCC | Y |  |
| ZTE | Y |  |
| OPPO | Y |  |
| Samsung |  | If all other companies insist to capture Rx reduction without MIMO layer reduction, we like to add a sentence in the description:  Note that, reduced of the number of UE Rx branches will naturally reduced the max support of MIMO layers. That is, the supported of MIMO layer cannot be larger than the number of UE Rx branches. |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | Y |  |

**Device size:**

In addition to reduction in cost/complexity benefits, the contributions [1, 2, 4, 5, 6, 8, 10, 12, 16, 19, 21, 28] have also highlighted that the reduction in number of UE Rx antennas is also beneficial in terms of reducing the size/form factor for devices, such as wearables in FR1. The contribution [2] has expressed the view that a RedCap technique, such as reduction of the number of antennas, shall not be considered a requirement to achieve a compact form factor for any use case. The contribution [28] has also expressed a similar view. More specifically, it is proposed in [28] to clarify that size reduction of device is neither an objective for RedCap study, nor within cost/complexity reduction study scope, and cannot be used to justify the choice of reduction mechanisms for RedCap UE.

With regards to the device size reduction in FR2, the contribution [28] has indicated that form factor consideration does not justify 1 Rx for RedCap in FR2. It is mentioned in [1] that reducing only the Rx branches has limited impact on reducing the device size in FR2. In [26], it is mentioned that in FR2 depending on the power, complexity, and form factor of the RedCap UE, 1Rx or 2 Rx may be selected.

Some companies say the device size is expected to increase with an increase in the number of supported bands [1, 4]. Such increase may depend on UE implementation and frequency band separation. [1]

Note that the following agreement was reached in RAN1#101e:

|  |
| --- |
| Agreements:   * [...] * Potential benefits in terms of reduced device size can be mentioned where applicable in the TR (e.g. in the section on reduced number of antennas), but the SI will not aim to quantify such benefits. |

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| The reduction of number of UE Rx branches, relative to that of the reference NR device, may be beneficial in terms of reducing the device size in FR1. This does not imply that a non-RedCap NR UE cannot be used in a compact or small form factor. |

**Phase 2: Proposal 7.2.2-1: Adopt the above description of the benefit of reduced number of UE Rx branches in terms of reducing the device size in FR1 as a baseline text for TR 38.875.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| LG | Y |  |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm |  | This SI is about the study of RedCap UE, and does not investigate how to make a non-RedCap UE achieve compact or small form factor. Therefore, we suggest to keep the 1st sentence only and remove the second one, i.e.  The reduction of number of UE Rx branches, relative to that of the reference NR device, may be beneficial in terms of reducing the device size in FR1. This does not imply that a non-RedCap NR UE cannot be used in a compact or small form factor. |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | Y | Agree with Qualcomm’s suggestion. This observation is about potential benefit and it’s sufficient without the last sentence. |
| OPPO | Y |  |
| Xiaomi |  | Similar comment with QC.  Let’s just focus on the issues and desctiption related to Redcap UEs |
| CATT | Y |  |
| Huawei, HiSilicon | Y |  |
| FL | The second sentence in the above TP was an explicit request in some received responses in FLS4 ([R1-2009394](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009394.zip)), and it seems that it may be difficult to agree the TP without it, so it would be good if the proposal can be agreed as is.  **FL1: Phase 2: Proposal 7.2.2-1: Adopt the above description of the benefit of reduced number of UE Rx branches in terms of reducing the device size in FR1 as a baseline text for TR 38.875.** | |
| Ericsson | Y |  |
| Qualcomm | Y |  |
| Intel | Y |  |
| Nokia, NSB | Y |  |
| DOCOMO | Y |  |
| LG | Y |  |
| CATT | Y |  |
| SONY6 | Y |  |
| CMCC | Y |  |
| ZTE | Y |  |
| OPPO | Y |  |
| Samsung | Y |  |
| Sequans | Y |  |
| Huawei, HiSilicon | Y |  |

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| It is unclear whether the reduction of number of UE Rx branches, relative to that of the reference NR device, may be beneficial in terms of reducing the device size in FR2. This does not imply that a non-RedCap NR UE cannot be used in a compact or small form factor. |

**Phase 2: Proposal 7.2.2-2: Adopt the above description of the benefit of reduced number of UE Rx branches in terms of reducing the device size in FR2 as a baseline text for TR 38.875.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| LG | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Ericsson | Y |  |
| Intel | Y |  |
| CATT | Y |  |
| Huawei, HiSilicon | Y |  |
| FL | **FL1: Phase 2: Proposal 7.2.2-2: Adopt the above description of the benefit of reduced number of UE Rx branches in terms of reducing the device size in FR2 as a baseline text for TR 38.875.** | |
| MediaTek | Y |  |
| Ericsson | Y |  |
| Qualcomm | Y |  |
| Intel | Y |  |
| Nokia, NSB | Y |  |
| DOCOMO | Y |  |
| LG | Y |  |
| CATT | Y |  |
| CMCC | Y |  |
| ZTE | Y |  |
| Samsung | Y |  |
| Sequans | Y |  |
| Huawei, HiSilicon | Y |  |

### 7.2.3 Analysis of performance impacts

According to the SID [36],

|  |
| --- |
| The study includes evaluations of the impact to coverage, network capacity and spectral efficiency |

In addition, RAN1#101e made the following agreement:

|  |
| --- |
| Agreements:   * The evaluation of performance impacts includes at least peak data rate, latency and reliability (as needed for the use cases). Other performance metrics such as power consumption, spectral efficiency and PDCCH blocking probability may also be considered if appropriate for a specific technique. |

**Coverage:**

* P0: Most companies have reported a loss in DL coverage/performance, either quantitatively or qualitatively, when reducing the number of Rx antennas [1, 2, 3, 4, 5, 6, 9, 11, 12, 14, 15, 16, 19, 20, 21, 22, 23, 26, 27, 28] . It is the recommendation of the FL that the discussion on quantitative values of the coverage loss and bottleneck channels be considered under AI 8.6.3.

Based on submitted contributions and email discussion responses, the following TP can be considered. More text on coverage can be captured after further progression of the discussion under AI 8.6.3.

|  |
| --- |
| **Coverage:**  In general, degradation of downlink performance is expected when reducing the number of Rx branches, which may affect the coverage. The amount of degradation depends on the number of Rx branches. Quantitative evaluation results are provided in clause 9. |

**Phase 2: Question 7.2.3-2: Can the above observations of the impact on coverage for reduced number of UE Rx antennas be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| LG | Y |  |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y | Can further revised it based on evaluation result in AI 8.6.3 |
| Ericsson | Y |  |
| Intel | Y |  |
| Spreadtrum | Y |  |
| OPPO | Y | Agree with Samsung. Even for 1Rx UE, the bottleneck for coverage may not be downlink channels. |
| Xiaomi | Y |  |
| CATT | Y |  |
| Huawei, HiSilicon | Y |  |
| FL | **FL2: Phase 2: Question 7.2.3-2: Can the above observations of the impact on coverage for reduced number of UE Rx antennas be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Samsung | Y | Better to clarify that, it can further revise it based on evaluation result in AI 8.6.3 |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | Y |  |
| LG | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Network capacity and spectral efficiency:**

* P7: [1, 2, 3, 5, 12, 13, 15, 16, 18, 19, 21, 23, 24, 27, 28] has reported a loss in spectral efficiency/network capacity. In [4], it has been reported that the spectral efficiency decrease, but cell capacity (cell served throughput) increases. In [6], it has been noted that degree of spectral efficiency loss depends on the proportion of RedCap UE, traffic model and traffic load. The quantitative values of the loss can be discussed under AI 8.6.3.
* P8: [11] has reported the loss is sector/cell edge spectral efficiency when reducing the number of Rx antennas.
* P9: In [6], it is also noted that the impact can be managed by network by access control mechanism.
* P11: In [26], it is observed that for FR2, the number of users that can be supported is impacted by almost 50% if the number of UE Rx antennas is reduced from 2 to 1. It is also observed that 1 Rx antenna at the UE may be able to support a high number of users. It has been noted in [24] and [28] have also reported a reduction in the number of users supported. In [24], it has been mentioned that this aspect should be discussed under AI 8.6.3.

Based on submitted contributions and email discussion responses, the following TP can be considered. More text on network capacity and spectral efficiency can be captured after further progression of the discussion under AI 8.6.3.

|  |
| --- |
| **Network capacity and spectral efficiency:**  A loss in network capacity and spectral efficiency is expected when reducing the number of UE Rx branches. The magnitude of the loss depends on the proportion of RedCap UEs, the traffic characteristics, as well as on the number of Rx branches. Quantitative evaluation results are provided in clause X. |

**Phase 2: Question 7.2.3-3: Can the above observations of the impact on network capacity and spectral efficiency for reduced number of UE Rx antennas be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| LG | Y |  |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y | Editorial: The magnitude of the loss depends on the proportion of ~~the~~ RedCap UEs |
| FUTUREWEI | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Samsung | Y | Can further revised it based on evaluation result in AI 8.6.3 |
| Ericsson | Y |  |
| Intel | Y |  |
| OPPO | Y |  |
| Xiaomi | Y |  |
| CATT | Y |  |
| Huawei, HiSilicon | Y |  |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.2.3-3a: Can the above observations of the impact on network capacity and spectral efficiency for reduced number of UE Rx antennas be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Samsung | Y | Better to clarify that, it can further revise it based on evaluation result in AI 8.6.3 |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | Y |  |
| LG | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Data rate:**

* P1: [1, 2, 3, 4, 5, 6, 15, 16, 18, 19, 20, 22, 23, 24, 28] have indicated that there will be negative impact on DL data rate/throughput when reducing the number of Rx antennas. The main reason is that reducing the number of Rx antennas will also reduce the number of transmission layers that can be transmitted in the DL. However, [3, 4, 14, 16, 19, 22, 24, 26] have also highlighted that in spite of the reduction in Rx antennas, the UEs will be able to fulfil the data rate requirements of most RedCap use cases (except high-end wearables in FR1), as given in the SID.

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Data rate:**  Reducing the number of Rx branches at the UE will lower the downlink peak data rate. This is due to the reduction in number of downlink MIMO layers that can be supported when the number of Rx branches is reduced.   * Reduction from 2 Rx branches to 1 Rx branch decreases the downlink peak rate by ~50%. * Reduction from 4 Rx branches to 2 Rx branches decreases the downlink peak rate by ~50%. * Reduction from 4 Rx branches to 1 Rx branch decreases the downlink peak rate by ~75%.   Despite this reduction in peak data rate, a UE with reduced number of Rx branches and downlink MIMO layers will be able to sufficiently fulfil the peak data rate requirements for the RedCap use cases. For peak rate impacts from other combinations of UE complexity reduction techniques, see clause 7.8.3. |

**Phase 2: Question 7.2.3-4: Can the above observations of the impact on data rate for reduced number of UE Rx antennas be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| LG | Y(partially) | The sentence starting with “Despite …” may not be entirely correct. For example, 1 Rx cannot support the highest peak rate in the SID. We would not be at least incorrect with the following changes:  “Despite this reduction in peak data rate, the UE will be able to sufficiently fulfil most of the peak data rate requirements for the RedCap uses cases.” |
| ZTE | Partially Y | For reduction from 4 Rx branches to 2 Rx branches, the decreasing ratio of downlink peak rate should be determined according to number of MIMO layers. |
| vivo | Y | We are also fine with LG’s proposed update |
| SONY5 | Y | Also OK with LG’s proposed update |
| FUTUREWEI | Y | The peak data rate in the SID has “up to” so this is OK. |
| Qualcomm | Y |  |
| DOCOMO | Partially Y | Agree with LG that the highest peak data rate requirement is not satisfied with 1 Rx branch and support LG’s modification |
| Sierra Wireless | Y | Ok with LG’ proposal |
| Samsung |  | Suggest to delete the following sentence  ~~The lower MCS that may need to be applied to compensate for the performance loss may have a negative impact on the achievable data rate.~~  In addition, we only agree to capture the bullets if table 7.2.2.-1 is deleted. There is no reduction on HARQ buffer and LDPC decoding, which implied no peak data rate reduction. |
| Ericsson | Y | Perhaps it can be clarified in the text that the statement concerns reduced number of Rx branches with a corresponding reduction of the number of MIMO layers, but not combinations with other techniques (such as reduced bandwidth). |
| Intel | Y (partially) | Propose to remove the last sentence – “performance loss” is unclear, and if it is referring to link reliability/coverage, then the essence of it is already covered in the first part (“… will lower the DL peak data rate”). |
| OPPO | Y | Ok with LG’ proposal |
| Xiaomi |  | * + 1. The peak data rate depends on the the number of MIMO layer, the maximum UE BW and the MCS. Maybe, it is not so rigorous without saying the assumption of UE bandwidth and MCS. For example, different UE bandwidth assumption would result in different conclunsion.     2. Since the the reduction to 2Rx and reduction to 1Rx face different situation, then we suggest to describle them separately.   Hence, We suggest the following update for the sentence starting with ” Despite…”  “Despite this reduction in peak data rate,   * + - the Redcap UE with 2Rx will be able to sufficiently fulfil the peak data rate requirements for the RedCap uses cases with the assumption of 20MHz maximum UE bandwith and 64QAM in DL     - the Redcap UE with 1Rx will be able to sufficiently fulfil most of the peak data rate requirements for the RedCap uses cases with the assumption of 20MHz maximum UE bandwith and 64QAM in DL     - the Redcap UE with 1Rx will be able to sufficiently fulfil the peak data rate requirements for the RedCap uses cases with the assumption of 40MHz maximum UE bandwith and 64QAM in DL” |
| CATT | Y, partially | For the 2nd paragraph, we agree with LG. We think ‘most of’ should be added before ‘the RedCap uses cases’. It is not sure whether all uses cases can be fulfilled, especially if the BW is also reduced (to 20MHz).  For the 3rd paragraph, we are appreciated if we can hear some clarifications. Is it talking about the achievable data rate but not peak data rate, e.g. the result from ‘1 layer, 2Rx’ to ‘1 layer, 1Rx’? If so, we are OK for it. |
| Huawei, HiSilicon | Y |  |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.2.3-4a: Can the above observations of the impact on data rate for reduced number of UE Rx antennas be used as a baseline text for TR 38.875?** | |
| CATT | Y | We think it is somewhat obvious that the UE can fulfill the data rate requirement when only the Rx number is reduced. But we are fine with the current verson. |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Samsung | Y |  |
| Huawei, HiSilicon | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Latency and reliability:**

* P2: In [26], it is observed that in FR2, support of 1 Rx antenna at the UE can satisfy the latency requirements for industrial wireless sensors and video surveillance cameras (with 100 MHz).
* P3: In [19], it is observed that reducing the number of receive antennas does not affect the reliability and latency in most cases. However, if the UE is in the cell-edge the latency can increase. In [1], it is highlighted that the UEs with reduced of number of UE Rx branches can sufficiently fulfil the latency and reliability requirements of all RedCap use cases.

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Latency and reliability:**  Reducing the number of UE Rx branches has limited impact on the latency in most cases. However, if the UE is near the cell edge, the latency can increase. Nevertheless, the latency requirements of RedCap use cases can be sufficiently fulfilled, in both FR1 and FR2.  The reliability requirements for the RedCap use cases can still be fulfilled with reduced number of UE Rx branches. However, in some cases, the reliability can only be maintained at the cost of downlink spectral efficiency loss. |

**Phase 2: Question 7.2.3-5: Can the above observations of the impact on latency and reliability for reduced number of UE Rx antennas be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Partially Y | Change “Reducing the number of UE Rx branches does not affect the reliability” to “Reducing the number of UE Rx branches can fulfil the reliability requirements.” |
| vivo | Y |  |
| SONY5 | Y | Editorial: Nevertheless, the latency requirements of RedCap use cases can be sufficiently fulfilled, in both FR1 and FR2. |
| FUTUREWEI | wait | Let us see the 8.6.3 progress and how much we will compensate |
| Qualcomm | Y |  |
| DOCOMO | Y | Also fine with ZTE’s modification |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y | Also fine with ZTE’s revision |
| Intel | Y (partially) | Propose to remove the last sentence – it is not necessary and essentially repeating the peak data rate/spectral efficiency impact from previous point. |
| OPPO | Y |  |
| Xiaomi | Y |  |
| CATT | Y |  |
| LG | Y | Also fine with ZTE’s wording. |
| Huawei, HiSilicon | FFS | The reliability is related to the coverage. So saying reliability is not affected may not be correct. |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.2.3-5a: Can the above observations of the impact on latency and reliability for reduced number of UE Rx antennas be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Samsung | Y |  |
| Huawei, HiSilicon | Y |  |
| LG | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Power consumption:**

* P4: [4] and [16] have noted that power consumption is also saved by fewer RF chains and by less complexity of multi-antenna processing. In [6], it has been noted that the power consumption of 1 Rx UE is lower than that of a 2 Rx UE.
* P5: [1, 11, 13, 15, 19, 27, 28] have noted that although the reduction in Rx antenna can reduce power consumption in the RF and the baseband modules, due to longer reception time needed for downlink channels, the power consumption will be increased. In [1, 15], it has been highlighted that the actual impact depends on the DL traffic.
* P6: The evaluation results in [4] show that the power saving gains when reducing the number of UE Rx antennas from 2 to 1 are about 14% for instant messaging traffic, 11% for Heartbeat traffic and 15% for VoIP traffic. In [24], it has been mentioned that more evaluations are needed to understand the impact on overall power consumption due to lower consumption in RF/baseband modules and longer reception time.

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Power consumption:**  The instantenous power consumption in the RF and the baseband modules of the UE is expected to be reduced due to the use of fewer RF chains and the reduction in the complexity of multi-antenna processing. However, depending on the traffic characteristics, the average power consumption of the UE can increase or decrease. The average power consumption may increase since the reduced downlink spectral efficiency may require larger coded blocks or a longer reception time for the PDSCH to deliver the same amount of data. |

**Phase 2: Question 7.2.3-6: Can the above observations of the impact on power consumption for reduced number of UE Rx antennas be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | N | Regarding the last sentence, it seems no evaluation results showing that with what traffic model, the average power consumption will increase due to reduced Rx? |
| SONY5 | Y | Editorial: “fewer ~~number of~~ RF chains”.  In response to vivo: if the reduced number of RX antennas caused a halving of MCS, then the UE would have to be “on” for twice as long to receive the data. This would tend to increase the power consumption. A related observation was made in TR36.888 (section 6.3.2.2): “*Reduced downlink spectral efficiency would require larger coded blocks or a longer reception time for the PDSCH to deliver the same amount of data. This would increase the average power consumption*”. We think that this effect occurs both in LTE and in NR. |
| FUTUREWEI | Y | This balanced style of observation seems fair and about as good as we can get. |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung |  | The observation can be made based on the result in AI 8.6.2 |
| Ericsson | Y |  |
| Intel | N | Agree with Vivo that the “increase” part is not very obvious and such may not occur in many cases. Reduction in Rx antenna may not necessarily lead to longer DL reception. The UE could still be scheduled over the same time resources with larger BW or with power boosting. Thus, further conditioning/clarifications would be necessary if we want to capture possibility of power consumption increase. |
| OPPO | N | Agree with vivo. The last sentence shall be further proved? |
| Xiaomi | Y |  |
| CATT | Y |  |
| LG | N | Agree with the comments above from vivo, Intel and OPPO. |
| Huawei, HiSilicon | FFS | The last sentence is being studied in other sessions. May need to calrify as vivo commented. |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.2.3-6a: Can the above observations of the impact on power consumption for reduced number of UE Rx antennas be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | N | Need to align with the outcome of AI 8.6.2 |
| vivo | N | We disagree with the updated proposal. As commented before, there is no evaluation results showing that reduced Rx can actually increase UE power consumption. However, we had provided simuatio results in R1-2009212 section 2.3 showing that reducing Rx can provide power saving benefit based on the agreed agreed power model and traffic mode. |
| ZTE | Y |  |
| Samsung |  | We think P6 is worthwhile to capture. So, some changes is proposed:  The instantenous power consumption in the RF and the baseband modules of the UE is expected to be reduced due to the use of fewer RF chains and the reduction in the complexity of multi-antenna processing. ~~However, depending on the traffic characteristics, the average power consumption of the UE can increase or decrease.~~ The average power consumption may increase since the reduced downlink spectral efficiency may require larger coded blocks or a longer reception time for the PDSCH to deliver the same amount of data. However, for typical traffic for Redcap UE, i.e., instant messaging traffic, Heartbeat traffic and VoIP traffic, 11%~15% of power saving is observed by one soucing company.  In addition, we suggest to clarify that the TP can be updated based on output of AI 8.6.2 |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | Y |  |
| LG | N | We don’t agree on this analysis. Larger coded bits given the same amount of payload and slightly increased number of repetitions doesn’t always result in net incease in the power consumption. It would be okay to us if the last two sentences (or at least the last sentence) are removed. |
| FUTUREWEI3 | Y |  |
| Ericsson | Y | Regarding the last sentence proposed by Samsung, if the evaluations have been made under the assumption that the traffic is DL only, we think that would need to be clarified in the sentence if any such sentence is to be included. We prefer to not include any quantitative analysis here. |
| SONY7 | Y | Agree with proposal.  Agree with Ericsson about quantitative analysis in these sections: the text in these 7.x.3 sections tends to be more qualitative than quantitative.  A couple of responses to comments from other companies:  Vivo: do you disagree with the text in TR36.888 (section 6.3.2.2): “*Reduced downlink spectral efficiency would require larger coded blocks or a longer reception time for the PDSCH to deliver the same amount of data. This would increase the average power consumption*”? Why would we reach a different conclusion for NR relative to LTE?  LG: Regarding the red part of your comment: “Larger coded bits given the same amount of payload and slightly increased number of repetitions doesn’t always result in net incease in the power consumption.”. We think the FL proposal doesn’t contradict your point (see red, again): “The average power consumption may increase” |

**PDCCH blocking probability:**

* P10: [1,13, 15, 19, 23, 24, 28] have noted that there will be increase in PDCCH blocking probability. This is due to use of higher ALs in order to compensate for the performance degradation from a reduced number of Rx antennas.

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **PDCCH blocking probability:**  In order to compensate for the performance degradation resulting from a reduced number of UE Rx branches, higher aggregation levels may need to be used. This can lead to increase in PDCCH blocking probability if the amount of PDCCH resources is not increased. |

**Phase 2: Question 7.2.3-7: Can the above observations of the impact on PDCCH blocking probability for reduced number of UE Rx antennas be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | modifications | In order to compensate for the performance degradation resulting from a reduced number of UE Rx branches, higher aggregation levels may need to be used. This can lead to increase in PDCCH blocking probability if the amout of PDCCH resource is not increased. |
| SONY5 | Y | Editorial: This can lead to an increase in PDCCH blocking probability |
| FUTUREWEI | Y |  |
| DOCOMO | Y |  |
| Samsung | Y |  |
| Ericsson | Y | Also fine with Vivo’s revision |
| Intel | Y |  |
| Xiaomi |  | Agree with vivo’s update |
| CATT | Y |  |
| LG | Y |  |
| Huawei, HiSilion | Y |  |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.2.3-7a: Can the above observations of the impact on PDCCH blocking probability for reduced number of UE Rx antennas be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Huawei, HiSilion | Y |  |
| Spreadtrum | Y |  |
| LG | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

### 7.2.4 Analysis of coexistence with legacy UEs

Several contributions have analyzed coexistence issues with legacy UEs. The finding can be listed as follows:

* C1: There will be coexistence impact depending on the coverage recovery solutions and other enhancements (e.g., early RedCap indication in RACH) adopted for RedCap during the initial access stage [1, 2, 5, 9, 11, 15, 21, 24]. Note that depending on the outcome of discussions taking place under AI 8.6.3, no coverage recovery may be needed to compensate for the performance loss due to reduced number of UE Rx antennas.
* C2: Blocking impacts if RedCap UE need to use higher aggregation levels for PDCCH reception [1, 2, 5, 24].
* C3: There will be coexistence issues if common DL broadcast channels (e.g., SIBx/RAR/paging) are used for both legacy UEs and RedCap UEs [1, 5, 15, 16, 24]. This is because the system treating the UEs the same will mean conservative handling of all UEs. It has also been noted in [16] that the common channels can be transmitted separately for redcap UE and normal NR UE, which can be realized by the gNB’s scheduling implementation.
* C4: RedCap UEs with reduced number of Rx antennas can coexist with legacy UEs in general [4, 11, 15, 16, 19].
* C5: The network deployment (cell planning) may be required to be adjusted [24]. It is also been mentioned in [24] that this aspect can be considered in RAN4.
* C6: 1 Rx RedCap UEs would cause significant performance degradation to legacy UEs due to coexistence needs or may cause network block for RedCap UEs accessing when the number of UEs in one cell is large [3].

**Phase 3: Question 7.2.4-1: Can the above list (C1-C6) be used as a baseline for the TP drafting for TR section 7.2.4?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| vivo |  | Agree to capture:   * C3, C4   Do not agree to capture:   * C5 (The aim of coverage recovery is to allow RedCap UE to access the network without changing the deployment)   To discuss further in AI 8.6.3 based on the evaluation results:   * C1, C6   To discuss further in AI 8.6.2 based on the evaluation results:   * C2 |
| ZTE | Y | C1, C2, C3 |
| Spreadtrum | Y | C1, C2, C3 |
| OPPO |  | C1,C3, C4 can be captured. |
| Samsung |  | Support to capture: C1 (only first sentence without Note), C2 (with change), C3(except the last sentence), C4  Don’t agree to capture: C5, C6 (should be discussed in RAN 2)  Additiona comment:   * C1: There will be coexistence impact depending on the coverage recovery solutions and other enhancements (e.g., early RedCap indication in RACH) adopted for RedCap during the initial access stage [1, 2, 5, 9, 11, 15, 21, 24]. Note that depending on the outcome of discussions taking place under AI 8.6.3, no coverage recovery may be needed to compensate for the performance loss due to reduced number of UE Rx antennas. * Even no coverage recovery is needed, gNB need to knows the coverage different for DL early, otherwise, it has to assume all UEs, including NR UEs, only have single Rx, so that the resource for DL transmission will increased. * C2: Blocking impacts if RedCap UE need to use higher aggregation levels for PDCCH reception [1, 2, 5, 24], especially for common search space(s) before RRC connection since all the UEs monitor the same search space. * Suggest to add text in red. * C3: There will be coexistence issues if common DL broadcast channels (e.g., SIBx/RAR/paging) are used for both legacy UEs and RedCap UEs [1, 5, 15, 16, 24]. This is because the system treating the UEs the same will mean conservative handling of all UEs. It has also been noted in [16] that the common channels can be transmitted separately for redcap UE and normal NR UE, which can be realized by the gNB’s scheduling implementation. * The last sentence need to be further discussed. With current spec, we don’t think this can be solved by gNB implementation. Separated configuration for RACH procedure and dedicated SIB is needed. |

### 7.2.5 Analysis of specification impacts

Several contributions [1, 2, 3, 4, 5, 9, 11, 12, 13, 15, 16, 19, 20, 21, 22, 23, 24, 28] also point out the specification impacts from reducing the number of UE Rx antennas. Potential RAN1 impacts depend on the techniques that may be used to compensate for the coverage and spectral efficiency loss. The extent of RAN1 impacts would also depend on the outcome of link budget analysis that is taking place under AI 8.6.3.

Some techniques highlighted in different contributions that will have RAN1 specification impacts are:

* S1: PDCCH repetition: [12, 15, 22, 24]
* S2: Additional repetitions for PDSCH: [12, 22, 24]
* S3: AL greater than 16: [11, 15, 24]
* S4: Compact DCI: [15, 24]
* S5: CSI report enhancement to improve spectral efficiency: [15]
* S6: Early indication of RedCap UE in random access: [1, 22, 15]
* S7: Group scheduling to reduce PDCCH overhead and solve PDCCH blocking issue [15]
* S8: Cross-repetition channel estimation [12]

It has been noted in [3] that depending on the performance target, e.g., peak data rate and coverage recovery, there could be no/marginal specification impacts for UEs with 2Rx (20MHz) but there would be specification impact for 1Rx UEs even with larger bandwidth (for coverage/throughput improvement).

Several contributions [1, 2, 4, 5, 13, 15, 16, 19, 20, 28] have mainly also highlighted potential RAN4 specification impacts, including RRM, receiver characteristics, demodulation performance requirements, CSI reporting requirements, RF, and procedure requirements (e.g., cell change, radio link management, beam management, etc.). It is also mentioned in [5] that RAN4 needs to evaluate and specify the new minimum number of Rx antennas for different bands. In [5], it also suggested that UL transmit antenna gain should be evaluated in RAN4 for size-limited RedCap UEs, e.g. some wearables. In [1, 28], it is indicated that the impact is more significant when reducing the number of receiver branches to 1. It has been mentioned in [1] that the impacts are manageable and comparable (at least for FR1) to the corresponding changes done for Cat M1 UEs in LTE.

In addition, [19] has indicated that there would be potential RAN2 impact due to signalling of reduced antenna capability. It has also been noted in [1] that early indication (S6) will also have RAN2 specification impacts.

**Phase 4: Question 7.2.5-1: Should RAN4 specification impacts be captured in TR 38.875 for UE antenna reduction? If yes, list the most critical ones to be captured.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments** |
| vivo | N | It seems all the above proposals are relevant other agenda items rather than 8.6.1, to be more specific  To discuss further in AI 8.6.3 based on the evaluation results:   * S1, S2, S3, S4, S5, S8   To discuss further in AI 8.6.5   * S6   To discuss further in AI 8.6.2   * S7 |
| ZTE | Y | RF, RRM, demodulation performance and CSI reporting requirements. |
| Panasonic | Y | RRM, demodulation performance and CSI reporting requirements |
| Spreadtrum | Y | Should consider RAN4 impact |
| OPPO |  | May have some RAN4 impact, but it shall be decided by RAN4. |
| Samsung |  | At least RRM, demo requirement is needed to support Rx reduction. If captured, it is suggested to capture RAN 4 requirement (if any) for all the techniques has potentially RAN 4 impact. We can also live with focus on RAN 4 spec inpact. |
| Qualcomm | Y | At least RF, RRM, DL demodulation, CSI measurements/reporting and SSB/SIB acquisition.  FFS techniques for coverage recovery of RedCap UE. |

**Phase 4: Question 7.2.5-2: Can the above list (S1-S8) be used as a baseline for the TP drafting for TR section 7.2.5?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| vivo | N | As commented above, S1~S8 should be discussed in the corresponding agenda items, with the potential TPs as the discussion outcome. |
| OPPO |  | S6 may be needed, but it depends on the output of the evaluation in 8.6.3. |
|  |  |  |
| Samsung |  | S1, S3, S4, can be combined as PDCCH coverage recovery. S3, S6 can be discussed in other AI.  Support to capture S5, S7,  FFS for S8, considering CE SI. |
| Qualcomm |  | S1 to S7 can be considered. |

## 7.3 UE bandwidth reduction

### 7.3.1 Description of feature

RAN1#103e agreement:

* Adopt the TP in [R1-2009393](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009393.zip) for TR clause 7.3.1.

### 7.3.2 Analysis of UE complexity reduction

RAN1#103e agreement:

* Adopt the TP in [R1-2009393](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009393.zip) as baseline text for TR clause 7.3.2.
  + Companies are invited to double-check their entries in the cost reduction spreadsheet with respect to the above comments (and to catch potential typos).
  + The table will be further updated with potential updated cost estimates.

### 7.3.3 Analysis of performance impacts

According to the SID [36],

|  |
| --- |
| The study includes evaluations of the impact to coverage, network capacity and spectral efficiency |

In addition, RAN1#101e made the following agreement:

|  |
| --- |
| Agreements:   * The evaluation of performance impacts includes at least peak data rate, latency and reliability (as needed for the use cases). Other performance metrics such as power consumption, spectral efficiency and PDCCH blocking probability may also be considered if appropriate for a specific technique. |

**Coverage:**

* P23: The impact of reduced BW on DL and UL channels would not be large; some negligible loss may be observed due to reduced frequency diversity [1, 11, 15, 19, 27].
* P24: (FR1) UE bandwidth 20 MHz is enough to support PDCCH AL 16 in FR1 [1].
* P25: (FR2) For some use cases, increasing the max UE BW from 50 to 100 MHz may lead to an increase in mean SINR [26].
* P26: (FR2) RedCap UE may not receive AL8/16 [24].
* P27: (FR2) Due to not enough number of CCEs in the CORESET, AL 16 cannot be supported without performance loss for 50 MHz UE BW and SCS = 120 kHz [1, 26].
* P28: (FR2), Reducing the bandwidth to 50 MHz will have impact on PBCH coverage if the SSB is configured with 240 kHz SCS [1, 2, 8, 11, 27, 28].
  + The loss is assessed to be less than 1 dB [1, 11, 27].
* P29: (FR2) Reducing the bandwidth to 50 MHz will have impact on PDCCH coverage if CORESET#0 is configured to have 69.12 MHz bandwidth [1, 2, 4, 8, 16, 27, 28].
  + The loss is assessed to be ~ 1.5 – 3 dB [1, 2, 8].
* P30: (FR2) Reducing the bandwidth to 50 MHz will have impact on initial access (message 2/3/4) if CORESET#0 is configured to have 69.12 MHz bandwidth [3, 20, 23, 27].

Based on submitted contributions and email discussion responses, the following TP can be considered. More text on coverage can be captured after further progression of the discussion under AI 8.6.3.

|  |
| --- |
| **Coverage:**  The impact of reduced bandwidth on the coverage of downlink and uplink channels would not be large, although a small loss may be observed due to reduced frequency diversity.  For PDCCH coverage, one important aspect is whether the larger aggregation levels (AL), e.g. 8 and 16, can be supported after bandwidth reduction. In FR1, UE bandwidth 20 MHz is enough for supporting AL 16 for any CORESET#0 configuration. In FR2, UE bandwidth 100 MHz is also enough for supporting AL 16 for any CORESET#0 configuration. However, reducing the UE bandwidth to 50 MHz in FR2 will have impact on PDCCH coverage when CORESET#0 is configured to have 69.12 MHz bandwidth. The loss is assessed to be ~1.5-3.0 dB. Reducing the UE bandwidth to 50 MHz will have impact on PBCH coverage if the SSB is configured with 240 kHz SCS. The loss is assessed to be within 1 dB. Furthermore, reducing the UE bandwidth to 50 MHz may also impact the coverage of initial access messages if CORESET#0 is configured to have 69.12 MHz bandwidth. |

**Phase 2: Question 7.3.3-2: Can the above observations of the impact on coverage for UE bandwidth reduction be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung |  | OK with first sentence.  For the second paragraph, we sugget to wait for AI 8.6.3. |
| Ericsson | Y |  |
| Intel | Y |  |
| OPPO | Y |  |
| CATT | Y |  |
| LG | Y |  |
| Huawei, HiSilicon | Y |  |
| FL | **FL2: Phase 2: Question 7.3.3-2: Can the above observations of the impact on coverage for UE bandwidth reduction be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Samsung |  | In addition, we suggest to clarify that the TP can be updated based on output of AI 8.6.3 |
| Huawei, HiSilion | Y |  |
| LG | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Network capacity and spectral efficiency:**

* P34: Bandwidth reduction will not have a significant impact on capacity and spectral efficiency [1, 11, 19].
* P35: There may be some degradation in DL and UL spectral efficiency due to the loss in frequency selective scheduling gain [15].
* P36: Network capacity may be impacted for initial access [15].
* P37: The spectral efficiency may be affected due to an increase in PDCCH blocking probability resulting from the use of a smaller CORESET bandwidth [13].
* P38: (FR2) The number of users that can be supported is impacted by almost 50% if the max UE BW is reduced from 100 MHz to 50 MHz [26].
* P39: (FR2) If dedicated channel for RedCap is introduced for supporting maximum UE bandwidth of 50 MHz, the network capacity would be impacted [20].

Based on submitted contributions and email discussion responses, the following TP can be considered. More text on network capacity and spectral efficiency can be captured after further progression of the discussion under AI 8.6.3.

|  |
| --- |
| **Network capacity and spectral efficiency:**  Bandwidth reduction in FR1 will not have a significant impact on capacity and spectral efficiency, although there may be some minor degradation due to the loss in frequency selective scheduling gain.  Bandwidth reduction in FR2 may be associated with more noticable loss in capacity and spectral efficiency if analog beamforming is being used. In this case, the loss will be larger for 50 MHz UE bandwidth than for 100 MHz UE bandwidth. |

**Phase 2: Question 7.3.3-3: Can the above observations of the impact on network capacity and spectral efficiency for UE bandwidth reduction be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm |  | Y for FR1, when the reduced UE BW if no less than 20 MHz on a single carrier.  N for FR2, if the reduced UE BW is less than 100 MHz. Some results show that depending on the deployment scenario, there may be some degradation to the network capacity |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y | Can be revised with observation in AI 8.6.3 |
| Ericsson | Y |  |
| Intel | Y |  |
| OPPO | Y |  |
| Xiaomi | Y |  |
| CATT | Y |  |
| LG | Y |  |
| Huawei. HiSilicon | Y |  |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.3.3-3a: Can the above observations of the impact on network capacity and spectral efficiency for UE bandwidth reduction be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Huawei, HiSilion | Y |  |
| Spreadtrum | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y | Not convinced about the spelling of “analog”… 😊  [no need to update] |

**Data rate:**

* P1: (FR1) There is an impact on peak data rate due to BW reduction [2, 15, 19, 20, 24].
* P2: (FR1) The most demanding DL peak rate requirements (150 Mbps) can be met by 20 MHz UE BW with 2 MIMO layers [3, 4, 6, 8, 10, 12, 14, 23, 24, 26].
* P3: (FR1) The most demanding DL peak rate requirements (150 Mbps) can be met by larger than 20 MHz UE BW, e.g. 40 MHz [4, 5, 8, 12, 26].
* P4: (FR1) The most demanding UL peak rate requirements (50 Mbps) can be met by 20 MHz UE BW [8].
* P5: (FR1) Single MIMO layer, 20 MHz UE BW, and 64QAM can meet the peak bit rate requirements of most use cases [1, 2, 4, 6, 8, 14, 26].
* P6: (FR2) All the data rate requirement can be met by 50 MHz and 100 MHz BW [1, 4, 14, 24].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Data rate:**  Bandwidth reduction results in a reduction in the achievable peak data rate. However, all the bandwidth options (20 MHz in FR1, and 50 MHz or 100 MHz in FR2) considered in the RedCap study are enough for meeting the peak data rate requirements for the RedCap use cases. For peak rate impacts from combinations of UE complexity reduction techniques, see clause 7.8.3. |

**Phase 2: Question 7.3.3-4: Can the above observations of the impact on data rate for UE bandwidth reduction be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| LG | Y(partially) | Same concern as in **Phase 2: Question 7.2.3-4**. Consider changes suggested there. |
| ZTE | N | For 20 MHz in FR1, single-Rx RedCap UE cannot meet 150 Mbps peak data rate requirement. |
| vivo |  | Agree with ZTE’s point, maybe we should say “enough for meeting the peak data rate requirements for most of the RedCap use cases” |
| SONY5 | Y |  |
| FUTUREWEI | Y | The SID says “up to”. Let us not repeat that discussion. |
| Qualcomm |  | Agree with the suggestion of Vivo. |
| DOCOMO | Partially Y | Agree with LG |
| Sierra Wireless | Y | The proposal looks Ok. With the optional features the RedCap device should meet the requirements. For the highest of the rates, the SID says “up to”. |
| Samsung | Y |  |
| Ericsson | Y | Perhaps it can be clarified in the text that the statement concerns the individual technique, not combinations with other techniques. |
| Intel | Y |  |
| OPPO |  | Agree with ZTE and LG.  Vivo’s revision can be considered. |
| Xiaomi |  | Agree with ZTE and vivo |
| CATT | Y, partially | Like 7.2.3-4, we think ‘most of’ should be added before ‘the RedCap uses cases’. It is not sure whether all uses cases can be fulfilled, especially if the BW is also reduced (to 20MHz). |
| Huawei, HiSilicon | Y |  |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.3.3-4a: Can the above observations of the impact on data rate for UE bandwidth reduction be used as a baseline text for TR 38.875?** | |
| CATT | Y | We think it is somewhat obvious that the UE can fulfill the data rate requirement when only the BW is reduced. But we are fine with the current verson. |
| Qualcomm | Y |  |
| ZTE |  | Need to mention that only bandwidth is reduced |
| Samsung | Y |  |
| Huawei, HiSilion | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Latency and reliability:**

* P7: The latency requirements for industrial wireless sensors can be satisfied [1, 19].
* P8: For video surveillance cameras, the latency requirements can be satisfied [1].
* P9: For the use cases that are considered in this study, the latency associated with increased transmission time (due to the reduced bandwidth) is likely to be insignificant compared to the latency associated with the DRX functionality [19].
* P10: For larger message sizes, the latency can be increased if the large messages need to be segmented into multiple transport blocks and sent over multiple slots [19].
* P11: (FR2) The latency requirements for industrial wireless sensors may be satisfied with UE BW as small as 20 MHz. For video surveillance cameras, the latency requirements can be satisfied using 20 MHz BW for small file sizes. For larger file sizes, BW needs to be increased to ~100MHz to get more UE multiplexing capacity. 20 MHz active BWP may be enough for most cases [26].
* P12: (FR2) Bandwidth reduction results in a longer SSB/SIB1 acquisition time. However, it is not necessary to have stringent SSB acquisition requirements for RedCap use cases [1].
* P13: (FR2) To minimize the SSB/CORESET acquisition time (for multiplexing patterns 2 and 3), it may be beneficial to support 100 MHz as the max UE BW [5, 26].
* P14: (FR2) For both 50 MHz and 100 MHz bandwidth options in FR2, there will be longer SSB/SIB1 acquisition time for certain SSB and Type 0 PDCCH configurations [2, 5, 24, 25].
* P15: Longer SSB/CORESET acquisition time issue only occurs for SSB and CORESET multiplexing 2 with 240 kHz SCS SSB + 120 kHz SCS 48RB CORESET 0 if the maximum UE bandwidth is 100 MHz [5].
* P16: Reliability should not be impacted as it is envisaged that BLER targets can still be achieved at a reduced bandwidth [19].
* P17: All the RedCap bandwidth options can meet the reliability target of RedCap use cases [1].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Latency and reliability:**  All the latency and reliability requirements for the RedCap use cases can be satisfied by all the bandwidth options (20 MHz in FR1, and 50 MHz or 100 MHz in FR2)  In FR2, UE bandwidth reduction may result in a longer SSB/SIB1 acquisition time for certain configurations for SSB/CORESET multiplexing patterns 2 and 3. To minimize the SSB/SIB1 acquisition time, it may be beneficial to support an FR2 RedCap UE bandwidth of 100 MHz. |

**Phase 2: Question 7.3.3-5: Can the above observations of the impact on latency and reliability for UE bandwidth reduction be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm |  | Y for FR1.  N for FR2.  In FR2, UE bandwidth reduction may result in a longer SSB/SIB1 acquisition time for certain configurations for SSB/CORESET multiplexing patterns 2 and 3. However, it is not necessary to have stringent SSB/SIB1 acquisition requirements for RedCap use cases. To minimize the SSB/SIB1 acquisition time, it may be beneficial to support an FR2 RedCap UE bandwidth of 100 MHz. |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | Y (partly) | Support the modification from Qualcomm. |
| OPPO | Y |  |
| CATT | Y | Y for the 1st paragraph. When studing latency and reliability, it is more general to consider that the PUSCH/PDSCH in RRC\_CONNECT mode is evaluated.  Regarding to the 2nd paragraph, we are fine with Qualcomm’s modification. |
| LG | Y | Prefer the wording suggested by Qualcomm. |
| Huawei, HiSilicon | Y |  |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.3.3-5a: Can the above observations of the impact on latency and reliability for UE bandwidth reduction be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Samsung | Y |  |
| Huawei, HiSilion | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Power consumption:**

* P18: UE bandwidth reduction may reduce power consumption [4, 11, 13].
* P19: Evaluation is needed to assess the effects of less RF/BB modules vs longer Rx time [19, 24].
* P20: There is no clear power consumption advantage or disadvantage due to UE bandwidth reduction. It may depend on the specific traffic scenario [1].
* P21: BW reduction has no impact on the power consumption of data channels [13].
* P22: In connected mode, when the RedCap UE operates in initial DL/UL BWP larger than maximum UE bandwidth of RedCap UEs, more power consumption would be expected due to RF retuning [5].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Power consumption:**  UE bandwidth reduction reduces the instantaneous power consumption of the RF and baseband modules during transmission and reception. However, depending on the traffic characteristics, the average power consumption of the UE can increase or decrease. The average power consumption may increase since the reduced downlink peak data rate may require larger coded blocks or a longer reception time for the PDSCH to deliver the same amount of data. |

**Phase 2: Question 7.3.3-6: Can the above observations of the impact on power consumption for UE bandwidth reduction be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo |  | It is not clear whether increase of power consumption can be justified in the 2nd sentence. |
| SONY5 | Y | In response to vivo: if there is an increase in transmission time due to bandwidth reduction (either due to a lower MCS from frequency diversity loss, or due to a TB not “fitting into” 20MHz), then the UE needs to be “on” for longer, which would potentially cause an increase in power consumption. |
| FUTUREWEI | Y | Similar comment as before, balanced approach is appropriate. |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y | Can be revised with observation in AI 8.6.3 |
| Ericsson | Y |  |
| Intel |  | We tend to agree with Vivo here.  While the proposes last sentence may be true in general, for the data rate requirements considered for RedCap, we are not sure if there would be an increase in power consumption with reduced UE BW (to 20 MHz and 100 MHz respectively). |
| OPPO |  | Agree with intel and vivo.  The last sentence shall be further proved. |
| Xiaomi | Y |  |
| CATT | Y |  |
| LG |  | Agree with vivo, Intel and OPPO. |
| Huawei, HiSilicon | Y | And also fine with vivo suggestion |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.3.3-6a: Can the above observations of the impact on power consumption for UE bandwidth reduction be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | FFS | Need to align with the outcome of AI 8.6.2 |
| vivo | N | We disagree with the updated proposal. Technically 20MHz can still provide enough data rate so that the active time for data transmission does not necessarily increase, especially for RedCap use case which typically has smaller data packets.  Since there are no evaluation results avaiable, we can go with more simpler version, i.e. 1st sentence only  **Power consumption:**  UE bandwidth reduction reduces the instantaneous power consumption of the RF and baseband modules during transmission and reception. ~~However, depending on the traffic characteristics, the average power consumption of the UE can increase or decrease. The average power consumption may increase since the reduced downlink peak data rate may require larger coded blocks or a longer reception time for the PDSCH to deliver the same amount of data.~~ |
| ZTE | Y |  |
| Samsung |  | Support vivo’s proposal |
| Huawei, HiSilion | Y |  |
| Spreadtrum | Y |  |
| LG | N | We don’t agree on this analysis. Larger coded bits given the same amount of payload and slightly increased number of repetitions doesn’t always result in net incease in the power consumption. We are okay with vivo’s suggestion. |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y | Agree with proposal.  A couple of responses to comments from other companies:  Vivo: do you disagree with the text in TR36.888 (section 6.2.2.3): “*the reception time may become larger if the performance degradation on PDSCH results in a longer transmission time, thus possibly increasing the power consumption*”? Why would we reach a different conclusion for NR relative to LTE? We think we need to be talking about average power consumption, rather than instantaneous power consumption.  LG: Regarding the red part of your comment: “Larger coded bits given the same amount of payload and slightly increased number of repetitions doesn’t always result in net incease in the power consumption.”. We think the FL proposal doesn’t contradict your point (see red, again): “The average power consumption may increase”  the reception time may become larger if the performance degradation on PDSCH results in a longer transmission time, thus possibly increasing the power consumption |

**PDCCH blocking probability:**

* P31: PDCCH blocking probability may be increased due to small CORESET bandwidth [13].
* P32: (FR2) Using 50 MHz instead of 100 MHz may cause considerable reduction in the PDCCH multiplexing capacity and PDCCH blocking probability [24, 26].
* P33: (FR2) PDCCH blocking probability is only slightly increased if the maximum UE bandwidth is further reduced from 100 MHz to 50 MHz [1].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **PDCCH blocking probability:**  If CORESET is configured according to the RedCap UE capability and shared by both RedCap and non-RedCap UEs, this may result in increased PDCCH blocking probability. In that case, the impact of an FR2 RedCap UE bandwidth of 50 MHz would be greater than for 100 MHz. |

**Phase 2: Question 7.3.3-7: Can the above observations of the impact on PDCCH blocking probability for UE bandwidth reduction be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y | We think the text is OK. Although a lot of the text talks about FR2, we feel that the issue also exists for FR1. However, we think the text is OK. |
| FUTUREWEI | almost | Prefer not to include the “However” solution |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | Y |  |
| OPPO | Y |  |
| Xiaomi | Y |  |
| CATT | Y, partially | We suggest removing the 3rd sentence: ‘However, if it is possible…may be insignificant’. The direct result of separate CORESET is that the non-RedCap UE will not be impacted by the RedCap UE. However, for RedCap UE themselves, the PDCCH blocking probability may not be insignificant, due to reduced BW. Also, it seems P32 is contradictory to P33. |
| LG | Y |  |
| Huawei, HiSilicon | FFS | Detailed observation may wait for the output of study in other session. |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.3.3-7a: Can the above observations of the impact on PDCCH blocking probability for UE bandwidth reduction be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Samsung | Y |  |
| Huawei, HiSilion | Y |  |
| Spreadtrum | Y |  |
| LG | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

### Analysis of coexistence with legacy UEs

Many contributions analyze the coexistence impacts if bandwidth reduction is introduced for RedCap UEs. The findings are summarized below. Note that some of the findings reflect different views in different contributions. Further discussions are needed to resolve these conflicting views. In the summary below, if an impact is specific to only FR1 or only FR2, it is denoted accordingly.

**General:**

* C1: (FR1) For FR1, with 20MHz bandwidth capability, Redcap UEs should be able to coexist with the legacy UE [1, 11, 16, 19].
* C2: (FR2) For FR2, with 100MHz bandwidth capability, there is no coexistence impact [1, 11, 16].
* C3: There may or may not be impacts on the coexistence with legacy UEs, depending on the cell load and the solutions for RedCap and normal UEs camped on the same cell [4].

**Initial access and initial BWP:**

* C4: There may be issues with frequency-division multiplexed RACH Occasions [24].
* C5: (FR1) For initial access in FR1, the RedCap UEs can share SSB, SIB1, other Sis, RAR and Msg4 configured for normal NR UEs [5].
* C6: (FR2) The RedCap UEs with 100 MHz maximum UE bandwidth can share SSB, SIB1, other Sis, RAR and Msg4 configured for normal NR UEs [5].
* C7: (FR2) Compared with maximum UE bandwidth of 100 MHz, to support the RedCap UEs with 50 MHz maximum UE bandwidth, more serious configuration or scheduling restrictions to normal NR UEs would be expected. It may reduce the configuration or scheduling flexibility of legacy NR UEs [5].
* C8: Separate SIB1 for RedCap devices can be configured to solve coexistence problems [9].
* C9: (FR2) Limiting the supported SCS combinations for SSB/CORESET0 may be considered [9].
* C10: (FR2) There may be issues, such as backward compatibility or configuration restriction, with SSB and CORESET0 for supporting RedCap UE with 50MHz bandwidth [2, 4, 8, 15, 17, 23, 24].
  + Two initial access procedures will have to coexist: one for ‘regular’ UEs, one for RedCap UEs [2].
* C11: (FR2) With 50MHz UE BW, there may be misalignment between Redcap UE’s receiving bandwidth and the scheduling bandwidth of PDSCH for common channel during initial access procedure [16].
* C12: Supporting RedCap UEs may result in a high load in the initial BWP [24].
* C13: RedCap UEs may not support the bandwidth of the initial UL BWP configured for normal UEs in SIB1 depending on Rel-15 cell configuration [1, 5, 8, 9, 10].
  + This impacts Msg3 [1, 5] and PUCCH for Msg4 [1].
  + A separate UL BWP for RedCap devices can be configured to solve coexistence problems [9].
* C14: For both IDLE/INACTIVE and RRC-CONNECTED modes, if RedCap UEs are offloaded to a different BWP than initial BWP, it is beneficial from UE implementation perspective to have SSB transmitted in the operating BWP for RedCap UEs [4].

**Other aspects:**

* C15: Paging capacity may be an issue [24].
* C16: (FR2) In Idle mode, if the maximum UE bandwidth of RedCap UEs is 50 MHz, paging configuration for normal NR UEs may need to be restricted if the RedCap UEs and normal NR UEs share the same paging resources [5].
* C17: PDCCH blocking probability will increase with bandwidth reduction [15].
* C18: A reduced bandwidth Redcap UE is unable to measure the PRS across a wide bandwidth [19].
* C19: Legacy UE performance might be impacted if RedCap UEs accessing the cell with full backward compatibility [17].
* C20: RedCap UEs performance might not be guaranteed if accessing the cell with full backward compatibility. [17].

**Phase 3: Question 7.3.4-1: Can the above list (C1-C20) be used as a baseline for the TP drafting for TR section 7.3.4?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
|  |  |  |
|  |  |  |
|  |  |  |

### Analysis of specification impacts

Many contributions analyze the specification impacts if bandwidth reduction is introduced for RedCap UEs. The findings are summarized below. Note that some of the findings reflect different views in different contributions. Further discussions are needed to resolve these conflicting views. In the summary below, if an impact is specific to only FR1 or only FR2, it is denoted accordingly.

**General:**

* S1: (FR1) The specification impact is expected to be small in FR1 [11, 13, 21, 27],
* S2: (FR2) RAN1 specification impact is expected to be small for UE with 100 MHz bandwidth in FR2 [11].

**Initial access and initial BWP:**

* S3: (FR1) Rel-15 SSB and/or CORESET0 should be reused [12, 20].
* S4: (FR1) No spec impacts related to cell search, system information acquisition, RAR and Msg4 reception are expected for RedCap UEs [5].
* S5: (FR2) No spec impacts related to cell search, system information acquisition, RAR and Msg4 reception are expected for RedCap UEs with 100 MHz maximum UE bandwidth [5].
* S6: Support dedicated initial BWP or dedicated initial access procedure for RedCap [5, 7, 10, 12, 15, 16, 17, 24].
* S7: There is no need to define a dedicated initial BWP for RedCap UEs [1].
* S8: There are solutions that can be used to support RedCap UEs camping on a cell with initial DL or UL BWP bandwidth larger than the maximum UE bandwidth [1].
* S9: It is feasible to allow a RedCap UE to camp on a cell even when the initial DL or UL BWP configured in the cell is larger than the maximum UE bandwidth [1].
* S10: Support RF retuning for frequency-division multiplexed RACH Occasions or SSB/CORESET0 [1, 10, 24, 25].
* S11: During initial access procedure, if size of initial UL BWP configured for normal NR UEs is larger than the bandwidth of the RedCap UEs, Msg3 transmission of the RedCap UE can be flexibly scheduled and Msg3 hopping can be enabled if dedicated initial UL BWP is configured for the RedCap UEs [5].
* S12: For frequency-hopping Msg4 PUCCH or Msg3 PUSCH transmissions, the UE needs to frequency hop within the initial UL BWP, which may have a bandwidth larger than the maximum RedCap UE bandwidth [1].
* S13: Support configuring separated CD-SSB for RedCap UEs [17].

**Specification impact if dedicated initial BWP, dedicated initial access procedure, or dedicated BWP is introduced:**

* S14: Support initial BWP enhancement including at least one of following: multiple initial BWPs, enhancement on CORESET0, or narrow band Redcap UEs operate in a wide band system [15].
* S15: Using a separate DL BWP for SIB transmissions towards RedCap UEs [10].
* S16: Using a separate UL BWP for initial access of RedCap UEs (as well as common UL BWP shared with normal UEs) [10].
* S17: Initial BWP with non-CD SSB transmission dedicated for RedCap UEs [4].
* S18: Support dedicated BWP for RedCap [5, 7, 24].
* S19: UE switching to the dedicated BWP immediately after random access procedure may be considered to offload UEs from initial BWP [7, 26].
* S20: Mechanism for RedCap BWP switching (e.g., for switching UE from initial BWP to the dedicated BWP quickly or for other performance optimization considerations) [7, 26].
* S21: Introduce longer CORESET duration (Should be discussed in AI 8.6.3) [12, 24].
* S22: Introduce simplified BWP operation for RedCap [16].
* S23: Decouple the DL and UL BWP design for RedCap UE [16].
  + Support small DL bandwidth and large UL bandwidth.
  + Support fewer DL BWP configurations than that of UL.
* S24: Support SRS transmission or CSI report for inactive BWP(s) [15].

**System information:**

* S25: A new set of system information may be needed to indicate whether the cell supports RedCap UEs and to provide RRC configuration information [1].
* S26: System information that is needed for supporting RedCap UEs may be added as new information elements to existing SI blocks or as new SI blocks [1].
* S27: Support configuring separated resources for RedCap UEs in legacy SIB1 for RACH and paging [17].

**Paging:**

* S28: In Idle mode, dedicated paging occasions are considered for the RedCap UEs [5, 24].
* S29: The legacy paging procedure will work fine for RedCap UEs with 20 MHz bandwidth in FR1 and 50 MHz or 100 MHz bandwidth in FR2 [1].

**UE identification and capability signaling:**

* S30: Earlier identification of the RedCap UEs should be considered [5, 21].
  + S1: Identification of the RedCap UE before Msg3 transmission is needed if size of initial UL BWP configured for normal NR UEs is larger than the bandwidth of the RedCap UEs [5].
  + S1: The type of RedCap UE needs to be identified before RAR/Msg4 transmission [5].
* S31: Capability signaling defining that the UE supports a reduced bandwidth [4, 19, 21].

**RAN4:**

* S32: Most RF core requirements can be reused for supporting RedCap UE bandwidth reduction. However, certain modifications may be considered to reflect that the UE may not measure on the SSB at all times, if scheduled in other parts of the carrier [1].
* S33: There may be some minor performance impacts that need to be considered in RAN4 [19].

**Other aspects:**

* S34: In RRC\_CONNECTED, the RedCap UE can be scheduled within the maximum reception bandwidth even though the initial DL BWP configured for normal NR UEs is larger than the maximum UE bandwidth of RedCap UEs [5].
* S35: UE behavior, such as not expecting resource allocations exceeding the number of PRBs corresponding to BW limitation [2].
* S36: Support for RedCap UEs to be able to perform processing of the wider bandwidth PRS over a longer time period [19].
* S37: Study the maximum number BWPs for RedCap UEs [7].

**Additional specification impacts due to supporting 50 MHz UE in FR2:**

* S38: If the maximum UE bandwidth of RedCap UEs is 50 MHz, to guarantee the performance of RedCap UEs, dedicated common CORESET may need to be configured for system information acquisition, RAR and Msg4 reception [5].
* S39: Specification impact for reading system information [3]
* S40: Define a separate CORESET0 for RedCap UEs [27].
* S41: To allow the 240 kHz SCS SSB configuration to be used UEs with 50 MHz maximum bandwidth, the minimum guardband for SSB reception needs to be specified [1].
* S42: UE performance requirements may have to be defined for both SSB and CORESET0 in case of 50 MHz UE [11].
* S43: Enhancements are needed to compensate for potential PDCCH coverage reduction if FR2 50MHz maximum UE bandwidth is supported for initial access [9].
* S44: Reducing the UE RF bandwidth to 50MHz in FR2 may have significant specification for SSB/CORESET0 configurations using 240 kHz SCS [11, 21].
  + Potential solutions needed to address this issue require specification work
    - S45: Cell barring for the RedCap UEs. For example, the above-mentioned bandwidth is larger than the supportable maximum bandwidth of the RedCap UEs [21].
    - S46: Allowing to omit reception of channel/signal outside of its supportable maximum bandwidth, and so on [21].
    - S47: Additional or separate DL BWPs for RedCap UEs at least for some, if not all, common control [8].
    - S48: Some limitations or modifications may also need to be captured for FR2 50MHz e.g for multiplexing or retuning [2].

**Phase 4: Question 7.3.5-1: Can the above list (S1-S48) be used as a baseline for the TP drafting for TR section 7.3.5?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
|  |  |  |
|  |  |  |
|  |  |  |

## 7.4 Half-duplex FDD operation

### 7.4.1 Description of feature

RAN1#103e agreement:

* Adopt the TP in [R1-2009393](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009393.zip) as baseline text for TR clause 7.4.1.

### 7.4.2 Analysis of UE complexity reduction

The tables with device cost evaluation results in this contribution are based on [RedCapCost-v048-FL-Samsung2.xlsx](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Inbox/drafts/8.6/EvaluationResults/RedCapCost/RedCapCost-v048-FL-Samsung2.xlsx). They will eventually be updated with new results from the email discussion [103-e-NR-RedCap-EvaluationResults].

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| The estimated cost for an HD-FDD only device, relative to the reference NR device (see evaluation methodology described in clause 6.1) and averaged over the results provided by the sourcing companies, is summarized in Table 7.4.2-1.  For Type A HD-FDD, a high proportion of the cost saving occurs because the duplexer can be replaced with a switch and a lowpass filter.  For Type B HD-FDD, uplink and downlink can share one local oscillator, therefore, some additional saving on RF transceiver can be obtained.  By comparing Table 7.4.2-1 with the reference NR device cost breakdown in clause 6.1, it can be observed that the main contributor of the cost reduction is the duplexer/switch block. Depending on the implementation, as indicated by some sourcing companies, removing the duplexer may also reduce the insertion loss in both the Rx and Tx chains and as a result, the PA power can be reduced, and the LNA sensitivity requirement can be relaxed which allows for potential UE complexity reduction.  As can be seen in the last row for the total cost, the average estimated cost reduction achieved by Type A and Type B HD-FDD is approximately ~7% and ~10%, respectively.  Furthermore, all sourcing companies indicated that the RF cost savings (but not the baseband cost savings) accumulate across supported bands.  **Table 7.4.2-1: Estimated relative device cost for an HD-FDD device**   |  |  |  | | --- | --- | --- | | **Half-duplex FDD operation** | **HD-FDD operation (Type A)** | **HD-FDD operation (Type B)** | | RF: Antenna array | - | - | | RF: Power amplifier | 24.1% | 23.9% | | RF: Filters | 10.6% | 10.7% | | RF: Transceiver (including LNAs, mixer, and local oscillator) | 44.4% | 37.8% | | RF: Duplexer / Switch | 4.8% | 4.9% | | **RF: Total relative cost** | **83.9%** | **77.3%** | | BB: ADC / DAC | 10.0% | 10.0% | | BB: FFT/IFFT | 3.8% | 3.7% | | BB: Post-FFT data buffering | 9.9% | 9.9% | | BB: Receiver processing block | 24.0% | 24.0% | | BB: LDPC decoding | 10.0% | 10.0% | | BB: HARQ buffer | 14.0% | 14.0% | | BB: DL control processing & decoder | 4.8% | 4.8% | | BB: Synchronization / cell search block | 9.0% | 9.0% | | BB: UL processing block | 4.8% | 4.8% | | BB: MIMO specific processing blocks | 9.0% | 9.0% | | **BB: Total relative cost** | **99.4%** | **99.2%** | | **RF+BB: Total relative cost** | **93.2%** | **90.4%** | |

One response in FLS4 ([R1-2009394](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009394.zip)) requested more discussion about the assumtions behind the cost estimates before the results are agreed to be captured in the TR.

**Phase 1: Proposal 7.4.2-1d: Adopt the TP above as baseline text for TR clause 7.4.2.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Nokia, NSB | Y |  |
| SONY | Y | Our analysis on the complexity reduction from HD-FDD is unchanged from the previous version of this document. Removing the duplexer leads to a significant decrease in the cost of the duplexer and any cost increase in the filter that goes into the “duplex / switch” is not significant. Our analysis seems to be consistent with that of TR36.888.  Our preference would be that companies would note a lower PA cost due to the lower insertion loss. However, we understand that other companies do not see that benefit. We are OK with other companies having a different view to us on this. We think there is no additional filtering cost that needs including from removing the duplexer and we hope that other companies are similarly OK with our view on this. |
| FUTUREWEI | Y | OK as baseline, can be updated as needed |
| DOCOMO | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | Y |  |
| Spreadtrum | Y |  |
| LG | Y |  |
| Huawei, HiSilicon | Y with minor | Modifications as “The estimated cost for an HD-FDD only device,” since the cost is not reduced when the UE is also support FD-FDD. |
| FL | The TP above has been updated based on the received responses.  **FL1: Phase 1: Proposal 7.4.2-1e: Adopt the TP above as baseline text for TR clause 7.4.2.** | |
| FUTUREWEI2 | Y |  |
| MediaTek | Y |  |
| Ericsson | Y |  |
| Qualcomm | Y |  |
| Intel | Y |  |
| Nokia, NSB | Y |  |
| DOCOMO | Y |  |
| LG | Y |  |
| CATT | Y |  |
| SONY6 | Y |  |
| CMCC | Y |  |
| ZTE | Y |  |
| OPPO | Y |  |
| Samsung | Y |  |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | Y |  |

**Device size:**

In addition to reduction in cost/complexity benefits, contribution [18] points out that HD-FDD is expected to reduce device size. Note that the following agreement was reached in RAN1#101e:

|  |
| --- |
| Agreements:   * […] * Potential benefits in terms of reduced device size can be mentioned where applicable in the TR (e.g. in the section on reduced number of antennas), but the SI will not aim to quantify such benefits. |

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| It is unclear whether the HD-FDD operation may be beneficial in terms of reducing the device size in FR1 FDD. |

**Phase 2: Proposal 7.4.2-2: Adopt the above description of the benefit of HD-FDD operation in terms of reducing the device size in FR1 FDD as a baseline text for TR 38.875.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y | Although we think that there could potentially be a small size decrease, we are OK with the [somewhat ambiguous] text that is proposed. |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson |  | No strong view |
| Intel | Y |  |
| OPPO | Y |  |
| Xiaomi | Y |  |
| CATT | Y |  |
| LG | Y |  |
| Huawei, HiSilicon | Y |  |
| FL | **FL1: Phase 2: Proposal 7.4.2-2: Adopt the above description of the benefit of HD-FDD operation in terms of reducing the device size in FR1 FDD as a baseline text for TR 38.875.** | |
| MediaTek |  | No objection, although in our view sparing the duplexers helps in reducing the device size. |
| Ericsson | Y |  |
| Qualcomm | Y | We can live with this proposal for the sake of progress. |
| Intel | Y |  |
| Nokia, NSB | Y |  |
| DOCOMO | Y |  |
| LG | Y |  |
| CATT | Y |  |
| SONY6 |  | Agree with Mediatek view |
| ZTE | Y |  |
| OPPO | Y |  |
| Samsung | Y |  |
| Sequans | Y |  |
| Huawei, HiSilicon | Y |  |

### 7.4.3 Analysis of performance impacts

According to the SID [36],

|  |
| --- |
| The study includes evaluations of the impact to coverage, network capacity and spectral efficiency |

In addition, RAN1#101e made the following agreement:

|  |
| --- |
| Agreements:   * The evaluation of performance impacts includes at least peak data rate, latency and reliability (as needed for the use cases). Other performance metrics such as power consumption, spectral efficiency and PDCCH blocking probability may also be considered if appropriate for a specific technique. |

**Coverage:**

* P6: HD-FDD will not result in coverage loss and the coverage of HD-FDD UEs is expected to be at least as good as that of FD-FDD UEs [1, 4, 10, 11, 13, 15, 19, 22, 26].
* P7: HD-FDD will result in coverage loss if the same data rate needs to be maintained [3, 6].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Coverage:**  If there are no stringent requirements on latency and data rate, then HD-FDD will not result in coverage loss, otherwise a coverage loss can be expected. |

**Phase 2: Question 7.4.3-2: Can the above observations of the impact on coverage for HD-FDD operation be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo |  | We are not sure if the last sentence is true respective to better coverage for HD-FDD UE compared to FD-FDD UE. |
| SONY5 | Y | Editorial: and the coverage for HD-FDD UEs is expected to be similar ~~as~~ to that for FD-FDD UEs,  We have some sympathy with the view from vivo. The coverage is related to the radiated power, which is set by the power class. The insertion loss affects how much battery power is required to produce that amount of radiated power. The lower insertion loss is a good thing, whether it directly impacts coverage is unclear. |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung |  | Suggest to simplify as:  If there are no stringent requirements on latency and data rate, then HD-FDD will not result in coverage loss~~, otherwise a coverage loss can be expected. No RedCap use case requires both low latency and~~ high data rate, so no coverage loss is expected for the RedCap use cases, and the coverage for HD-FDD UEs is expected to be similar as for FD-FDD UEs, or possibly even slightly better due to lower insertion loss. |
| Ericsson | Y |  |
| Intel | Y |  |
| CATT | Y, partially | Suggest following change: ‘If ~~N~~no RedCap use case requires both low latency and high data rate, ~~so~~ no coverage loss is expected for the RedCap use cases, and the coverage…’ RedCap UE may be deployed as real time video monitoring device. It is possible to have demand on both low latency and high data rate. |
| LG | Y |  |
| Huawei, HiSilicon | N | If there are no stringent requirements on latency and data rate, then HD-FDD will not result in coverage loss, otherwise a coverage loss can be expected. The potential coverage loss highly depends on UL and DL ratio subject to gNB scheduling and the Tx-Rx switching time, HARQ re-transmission times for a given data rate and latency/reliability requirements. It is in general understood that HD-FDD has worse coverage than FD-HDD while the potential lower insertion loss may slightly compensate the coverage loss, depending on the implementations. ~~No RedCap use case requires both low latency and high data rate, so no coverage loss is expected for the RedCap use cases, and the coverage for HD-FDD UEs is expected to be similar as for FD-FDD UEs, or possibly even slightly better due to lower insertion loss.~~ |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.4.3-2a: Can the above observations of the impact on coverage for HD-FDD operation be used as a baseline text for TR 38.875?** | |
| CATT | Y | Fine to keep it simple. |
| Qualcomm | Y | We can live with it for the sake of progress |
| ZTE | Y |  |
| Samsung | Y |  |
| Huawei, HiSilion | Y |  |
| Spreadtrum | Y |  |
| LG | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Network capacity and spectral efficiency:**

* P17: HD-FDD results in lower spectral efficiency [4, 24].
* P18: HD-FDD has minor or no impact on spectral efficiency and capacity [1, 11, 13, 15, 19].
* P19: The lower noise figure of an HD-FDD UE leads to a moderate improvement in cell spectral efficiency and capacity [19].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Network capacity and spectral efficiency:**  HD-FDD operation has minor impact on spectral efficiency and capacity. |

**Phase 2: Question 7.4.3-3: Can the above observations of the impact on network capacity and spectral efficiency for HD-FDD operation be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo |  | We are not sure the 2nd bullet is true, since HD-FDD will restrict the network secheduling flexibility so the spectral efficienc is not expected to increase? |
| SONY5 | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | Y |  |
| CATT | Y, partially | Similar concern as vivo. |
| LG | Y |  |
| Huawei, HiSilicon | N | Same view as vivo.  HD-FDD operation is expected to have negative ~~has minor~~ impact on spectral efficiency and capacity. ~~Depending on the implementation, the potentially lower noise figure of an HD-FDD UE may lead to a moderate improvement in cell spectral efficiency and capacity.~~ |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.4.3-3a: Can the above observations of the impact on network capacity and spectral efficiency for HD-FDD operation be used as a baseline text for TR 38.875?** | |
| CATT | Y | Fine to keep it simple. |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Samsung | Y |  |
| Huawei, HiSilion | Y |  |
| Spreadtrum | Y |  |
| LG | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Data rate:**

* P1: HD-FDD reduces data rate compared to FD-FDD [2, 3, 4, 6, 19, 24].
* P2: HD-FDD Redcap UEs can fulfil all the RedCap data rate requirements [1, 5, 22].
* P3: Type A HD-FDD has minor data rate and latency degradation [18].
* P4: Type B HD-FDD has a significant impact on the throughput and/or latency performance [6, 18].
* P5: It might be problematic for HD-FDD UEs to fulfill the data rate requirements of high-end wearables (e.g. 50/150 Mbps peak bitrate in UL/DL) without relying on high modulation order, MIMO and/or carrier aggregation capability [28].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Data rate:**  HD-FDD reduces user throughput compared to FD-FDD, especially in case of simultaneous downlink and uplink traffic. |

**Phase 2: Question 7.4.3-4: Can the above observations of the impact on data rate for HD-FDD operation be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo |  | HD-FDD reduces data rate compared to FD-FDD, but the peak data rate requirements of some RedCap use cases can still be fulfilled. |
| SONY5 | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y | Perhaps it can be clarified in the text that the statement concerns the individual technique, not combinations with other techniques. |
| Intel | Y |  |
| CATT | Y, partially | Better to add ‘most of’ or ‘some’ before the ‘RedCap use cases’. If the use case requires both DL and UL data rate at the same time (e.g. real time video interaction), it is possible that the data rate requirement can not be fulfilled. |
| LG | Y | Also fine with the clarification from vivo, and Ericsson. |
| Huawei, HiSilicon | N | We are not sure about the observation. It will depend on the UL:DL ratio and the peak data rate may only be satisfied in either DL or UL but not both. |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.4.3-4a: Can the above observations of the impact on data rate for HD-FDD operation be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y | But we prefer the original TP. |
| Samsung |  | We suggest to add the following if changing data rate to User throughput.  There is minor impact on instant data rate for uplink or downlink. |
| Huawei, HiSilion | Y but | Is it user throughput or data rate? |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Latency and reliability:**

* P8: HD-FDD introduces longer latency than FD-HDD [3, 6, 19, 24, 28].
* P9: An HD-FDD UE in RRC\_CONNECTED can meet the 5-10 ms latency requirement for safety related sensors [1, 4].
* P10: HD-FDD has less impact on latency compared to TDD [19].
* P11: The latency requirement can be met if NR dynamic TDD is reused for HD-FDD [5].
* P12 The safety sensor use case has strict latency requirements of 5-10 ms which seems difficult for an HD-FDD device to meet [28].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Latency and reliability:**  HD-FDD introduces longer latency than FD-HDD, especially in case of simultaneous downlink and uplink traffic, but the latency and reliability requirements of RedCap use cases can still be fulfilled at least for one direction (i.e., either downlink or uplink). |

**Phase 2: Question 7.4.3-5: Can the above observations of the impact on latency and reliability for HD-FDD operation be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo |  | HD-FDD introduces longer latency than FD-HDD, but the latency and reliability requirements of most of RedCap use cases can still be fulfilled. |
| SONY5 | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | Y |  |
| OPPO |  | Share similar view with vivo |
| CATT | Y, partially | Similar to vivo. Better to add ‘most of’ or ‘some’ before the ‘RedCap use cases’. |
| LG | Y | Also fine with the modification from vivo. |
| Huawei, HiSilicon | N | HD-FDD introduces longer latency than FD-HDD, but the latency and reliability requirements of RedCap use cases can still be fulfilled at least in one way (i.e. either UL or DL) depending on gNB scheduling and Rx-Tx swictching time capability, HARQ retransmission times. |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.4.3-5a: Can the above observations of the impact on latency and reliability for HD-FDD operation be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y | But we prefer the original TP. |
| Samsung | Y |  |
| Huawei, HiSilion | Y |  |
| LG | N | Not sure if we need to separate DL and UL latency and also not sure if there are separate requirements for DL and UL. We would like to keep it simple as follows:  HD-FDD introduces longer latency than FD-HDD, especially in case of simultaneous downlink and uplink traffic, but the latency and reliability requirements of RedCap use cases can still be fulfilled for most of the RedCap use cases. |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y | OK, but prefer original TP. |

**Power consumption:**

* P13: The lower insertion loss of an HD-FDD UE leads to a higher power efficiency in the transmit chain and improved power consumption when transmitting [1, 11, 19, 23].
* P14: HD-FDD has lower power consumption compared to FD-FDD [4, 10, 19, 24, 26].
  + HD-FDD has a negative impact on UE power consumption because the UE will be “on” for a longer time before being able to return to a lower power light sleep / deep sleep state. This loss is expected to be less than the gain from the lower insertion loss [19].
* P15: Compared to the reference NR modem, half duplex operation means some components can work in a reduced power state until required [13].
* P16: The impact on power consumption of HD-FDD depends on implementation [5].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Power consumption:**  The lower insertion loss of an HD-FDD UE may enable a higher power efficiency in the transmit chain and reduce power consumption. Furthermore, compared to the reference NR modem, half-duplex operation means some components can work in a reduced power state until required. However, on the other hand, HD-FDD may have a negative impact on UE average power consumption because the UE will be active for a longer time before being able to return to a lower power light sleep or deep sleep state. The impact on power consumption of HD-FDD depends on implementation and traffic characteristics. |

**Phase 2: Question 7.4.3-6: Can the above observations of the impact on power consumption for HD-FDD operation be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Ericsson | Y |  |
| Intel | Y |  |
| OPPO | Y |  |
| CATT | Y |  |
| LG | Y |  |
| Huawei, HiSilicon | Y |  |
| FL | **FL2: Phase 2: Question 7.4.3-6: Can the above observations of the impact on power consumption for HD-FDD operation be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Huawei, HiSilion | Y |  |
| Spreadtrum | Y |  |
| LG | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**PDCCH blocking probability:**

* P20: HD-FDD reduces available PDCCH monitoring occasion [6].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **PDCCH blocking probability:**  HD-FDD operation may potentially reduce the available PDCCH monitoring occasions when the UE is transmitting rather than receiving. |

**Phase 2: Question 7.4.3-7: Can the above observations of the impact on PDCCH blocking probability for HD-FDD operation be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | N |  |
| Vivo | Y |  |
| SONY5 | N | We don’t have a strongly negative view here. Our understanding is that PDCCH blocking is about blocking within a PDCCH monitoring occasion and not about blocking between monitoring occasions. |
| FUTUREWEI | Y |  |
| Qualcomm | N | We don’t think there is an impact on PDCCH blocking probability because:  • The DL/UL resources are configured by gNB.  • The PDCCH is also scheduled by gNB. |
| DOCOMO | Y |  |
| Sierra Wireless | N |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | N | Agree with Qualcomm and, in addition, for type A, we expect that the switching times can be accommodated to not impact PDCCH monitoring opportunities. |
| OPPO | Y |  |
| CATT | Y | PDCCH blocking probability can be increased due to larger number of UEs within the same PDCCH monitoring occasions, due to less available DL slots in general. Since ‘may’ and ‘potentially’ are included, we think the observation is fine. |
| Huawei, HiSilicon | Y | We think it is proper. Although it is configured/scheduled by gNB, the CORESET configurations for FD-FDD and HD-FDD UEs will naturally be different given the Rx-Tx gap and lack of capability of simulatenous UL and DL for HD-FDD. |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.4.3-7a: Can the above observations of the impact on PDCCH blocking probability for HD-FDD operation be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| ZTE | Y |  |
| Samsung | Y |  |
| Huawei, HiSilion | Y |  |
| FUTUREWEI3 | Y | Can accept, but it says blocking potentially may be increased which is true. If potentially not good enough, perhaps a ‘may or may not’. |
| Ericsson | Y |  |
| SONY7 | Y |  |

### 7.4.4 Analysis of coexistence with legacy UEs

Many contributions analyze the coexistence impacts if HD-FDD operation is introduced for RedCap UEs. The findings are summarized below. Note that some of the findings reflect different views in different contributions. Further discussions are needed to resolve these conflicting views.

* C1: Introducing HD-FDD operation will make gNB scheduling more complicated [2, 10, 24].
* C2: HD-FDD may introduce scheduling constraints to URLLC services and may introduce issues with pre-emption indicator monitoring [3, 19, 28].
* C3: Introducing HD-FDD operation has no impact on initial access procedure as it is not likely to require simultaneous uplink and downlink transmission in legacy implementations during initial access [1, 11, 19].
* C4: Potential impact on RACH procedure to support Type B HD-FDD UE can be expected, e.g., switching time from PRACH to Msg2 for Type B HD-FDD [15, 24].
* C5: Introducing the support of Type-A HD-FDD operation will not introduce any coexistence issues with legacy UEs [1, 5].
* C6: Introducing the support of Type B HD-FDD operation may require longer time gaps between subsequent messages in the random-access procedure and may therefore introduce longer delay in the random-access procedure for legacy UEs [1].
* C7: Introducing Type B HD-FDD operation has a significant impact on the gNB scheduler [1].
* C8: HD-FDD introduces limitation on the configuration of some common RS/channels for both legacy and RedCap UEs [3].
* C9: Scheduling effectiveness is not compromised by supporting Type-A HD-FDD UE’s in paired spectrum, since each UE could switch between DL and UL at independent points in time, according to their respective scheduled or configured uplink transmissions [23].
* C10: With Type A HD FDD, only the duplexer is dropped, and the same (full-duplex) UE modem can be reused in full-duplex and half-duplex FDD UE designs, thus avoiding UE modem market fragmentation [23].

This potential impact has been moved here from Section 7.4.3 of this document where it was known as P21:

* C11: BWP adaptation may have an impact on HD-FDD operation. [7].

**Phase 3: Question 7.4.4-1: Can the above list (C1-C11) be used as a baseline for the TP drafting for TR section 7.4.4?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Samsung |  | Support: C3, combined C4 and C6 , C5  FFS for C1  Don’t support: C1, C2, C7, C8, C9, C10 (not belong to this AI, and don’t agree with the statement) |
| Qualcomm |  | We support C3, C4, C5, C6, C7, C9, C10. |
|  |  |  |

### 7.4.5 Analysis of specification impacts

Many contributions analyze the specification impacts if HD-FDD operation is introduced for RedCap UEs. The findings are summarized below. Note that some of the findings reflect different views in different contributions. Further discussions are needed to resolve these conflicting views.

* S1: RAN1 specification impact is expected to be minor [11, 17].
* S2: RAN1 specification impact is expected to be small for supporting Type A HD-FDD [1, 21].
* S3: Introducing Type B HD-FDD operation would have much more specification impacts than Type A [1].
* S4: Need to specify DL-to-UL and UL-to-DL switching time [1, 3, 4, 5, 6, 8, 12, 13, 19, 21, 22, 24].
* S5: RAN4 should decide on switching time requirements during the work item phase [19].
* S6: Need to specify HD-FDD capability signaling [1, 4, 5, 19, 21].
* S7: Need to specify how to handle DL/UL collision [1, 4, 8, 24].
* S8: For Type A HD-FDD, the guard period for DL-to-UL and UL-to-DL switching may be relaxed compared to the minimum Rx-to-Tx and Tx-to-Rx switching times defined in Rel-15 for a UE not supporting full-duplex communication [8].
* S9: The DL-to-UL and UL-to-DL switching time for a Type A HD-FDD device can reuse the same values of and specified in Table 4.3.2-3 of TS 38.211 [1].
* S10: The values of and specified in Table 4.3.2-3 of TS 38.211 cannot be used as DL-to-UL and UL-to-DL switching time for a Type B HD-FDD device [1].
* S11: Need to define applicable bands and performance requirements for HD-FDD operation [4].
* S12: RAN4 specification changes such as new reference sensitivity, RRM, and performance requirements can be expected, due to the lack of a duplexer, thus less insertion loss [1].
* S13: Thanks to the flexibility in the TDRA and HARQ timing in NR, there is less motivation to adopt features such as increasing the number of HARQ processes, multi-TB scheduling, and HARQ-ACK bundling, if Type A HD-FDD is introduced for RedCap [1].
* S14: If for unforeseeable reasons, features such as increasing the number of HARQ processes, multi-TB scheduling, and HARQ-ACK bundling, need to be introduced for enhancing the throughput for an HD-FDD UE, the specification impacts will be very significant [1].
* S15: Need to specify how DL pre-emption and UL cancellation work when HD-FDD UEs share resources with URLLC UEs [19].
* S16: Need to specify how to prioritize between eMBB traffic and URLLC traffic for the cases of (1) eMBB DL and URLLC UL and (2) eMBB UL and URLLC DL [19].
* S17: The gNB should be able to configure DL or UL durations for HD-FDD UE [12].
* S18: Type A HD-FDD operation will not impact BWP switch delay requirements [1].
* S19: Type B HD-FDD operation will require defining new BWP switch delay requirements [1].
* S20: RedCap UEs in HD-FDD mode should support BWP switching for power saving [7].

**Phase 4: Question 7.4.5-1: Can the above list (S1-S20) be used as a baseline for the TP drafting for TR section 7.4.5?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
|  |  |  |
|  |  |  |
|  |  |  |

## 7.5 Relaxed UE processing time

### 7.5.1 Description of feature

Based on earlier RAN1 agreements [37], the following text proposal for the TR can be considered.

|  |
| --- |
| In the RedCap study item, relaxed UE processing time is considered in terms of more relaxed N1/N2 values compared to those of UE processing time capability 1.  In the study, for the purpose of evaluation, the relaxed UE processing time in terms of N1/N2 are assumed to be doubled compared to those of capability 1, i.e.,   * N1 = 16, 20, 34, and 40 symbols for 15, 30, 60, and 120 kHz SCS (assuming only front-loaded DMRS) * N2 = 20, 24, 46, and 72 symbols for 15, 30, 60, and 120 kHz SCS |

In FLS4, different views were expressed regarding the two last sentence in the first paragraph in the TP for TR clause 7.5.1. Perhaps one possible compromise is to keep the first of these two sentences and remove the last one.

**Phase 1: Proposal 7.5.1-2a: Adopt the TP above as baseline text for TR clause 7.5.1.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | Y | We can live with this. The important thing to discuss is the individual discussion points that may lead to different observations/conclusions. |
| CATT | Y |  |
| CMCC | Y |  |
| LG | Y |  |
| ZTE | Y |  |
| vivo | Y |  |
| Nokia, NSB | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung |  | Move the following sentence to 7.5.2  *Relaxed UE processing time in terms of N1/N2 potentially reduces UE complexity by allowing a longer time for the processing of PDCCH and PDSCH and preparing PUSCH and PUCCH*. |
| Ericsson | Y |  |
| Intel | Y |  |
| Spreadtrum | Y |  |
| OPPO | Y |  |
| FL | Based on received responses, a sentence has been moved from the 7.5.1 TP to the 7.5.2 TP.  **FL1: Phase 1: Proposal 7.5.1-2b: Adopt the TP above as baseline text for TR clause 7.5.1.** | |
| FUTUREWEI2 | Y |  |
| MediaTek | Y |  |
| Ericsson | Y |  |
| Qualcomm | Y |  |
| Intel | Y |  |
| Nokia, NSB | Y |  |
| DOCOMO | Y |  |
| LG | Y |  |
| CATT | Y |  |
| SONY6 | Y |  |
| CMCC | Y |  |
| ZTE | Y |  |
| Samsung | Y |  |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | Y |  |

According to guidance from the RAN1 chairman communicated in the RedCap GTW session on Tuesday 3rd November (UTC), if some companies have studied relaxed CSI computation time, this can be reflected in the TR.

**Phase 1: Question 7.5.1-3: What should be captured in the TR regarding relaxed CSI computation?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Comments** | |
| Huawei, HiSilicon | It can briefly describe what is being assumed for the presented results, as well as the results, similar to the handling of other techniques. Recommandation should be a separate discussion. One example for consideration:  “In the study, for the purpose of evaluation, there are also results for CSI computation time relaxation as below, assuming doubled Z/Z' compared to the values defined in section 5.4 TS 38.214.  [Xxx, the sourcing results]  ” | |
| SONY5 | It’s not clear how we would capture relaxed CSI computation in the TR. If it is were captured in section 7.5, then it would some that there would need to be short mentions of relaxed CSI computation in each of sections 7.5.1 -> 7.5.5. Another option would be to have a section 7.9 on “other technqiues” where short descriptions of / observations about other techniques could be captured. | |
| FUTUREWEI | Above proposal seems in line with GTW | |
| DOCOMO | Fine with the proposal from Huawei | |
| Ericsson | Huawei’s TP above can be a starting point. | |
| Intel | Support the proposal from Huawei. | |
| FL | Based on received responses, the following TP can be considered.   |  | | --- | | In the study, for the purpose of evaluation, relaxed CSI computation time was also considered, assuming doubled Z/Z' compared to the values defined in TS 38.214 clause 5.4. |   **FL1: Phase 1: Proposal 7.5.1-3: Adopt the TP above as baseline text regarding relaxed CSI computation, either in TR clause 7.5.1 or in a TR (sub)clause on relaxed CSI computation.** | |
| FUTUREWEI2 | Y |  |
| Ericsson | Y | Okay with the TP. Good to keep it short. |
| Qualcomm | Y | We can live with this proposal for the sake of progress. |
| Intel | Y |  |
| DOCOMO | Y |  |
| LG | Y |  |
| CATT | Y |  |
| SONY6 | Y |  |
| CMCC | Y |  |
| ZTE | Y |  |
| Samsung | Y |  |
| Huawei, HiSilicon | Y |  |

### 7.5.2 Analysis of UE complexity reduction

The tables with device cost evaluation results in this contribution are based on [RedCapCost-v048-FL-Samsung2.xlsx](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Inbox/drafts/8.6/EvaluationResults/RedCapCost/RedCapCost-v048-FL-Samsung2.xlsx). They will eventually be updated with new results from the email discussion [103-e-NR-RedCap-EvaluationResults].

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| The estimated cost for a device with relaxed UE processing time (see evaluation methodology described in clause 6.1) and averaged over the results provided by the sourcing companies, is summarized in Table 7.5.2-1. As can be seen in the last row for the total cost, the average estimated cost reduction is ~6% for FR1 FDD, ~6% for FR1 TDD, and ~6% for FR2 TDD.  Relaxed UE processing time in terms of N1/N2 potentially reduces UE complexity by allowing a longer time for the processing of PDCCH and PDSCH and preparing PUSCH and PUCCH. By comparing Table 7.5.2-1 with the reference NR device cost breakdown in clause 6.1, it can be observed that the cost of the following functional blocks can be reduced:   * Baseband: Receiver processing block * Baseband: LDPC decoding * Baseband: DL control processing & decoder * Baseband: UL processing block   Whether the relaxed UE processing time may reduce the cost/complexity in the ‘DL control processing & decoder’ block depends on the UE implementation.  Furthermore, all sourcing companies indicated that these cost savings do not accumulate across supported bands.  **Table 7.5.2-1: Estimated relative device cost for relaxed UE processing time**   |  |  |  |  | | --- | --- | --- | --- | | **Relaxed processing time (doubled N1 and N2)** | **FR1 FDD** | **FR1 TDD** | **FR2 TDD** | | RF: Antenna array | - | - | 33.0% | | RF: Power amplifier | 25.0% | 25.0% | 18.0% | | RF: Filters | 10.0% | 14.7% | 8.0% | | RF: Transceiver (including LNAs, mixer, and local oscillator) | 45.0% | 54.3% | 41.0% | | RF: Duplexer / Switch | 20.0% | 6.0% | 0.0% | | **RF: Total relative cost** | **100.0%** | **100.0%** | **100.0%** | | BB: ADC / DAC | 10.0% | 9.0% | 4.0% | | BB: FFT/IFFT | 4.0% | 4.0% | 4.0% | | BB: Post-FFT data buffering | 10.0% | 10.0% | 11.0% | | BB: Receiver processing block | 20.3% | 24.6% | 19.5% | | BB: LDPC decoding | 6.6% | 5.9% | 5.9% | | BB: HARQ buffer | 14.0% | 12.0% | 11.0% | | BB: DL control processing & decoder | 4.1% | 3.3% | 4.0% | | BB: Synchronization / cell search block | 9.0% | 9.0% | 7.0% | | BB: UL processing block | 3.7% | 3.6% | 5.0% | | BB: MIMO specific processing blocks | 8.8% | 8.8% | 17.5% | | **BB: Total relative cost** | **90.5%** | **90.1%** | **88.9%** | | **RF+BB: Total relative cost** | **94.3%** | **94.1%** | **94.4%** | |

In FLS4, one response in expressed the view that the averaging of cost estimates from different sources should be done by excluding outlier numbers. This aspect is treated in the new Question 6.1-3 in Section 6.1 of this document. The TP for TR clause 7.5.2 above is unchanged compared to the TP in FLS4.

**Phase 1: Proposal 7.5.2-1d:**

* **Adopt the TP above as baseline text for TR clause 7.5.2.**
  + **Companies are invited to double-check their entries in the cost reduction spreadsheet with respect to the above comments (and to catch potential typos).**
  + **The table will be further updated with potential updated cost estimates.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | Y | We can live with the FL handling of ‘DL control processing & decoder’. |
| CATT | Y |  |
| LG | Y |  |
| ZTE | Y |  |
| vivo | Y |  |
| Nokia, NSB | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y | Additional, add the senteces removed in 7.5.1 |
| Ericsson | Y |  |
| Intel | Y |  |
| Spreadtrum | Y |  |
| OPPO | Y |  |
| Xiaomi | Y |  |
| FL | Based on received responses, a sentence has been moved from the 7.5.1 TP to the 7.5.2 TP.  **FL1: Phase 1: Proposal 7.5.2-1e: Adopt the TP above as baseline text for TR clause 7.5.2.** | |
| FUTUREWEI2 | Y |  |
| Ericsson | Y |  |
| Qualcomm | Y |  |
| Intel | Y |  |
| Nokia, NSB | Y |  |
| DOCOMO | Y |  |
| LG | Y |  |
| CATT | Y |  |
| SONY6 | Y |  |
| CMCC | Y |  |
| ZTE | Y |  |
| OPPO | Y |  |
| Samsung | Y |  |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | Y |  |

### 7.5.3 Analysis of performance impacts

According to the SID [36],

|  |
| --- |
| The study includes evaluations of the impact to coverage, network capacity and spectral efficiency |

In addition, RAN1#101e made the following agreement:

|  |
| --- |
| Agreements:   * The evaluation of performance impacts includes at least peak data rate, latency and reliability (as needed for the use cases). Other performance metrics such as power consumption, spectral efficiency and PDCCH blocking probability may also be considered if appropriate for a specific technique. |

**Coverage:**

* P6: Contributions [1, 2, 4, 11, 15, 24] note that no significant coverage impact is expected from a more relaxed UE processing time.

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Coverage:**  No coverage impact is expected from a more relaxed UE processing time. |

**Phase 2: Question 7.5.3-2: Can the above observations of the impact on coverage for UE with relaxed UE processing time be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | Y |  |
| Spreadtrum | Y |  |
| OPPO | Y |  |
| CATT | Y |  |
| LG | Y |  |
| Huawei, HiSilicon | Y with modificatioins | Please remove “significant”. This can be obvious similar to that no coverage loss comparing Cap#1 with Cap#2. |
| Nokia, NSB | Y |  |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.5.3-2a: Can the above observations of the impact on coverage for UE with relaxed UE processing time be used as a baseline text for TR 38.875?** | |
| Ericsson | Y | The ‘Phase 2’ tag was missing in this updated question. We have inserted the missing tag now, but it seems that many companies may have missed the updated question. |
| SONY7 | Y |  |

**Network capacity and spectral efficiency:**

* P7: Contributions [1, 3, 4, 11, 15] note that no impact on spectral efficiency or network capacity is expected since it is up to gNB to schedule other UEs on available resources.

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Network capacity and spectral efficiency:**  Depending on the gNB scheduler implementation, there may be no or minor impact on network capacity or spectral efficiency from a more relaxed UE processing time. |

**Phase 2: Question 7.5.3-3: Can the above observations of the impact on network capacity and spectral efficiency for UE with relaxed UE processing time be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | N | The last part of the sentence should be deleted: “since it is up to gNB to schedule other UEs on available resources.”. Can’t the Redcap UE be scheduled on all available resources anyway? If the UE could not be scheduled on all available resources, then wouldn’t the peak data rate to impacted (following proposal). |
| FUTUREWEI | Y |  |
| Qualcomm | N | Limitation on scheduler will impact (reduce) at least the SE. |
| DOCOMO | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | Y |  |
| OPPO | Y |  |
| CATT | Y | Better to clarify that ‘other UEs’ includes other RedCap UEs and normal UEs. |
| LG | Y | Also okay to remove the last part as suggested by SONY. |
| Huawei, HiSilicon | Y with modifications | Please remove “significant”. Similarly, Cap#1 vs Cap#2 will not have capacity loss.  The last part from “since” is fine but no cocnern to remove, simply as e.g. a Cap#2 UE being configured in Cap#1 mode will not reduce the capacity. |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.5.3-3a: Can the above observations of the impact on network capacity and spectral efficiency for UE with relaxed UE processing time be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| ZTE | Y |  |
| Huawei, HiSilion | Y |  |
| LG | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Data rate:**

* P5: Contributions [1, 2, 15, 24, 26] mention that sustained data rate may be impacted due to longer HARQ RTT because of the relaxed UE processing time.

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Data rate:**  No impact on peak data rate is expected. It is unclear whether the sustained data rate which considers HARQ retransmissions may be impacted due to longer HARQ round-trip time caused by the relaxed UE processing time in terms of N1/N2. |

**Phase 2: Question 7.5.3-4: Can the above observations of the impact on data rate for UE with relaxed UE processing time be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| SONY5 | Partially Y | Presumably, the second sentence assumes that there is no increase in the number of HARQ processes (which is probably a reasonable assumption) |
| FUTUREWEI | Y |  |
| DOCOMO | Y |  |
| Samsung | Y |  |
| Ericsson | Y | Perhaps it can be clarified in the text that the statement concerns the individual technique, not combinations with other techniques. |
| Intel | N | We do not think that, with 16 HARQ processes, there will be an adverse impact to achievable sustained data rate in all FDD and most typical TDD configurations. Certainly, there can be extreme TDD configurations where there could be an impact, but these may be rather atypical. Thus, prefer to remove the second sentence. |
| OPPO | Partially Y | We are wondering whether there is date rate impact with 16 HARQ processes. |
| CATT | Y |  |
| Huawei, HiSilicon | Y |  |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.5.3-4a: Can the above observations of the impact on data rate for UE with relaxed UE processing time be used as a baseline text for TR 38.875?** | |
| vivo |  | The 2nd sentence after adding “It is unclear whether” is confusing to readers, suggest to delete the whole sentence if it is not sure yet. |
| Ericsson | Y | The ‘Phase 2’ tag was missing in this updated question. We have inserted the missing tag now, but it seems that many companies may have missed the updated question. |
| SONY7 | Y | Would also be OK to delete the second sentence. |

**Latency and reliability:**

* P1: Contributions [1, 4, 5, 6, 9, 13, 16, 23, 24, 26, 28] mentioned the impact of relaxed UE processing time capability on latency, where [1, 4, 5, 23] provide some numerical examples of the impact on UL and DL latency for the initial transmission and different number of retransmissions.
* P2: Contributions [1, 3, 4, 5, 16, 21, 23, 24] observe that many RedCap use cases have rather relaxed latency requirements of up to 100 ms or 500 ms and thus can afford to have more relaxed UE processing time if the trade-off between cost reduction benefits and impacts is justified.
* P3: It is mentioned in several contributions [1, 2, 5, 6, 13, 23, 24, 26, 28] that for some use cases such as safety-related sensors, rather strict latency may be required, and a more relaxed UE processing may not be feasible.

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Latency and reliability:**  Relaxed UE processing time in terms of N1/N2 has impact on latency. For downlink transmission, relaxed N1 value impacts how fast HARQ-ACK feedback can be sent after the reception of PDSCH. For uplink transmission, relaxed N2 value impacts how fast PUSCH can be scheduled with respect to the UL grant. How significant the impact on latency is depends on use cases and scheduled number of retransmissions. Among the RedCap use cases, some safety-related sensor use cases may have rather strict latency requirements, for which relaxed UE processing time may not be feasible at least for some TDD configurations. For the other RedCap use cases, the latency requirements can be fulfilled. |

**Phase 2: Question 7.5.3-5: Can the above observations of the impact on latency and reliability for UE with relaxed UE processing time be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| SONY5 | Y |  |
| Qualcomm |  | We agree with most part of the proposal, and suggest to remove the last sentence as follows:  Relaxed UE processing time in terms of N1/N2 has impact on latency. For downlink transmission, relaxed N1 value impacts how fast HARQ-ACK feedback can be sent after the reception of PDSCH. For uplink transmission, relaxed N2 value impacts how fast PUSCH can be scheduled with respect to the UL grant. How significant the impact on latency is depends on use cases and targeted number of retransmissions. Among the RedCap use cases, some safety-related sensor use cases may have rather strict latency requirements, for which relaxed UE processing time may not be feasible. For the other RedCap use cases, the latency requirements can be fulfilled. |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | N | We suggest removing this sentence:  “Among the RedCap use cases, some safety-related sensor use cases may have rather strict latency requirements, for which relaxed UE processing time may not be feasible.”  We do not agree that it is not feasible to achieve 5-10 ms latency performance with doubling of N1/N2 values from Cap #1 numbers for low throughput data as identified for IWSN (even targeting 99.99% reliability). In fact, it should also be possible to accommodate reTx as well, except possibly some particular TDD configurations (and one can find such even for NR). Note that, for latency estimates, the NW component of the latency could still be assumed to operate at Cap #1 equivalent (i.e., need not be assumed to be relaxed as well). |
| OPPO |  | Agree with intel. |
| CATT | Y |  |
| Huawei, HiSilicon | N | The observation needs modifications. Given certain TDD configuration and specific deployment scenairos, it is still with large possibility that doubled processing time can meet the latency requirement even for safety related sensors, just with less retransmission times. The latency due to more HARQ retransmissions also hold for other techniques, e,g. HD-FDD. Suggest to  Relaxed UE processing time in terms of N1/N2 has impact on latency. For downlink transmission, relaxed N1 value impacts how fast HARQ-ACK feedback can be sent after the reception of PDSCH. For uplink transmission, relaxed N2 value impacts how fast PUSCH can be scheduled with respect to the UL grant. How significant the impact on latency ~~is~~ depends on use cases and ~~targeted~~ scheduled number of retransmissions. Among the RedCap use cases, some safety-related sensor use cases may have rather strict latency requirements, for which there may be less HARQ retramissions performed with relaxed UE processing time ~~ay not be feasible~~. For the other RedCap use cases, the latency requirements can be fulfilled. |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.5.3-5a: Can the above observations of the impact on latency and reliability for UE with relaxed UE processing time be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | N | We can agree with this proposal if the last sentence is removed, i.e.  For the other RedCap use cases, the latency requirements can be fulfilled. |
| ZTE | Y |  |
| Huawei, HiSilion | Y with modificiation | Typo: “latency is depends”. Not sure about QC concern on the last.  “for which relaxed UE processing time may not be feasible at least for some TDD configurations depending on the possible number of HARQ retransmissions within the latency requirement” |
| Spreadtrum | Y |  |
| LG |  | It would be okay to us if the last two senstences (starting from Among …) are removed. |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y | The “is” in “latency is depends” should be there (or something like “The significance of the impact on latency depends…”). We are OK with the text as is, as we probably don’t want to deal with an updated proposal. |

**Power consumption:**

* P8: Contributions [3, 5, 13, 16] mention that relaxed processing timeline can allow for lower clock frequency and lower voltage which has an impact on the UE power consumption.
* P9: Contributions [4, 16] mentioned that power saving benefit from cross-slot scheduling can be obtained from relaxed UE processing time.
* P10: Contributions [5, 6, 11, 24, 26, 28] noted that the UE power saving gain may not be clear or may even be degraded as UE may need to stay active longer due to more relaxed UE processing time, and that it may also depend on specific implementation.
* P11: Contribution [1] notes that the NW can configure RedCap UEs to achieve power saving gain from cross-slot scheduling even if no relaxed UE processing time capability is defined.

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Power consumption:**  Relaxed UE processing time in terms of N1/N2 may allow for processing with lower clock frequency and lower voltage which has an impact on the UE power consumption. The impact on power consumption of relaxed UE processing time depends on implementation and traffic characteristics. |

**Phase 2: Question 7.5.3-6: Can the above observations of the impact on power consumption for UE with relaxed UE processing time be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Partially Y | The last sentence should be “The impact on power consumption of relaxed UE processing time depends on implementation and traffic characteristics.” |
| vivo |  | We are not sure if the 2nd sentence is true and propose to delete it. One simple example, do we expect a Cap#1 NR UE will be more power consuming than a Cap#2 NR UE?  Relaxed UE processing time in terms of N1/N2 may allow for processing with lower clock frequency and lower voltage which has an impact on the UE power consumption. ~~However, on the other hand, relaxed UE processing time may have a negative impact on UE average power consumption because the UE will be active for a longer time before being able to return to a lower power light sleep or deep sleep state.~~ The impact on power consumption of HD-FDD depends on implementation and traffic characteristics. |
| SONY5 | Y | Agree with ZTE. OK with all the sentences. |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y | Agree with ZTE correction. |
| Samsung | Y |  |
| Ericsson | Y | Fine assuming the typo pointed out by ZTE is fixed |
| Intel | N | Agree with Vivo that the second sentence should be removed since it is not necessarily true. It is not necessarily the case that the UE can transition to lower power states with Cap #1 vs. doubling the Cap #1 numbers, and when considering support of multiple HARQ processes.  ~~However, on the other hand, relaxed UE processing time may have a negative impact on UE average power consumption because the UE will be active for a longer time before being able to return to a lower power light sleep or deep sleep state.~~ |
| OPPO |  | Agree with vivo and intel |
| CATT | Y |  |
| Huawei, HiSilicon |  | Share the view with vivo. As replied in FL4, the power comsumption benefits due to low voltage is exponential contribution, which would be larger on the negative impact due to longer active time. |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.5.3-6a: Can the above observations of the impact on power consumption for UE with relaxed UE processing time be used as a baseline text for TR 38.875?** | |
| CATT | Y | Fine to keep it simple. |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | Y |  |
| LG | Y | We are okay with this proposal, but we prefer the following wording as the word “impact” feels just neutral.  Relaxed UE processing time in terms of N1/N2 may allow for processing with lower clock frequency and lower voltage which helps reducing the UE power consumption |
| FUTUREWEI3 | Y | OK with LGE update |
| Ericsson | Y |  |
| SONY7 | Y |  |

### 7.5.4 Analysis of coexistence with legacy UEs

Contributions [1, 2, 23, 24] express that multiple UE processing timelines may increase complexity at the scheduler to handle and ensure coexistence with legacy UEs.

Contributions [1, 5, 8, 9, 10, 11, 15, 16, 21, 24] observe that there can be potential coexistence issues with legacy UEs during initial access/random access if a new, more relaxed UE processing time capability is introduced. For example, there exist the timing requirement for scheduling of Msg3 which depends on N1 and N2 values of UE processing time capability #1. If gNB schedules according to legacy UEs, RedCap UEs with relaxed N1/N2, if supported, may not be able to access the cell. On the other hand, if gNB considers potential presence of UEs with relaxed processing time in a cell, it would schedule according to the worst-case timing which would degrade the performance of legacy UEs. Similarly, timing of HARQ-ACK for Msg4 is also identified as a potential coexistence issue with legacy UEs in contributions [8, 9, 10, 15]. In order to support relaxed UE processing time capability during initial access, contributions [3, 8, 9, 10, 15] mention that methods for identifying RedCap UEs, e.g., before Msg3 scheduling may need to be studied.

These identified issues are listed below.

* C1: May make scheduler more complex [1, 2, 23, 24]
* C2: Identification of RedCap UEs before Msg3 may be needed [3, 8, 9, 10, 15].

This potential impact has been moved here from Section 7.5.3 of this document where it was known as P4:

* C3: Contributions [1, 4, 6, 23, 24, 26] observe negative impacts of relaxed UE processing time on scheduling complexity, especially when taking into account different scheduling timing restriction related to N1/N2 and the fact that there already exist two UE processing time capabilities in NR.

**Phase 3: Question 7.5.4-1: Can the above list (C1-C3) be used as a baseline for the TP drafting for TR section 7.5.4?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
|  |  |  |
|  |  |  |
|  |  |  |

### 7.5.5 Analysis of specification impacts

Contributions [1, 2, 3, 4, 13, 15, 23, 24] mention the specification impact of defining a new relaxed UE processing time capability and new values of N1/N2. Contributions [2, 23] note that the standardization effort can be high as it requires inputs and agreement from all UE manufacturers.

Other potential impacts on scheduling timing related to the existing default TDRA tables and HARQ-ACK timing range are mentioned by contributions [5, 9, 16, 21, 24]. On the other hand, contributions [1, 3, 4] note that no specification impacts beyond new definition of relaxed UE processing time are expected unless the relaxation of N1/N2 values is too excessive.

These identified impacts are listed below.

* S1: Definition of relaxed UE processing time capability and N1/N2 values [1, 2, 3, 4, 13, 15, 23, 24]
* S2: Scheduling time related to default TDRA tables and HARQ-ACK timing range [5, 9, 16, 21, 24]

**Phase 4: Question 7.5.5-1: Can the above list (S1-S2) be used as a baseline for the TP drafting for TR section 7.5.5?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
|  |  |  |
|  |  |  |
|  |  |  |

## 7.6 Relaxed maximum number of MIMO layers

### 7.6.1 Description of feature

RAN1#103e agreement:

* Adopt the TP in [R1-2009393](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009393.zip) as baseline text for TR clause 7.6.1.

### 7.6.2 Analysis of UE complexity reduction

RAN1#103e agreement:

* Adopt the TP in [R1-2009393](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009393.zip) as baseline text for TR clause 7.6.2.

### 7.6.3 Analysis of performance impacts

According to the SID [36],

|  |
| --- |
| The study includes evaluations of the impact to coverage, network capacity and spectral efficiency |

In addition, RAN1#101e made the following agreement:

|  |
| --- |
| Agreements:   * The evaluation of performance impacts includes at least peak data rate, latency and reliability (as needed for the use cases). Other performance metrics such as power consumption, spectral efficiency and PDCCH blocking probability may also be considered if appropriate for a specific technique. |

**Coverage:**

* P7: No impact on coverage [1, 4, 11, 15, 24].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Coverage:**  Reducing the maximum number of MIMO layers does not impact the coverage. |

**Phase 2: Question 7.6.3-2: Can the above observations of the impact on the coverage for UE with relaxed maximum number of MIMO layers be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | Y |  |
| OPPO | Y |  |
| Xiaomi | Y |  |
| CATT | Y |  |
| LG | Y |  |
| Huawei, HiSilicon | Y |  |
| FL | **FL2: Phase 2: Question 7.6.3-2: Can the above observations of the impact on the coverage for UE with relaxed maximum number of MIMO layers be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Huawei, HiSilicon | Y |  |
| LG | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Network capacity and spectral efficiency:**

* P8: [1] noted that spectral efficiency is expressed as bit rates per Hz, as reducing the maximum number of MIMO layers will decrease the peak data rates. It is expected that the maximum number of MIMO layers will degrade the spectral efficiency. However, as higher MIMO layers are scheduled when SNR is relatively high. Thus, impacts on spectral efficiency may only be observed under good channel conditions.
* P9: Cell spectral efficiency will be impacted/reduced due to reduced data rate/throughput [1, 2, 4, 5, 6, 11, 15, 24].
* P10: Capacity will be impacted/reduced due to reduced data rate [5, 24].

Based on submitted contributions and email discussion responses, the following TP can be considered. More text on network capacity and spectral efficiency can be captured after further progression of the discussion under AI 8.6.3.

|  |
| --- |
| **Network capacity and spectral efficiency:**  Since reducing the maximum number of MIMO layers reduces the peak data rate, it degrades the network capacity and spectral efficiency. Especially, the reduction of maximum number of MIMO layers mainly degrades the spectral efficiency for UEs in good channel conditions. |

**Phase 2: Question 7.6.3-3: Can the above observations of the impact on the network capacity and spectral efficiency for UE with relaxed maximum number of MIMO layers be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| DOCOMO | Y |  |
| Samsung |  | We suggest to simply as:  Since reducing the maximum number of MIMO layers reduces the peak data rate, it degrades the network capacity and spectral efficiency. ~~However, the impact depends on the channel condition which affects the number of MIMO layers that are used. For example, using a high number of MIMO layers is typically considered in good channel conditions. Therefore,~~ Especially, the reduction of maximum number of MIMO layers mainly degrades the spectral efficiency for UEs in good channel conditions. |
| Ericsson | Y |  |
| Intel | Y |  |
| OPPO |  | Agree with Samsung. |
| Xiaomi |  | Same view with Samsung |
| CATT | Y |  |
| LG | Y |  |
| Huawei, HiSilicon | Y |  |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.6.3-3a: Can the above observations of the impact on the network capacity and spectral efficiency for UE with relaxed maximum number of MIMO layers be used as a baseline text for TR 38.875?** | |
| CATT | Y | Fine to keep it simple. |
| ZTE | Y |  |
| Samsung | Y |  |
| Huawei, HiSilicon | Y |  |
| LG | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Data rate:**

* P1: With the agreed number of MIMO layers to study, peak data rates will be reduced but it can still adequately achieve the data rate requirements for all RedCap use cases [1].
* P2: Peak/max data rate will be impacted or reduced [2, 4, 9, 15, 22, 24]. One contribution [5] further noted that data rate will be reduced by 50% and 75% when the maximum number of MIMO layers is reduced from 4 to 2 or 2 to 1 layer, and from 4 to 1 layer respectively.
* P3: Reducing to 2 MIMO layers in FR1, it can provide the capability of achieving the upper bound data rate requirements [3].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Data rate:**  Reducing the maximum number of downlink MIMO layers will lower the downlink peak data rate.   * Reduction from 2 layers to 1 layer decreases the downlink peak rate by ~50%. * Reduction from 4 layers to 2 layers decreases the downlink peak rate by ~50%. * Reduction from 4 layers to 1 layer decreases the downlink peak rate by ~75%.   Despite this reduction in peak data rate, the UE with reduced number of downlink MIMO layers will be able to sufficiently fulfil the peak data rate requirements for the RedCap uses cases. For peak rate impacts from combinations of UE complexity reduction techniques, see clause 7.8.3. |

**Phase 2: Question 7.6.3-4: Can the above observations of the impact on the data rate for UE with relaxed maximum number of MIMO layers be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Paritally Y | As commented to **Phase 2: Question 7.2.3-4**, highest peak data rate requirement is not satisfied with 1 layer. We suggest to modify to “Despite this reduction in peak data rate, the UE will be able to sufficiently fulfil the peak data rate requirements for most of the RedCap uses cases.” |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y | Perhaps it can be clarified in the text that the statement concerns the individual technique, not combinations with other techniques. |
| Intel | Y |  |
| OPPO | Y |  |
| Xiami |  | **Same comment with that in Phase 2: Question 7.2.3-4** |
| CATT | Paritally Y | Agree with DOCOMO. Better to add ‘most of’ before the ‘RedCap use cases’. |
| LG | Y(Partially) | Agree with DOCOMO. Or, to make a progress, we put [ ] around the last sentence and can come back to it later. |
| Huawei, HiSilicon | Y |  |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.6.3-4a: Can the above observations of the impact on the data rate for UE with relaxed maximum number of MIMO layers be used as a baseline text for TR 38.875?** | |
| CATT | Y | We think it is somewhat obvious that the UE can fulfill the data rate requirement when only the number of maximum MIMO layers is reduced. But we are fine with the current verson. |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Huawei, HiSilicon | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Latency and reliability:**

* P4: No latency impact [24].
* P5: [1] noted that reducing the maximum number of MIMO layers may increase latency. However, the end-to-end latency requirements of RedCap use cases are relaxed (e.g. less than 100 ms for industrial wireless sensors and 500 ms for video surveillance), except the 5-10 ms requirement for safety related sensors. However, data rate of ~80 Mbps can be achieved with 20 MHz with 64QAM per MIMO layer in FR1. This allows transmitting payload up to 10 Kbytes in 1ms in layer 1 which is more than enough for small packet size expected for safety related message and enough to ensure the 5-10 ms latency requirement for safety related sensors. In FR2, it allows larger bandwidth thus higher bit rates can be achieved. Restricting the maximum number of MIMO layers can still sufficiently fulfil the latency requirements of all RedCap use cases.
* P6: Reliability should not be impacted [1, 24], as it is envisaged that BLER targets can still be achieved. [1].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Latency and reliability:**  Reducing the number of MIMO layers does not impact the latency and reliability significantly. The reduction of the maximum number of MIMO layers is only expected to affect the achievable latency for UEs in good channel conditions. The latency requirements of most RedCap use cases can still be sufficiently fulfilled. |

**Phase 2: Question 7.6.3-5: Can the above observations of the impact on the latency and reliability for UE with relaxed maximum number of MIMO layers be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo |  | Suggest to add one more sentence (from P5)  Reducing the number of MIMO layers does not impact the latency and reliability significantly. The reduction of the maximum number of MIMO layers is only expected to affect the achievable latency for UEs in good channel conditions. Restricting the maximum number of MIMO layers can still sufficiently fulfil the latency requirements of most RedCap use cases. |
| SONY5 | Y |  |
| FUTUREWEI | Y | Same “up to” comment |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Samsung | Y |  |
| Ericsson | Y | Also fine with Vivo’s revision |
| Intel | Y |  |
| OPPO | Y |  |
| CATT | Y |  |
| LG | Y | Also fine with what vivo suggested. |
| Huawei, HiSilicon | Y |  |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.6.3-5a: Can the above observations of the impact on the latency and reliability for UE with relaxed maximum number of MIMO layers be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Huawei, HiSilicon | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Power consumption:**

* P11: In [1], it is noted that Reducing the maximum DL/UL modulation order and/or DL MIMO support may reduce power consumption due to reduced complexity in processing a smaller maximum TB. However, the amount of power saved may not be significant if the RedCap UEs would mostly be in RRC\_IDLE/INACTIVE states. Furthermore, reducing the maximum number of DL MIMO layers can fulfil the date rate requirements of most RedCap uses cases. In many use cases, long transmission times for large TB sizes are not expected to occur frequently for RedCap use cases. Thus, a negative impact on UE power consumption is not expected. In use cases where large TB sizes occur more often, and long transmission times might become a consequence of modulation order and MIMO layer reduction for UEs in good coverage. In such cases, there will be more pronounced negative impact on UE power consumption. In summary, the impact on UE power consumption depends on the traffic and coverage scenarios.
* P12: Reduced power consumption as higher data rate consume higher power or less processing energy is required for smaller TB sizes [1, 4, 13].
* P13: No impacts on power consumption [24].
* P14: As the number of DL antennas is kept the same, there is no power saving. And since the data rate is reduced, longer receiving time is needed to receive a DL TB. Thus, it will have negative impact on UE power saving [15].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Power consumption:**  The reduced number of MIMO layers can result in a lower instantaneous power consumption due to the reduced peak data rate and reduced complexity in processing a smaller maximum transport block size. However, it is not clear whether the average power consumption of the UE is increased or decreased. |

**Phase 2: Question 7.6.3-6: Can the above observations of the impact on the power consumption for UE with relaxed maximum number of MIMO layers be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | N | The 2nd sentence is definitely not true. TR38.840 had concluded the power saving benefit by reducing the number of MIMO layers. |
| SONY5 | Y | In response to vivo: wasn’t the TR38.840 conclusion based on certain assumptions? In the Redcap case, for a UE in channel conditions that would support 2 layers, if the Redcap UE only supported a single layer, wouldn’t the UE need to be “on” for longer, thereby increasing power consumption? |
| FUTUREWEI |  | Not sure this one is correct |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | N | We don’t agree on the power consumption reduction. We sugget to change to:  The UE power comsumption impact is not clear. |
| Ericsson | Y |  |
| Intel | N | While the second statement may be true in general, we do not think it applies for the UE BW and data rate requirements we are considering for RedCap use-cases. Thus, to SONY’s comment, the UE need not be “ON” for longer only if the traffic demands dictate such, and we do not see such for the targeted data rates and traffic models considered for RedCap. |
| CATT | Y |  |
| Huawei, HiSilicon | Y |  |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.6.3-6a: Can the above observations of the impact on the power consumption for UE with relaxed maximum number of MIMO layers be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| vivo | N | Saying something is unclear is confusing to the reader. In section 2.3 of R1-2009212, we provided results assuming MIMO layer is reduced together with number of Rx, and power saving gain is shown for all the agreed traffic model. However, no other evaluations results are available so far showing the power consumption can increase based on the agreed assumptions. |
| ZTE | Y |  |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

### 7.6.4 Analysis of coexistence with legacy UEs

The following potential coexistence impacts were identified in the contributions:

* C1: There is no or no significant coexistence impact. [1, 2, 4, 5, 11, 15]. In [1], it is further noted that prior to the completion of initial access, it is not possible for the gNB to send the rank indication to the UE. Furthermore, a UE’s MIMO layer support could only be known to the gNB after it has retrieved the UE capability from the UE. Due to the limitation in the current specifications, legacy UEs can only be scheduled with single MIMO layer for initial access. Having a RedCap UE with reduced maximum MIMO layer support in the same network, will not affect the number of MIMO layers to be scheduled for the legacy UEs or the RedCap UEs for initial access transmissions.
* C2: Restricted to 2 MIMO layers in FR1 have no obvious coexistence issue is envisioned [3].
* C3: Implicit restrictions on TBS may impact on SIB/Msg4/Paging [24].

**Phase 3: Question 7.6.4-1: Can the above list (C1-C3) be used as a baseline for the TP drafting for TR section 7.6.4?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
|  |  |  |
|  |  |  |
|  |  |  |

### 7.6.5 Analysis of specification impacts

The following potential specification impacts were identified in the contributions:

* S1: UE capability indication to notify the NW of UE’s reduced capability [1, 4, 13].
* S2: Small RAN1 specification impacts [11]
* S3: Limited or no significant specification impacts [2, 15]
* S4: Reduced to 2 MIMO layers in FR1 can provide minimized specification impacts [3].
* S5: No RI and LI report are reduced for single MIMO layer support. Thus, can consider adding the descriptions with report to no RI and LI in the specifications [5].
* S6: Demodulation performance requirements for single layer may be specified in RAN4 [5].

**Phase 4: Question 7.6.5-1: Can the above list (S1-S6) be used as a baseline for the TP drafting for TR section 7.6.5?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
|  |  |  |
|  |  |  |
|  |  |  |

## 7.7 Relaxed maximum modulation order

### 7.7.1 Description of feature

RAN1#103e agreement:

* Adopt the TP in [R1-2009394](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009394.zip) for TR clause 7.7.1.

### 7.7.2 Analysis of UE complexity reduction

RAN1#103e agreement:

* Adopt the TP in [R1-2009393](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009393.zip) as baseline text for TR clause 7.7.2.
  + Companies are invited to double-check their entries in the cost reduction spreadsheet with respect to the above comments (and to catch potential typos).
  + The table will be further updated with potential updated cost estimates.

### 7.7.3 Analysis of performance impacts

According to the SID [36],

|  |
| --- |
| The study includes evaluations of the impact to coverage, network capacity and spectral efficiency |

In addition, RAN1#101e made the following agreement:

|  |
| --- |
| Agreements:   * The evaluation of performance impacts includes at least peak data rate, latency and reliability (as needed for the use cases). Other performance metrics such as power consumption, spectral efficiency and PDCCH blocking probability may also be considered if appropriate for a specific technique. |

**Coverage:**

* P7: No impact on coverage [1, 4, 11, 15, 24].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Coverage:**  Relaxation of maximum mandatory modulation orders does not impact the coverage. |

**Phase 2: Question 7.7.3-2: Can the above observations of the impact on coverage for UE with relaxed maximum modulation orders be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| LG | Y |  |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | Y |  |
| OPPO | Y |  |
| CATT | Y |  |
| Huawei, HiSilicon | Y |  |
| FL | **FL2: Phase 2: Question 7.7.3-2: Can the above observations of the impact on coverage for UE with relaxed maximum modulation orders be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Huawei, HiSilicon | Y |  |
| LG | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Network capacity and spectral efficiency:**

* P8: [1] noted that Spectral efficiency is expressed as bit rates per Hz, as reducing the maximum modulation orders in DL/UL will decrease the peak data rates. It is expected that reducing the maximum number of MIMO layers will degrade the spectral efficiency. However, as higher MIMO layers are scheduled when SNR is relatively high. Thus, impacts on spectral efficiency may only be observed under good channel conditions.
* P9: Cell spectral efficiency will be impacted/reduced due to reduced data rate/throughput [1, 2, 4, 5, 6, 11, 15, 24].
* P10: [2] noted the impact on spectral efficiency will be substantial. [3, 11] further observed substantial cell spectral efficiency loss about 23.6% - 43.6% due to UL modulation order restriction from 64QAM to 16QAM in FR1 and about 6.43% spectral efficiency reduction due to DL modulation order restriction from 256QAM to 64QAM in FR1.
* P11: Capacity will be impacted/reduced due to reduced data rate [5, 24].

Based on submitted contributions and email discussion responses, the following TP can be considered. More text on network capacity and spectral efficiency can be captured after further progression of the discussion under AI 8.6.3.

|  |
| --- |
| **Network capacity and spectral efficiency:**  Relaxation of maximum mandatory modulation orders will reduce both network capacity and spectral efficiency due to reduced peak data rate. |

**Phase 2: Question 7.7.3-3: Can the above observations of the impact on network capacity and spectral efficiency for UE with relaxed maximum modulation orders be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| LG | Y |  |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | Y |  |
| OPPO | Y |  |
| CATT | Y |  |
| Huawei, HiSilicon | Y |  |
| FL | **FL2: Phase 2: Question 7.7.3-3: Can the above observations of the impact on network capacity and spectral efficiency for UE with relaxed maximum modulation orders be used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | N | The impacts on network capacity are not clear, since the network can admit more RedCap UEs with lower data rates. |
| ZTE | Y |  |
| Huawei, HiSilicon | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y | Regarding the Qualcomm comment, shouldn’t the network capacity be based on the number of UEs that can be supported with the same data rate? For the same data rate, it seems that the network capacity would be reduced. |

**Data rate:**

* P1: With the agreed maximum modulation orders to study, peak data rates will be reduced but it can still adequately achieve the data rate requirements for all RedCap use cases [1].
* P2: Peak/max data rate will be impacted or reduced [2, 3, 4, 5, 9, 11, 15, 22, 24]. Contribution [5, 23] further noted that data rate will be reduced by ~20% and ~33% when the maximum modulation order is restricted from 256QAM to 64QAM, and from 64QAM to 16QAM respectively.

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Data rate:**  Reducing the maximum modulation orders will lower the downlink peak data rate.   * Reduction from 256QAM to 64QAM decreases the downlink peak rate by ~25%. * Reduction from 64QAM to 16QAM decreases the downlink peak rate by ~33%.   Despite this reduction in peak data rate, the UE will be able to sufficiently fulfil the peak data rate requirements for the RedCap uses cases. For peak rate impacts from combinations of UE complexity reduction techniques, see clause 7.8.3. |

**Phase 2: Question 7.7.3-4: Can the above observations of the impact on data rate for UE with relased maximum modulation order be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| LG |  | Depending on the supported bandwidth and the number of MIMO layers, the sentence starting with “Despite …” may or may not be correct. We can comeback to this question later. |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y | Perhaps it can be clarified in the text that the statement concerns the individual technique, not combinations with other techniques. |
| Intel | Y |  |
| OPPO | Y |  |
| CATT | Y, partially | Not sure whether ‘Despite …’ is correct. Is it under the assumption that the BW and Rx antenna number remains unchanged compared to the reference NR UE? If so, we are OK with it. |
| Huawei, HiSilicon |  | Share the view with LG. |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.7.3-4a: Can the above observations of the impact on data rate for UE with relased maximum modulation order be used as a baseline text for TR 38.875?** | |
| CATT | Y | We think it is somewhat obvious that the UE can fulfill the data rate requirement when only the maximum modulation order is reduced. But we are fine with the current verson. |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Huawei, HiSilicon | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Latency and reliability:**

* P3: [1] noted that restricting the DL/UL maximum modulation orders may increase latency. However, the end-to-end latency requirements of RedCap use cases are relaxed (e.g. less than 100 ms for industrial wireless sensors and 500 ms for video surveillance), except the 5-10 ms requirement for safety related sensors. Data rate of ~80 Mbps can be achieved with 20 MHz with 64QAM per MIMO layer in FR1 DL. This allows transmitting payload up to 10 Kbytes in 1ms in layer 1 which is more than enough for small packet size expected for safety related message and enough to ensure the 5-10 ms latency requirement for safety related sensors. In FR2, it allows larger bandwidth thus higher bit rates can be achieved. Restricting the DL/UL modulation orders can also sufficiently fulfil the latency requirements of all RedCap use cases.
* P4: No latency impact [24].
* P5: Slightly increased latency but acceptable for RedCap use cases [16].
* P6: Reliability should not be impacted [1, 24], as it is envisaged that BLER targets can still be achieved. [1].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Latency and reliability:**  Relaxing the maximum modulation orders may increase the latency slightly. Nevertheless, all the latency and reliability requirements for the RedCap use cases can be satisfied by all the studied options for relaxed maximum modulation orders. |

**Phase 2: Question 7.7.3-5: Can the above observations of the impact on latency and reliability for UE with relaxed maximum modulation orders used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| vivo | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | Y |  |
| OPPO | Y |  |
| CATT | Y |  |
| LG | Y |  |
| Huawei, HiSilicon | Y |  |
| FL | **FL2: Phase 2: Question 7.7.3-5: Can the above observations of the impact on latency and reliability for UE with relaxed maximum modulation orders used as a baseline text for TR 38.875?** | |
| CATT | Y |  |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Huawei, HiSilicon | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y |  |

**Power consumption:**

* P12: [1] noted that Reducing the maximum DL/UL modulation order may reduce power consumption due to reduced complexity in processing a smaller maximum TB. Furthermore, reducing the DL/UL maximum modulation order may also reduce the ADC/DAC power consumption. However, the amount of power saved may not be significant if the RedCap UEs would mostly be in RRC\_IDLE/INACTIVE states. Furthermore, reducing the maximum modulation order can adequately fulfil the date rate requirements of all RedCap uses cases. In many use cases, long transmission times for large TB sizes are not expected to occur frequently for RedCap use cases. Thus, a negative impact on UE power consumption is not expected. In use cases where large TB sizes occur more often, and long transmission times might become a consequence of modulation order and MIMO layer reduction for UEs in good coverage. In such cases, there will be more pronounced negative impact on UE power consumption. In summary, the impact on UE power consumption depends on the traffic and coverage scenarios.
* P13: Reduced power consumption as higher data rate consume higher power or less processing energy is required for RF components [3, 4, 11, 13, 16].
* P14: [11] noted that power saving would be marginal.
* P15: No impacts on power consumption [24].
* P16: There will have some saving on RF part, but the receive/transmit time may be longer for high data rate case [15].

Based on submitted contributions and email discussion responses, the following TP can be considered.

|  |
| --- |
| **Power consumption:**  Relaxation of maximum modulation orders can reduce power consumption of the RF and baseband modules marginally during transmission and reception. |

**Phase 2: Question 7.7.3-6: Can the above observations of the impact on power consumption for UE with relaxed maximum modulation orders be used as a baseline text for TR 38.875?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| ZTE | Y |  |
| SONY5 | Y | The power consumption reduction would be marginal, but we are OK with the text proposal. |
| DOCOMO | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Intel | Y |  |
| OPPO | Y |  |
| CATT | Y |  |
| LG | Y |  |
| Huawei, HiSilicon |  | Not needed about “However, the overall impact on UE power consumption depends on the traffic and coverage scenarios.” |
| FL | The proposal has been updated based on received responses.  **FL2: Phase 2: Question 7.7.3-6a: Can the above observations of the impact on power consumption for UE with relaxed maximum modulation orders be used as a baseline text for TR 38.875?** | |
| CATT | Y | Fine to keep it simple. |
| Qualcomm | Y |  |
| ZTE | Y |  |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | Y |  |
| LG | Y |  |
| FUTUREWEI3 | Y |  |
| Ericsson | Y |  |
| SONY7 | Y | While we are OK with the text, we would have thought that a relaxed modulation order would tend to increase power consumption for cell centre UEs. If the UE takes a longer time to transmit / receive a packet, it is “on” for longer. Maybe this isn’t such a big issue as the power consumption of the cell edge UE should be the greater concern. |

### 7.7.4 Analysis of coexistence with legacy UEs

The following potential coexistence impacts were identified in the contributions:

* C1: There is no or no significant coexistence impact. [1, 4, 9, 11, 15, 16]. Contribution [1] further noted that During initial access, for the reception of paging indication or broadcasting information (SIBx), PDSCH is not expected to be scheduled with modulation order higher than QPSK. And the scheduling information for Msg3 would be carried in PDCCH using DCI format 0\_1 which allows modulation order <= 16QAM to be sent in the DCI. From modulation order perspective, there will be no impacts by restricting the UL and/or DL maximum modulation order based on the current agreement.
* C2: For the initial access procedure, lower MCS and single layer for broadcast downlink transmission and initial uplink scheduling will be used to ensure decoding performance or poor UE channel condition. In this case, RedCap UEs are still able to finish the access procedure [9].
* C3: Implicit restrictions on TBS may impact on SIB/Msg4/Paging [24].

**Phase 3: Question 7.7.4-1: Can the above list (C1-C3) be used as a baseline for the TP drafting for TR section 7.7.4?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
|  |  |  |
|  |  |  |
|  |  |  |

### 7.7.5 Analysis of specification impacts

The following potential specification impacts were identified in the contributions:

* S1: UE capability indication to notify the NW of UE’s reduced capability [1, 4, 13]
* S2: To minimize specification impacts, there should be no optimization (only reuse) of all existing tables [2]. [5] noted that restricting to 64QAM, one possible solution is to reuse the existing 64QAM table.
* S3: Limited specification impacts [15].
* S4: Small RAN1 specification impacts [1, 4, 5, 11, 20, 24]
  + Change of DCI size, CQI table and MCS table due to restricted maximum modulation order is possible but not essential [1, 4].
  + If the maximum modulation order is restricted to 16QAM, new MCS/DCI tables are introduced [5, 20] with lower/higher spectral efficiency for UE specific allocation case [20] to achieve more scheduling flexibility. It is further noted that the standardization effort would be small if the values from Rel-15/16 tables are reused [20].
* S5: RAN4 CQI performance requirement if new CQI tables are introduced [1].

**Phase 4: Question 7.7.5-1: Can the above list (S1-S5) be used as a baseline for the TP drafting for TR section 7.7.5?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
|  |  |  |
|  |  |  |
|  |  |  |

## 7.8 Combinations of UE complexity reduction features

### 7.8.1 Description of feature combinations

Draft TPs will be provided later.

### 7.8.2 Analysis of UE complexity reduction

RAN1#103e agreements:

* For evaluating complexity reduction, to come up with a set of combinations of techniques:
  + For each case (FR1 FDD, FR1 TDD, & FR2), target up to 6 to 8 combinations
    - Detailed combinations are FFS
* For TR section 7.2.2 (on reduced number of Rx antennas), the following combinations of complexity reduction techniques are evaluated.
  1. FR1 FDD: 1 layer, 1 Rx
  2. FR1 TDD: 1 layer, 1 Rx
  3. FR1 TDD: 2 layers, 2 Rx
  4. FR2: 1 layer, 1 Rx
* For FR1 FDD, the following combinations of complexity reduction techniques are evaluated:

1. 1 layer, 1 Rx, 20 MHz
2. 1 layer, 1 Rx, 20 MHz, HD-FDD type A
3. 1 layer, 1 Rx, 20 MHz, relaxed modulations for DL & UL
4. 1 layer, 1 Rx, 20 MHz, doubled processing time for N1 & N2 only
5. 1 layer, 1 Rx, 20 MHz, relaxed modulations for DL & UL, doubled processing time for N1 & N2 only
6. 1 layer, 1 Rx, 20 MHz, relaxed modulations for DL & UL, HD-FDD type A, doubled processing time for N1 & N2 only
7. 2 layers, 2 Rx, 20 MHz, HD-FDD type A
8. 2 layers, 2 Rx, 20 MHz, doubled processing time for N1 & N2 only

* For FR1 TDD, the following combinations of complexity reduction techniques are evaluated:

1. 1 layer, 1 Rx, 20 MHz
2. 1 layer, 1 Rx, 20 MHz, relaxed modulations for DL & UL
3. 1 layer, 1 Rx, 20 MHz, doubled processing time for N1 & N2 only
4. 1 layer, 1 Rx, 20 MHz, relaxed modulations for DL & UL, doubled processing time for N1 & N2 only
5. 2 layers, 2 Rx, 20 MHz
6. 2 layers, 2 Rx, 20 MHz, relaxed modulations for DL & UL
7. 2 layers, 2 Rx, 20 MHz, doubled processing time for N1 & N2 only
8. 2 layers, 2 Rx, 20 MHz, relaxed modulations for DL & UL, doubled processing time for N1 & N2 only

* For FR2, the following combinations of complexity reduction techniques are evaluated:

1. 1 layer, 1 Rx, 100 MHz
2. 1 layer, 1 Rx, 100 MHz, relaxed modulations DL & UL
3. 1 layer, 1 Rx, 100 MHz, doubled processing time for N1 & N2 only
4. 1 layer, 1 Rx, 100 MHz, relaxed modulations DL & UL, doubled processing time for N1 & N2 only
5. 2 layers, 2 Rx, 100 MHz, relaxed modulations DL & UL
6. 2 layers, 2 Rx, 100 MHz, doubled processing time for N1 & N2 only
7. 2 layers, 2 Rx, 100 MHz, relaxed modulations DL & UL, doubled processing time for N1 & N2 only

The tables with device cost evaluation results in this contribution are based on [RedCapCost-v048-FL-Samsung2.xlsx](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Inbox/drafts/8.6/EvaluationResults/RedCapCost/RedCapCost-v048-FL-Samsung2.xlsx). They will eventually be updated with new results from the email discussion [103-e-NR-RedCap-EvaluationResults].

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| The estimated costs and estimated cost reductions for devices employing one or more of the UE complexity reduction techniques (see descriptions in clauses 7.2 through 7.7), relative to the reference NR device (see evaluation methodology described in clause 6.1) and averaged over the results provided by the sourcing companies, are summarized in Table 7.8.2-1 for FR1 FDD, Table 7.8.2-2 for FR1 TDD, and Table 7.8.2-3 for FR2.  **Table 7.8.2-1: Estimated relative device cost and estimated relative device cost reduction for UE complexity reduction technique(s) for FR1 FDD**   |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | | **FR1 FDD UE complexity reduction technique(s)** | **RF cost metric** | **BB cost metric** | **Total cost metric** | **RF reduction** | **BB reduction** | **Total reduction** | | 20 MHz (instead of 100 MHz) | 97.7% | 48.4% | 68.1% | 2.3% | 51.6% | 31.9% | | 1 layer (instead of 2 layers) | 100.0% | 79.3% | 87.6% | 0.0% | 20.7% | 12.4% | | 1 Rx (instead of 2 Rx) | 74.8% | 75.7% | 75.4% | 25.2% | 24.3% | 24.6% | | HD-FDD type A (instead of FD-FDD) | 83.9% | 99.4% | 93.2% | 16.1% | 0.6% | 6.8% | | HD-FDD type B (instead of FD-FDD) | 77.3% | 99.2% | 90.4% | 22.7% | 0.8% | 9.6% | | Double N1 and N2 | 100.0% | 90.5% | 94.3% | 0.0% | 9.5% | 5.7% | | DL 64QAM (instead of DL 256QAM) | 97.8% | 91.8% | 94.2% | 2.2% | 8.2% | 5.8% | | UL 16QAM (instead of UL 64QAM) | 97.1% | 98.3% | 97.8% | 2.9% | 1.7% | 2.2% | | 1 layer, 1 Rx | 74.2% | 55.9% | 63.2% | 25.8% | 44.1% | 36.8% | | 20 MHz, 1 layer, 1 Rx | 67.5% | 25.8% | 42.5% | 32.5% | 74.2% | 57.5% | | 20 MHz, 1 layer, 1 Rx, HD-FDD type A | 53.2% | 25.6% | 36.6% | 46.8% | 74.4% | 63.4% | | 20 MHz, 1 layer, 1 Rx, DL 64QAM, UL 16QAM | 64.2% | 24.3% | 40.2% | 35.8% | 75.7% | 59.8% | | 20 MHz, 1 layer, 1 Rx, double N1/N2 | 67.5% | 22.9% | 40.7% | 32.5% | 77.1% | 59.3% | | 20 MHz, 1 layer, 1 Rx, DL 64QAM, UL 16QAM, double N1/N2 | 64.6% | 21.7% | 38.9% | 35.4% | 78.3% | 61.1% | | 20 MHz, 1 layer, 1 Rx, DL 64QAM, UL 16QAM, HD-FDD type A, double N1/N2 | 50.2% | 21.4% | 32.9% | 49.8% | 78.6% | 67.1% | | 20 MHz, 2 layers, 2 Rx, HD-FDD type A | 81.3% | 46.0% | 60.1% | 18.8% | 54.0% | 39.9% | | 20 MHz, 2 layers, 2 Rx, double N1/N2 | 97.6% | 42.6% | 64.6% | 2.4% | 57.4% | 35.4% |   **Table 7.8.2-2: Estimated relative device cost and estimated relative device cost reduction for UE complexity reduction technique(s) for FR1 TDD**   |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | | **FR1 TDD UE complexity reduction technique(s)** | **RF cost metric** | **BB cost metric** | **Total cost metric** | **RF reduction** | **BB reduction** | **Total reduction** | | 20 MHz (instead of 100 MHz) | 96.4% | 46.7% | 66.6% | 3.6% | 53.3% | 33.4% | | 2 layers (instead of 4 layers) | 100.0% | 81.1% | 88.7% | 0.0% | 18.9% | 11.3% | | 1 layer (instead of 4 layers) | 100.0% | 71.9% | 83.2% | 0.0% | 28.1% | 16.8% | | 2 Rx (instead of 4 Rx) | 68.1% | 71.4% | 70.1% | 31.9% | 28.6% | 29.9% | | 1 Rx (instead of 4 Rx) | 51.9% | 57.3% | 55.1% | 48.1% | 42.8% | 44.9% | | Double N1 and N2 | 100.0% | 90.1% | 94.1% | 0.0% | 9.9% | 5.9% | | DL 64QAM (instead of DL 256QAM) | 96.2% | 92.1% | 93.7% | 3.8% | 7.9% | 6.3% | | UL 16QAM (instead of UL 64QAM) | 96.9% | 98.4% | 97.8% | 3.1% | 1.6% | 2.2% | | 1 layer, 1 Rx | 51.3% | 33.0% | 40.3% | 48.7% | 67.0% | 59.7% | | 2 layers, 2 Rx | 68.0% | 55.4% | 60.4% | 32.0% | 44.6% | 39.6% | | 20 MHz, 1 layer, 1 Rx | 50.6% | 18.6% | 31.4% | 49.4% | 81.4% | 68.6% | | 20 MHz, 1 layer, 1 Rx, relaxed mods | 47.1% | 17.5% | 29.3% | 52.9% | 82.5% | 70.7% | | 20 MHz, 1 layer, 1 Rx, double N1/N2 | 50.6% | 16.2% | 30.0% | 49.4% | 83.8% | 70.0% | | 20 MHz, 1 layer, 1 Rx, relaxed mods, double N1/N2 | 47.1% | 15.3% | 28.1% | 52.9% | 84.7% | 71.9% | | 20 MHz, 2 layers, 2 Rx | 66.8% | 27.8% | 43.4% | 33.3% | 72.2% | 56.6% | | 20 MHz, 2 layers, 2 Rx, relaxed mods | 61.8% | 26.1% | 40.4% | 38.2% | 73.9% | 59.6% | | 20 MHz, 2 layers, 2 Rx, double N1/N2 | 66.8% | 24.9% | 41.7% | 33.3% | 75.1% | 58.3% | | 20 MHz, 2 layers, 2 Rx, relaxed mods, double N1/N2 | 61.8% | 23.7% | 38.9% | 38.2% | 76.3% | 61.1% |   **Table 7.8.2-3: Estimated relative device cost and estimated relative device cost reduction for UE complexity reduction technique(s) for FR2**   |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | | **FR2 UE complexity reduction technique(s)** | **RF cost metric** | **BB cost metric** | **Total cost metric** | **RF reduction** | **BB reduction** | **Total reduction** | | 100 MHz (instead of 200 MHz) | 99.5% | 69.4% | 84.4% | 0.5% | 30.6% | 15.6% | | 50 MHz (instead of 200 MHz) | 99.0% | 54.0% | 76.5% | 1.0% | 46.0% | 23.5% | | 1 layer (instead of 2 layers) | 100.0% | 77.8% | 88.9% | 0.0% | 22.2% | 11.1% | | 1 Rx (instead of 2 Rx) | 64.3% | 76.2% | 70.3% | 35.7% | 23.8% | 29.7% | | Double N1 and N2 | 100.0% | 88.9% | 94.4% | 0.0% | 11.1% | 5.6% | | DL 16QAM (instead of DL 64QAM) | 97.8% | 91.0% | 94.4% | 2.2% | 9.0% | 5.6% | | UL 16QAM (instead of UL 64QAM) | 97.9% | 98.4% | 98.1% | 2.2% | 1.6% | 1.9% | | 1 layer, 1 Rx | 64.9% | 55.7% | 60.3% | 35.1% | 44.3% | 39.7% | | 100 MHz, 1 layer, 1 Rx | 64.8% | 40.3% | 52.5% | 35.2% | 59.7% | 47.5% | | 100 MHz, 1 layer, 1 Rx, relaxed mods | 61.6% | 37.0% | 49.3% | 38.4% | 63.0% | 50.7% | | 100 MHz, 1 layer, 1 Rx, double N1/N2 | 64.4% | 35.5% | 50.0% | 35.6% | 64.5% | 50.0% | | 100 MHz, 1 layer, 1 Rx, relaxed mods, double N1/N2 | 61.6% | 32.9% | 47.2% | 38.4% | 67.1% | 52.8% | | 100 MHz, 2 layers, 2 Rx, relaxed mods | 95.2% | 63.8% | 79.5% | 4.8% | 36.2% | 20.5% | | 100 MHz, 2 layers, 2 Rx, double N1/N2 | 99.4% | 62.4% | 80.9% | 0.6% | 37.6% | 19.1% | | 100 MHz, 2 layers, 2 Rx, relaxed mods, double N1/N2 | 95.2% | 57.8% | 76.5% | 4.8% | 42.2% | 23.5% | |

**FL1: Phase 1: Proposal 7.8.2-1: Adopt the TP above as baseline text for TR clause 7.8.2.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| FUTUREWEI2 | Y |  |
| Ericsson | Y |  |
| Qualcomm | Y |  |
| Intel | Y |  |
| Nokia, NSB | Y |  |
| DOCOMO | Y |  |
| LG | Y |  |
| CATT | Y mostly | In **Table 7.8.2-1,** relaxed modulation in *combinations* is marked as ‘DL 64QAM, UL 16QAM’, while in **Table 7.8.2-2** and **Table 7.8.2-3,** it is marked as ‘relaxed mods’.  We prefer to make them aligned, e.g., for **Table 7.8.2-2**, change to ‘DL 64QAM, UL 16QAM’, and for **Table 7.8.2-3,** change to ‘DL 16QAM, UL 16QAM’, respectively. |
| SONY6 | Y |  |
| CMCC | Y |  |
| ZTE | Y |  |
| OPPO | Y | Agree with CATT’s proposal |
| Samsung | N | It is not clear on what is MIMO layer assumption on 1Rx (instead of 2 Rx).  And We don’t agree to capture it in conclusion part. |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | Y |  |

### 7.8.3 Analysis of performance impacts

Draft TPs will be provided later (at least regarding peak data rates for different combinations of techniques).

### 7.8.4 Analysis of coexistence with legacy UEs

Draft TPs will be provided later.

### 7.8.5 Analysis of specification impacts

Draft TPs will be provided later.

# 12 Conclusions

RAN1#103e agreements:

* Capture the recommendation that maximum bandwidth of an FR1 RedCap UE is 20 MHz during and after initial access.
  + FFS: Whether an FR1 RedCap UE can optionally support a maximum bandwidth larger than 20 MHz after initial access
* Working assumption: Support that the maximum bandwidth of an FR2 RedCap UE is 100 MHz during initial access and 100MHz after initial access.

Based on submitted input (contributions, evaluation results, email discussion responses), the following can be considered.

**Phase 1: Proposal 12-10: Confirm the working assumption: Support that the maximum bandwidth of an FR2 RedCap UE is 100 MHz during initial access and 100MHz after initial access.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | Y |  |
| CATT | Y |  |
| CMCC | Y |  |
| LG | Y |  |
| ZTE | Y |  |
| vivo | Y |  |
| Nokia, NSB | Y |  |
| FUTUREWEI | Y |  |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| InterDigital | Y |  |
| Sierra Wireless | Y |  |
| Samsung |  | Wait until more clear observations for combinations |
| Ericsson | Y |  |
| Sharp | Y |  |
| Intel | Y |  |
| Spreadtrum | Y |  |
| OPPO | Y |  |
| NEC | Y |  |
| FL | **FL1: Phase 1: Proposal 12-10: Confirm the working assumption: Support that the maximum bandwidth of an FR2 RedCap UE is 100 MHz during initial access and 100MHz after initial access.** | |
| FUTUREWEI2 | Y |  |
| MediaTek | Y |  |
| Ericsson | Y |  |
| Qualcomm | Y |  |
| Intel | Y |  |
| Nokia, NSB | Y |  |
| DOCOMO | Y |  |
| LG | Y |  |
| CATT | Y |  |
| Lenovo, Motorola Moblity | Y |  |
| NEC | Y |  |
| CMCC | Y |  |
| ZTE | Y |  |
| OPPO | Y |  |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | Y |  |

**Phase 1: Proposal 12-20: Support that the minimum number of Rx branches of a RedCap UE is 1 for FR1 FDD bands where a non-RedCap UE is required to be equipped with a minimum of 2 Rx branches.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | N | Wait. We envision that the support 2Rx&2Layers in FDD FR1 for RedCap is important. It should be decided together with the support of 1Rx&1 Layer. |
| CATT | Y | Also fine to wait for conclusions from cost evaluations of combinations. |
| CMCC | Y |  |
| LG | Y |  |
| ZTE | Y |  |
| vivo | Y |  |
| Nokia, NSB | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | almost | Our comment from the last FLS still applies … we may be ok to support 1RX as long as 2RX/2MIMO layers is also supported as part of UE capability signaling. |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| InterDigital | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y | It should be clarified that this is a RAN1 recommendation. Per-band Rx requirements should be specified in RAN4. |
| Sharp | Y |  |
| Intel | Y |  |
| Spreadtrum | Y |  |
| OPPO | Y |  |
| NEC | Y |  |
| Xiaomi | Y |  |
| FL | Based on received responses, the following proposal can be considered as a way forward.  **FL1: Phase 1: Proposal 12-21: Recommend that the specification supports RedCap UEs with 1 Rx branch as well as RedCap UEs with 2 Rx branches for FR1 FDD bands where a non-RedCap UE is required to be equipped with a minimum of 2 Rx branches.** | |
| FUTUREWEI2 | Y | We can accept this, though our preference as expressed in the GTW is to decide now that initial access is based on 1RX and 2RX can be indicated as a UE capability. |
| MediaTek | N | We don’t support the proposal. If we don’t define different RedCap UEs, the gNB will have to assume 1Rx RedCap UEs. So, not sure what this will add compared to mandating the UE to support at least 1 Rx.  We do not see a need to introduce market fragmentation, especially if the same approach is adopted to other reduction features.  We should down select between the two options (1Rx or 2Rx). |
| Ericsson | Y |  |
| Qualcomm | N | As far as the **minimum** number of RX branches is concerned, we think 1 RX should be recommended for RedCap devices. |
| Intel | Y | Also, agree with the comment from FTW. |
| Nokia, NSB | Y |  |
| DOCOMO | Y |  |
| LG | Y | We can accept this proposal. Although we think the minimum should be 1Rx and the 2Rx should be optional if supported, we can discuss this later on. |
| CATT | Y | We can live with this for the sake of progress. |
| Lenovo, Motorola Mobility | Y |  |
| vivo | N | We think previous version (**Phase 1: Proposal 12-20**) which has been supported by almost all companies should be taken. |
| NEC | Y |  |
| CMCC | Y |  |
| ZTE | Y |  |
| OPPO |  | 1 RX shall be supported.  We don’t see the clear motivation to support 2RX for FDD FR1. |
| Samsung | N | We think 1 Rx should be recommended for Redcap devices.  We also support Proposal 12-20 |
| Sequans | Y |  |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | Y | Both 1 Rx and 2 Rx can be supported as the minimum capability. 2 Rx can support about 150Mbps DL peak data rate. |

**Phase 2: Question 12-30: Should RAN1 make a recommendation also regarding the minimum number of Rx branches of a RedCap UE for FR1 FDD bands where a non-RedCap UE is required to be equipped with a minimum of 4 Rx branches? If so, what should RAN1 recommend?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments** |
| ZTE |  | 1 Rx antenna is defined as the minimum number of Rx antennas. And 2 Rx antennas are supported as optional capability. |
| vivo | Y | Minimum number is 1 |
| SONY5 | Y | Minimum is 1 |
| FUTUREWEI | Y | Suggest to handle 4Rx FDD recommendation same as 4Rx TDD |
| Qualcomm | Y | 1 RX branch should be recommended by RAN1. |
| DOCOMO | N | The impact of reduced number of Rx branches for this case has not been evaluated. No recommendation is possible without any technical reasons. |
| InterDigital | Y | 1 Rx can be recomnended. |
| Sierra Wireless |  | 1 Rx as the minimum number of Rx antennas, and 2 Rx as optional capability. |
| Samsung | Y | 1 Rx |
| Ericsson | Y | Agree with Futurewei to recommend the same for the 4-Rx FR1 FDD cases as for the 4-Rx FR1 TDD cases. We are also fine with leaving this question to RAN4 WI phase. |
| Intel | Y | Considering impact on coverage performance and the tradeoff against UE complexity, 2Rx should be recommended.  On a related note, we propose to define 1 MIMO layer for this case (i.e., 2Rx) and support of max 2 DL MIMO layers can be optional RedCap UE feature. |
| Spreadtrum | Y | 1 Rx can be recomnended. |
| OPPO | Y | 1RX shall be recommended as in FR1 TDD. |
| Xiaomi |  | 1Rx is the basline, 2Rx can be optionally supported |
| CATT |  | We can handle this case referring to the 4Rx TDD case |
| Huawei, HiSilicon | N |  |
| FL | This question may be revisited later in this meeting. | |
|  |  |  |

**Phase 1: Proposal 12-40: Support that the minimum number of Rx branches of a RedCap UE is at least reduced from 4 to 2 for FR1 TDD bands where a non-RedCap UE is required to be equipped with a minimum of 4 Rx branches. Further reduction to 1 Rx is FFS.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | Y with minor | **Support that the ~~minimum~~ number of Rx branches of a RedCap UE ~~is~~ at least can be reduced from 4 to 2 for FR1 TDD bands where a non-RedCap UE is required to be equipped with a minimum of 4 Rx branches. Further reduction to 1 Rx is FFS.** |
| CATT | Y | Also fine to wait for conclusions from cost evaluations of combinations. |
| CMCC | Y |  |
| LG | N | No differentiation within the FR1 (b/w FDD and TDD, or b/w low and high frequency bands) is preferred as the low-end wearables and sensors which would have the most benefits from 1Rx will need to be deployed in the entire NR operating bands in FR1.  Our preference is to support 1 Rx also for this case. |
| ZTE |  | 1 Rx antenna is defined as the minimum number of Rx antennas. And 2 Rx antennas are supported as optional capability. |
| vivo | N | Agree with LG and ZTE |
| Nokia, NSB | Y |  |
| SONY5 | N | Agree with LG, ZTE, vivo |
| FUTUREWEI | Y | If a company says N to this proposal it actually means they do not support any reduction. “At least” covers 2RX and maybe 1RX. |
| Qualcomm | N | Min(1, 2)=1. Therefore,1 RX branch should be the minimum number recommended by RAN1. This is to ensure the wearable devices with 1 RX branch can operate in both TDD bands and FDD bands of FR1.  2 RX branches can be supported as an optional UE capability for RedCap devices. |
| DOCOMO | Y |  |
| InterDigital | N | Agree with LG; 1 Rx should be supported. |
| Sierra Wireless |  | 1 Rx as the minimum number of Rx antennas, and 2 Rx as optional capability. |
| Samsung | N | Support 1Rx for FR1 TDD bands |
| Ericsson | Y | We prefer 2 Rx in all 4-Rx FR1 TDD bands. It should be clarified that this is a RAN1 recommendation. Per-band Rx requirements should be specified in RAN4. |
| Sharp | Y |  |
| Intel | Y | Also, this case can be handled the same way as FR1 FDD bands with non-RedCap UE requirement of 4Rx (Question 12-30). |
| OPPO | N | Support 1Rx for FR1 TDD bands. Agree with LG. In addition, it shall consider to support wearables with 1RX. |
| NEC | Y | “at least” would cover Rx also if feasible. Support of 1 Rx might require feasibility study by RAN4. |
| Xiaomi | N | Same view with LG, ZTE, vivo, 1Rx should be supported |
| FL | Based on received responses, the following proposal can be considered as a way forward.  **FL1: Phase 1: Proposal 12-41: Recommend that the specification supports RedCap UEs with *N* Rx branches for FR1 TDD bands where a non-RedCap UE is required to be equipped with a minimum of 4 Rx branches. *N*=2 is supported, and *N*=1 is FFS.** | |
| FUTUREWEI2 | Y |  |
| MediaTek | Y | We have strong concerns on reducing the #Rx from 4 to 1. This has significant impact to the system spectral efficiency. As we have shown in our Tdoc R1-2009543, the resources usage for DL control (PDCCH) will be doubled by adopting 1Rx compared to 2Rx. This will significantly increase the PDCCH blockage probability (e.g. AL8 probability increased from 2% to 32%). |
| Ericsson | Y |  |
| Qualcomm | N | We think N=1 should be supported as the **minimum** number of RX branches.  As a compromise, we can accept the following proposal:  *For FR1 TDD bands where a non-RedCap UE is required to be equipped with a minimum of 4 Rx branches, recommend that the specification supports RedCap UEs with 1 Rx branch as well as RedCap UEs with 2 Rx branches.* |
| Intel | Y |  |
| Nokia, NSB | Y |  |
| DOCOMO | Y |  |
| LG | N | We think we need to support the RedCap UE with 1Rx also in this frequency band. We agree with Qualcomm in that the minimum should be 1Rx and the 2Rx can be supported in addition to 1Rx. Either the wording from the **FL1: Phase 1: Proposal 12-21** with the necessary changes, or the wording from QC would be okay to us as a way forward. |
| CATT | Y | We can live with this for the sake of progress. |
| SONY6 |  | We really would prefer that N=1 so that a 1 RX antenna device can work in both TDD and FDD bands. |
| Lenovo, Motorola Mobility | N | Similar view with LG. |
| vivo | N | We disagree with the updated proposal. We can accept the QC’s version as compromise. |
| NEC | Y |  |
| CMCC | Y | If N=1 is also supported as one of UE Rx branches capability, we are also fine with QC’s version. |
| ZTE | N | We show similar view as Qualcomm |
| OPPO | N | N=1 should be supported as the **minimum** number of RX branches.  We can accept Qualcomm’s suggested version as a compromise. |
| Samsung | N | We think N=1 should be supported as the **minimum** number of RX branches. |
| Sequans | Y |  |
| Huawei, HiSilicon | Y |  |
| Spreadtrum | N | Both 1 Rx and 2 Rx can be supported as the minimum capability. 1 Rx has benefit of lower cost. |

**Phase 2: Question 12-50: Should RAN1 make a recommendation also regarding the minimum number of Rx branches of a RedCap UE for FR1 TDD bands where a non-RedCap UE is required to be equipped with a minimum of 2 Rx branches? If so, what should RAN1 recommend?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments** |
| ZTE | Y | 1 Rx branch |
| vivo | Y | 1 Rx |
| SONY5 | Y | 1 RX |
| FUTUREWEI | Y | Suggest to handle 2Rx TDD recommendation same as 2Rx FDD |
| Qualcomm | Y | 1 RX branch |
| DOCOMO | N | The impact of reduced number of Rx branches for this case has not been evaluated. No recommendation is possible without any technical reasons. |
| InterDigital | Y | 1 Rx. |
| Sierra Wireless | Y | 1 Rx |
| Samsung | Y | 1Rx |
| Ericsson | Y | Agree with Futurewei to recommend the same for the 2-Rx FR1 TDD cases as for the 2-Rx FR1 FDD cases. We are also fine with leaving this question to RAN4 WI phase. |
| Sharp | Y | 1 Rx branch |
| Intel | Y | 1 Rx |
| Spreadtrum | Y | 1 Rx |
| OPPO | Y | 1RX |
| Xiaomi |  | 1Rx |
| CATT | Y | 1 Rx |
| Huawei, HiSilicon | N |  |
| FL | This question may be revisited later in this meeting. | |
|  |  |  |

**Phase 1: Proposal 12-60: Support that the minimum number of Rx branches of an FR2 RedCap UE is 1.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| CATT | Y | Also fine to wait for conclusions from cost evaluations of combinations. |
| LG | Y |  |
| ZTE | Y |  |
| vivo | Y |  |
| Nokia, NSB | Y |  |
| FUTUREWEI | almost | The results here seem not so stable, and we may need to discuss how much compensation we would apply in this case.  Our comment from the last FLS still applies … we may be ok to support 1RX as long as 2RX/2MIMO layers is also supported as part of UE capability signaling. |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| InterDigital | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Sharp | Y |  |
| Intel | Y |  |
| Spreadtrum | Y |  |
| OPPO | Y |  |
| NEC | Y |  |
| Xiaomi | Y |  |
| FL | Based on received responses, the following proposal can be considered as a way forward.  **FL1: Phase 1: Proposal 12-61: Recommend that the specification supports RedCap UEs with 1 Rx branch as well as RedCap UEs with 2 Rx branches for FR2 bands where a non-RedCap UE is required to be equipped with a minimum of 2 Rx branches.** | |
| FUTUREWEI2 | Y | We can accept this, though our preference as expressed in the GTW is to decide now that initial access is based on 1RX and 2RX can be indicated as a UE capability. |
| MediaTek | N | We don’t support the proposal. If we don’t define different RedCap UEs, the gNB will have to assume 1Rx RedCap UEs. So, not sure what this will add compared to mandating the UE to support at least 1 Rx.  We do not see a need to introduce market fragmentation, especially if the same approach is adopted to other reduction features.  We should down select between the two options (1Rx or 2Rx). |
| Ericsson | Y |  |
| Qualcomm | Y |  |
| Intel | Y |  |
| Nokia, NSB | N | We are not sure why 2Rx is needed here. As FL’s proposal is to support both 1Rx and 2Rx, we’d likely have to do coverage recovery for the 1Rx case anyway. So we don’t know why we need to also support 2Rx. |
| DOCOMO | Y |  |
| LG | Y | We can accept this proposal. We think 1Rx needs to be supported anyway perhaps with optional 2Rx, but we can discuss this later on. |
| CATT | Y | We can live with this for the sake of progress. |
| Lenovo, Motorola Mobility | Y |  |
| vivo | N | The previous version (**Phase 1: Proposal 12-60**) of proposal were supported by all companies, not sure the reason for the update. The previous one should be taken. |
| NEC | Y |  |
| CMCC | Y |  |
| ZTE | Y |  |
| OPPO |  | One RX shall be supported for FR2.  We don’t see clear motivation to support 2RX in FR2. |
| Samsung | N | We think N=1 should be supported as the **minimum** number of RX branches.  Same question as Vivo. We think we should go back to (**Phase 1: Proposal 12-60** |
| Huawei, HiSilicon | Y |  |

**Phase 1: Proposal 12-70: Support that the minimum number of supported DL MIMO layers of an FR1 FDD RedCap UE is 1.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | N | Wait. We envision that the support 2Rx&2Layers in FDD FR1 for RedCap is important. It should be decided together with the support of 1Rx&1 Layer. |
| CATT | Y | Also fine to wait for conclusions from cost evaluations of combinations. |
| LG | Y |  |
| ZTE | Y |  |
| vivo | Y |  |
| Nokia, NSB | Y |  |
| SONY5 | Y |  |
| FUTUREWEI | almost | 2RX/2MIMO layers also is supported by UE capability |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| InterDigital | Y |  |
| Sierra Wireless | Y |  |
| Samsung |  | No need to make recommendation for MIMO layer reduction itself. But OK with 1 Rx |
| Ericsson | Y |  |
| Sharp | Y |  |
| Intel | Y |  |
| Spreadtrum | Y |  |
| OPPO | Y |  |
| NEC | Y |  |
| Xiaomi | Y |  |
| FL | Based on received responses, the following proposal can be considered as a way forward.  **FL1: Phase 1: Proposal 12-71: Recommend that the specification supports RedCap UEs with max 1 DL MIMO layer as well as RedCap UEs with max 2 DL MIMO layers for FR1 FDD bands where a non-RedCap UE is required to be equipped with a minimum of 2 Rx branches.** | |
| FUTUREWEI | Y | We can accept this for progress, though more discussion may be needed later on the relation of RX and layer (e.g., is 2RX always 2 layer, or can also be 1 layer) |
| MediaTek | N | Number of DL MIMO layers should be the same as the #Rx. Please see our input to “FL1: Phase 1: Proposal 12-21”. |
| Ericsson | Y | We would also be fine to add a sub-bullet stating that the UE is not required to support a higher number of DL MIMO layers than the number of Rx branches, although it seems somewhat obvious. |
| Qualcomm | N | As far as UE capability is concerned for RedCap devices, we don’t support MIMO layer reduction beyond the number of RX antennas.  As a compromise, we can accept the following proposal:  *For FR1 FDD bands where a non-RedCap UE is required to be equipped with a minimum of 2 Rx branches, recommend that the specification supports RedCap UEs with 1 RX branch and max 1 DL MIMO layer.*  *FFS the support for RedCap UEs with 2 RX branches and max 2 DL MIMO layer for FR1 FDD bands where a non-RedCap UE is required to be equipped with a minimum of 2 Rx branches.* |
| Intel | Y | We support the proposal and do not agree to the idea that a UE should be mandated to support more than 1 layers for 2Rx cases, when there is no need from data rate perspective and can provide meaningful cost/complexity savings. |
| Nokia, NSB | Y | We think that the number of DL MIMO layers should be the same as the number of Rx antennas. But we are OK to accept this. |
| DOCOMO | Y | Share the same view with Intel |
| LG | Y | Also fine with the suggested addition from Ericsson. |
| CATT | Y | We can live with this for the sake of progress. |
| SONY6 | Y | Agree with Ericsson |
| Lenovo, Motorola Mobility | Y |  |
| vivo | N | The previous version (**Phase 1: Proposal 12-60**) of proposal were supported by all companies, not sure the reason for the update. The previous one should be taken. |
| NEC | Y |  |
| CMCC | Y |  |
| ZTE | Y | 2 MIMO layers could not be mandatory for 2Rx UE. |
| OPPO | N | The number of DL MIMO layers should be the same as the number of Rx antennas.  Agree with Qualcomm’s proposal as a compromise. |
| Samsung | N | We support 1 layer with 1 Rx.  We should agreed on # of Rx first and then discuss whether more relax of MIMO layer is needed or not.  We should go back to Proposal 12-60 |
| Sequans | Y | Same view as Intel |
| Huawei, HiSilicon | Y |  |
| Spreadtrum |  | Number of DL MIMO layers should be the same as the #Rx |

**Phase 1: Question 12-80: If RAN1 recommends 2 Rx for FR1 TDD, should RAN1 recommend 1 or 2 layers for FR1 TDD?**

|  |  |  |
| --- | --- | --- |
| **Company** | **1 or 2** | **Comments or suggested revisions** |
| Huawei, HiSilicon | Y | We are ok with #Layers=#Rx, i.e. 2 Layers. |
| CATT | 2 |  |
| CMCC | 2 layers |  |
| LG | 2 |  |
| ZTE |  | 1 MIMO layer is mandatory and 2 MIMO layers could be an optional capability. |
| vivo | 1 | Agree with ZTE |
| Nokia, NSB | 2 layers |  |
| SONY5 | 1 | Agree with ZTE, vivo |
| FUTUREWEI | 2 |  |
| Qualcomm |  | We don’t think DL MIMO layer reduction beyond the number of RX branches should be supported.  1 RX branch and 1 DL MIMO layer should be recommended as the minimum UE capabilities in FR1.  We are fine to support 2 RX branches and 2 DL MIMO layers as optional instead of minimum UE capabilities for RedCap devices. |
| DOCOMO |  | Agree with ZTE |
| InterDigital | Y | Agree with ZTE. |
| Sierra Wireless | 2 | Prefer to have # of layers = # Rx |
| Samsung |  | No need to make recommendation if # layer =# of Rx |
| Ericsson |  | No strong view |
| Sharp | 2 layers | As the combinations of complexity reduction techniques for evaluation, the number of layers is equal to the number of RXs. |
| Intel | 1 layer | 1 layer should be requirement; 2 layers can be UE capability for bands wherein UE is either: required to support, or optionally supports, 2Rx.  We do not agree to mandating 2 layers for FR1 TDD which is entirely unnecessary.  Also, the proposal as it stands, seems to indicate we might even end up requiring 2 layers in certain FR1 TDD bands with 1Rx support, but this may not be relevant if we go with 1 DL MIMO layer as the mandatory requirement. |
| Spreadtrum |  | Agree with ZTE |
| OPPO | 2 layers | What is the motivation to support 2Rx in FR1 TDD?  If it is for boosting peak data rate, 2 layer shall be supported for UE with 2RX. |
| NEC | 1 or 2 | Capability per CC |
| Xiaomi |  | Same view with ZTE |
| FL | Based on received responses, the following proposal can be considered as a way forward.  **FL1: Phase 1: Proposal 12-80: Recommend that the specification supports RedCap UEs with max 1 DL MIMO layer as well as RedCap UEs with max 2 DL MIMO layers for FR1 TDD bands where a non-RedCap UE is required to be equipped with a minimum of 4 Rx branches.** | |
| FUTUREWEI | Y | We can accept this for progress, though more discussion may be needed later on the relation of RX and layer (e.g., is 2RX always 2 layer, or can also be 1 layer) |
| MediaTek | N | DL MIMO layers reduction beyond the number of Rx branches shouldn’t be supported. |
| Ericsson | Y | We would also be fine to add a sub-bullet stating that the UE is not required to support a higher number of DL MIMO layers than the number of Rx branches, although it seems somewhat obvious. |
| Qualcomm | Y partially | For clarity, we suggest the following changes for this proposal:  *For FR1 TDD bands where a non-RedCap UE is required to be equipped with a minimum of 4 Rx branches, recommend that the specification supports RedCap UEs with max 1 DL MIMO layer and 1 RX branch, as well as RedCap UEs with max 2 DL MIMO layers and 2 RX branches.* |
| Intel | Y |  |
| Nokia, NSB | Y | We think that the number of DL MIMO layers should be the same as the number of Rx antennas. But we are OK to accept this. |
| DOCOMO | Y |  |
| LG | Y | Also okay with the suggested addition from Ericsson. |
| CATT | Y | We can live with this for the sake of progress. |
| SONY6 | Y | Agree with Ericsson |
| Lenovo, Motorola Mobility | Y |  |
| vivo | N | The proposal regarding MIMO layer should be pending until the conclusion of Rx antenna is made. |
| NEC | Y |  |
| CMCC | N | The number of layers should equals with number of Rx branches. |
| ZTE | Y |  |
| OPPO | N | Agree with vivo we shall firstly wait for the result of the discussion on the number of supported Rx in FR2.  In addition, the number of the maximum MIMO layer shall be the same as the number of supported Rx. There is no clear motivation to support smaller maximum MIMO layer than the number of supported Rx. |
| Samsung | N | We think N=1 should be supported together with 1Rx as the **minimum** number of RX branches.  We should agreed on # of Rx first and then discuss whether more relax of MIMO layer is needed or not. |
| Sequans | Y\* | Maybe with minor modification, to be aligned with conclusion proposals on Rx branches:  *Recommend that the specification supports RedCap UEs with ~~max~~ 1 DL MIMO layer as well as RedCap UEs with ~~max~~ 2 DL MIMO layers for FR1 TDD bands where a non-RedCap UE is required to be equipped with a minimum of 4 Rx branches.* |
| Huawei, HiSilicon | FFS |  |
| Spreadtrum |  | Number of DL MIMO layers should be the same as the #Rx |

**Phase 1: Proposal 12-90: Support that the minimum number of supported DL MIMO layers of an FR2 RedCap UE is 1.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| CATT | Y | Also fine to wait for conclusions from cost evaluations of combinations. |
| LG | Y |  |
| ZTE | Y |  |
| vivo | Y |  |
| Nokia, NSB | Y |  |
| FUTUREWEI | almost | 2RX/2MIMO layers also is supported by UE capability |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| InterDigital | Y |  |
| Sierra Wireless | Y |  |
| Samsung |  | No need to make recommendation for MIMO layer reduction itself. But OK with 1 Rx |
| Ericsson | Y |  |
| Sharp | Y |  |
| Intel | Y |  |
| Spreadtrum | Y |  |
| OPPO | Y |  |
| NEC | Y |  |
| Xiaomi | Y |  |
| FL | Based on received responses, the following proposal can be considered as a way forward.  **FL1: Phase 1: Proposal 12-91: Recommend that the specification supports RedCap UEs with max 1 DL MIMO layer as well as RedCap UEs with max 2 DL MIMO layers for FR2 bands where a non-RedCap UE is required to be equipped with a minimum of 2 Rx branches.** | |
| FUTUREWEI | Y | We can accept this for progress, though more discussion may be needed later on the relation of RX and layer (e.g., is 2RX always 2 layer, or can also be 1 layer) |
| MediaTek | N | DL MIMO layers reduction beyond the number of Rx branches shouldn’t be supported. |
| Ericsson | Y | We would also be fine to add a sub-bullet stating that the UE is not required to support a higher number of DL MIMO layers than the number of Rx branches, although it seems somewhat obvious. |
| Qualcomm |  | We suggest the following changes for this proposal:  *For FR2 bands where a non-RedCap UE is required to be equipped with a minimum of 2 Rx branches, recommend that the specification supports RedCap UEs with max 1 DL MIMO layer and 1 RX branch, as well as RedCap UEs with max 2 DL MIMO layers and 2 RX branches.* |
| Intel | Y |  |
| Nokia, NSB | N | As we don’t support 2Rx for FR2, we do not support 2 DL MIMO layers here. |
| DOCOMO | Y |  |
| LG | Y | Also okay with the suggested addition from Ericsson. |
| CATT | Y | We can live with this for the sake of progress. |
| Lenovo, Motorola Mobility | Y |  |
| vivo | N | First of all, no sure what is the intention to change the proposal from the previous one which has been supported by all companies.  Secondly, the proposal regarding MIMO layer should be pending until the conclusion of Rx antenna is made. |
| NEC | Y |  |
| ZTE | N | We cannot see the necessity to support two layers since one layer can meet the peak data requirement |
| OPPO | N | Agree with vivo we shall firstly wait for the result of the discussion on the number of supported Rx in FR2.  In addition, the number of the maximum MIMO layer shall be the same as the number of supported Rx. There is no clear motivation to support smaller maximum MIMO layer than the number of supported Rx. |
| Samsung | N | As we don’t support 2Rx for FR2, we do not support 2 DL MIMO layers here.  We should agreed on # of Rx first and then discuss whether more relax of MIMO layer is needed or not. |
| Sequans | Y\* | \*Same comment as for 4Rx case above:  *Recommend that the specification supports RedCap UEs with ~~max~~ 1 DL MIMO layer as well as RedCap UEs with ~~max~~ 2 DL MIMO layers for FR1 TDD bands where a non-RedCap UE is required to be equipped with a minimum of 2 Rx branches.* |
| Spreadtrum |  | Number of DL MIMO layers should be the same as the #Rx |

**Phase 1: Proposal 12-100: Recommend that HD-FDD type B is not supported for RedCap FR1 FDD UEs.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | Y |  |
| CATT | Y |  |
| CMCC | Y |  |
| LG | N | We don’t think this proposal is not needed. For the HD-FDD, **Proposal 12-110** seems to be enough. |
| ZTE | Y |  |
| vivo | Y |  |
| Nokia, NSB | Y |  |
| SONY5 | Y | We think that HD-FDD Type A is more important than HD-FDD Type B. While we prefer a single HD-FDD type, we don’t have a big aversion to HD-FDD Type B. |
| FUTUREWEI | Y | This seems to be aligned with the vast majority of companies results and preference |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| Samsung | N | No need to make recommendation to not support HD-FDD type B |
| Ericsson | Y |  |
| Sharp | Y |  |
| Spreadtrum | Y |  |
| OPPO | Y |  |
| FL | This question will be revisited later in this meeting. | |
|  |  |  |

**Phase 1: Proposal 12-110: Recommend that HD-FDD type A is optionally supported for RedCap FR1 FDD UEs.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | FFS | We have some questions for better understanding the cost saving of HD-FDD type A. Unless they are clarified, we don’t see clear benefits justifying the recommendation of Type A. It is not about different UE implementations, rather, there seems to be mis-calculation in most of others results that can significantly impact the observations for cost saving (see our comments regarding Duplexer v.s filters inside/outside the duplexer).  The performance in terms of coverage, capacity, and latency etc. shuld be clear for Type A, i.e. less than FD-HDD. Of course, similar to the doubled processing time, this can be minimized by network control.  The spec impact can be depending. Current spec only support HD operation for CA/DC/SUL case where an advanced UE is assumed. With redcued capability and introducing HD-FDD to single cell FDD band, new UE behavior such as partial canclation should be defined. This is not trivial since NR supports mini-slot based scheduling, unlike LTE subframe-based where canclation can be easier.  We think FD-FDD is at least supported/recommended. |
| CATT | Y | We are OK if type A HD-FDD is an optional feature. |
| LG | Y(Partially) | Do we need “optionally” in this proposal? Unless we can assume those proposals without “optionally” as “mandatory” or “not optional” now, it is suggested to remove the “optionally” in the proposal. |
| ZTE | Y |  |
| vivo |  | No strong view. Also fine with not recommend HD-FDD Type A |
| Nokia, NSB | Y |  |
| SONY5 | Y (partially) | Agree with LG. Do we need “optionally” at this stage?  There seems to be a high degree of agreement among companies, maybe with one outlier, that there is an RF cost saving of about 15% for HD-FDD. |
| FUTUREWEI | N | This is stronger than the last FLS proposal … optional means all the spec impacts will have to be worked on, perhaps at the expense of a feature that applies to all bands of interest. Can consider more if type B is clearly not recommended and the spec impacts are made clear and we see some of the recommendations for e.g. N1/N2, modulation, etc. |
| Qualcomm | Y (partially) | Agree with the comments of LG and Sony.  If a RedCap UE supports FD-FDD, it has no issue to support HD-FDD type A. Therefore, we don’t need to include “optional” here. HD-FDD type A should be supported as a mandatory instead of optional UE capability. |
| DOCOMO | Y |  |
| InterDigital | Y |  |
| Sierra Wireless | Y (partially) | Perhaps “optionally” is not needed at this stage.  The cost saving of HD-FDD for a real-world device that operates in multiple bands is significant. The single band analysis that is used in this study does not accurately reflect on this. The fact that HD-FDD results accumulate across bands on a multi-band device should not be lost.  For each FDD band, a FD-FDD device needs to have an expensive RF duplexer. Whereas with the HD-FDD a cheap switch can be used. This is one of the benefits of TDD, NB-IOT, and LTE-M.  As for the filter, from our analysis, if you use two separate components for the switch and low pass filter, the filter is around 1/10th of the price of the switch. If you use an integrated switch and filter part, the additional cost of filter is very insignificant. |
| Samsung | Y |  |
| Ericsson |  | No strong view. However, if HD-FDD type A is supported in the specification for RedCap UEs, then FD-FDD should also be supported in the specification for RedCap UEs, and then it is probably FD-FDD that should be considered the optional feature rather than HD-FDD type A (since gNB might have no choice but to treat the UE as a HD-FDD type A UE until the UE has reported its FD-FDD capability). |
| Sharp | Y |  |
| Intel | Y (partially) | Agree with LG and others that the current wording could be improved a bit in context of SI recomendations.  We propose to replace “is optionally supported” with “can be supported”, and then leave the optional/mandatory support details for the normative phase. |
| Spreadtrum | Y (partially) | Agree with LG |
| OPPO | Y | No strong views |
| Xiaomi | Y |  |
| FL | This question will be revisited later in this meeting. | |
|  |  |  |

**Phase 1: Question 12-120: Should the TR recommend relaxed UE processing time in terms of N1/N2 for RedCap UEs?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | Y | It should be clear that the cost saving from doubled N1/N2 can be obvious based on different implementation (ours is 5.5% referring to reference UE, which is several $ for an IoT device!). It also has a benefit to be applicable to all FDD, TDD, FR1 and FR2. For the UE vendors do not want to implement this, capability#1 can be reused but certain choise for achieveing an even cheaper RedCap without penalty on network performance should be allowed.  The impact of doubled N1/N2 to network scheduler can be minimized by access control or early identification. Or can be comparable to the impact of other reduced capabilities, e.g. the potential support of 1Rx leads to many UEs without MIMO supported, the potential support of HD-FDD lead to TDD-like scheduling for a FDD network (which scheduler is different from TDD).  The spec impact of introducing doubled N1/N2 is expected to be small – introducing the new values only in sections for defining N1/N2 so other sections referring to N1/N2 can remain unchanged. |
| CATT | N | 1) No significant cost reduction in consensus.  2) At the cost of increasing the scheduling complexity of gNB, inevitably.  3) Have negative and complex impact on Msg2/3/4 scheduling, if RedCap UE cannot be identified early. |
| LG | Y |  |
| ZTE | Y |  |
| vivo | Y |  |
| Nokia, NSB | N | No meaningful cost reduction and there may be an impact to legacy UEs as the timing between RAR grant and Msg3 depends on N1 and N2 values |
| SONY5 | N | The cost saving doesn’t merit including this feature. |
| FUTUREWEI |  | This is a small reduction that can be discussed with several others that are similar. |
| Qualcomm | N |  |
| DOCOMO | N | Agree with CATT |
| InterDigital | Y |  |
| Sierra Wireless | FFS | The current analysis shows that N1/N2 only reduces cost by ~1.5% e.g.   * 20 MHz, 1 layer, 1 Rx, relaxed mods = 43.9% * 20 MHz, 1 layer, 1 Rx, relaxed mods, double N1/N2 = 42.4%   Only a single band UE was used for the study, but real-world devices all support multiple bands. And this cost saving does not multiply when more RF bands are added so when e.g. 20 bands are supported the % saving would be even smaller. |
| Samsung |  | Wait until the summary of combinations. |
| Ericsson | N | The relatively small potential cost reduction from relaxed N1/N2, especially when the technique is in a combination with other complexity reduction techniques that reduce the baseband complexity, does not seem to be worth the identified impacts on scheduling flexibility, etc. |
| Sharp | Y |  |
| Intel | Y | We support the recommendation.  On gNB scheduler complexity, considering we already have two timelines and many other separate margins and special cases, the effective impact to scheduler complexity compared to what it may need to handle already is unclear.  On RedCap UE identification, this may anyway be necessary for coverage purposes. Thus, the timing relaxation can be accommodated using the same framework, and there would be no adverse impact to legacy UE in terms of initial access.  On the gain margins, in isolation this technique offers similar (if not higher) gains w.r.t. reference UE as for some others (e.g., max modulation orders, within which DL and UL were coupled), and thus, should be considered similarly, not based on a particular order of consideration of the relaxations. |
| Spreadtrum | Y |  |
| OPPO | Y |  |
| FL | This question will be revisited later in this meeting. | |
|  |  |  |

**Phase 1: Question 12-130: Should the TR recommend relaxed maximum mandatory DL modulation (from 256QAM to 64QAM) for FR1 RedCap UEs?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | Y |  |
| CATT | Y | About 6% cost reduction can be achieved (evaluated individually), and the highest required DL data rate can still be fulfilled. |
| CMCC | Y |  |
| ZTE | Y | No need to support 256QAM |
| vivo | Y |  |
| Nokia, NSB | N | Small cost reduction and some impact to efficiency (~6.4% reduction in spectral efficiency based on our analysis) |
| SONY | N | The cost saving doesn’t merit including this feature. |
| FUTUREWEI |  | This is a small reduction that can be discussed with several others that are similar.  The proposal should be to recommend that 256QAM DL is optional instead of mandatory. (If you already supported 256QAM efficiently in your chipset you should be able to keep supporting.) |
| Qualcomm | Y |  |
| DOCOMO | Y |  |
| InterDigital | Y |  |
| Sierra Wireless | Y |  |
| Samsung | Y |  |
| Ericsson | Y |  |
| Sharp | Y |  |
| Intel | Y |  |
| Spreadtrum | Y |  |
| OPPO | Y |  |
| NEC | Y |  |
| LG | Y |  |
| FL | This question will be revisited later in this meeting. | |
|  |  |  |

**Phase 1: Question 12-140: Should the TR recommend relaxed maximum mandatory UL modulation (from 64QAM to 16QAM) for FR1 RedCap UEs?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | N |  |
| CATT | N | We do not want to make the RedCap UE even weaker than a legacy LTE UE, which has already mandatorily support 64QAM in UL. This is against the SID direction.  Only 1~2% cost reduction can be achieved (evaluated individually), and has significant negative impact on UL SE. |
| CMCC | N | Same view as CATT |
| ZTE | Y |  |
| vivo | Y | To respond CATT, 64QAM for UL was a very late feature even for LTE, RAN4 requirement was defined late. Therefore there are many LTE UEs actually not supporting 64QAM in UL |
| Nokia, NSB | N | Very small cost reduction and significant impact to efficiency (~23.6% reduction in spectral efficiency based on our analysis) |
| SONY | N | The cost saving doesn’t merit including this feature. |
| FUTUREWEI | N |  |
| Qualcomm | Y |  |
| DOCOMO | N | Agree with CATT |
| InterDigital | N |  |
| Sierra Wireless | Y | Only a single band UE was used for the study, but real-world devices all support multiple bands. And this cost saving DOES multiply when more RF bands are added so when e.g. 20 bands are supported the % saving would be great then the 1-2% the current evaluation is indicating. |
| Samsung | Y |  |
| Ericsson |  | No strong view. We are fine with or without relaxed maximum mandatory UL modulation. |
| Sharp | N | Agree with CATT. No significant reduction. As even in individual evaluation, there is roughly 2% reduction. In addition, it would also impact the current usage of MCS table for uplink. |
| Intel | N |  |
| Spreadtrum | Y |  |
| OPPO | Y | There is cost reduction. And the spec. impact is expected to be minor. |
| FL | This question will be revisited later in this meeting. | |
|  |  |  |

**Phase 1: Question 12-150: Should the TR recommend relaxed maximum mandatory DL modulation (from 64QAM to 16QAM) for FR2 RedCap UEs?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | N |  |
| CATT | N | It is justified for the network to schedule RedCap UE with 64QAM when the SINR is high, to guarantee the DL SE. |
| CMCC | N |  |
| ZTE | Y | 16QAM is mandatory and 64QAM could be optional. |
| vivo | Y |  |
| Nokia, NSB | N |  |
| SONY | N | The cost saving doesn’t merit including this feature. |
| FUTUREWEI |  | The recommendation should be 64QAM is optional instead of mandatory. |
| Qualcomm | N |  |
| DOCOMO | N |  |
| InterDigital | N |  |
| Samsung | Y |  |
| Ericsson |  | No strong view |
| Sharp | N |  |
| Intel | N |  |
| OPPO | Y |  |
| FL | This question will be revisited later in this meeting. | |
|  |  |  |

**Phase 1: Question 12-160: Should the TR recommend relaxed maximum mandatory UL modulation (from 64QAM to 16QAM) for FR2 RedCap UEs?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments or suggested revisions** |
| Huawei, HiSilicon | N |  |
| CATT | N | It is justified for the network to schedule RedCap UE with 64QAM when the SINR is high, to guarantee the UL SE. In addition, the cost reduction of UL modulation order relaxation is too small (1~2% by indivitually evaluation). |
| CMCC | N |  |
| ZTE | Y |  |
| vivo | Y |  |
| Nokia, NSB | N |  |
| SONY | N | The cost saving doesn’t merit including this feature. |
| FUTUREWEI | N |  |
| Qualcomm | N |  |
| DOCOMO | N |  |
| InterDigital | N |  |
| Samsung | Y |  |
| Ericsson |  | No strong view. We are fine with or without relaxed maximum mandatory UL modulation. |
| Sharp | N |  |
| Intel | N |  |
| OPPO | Y | There is cost reduction. And the spec. impact is expected to be minor. |
| FL | This question will be revisited later in this meeting. | |
|  |  |  |

# References

|  |  |  |  |
| --- | --- | --- | --- |
| [1] | [R1-2008837](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2008837.zip) | Potential UE complexity reduction features for RedCap (revision of [R1-2007529](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2007529.zip)) | Ericsson |
| [2] | [R1-2007534](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2007534.zip) | Complexity reduction features for RedCap UEs | FUTUREWEI |
| [3] | [R1-2009318](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2009318.zip) | Potential UE complexity reduction features (revision of [R1-2007596](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2007596.zip)) | Huawei, HiSilicon |
| [4] | [R1-2009212](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009212.zip) | Complexity reduction for Reduced Capability NR devices (revision of [R1-2007668](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2007668.zip)) | vivo, Guangdong Genius |
| [5] | [R1-2007715](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2007715.zip) | Potential UE complexity reduction features | ZTE |
| [6] | [R1-2007862](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2007862.zip) | Discussion on UE complexity reduction features | CATT |
| [7] | [R1-2007887](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2007887.zip) | Potential UE complexity reduction features | TCL Communication Ltd. |
| [8] | [R1-2009025](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009025.zip) | On potential UE complexity reduction features for RedCap (revision of [R1-2007947](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2007947.zip)) | Intel Corporation |
| [9] | [R1-2008016](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008016.zip) | Discussion on UE complexity reduction features | CMCC |
| [10] | [R1-2008048](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008048.zip) | Discussion on potential UE complexity reduction features | LG Electronics |
| [11] | [R1-2008068](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008068.zip) | UE complexity reduction features | Nokia, Nokia Shanghai Bell |
| [12] | [R1-2008857](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008857.zip) | Discussion on the complexity reduction for reduced capability device (revision of [R1-2008084](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008084.zip)) | Xiaomi |
| [13] | [R1-2008100](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008100.zip) | Discussion on potential UE complexity reduction features | Spreadtrum Communications |
| [14] | [R1-2008114](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008114.zip) | Discussion on bandwidth related features for RedCap devices | NEC |
| [15] | [R1-2008875](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008875.zip) | UE complexity reduction (revision of [R1-2008170](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008170.zip)) | Samsung |
| [16] | [R1-2008260](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008260.zip) | Discussion on UE complexity reduction | OPPO |
| [17] | [R1-2008294](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008294.zip) | UE complexity reduction features for RedCap | Lenovo, Motorola Mobility |
| [18] | [R1-2008315](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008315.zip) | Reduced Capability UE Complexity Reduction Features | Sierra Wireless, S.A. |
| [19] | [R1-2008366](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008366.zip) | On potential complexity reduction techniques for NR devices | Sony |
| [20] | [R1-2008382](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008382.zip) | Discussion on potential UE complexity reduction features | Panasonic Corporation |
| [21] | [R1-2008394](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008394.zip) | Discussion on Potential UE complexity reduction features | Sharp |
| [22] | [R1-2008469](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008469.zip) | Potential UE complexity reduction features for RedCap | Apple |
| [23] | [R1-2009543](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2009543.zip) | On complexity reduction features for NR RedCap UEs (revision of [R1-2008510](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008510.zip)) | MediaTek Inc. |
| [24] | [R1-2008551](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008551.zip) | Discussion on potential UE complexity reduction features for RedCap | NTT DOCOMO, INC. |
| [25] | [R1-2008581](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008581.zip) | Discussion on potential UE complexity reduction features | ASUSTeK |
| [26] | [R1-2008620](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008620.zip) | Complexity Reduction for RedCap Devices | Qualcomm Incorporated |
| [27] | [R1-2008684](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008684.zip) | UE complexity reduction features for reduced capability NR devices | InterDigital, Inc. |
| [28] | [R1-2008738](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008738.zip) | Complexity reduction features for RedCap UE | Sequans Communications |
| [29] | [R1-2007599](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2007599.zip) | Framework and principles for reduced capability devices | Huawei, HiSilicon |
| [30] | [R1-2007671](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2007671.zip) | Framework and Principles for Reduced Capability NR devices | vivo, Guangdong Genius |
| [31] | [R1-2008019](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008019.zip) | Discussion on design principles and definition for RedCap device type | CMCC |
| [32] | [R1-2008101](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008101.zip) | Discussion on Framework and Principles for Reduced Capability | Spreadtrum Communications |
| [33] | [R1-2008623](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008623.zip) | Standardization Framework and Design Principles for NR RedCap Devices | Qualcomm Incorporated |
| [34] | [R1-2008741](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_103-e/Docs/R1-2008741.zip) | Framework and principles for RedCap UE | Sequans Communications |
| [35] | [R1-2007482](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_102-e/Docs/R1-2007482.zip) | FL summary on initial collection of RedCap evaluation results | Moderator (Ericsson, Apple, Qualcomm) |
| [36] | [RP-201677](https://www.3gpp.org/ftp/tsg_ran/TSG_RAN/TSGR_89e/Docs/RP-201677.zip) | Revised SID on Study on support of reduced capability NR devices | Ericsson |
| [37] | [RP-201676](https://www.3gpp.org/ftp/tsg_ran/TSG_RAN/TSGR_89e/Docs/RP-201676.zip) | SR for Study on support of reduced capability NR devices | Ericsson |
| [38] | [R1-2007476](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_102-e/Docs/R1-2007476.zip) | FL summary #1 for RedCap evaluation templates | Moderator (Ericsson, Apple, Qualcomm) |