**3GPP TSG RAN WG1 #106bis-e** **R1-210xxxx**

**e-Meeting, October 11th – 19th, 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **DRAFT CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.213** | **CR** |  | **rev** |  | **Current version:** | **16.7.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Introduction of UEs with reduced capabilities in NR | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Samsung | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | | 2021-11-01 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Introduction of UEs with reduced capabilities in NR. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add description related to operation of RedCap UEs. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incomplete support for UEs with reduced capabilities in NR. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 17 (new) | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 38.211, TS 38.212, TS 38.214 | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\*\*\* Unchanged text is omitted \*\*\*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications"

[2] 3GPP TS 38.201: "NR; Physical Layer – General Description"

[3] 3GPP TS 38.202: "NR; Services provided by the physical layer"

[4] 3GPP TS 38.211: "NR; Physical channels and modulation"

[5] 3GPP TS 38.212: "NR; Multiplexing and channel coding"

[6] 3GPP TS 38.214: "NR; Physical layer procedures for data"

[7] 3GPP TS 38.215: "NR; Physical layer measurements"

[8-1] 3GPP TS 38.101-1: "NR; User Equipment (UE) radio transmission and reception; Part 1: Range 1 Standalone"

[8-2] 3GPP TS 38.101-2: "NR; User Equipment (UE) radio transmission and reception; Part 2: Range 2 Standalone"

[8-3] 3GPP TS 38.101-3: "NR; User Equipment (UE) radio transmission and reception; Part 3: Range 1 and Range 2 Interworking operation with other radios"

[9] 3GPP TS 38.104: "NR; Base Station (BS) radio transmission and reception"

[10] 3GPP TS 38.133: "NR; Requirements for support of radio resource management"

[11] 3GPP TS 38.321: "NR; Medium Access Control (MAC) protocol specification"

[12] 3GPP TS 38.331: "NR; Radio Resource Control (RRC); Protocol specification"

[13] 3GPP TS 36.213: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical layer procedures"

[14] 3GPP TS 36.321: "Evolved Universal Terrestrial Radio Access (E-UTRA); Medium Access Control (MAC) protocol specification"

[15] 3GPP TS 37.213: "Physical layer procedures for shared spectrum channel access"

[16] 3GPP TS 38.473: "F1 application protocol (F1AP)"

[17] 3GPP TS 38.304: "NR; User Equipment (UE) procedures in Idle mode and RRC Inactive state"

[18] 3GPP TR 38.822: "NR; User Equipment (UE) feature list"

\*\*\* Unchanged text is omitted \*\*\*

## 17 UE with reduced capabilities

A UE with reduced capabilities (RedCap UE) supports all Layer-1 UE features that are mandatory without capability signalling as described in [18, TR 38.822].

## 17.1 RedCap UE procedures

Procedures for a RedCap UE are same as described for a UE in all other clauses of this document unless stated otherwise.

A RedCap UE expects the initial DL BWP and the active DL BWP after the RedCap UE (re)establishes dedicated RRC connection to be smaller than or equal to the maximum DL bandwidth that the UE supports. A RedCap UE can be provided a DL BWP by *initialDownlinkBWP* in *DownlinkConfigCommonRedCapSIB*, and an UL BWP by *initialUplinkBWP* in *UplinkConfigCommonRedCapSIB*.

## 17.2 Half-Duplex UE in paired spectrum

A half-duplex UE (HD-UE) in paired spectrum is not capable of simultaneous transmissions and receptions on a serving cell with paired spectrum. This clause is applicable for communication of a HD-UE on a serving cell with paired spectrum.

A HD-UE does not expect to detect a first DCI format scheduling a reception in a set of symbols of a slot and detect a second DCI format scheduling a transmission in the set of symbols of the slot.

If a HD-UE is configured by higher layers to receive a PDCCH, or PDSCH, or CSI-RS, or DL PRS in a set of symbols of a slot, the HD-UE receives the PDCCH, or PDSCH, or CSI-RS, or DL PRS if the HD-UE does not detect a DCI format that indicates to the HD-UE to transmit a PUSCH, or PUCCH, or PRACH, or SRS in at least one symbol of the set of symbols of the slot; otherwise, the HD-UE does not receive the PDCCH, or PDSCH, or CSI-RS, or DL PRS in the set of symbols of the slot. The HD-UE is not required to monitor PDCCH for detection of a DCI format 2\_4.

If a HD-UE is configured by higher layers to transmit SRS, or PUCCH, or PUSCH, or PRACH in a set of symbols of a slot and the UE detects a DCI format indicating to the HD-UE to receive CSI-RS or PDSCH in a subset of symbols from the set of symbols, then

- the HD-UE does not expect to cancel the transmission of the PUCCH or PUSCH or PRACH in the set of symbols if the first symbol in the set occurs within relative to a last symbol of a CORESET where the HD-UE detects the DCI format; otherwise, the HD-UE cancels the PUCCH, or the PUSCH, or an actual repetition of the PUSCH [6, TS38.214], determined from clauses 9 and 9.2.5 or clause 6.1 of [6, TS38.214], or the PRACH transmission in the set of symbols.

- the HD-UE does not expect to cancel the transmission of SRS in symbols from the subset of symbols that occur within relative to a last symbol of a CORESET where the HD-UE detects the DCI format. The HD-UE cancels the SRS transmission in remaining symbols from the subset of symbols.

is the PUSCH preparation time for UE processing capability 1 [6, TS 38.214] assuming and corresponds to the smallest SCS configuration between the SCS configuration of the PDCCH carrying the DCI format and the SCS configuration of the SRS, PUCCH, PUSCH or , where corresponds to the SCS configuration of the PRACH if it is 15 kHz or larger; otherwise .

A HD-UE does not expect to receive both dedicated higher layer parameters configuring transmission in a set of symbols of a slot and dedicated higher layer parameters configuring reception in the set of symbols of the slot. A HD-UE does not expect to receive both a Type-0/0A/1/2-PDCCH CSS set configuration for PDCCH reception in a set of symbols of a slot and dedicated higher layer parameters configuring transmission in the set of symbols of the slot.

If a HD-UE would transmit a PUSCH, or PUCCH, or SRS in a slot based on a configuration by higher layers and the HD-UE is indicated presence of SS/PBCH blocks by *ssb-PositionsInBurst* in *SIB1* or in *ServingCellConfigCommon* in a set of symbols of the slot, the HD-UE does not transmit PUSCH or PUCCH in the slot if a transmission would overlap with any symbol from the set of symbols and the HD-UE does not transmit SRS in the set of symbols of the slot.