**3GPP TSG-RAN WG1 Meeting #108-e R1-220XXXX**

**e-Meeting, February 21 – March 3, 2022**

**Agenda Item: 5**

**Source: Moderator (Huawei)**

**Title: Summary of [108-e-R16-V2X-08] Addition of Rel-16 NR V2X bands to TR 37.985**

**Document for: Discussion and Decision**

# Introduction

This document is created to collect company views on the [draft CR in [1]](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_108-e/Docs/R1-2202442.zip), to address an omission in   
[TR 37.985](https://www.3gpp.org/ftp/Specs/archive/37_series/37.985/37985-g00.zip) v16.0.0.

# Background

The LTE part of TR 37.985 summarizes in clause 5.1.3 the RAN4 listing of bands for PC5 operation (b47), and concurrent PC5-Uu operation, taken from TS 36.101 clause 5.5G. It also, separately, discusses   
LTE-V SL CA.

The equivalent listing of NR PC5 bands and PC5-Uu concurrent operation for NR was omitted in the   
Rel-16 TR, meaning the TR gives an incomplete understanding of Rel-16 technology to external readers, and is inconsistent between LTE-V2X and NR-V2X.

Recalling that this TR is supposed to give an overview of 3GPP V2X technologies to external organizations (hence the 900-series number), it is important not to omit this information of relevance to the NR-V2X industry.

# Discussion

## Revised draft CR

During the preparation phase, some companies noted concerns on use of “multicarrier” in the new clause 6.2.6 title. The editor notes that “multicarrier” is reused from the LTE clause title, where it is distinct from carrier aggregation, which is mentioned separately. The intention was that “multicarrier” addresses the concurrent PC5-Uu operation described in TS 36.101 and TS 38.101-1.

Recognizing these concerns, an alteration to the CR is proposed which aligns terminology more closely between TR 37.985 and TS 36.101/38.101-1, as follows (with temporary change-on-change):

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 5 LTE V2X  **<Unchanged parts omitted>**  5.1.3 Concurrent operation and carrier aggregation  V2X operation is defined in band 47 in TS 36.101 [11, clause 5.5G], which supports single-carrier and multi-carrier operation:  **Table 5.1.3-1: V2X operating band**   |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | **E‑UTRA Operating Band** | **E-UTRA V2X Operating Band** | **V2X UE transmit** | | | **V2X UE receive** | | | **Duplex Mode** | **Interface** | | **FUL\_low – FUL\_high** | | | **FDL\_low – FDL\_high** | | | | 47 | 47 | 5855 MHz |  | 5925 MHz | 5855 MHz |  | 5925 MHz | HD | PC5 |   The V2X sidelink in band 47 can be operated concurrently with Uu FDD bands 3, 5, 7, 8, 20, 28, and Uu TDD bands 34, 39, 41, and 71.  **<Unchanged parts omitted>**  6 NR V2X  **<Unchanged parts omitted>**  6.2.6 Concurrent operation  NR-V2X operation is defined in bands n38 and n47 in TS 38.101-1 [22, clause 5.2E], which support single-carrier operation:  **Table 6.2.6-1: NR-V2X operating bands**   |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | | **V2X Operating Band** | **Sidelink (SL) Transmission operating band** | | | **Sidelink (SL) Reception operating band** | | | **Duplex Mode** | **Interface** | |  | **FUL\_low – FUL\_high** | | | **FDL\_low – FDL\_high** | | |  |  | | n381 | 2570 MHz | - | 2620 MHz | 2570 MHz | - | 2620 MHz | HD | PC5 | | n47 | 5855 MHz | - | 5925 MHz | 5855 MHz | - | 5925 MHz | HD | PC5 | | Note 1: When this band is used for V2X SL service, the band is exclusively used for NR V2X in particular regions. | | | | | | | | |   The NR-V2X sidelink in band n47 can be operated concurrently with Uu band n71.  6.3 V2X sidelink resource allocation  **<Unchanged parts omitted>** |

## Companies views

**Does your company agree to endorse the above updated change text for a CR, and/or have any other comments?**

|  |  |  |
| --- | --- | --- |
| **Company** | **OK to endorse?** | **Comment, if any** |
| Huawei, HiSilicon | OK |  |
| Samsung | OK |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 

# Conclusions

TBD.

# References

1. R1-2202442, “Draft CR: Addition of Rel-16 NR V2X bands to TR 37.985”, Huawei (editor), RAN1#108-e.