TSG-RAN WG1 #112b-e R1-23xxxxx

e-meeting, April 17 – 26, 2023

Source: Ericsson

Title: Draft CR 38.211 – NR\_MC\_enh-Core

Agenda Item: 9.18

Document for: Discussion and Decision

# Introduction

This thread will discuss the draft CR to 38.211 for NR\_MC\_enh-Core.

# Discussion – first round

The draft CR is available in R1-2302741

First checkpoint: April 20, UTC 17.00

|  |  |
| --- | --- |
| Company | Comments |
| Xiaomi | On 6.4.1.1.1.2 of the draft CR:   |  | | --- | | For a CORESET configured by the *ControlResourceSet* IE:  […]  - if the higher-layer parameter *dmrs-UplinkTransformPrecoding* is configured, π/2-BPSK modulation is used for PUSCH, and the PUSCH transmission is not a msg3 transmission, and the transmission is not scheduled using DCI format 0\_0 in a common search space, is given by clause 5.2.3 with given by  where unless given by the DCI according to clause 7.3.1.1.2 in [4, TS38.212] for a transmission scheduled by DCI format 0\_1, or given by the DCI according to clause 7.3.1.1.3 in [4, TS38.212] for a transmission scheduled by DCI format 0\_2 if the antenna ports field in the DCI format 0\_2 is not 0 bit, or given by the DCI according to clause 7.3.1.1.4 in [4, TS38.212] for a transmission scheduled by DCI format 0\_3 if the antenna ports field in the DCI format 0\_3 is not 0 bit, or given by the higher-layer parameter *antennaPort* for a PUSCH transmission scheduled by a type-1 configured grant; and  - are given by the higher-layer parameters *pi2BPSK-ScramblingID0* and *pi2BPSK-ScramblingID1*, respectively, in the *DMRS-UplinkConfig* IE if provided and the PUSCH is scheduled by DCI format 0\_1, or by DCI format 0\_2 if the antenna ports field in the DCI format 0\_2 is not 0 bit, or by DCI format 0\_3 if the antenna ports field in the DCI format 0\_3 is not 0 bit, or by a PUSCH transmission with a configured grant;  - is given by the higher-layer parameter *pi2BPSK-ScramblingID0* in the *DMRS-UplinkConfig* IE if provided and the PUSCH is scheduled by DCI format 0\_0 with the CRC scrambled by C-RNTI, MCS-C-RNTI, or CS-RNTI, or by DCI format 0\_2 if the antenna ports field in the DCI format 0\_2 is 0 bit, or by DCI format 0\_3 if the antenna ports field in the DCI format 0\_3 is 0 bit; |   According to the CR for 38.212 [R1-2303803] and discussion paper of [R1-2212924], it seems that the *Antenna ports* field in the DCI format 0\_3 is designed referring to the  *Antenna ports* field in the DCI format 0\_1. In this case, the *Antenna ports* field in the DCI format 0\_3 may be impossible to occupy 0 bit. To align with the description of  [R1-2303803], the draft CR on 6.4.1.1.1.2 can be modified as follows:   |  | | --- | | For a CORESET configured by the *ControlResourceSet* IE:  […]  - if the higher-layer parameter *dmrs-UplinkTransformPrecoding* is configured, π/2-BPSK modulation is used for PUSCH, and the PUSCH transmission is not a msg3 transmission, and the transmission is not scheduled using DCI format 0\_0 in a common search space, is given by clause 5.2.3 with given by  where unless given by the DCI according to clause 7.3.1.1.2 in [4, TS38.212] for a transmission scheduled by DCI format 0\_1, or given by the DCI according to clause 7.3.1.1.3 in [4, TS38.212] for a transmission scheduled by DCI format 0\_2 if the antenna ports field in the DCI format 0\_2 is not 0 bit, or given by the DCI according to clause 7.3.1.1.4 in [4, TS38.212] for a transmission scheduled by DCI format 0\_3 ~~if the antenna ports field in the DCI format 0\_3 is not 0 bit~~, or given by the higher-layer parameter *antennaPort* for a PUSCH transmission scheduled by a type-1 configured grant; and  - are given by the higher-layer parameters *pi2BPSK-ScramblingID0* and *pi2BPSK-ScramblingID1*, respectively, in the *DMRS-UplinkConfig* IE if provided and the PUSCH is scheduled by DCI format 0\_1, or by DCI format 0\_2 if the antenna ports field in the DCI format 0\_2 is not 0 bit, or by DCI format 0\_3 ~~if the antenna ports field in the DCI format 0\_3 is not 0 bit~~, or by a PUSCH transmission with a configured grant;  - is given by the higher-layer parameter *pi2BPSK-ScramblingID0* in the *DMRS-UplinkConfig* IE if provided and the PUSCH is scheduled by DCI format 0\_0 with the CRC scrambled by C-RNTI, MCS-C-RNTI, or CS-RNTI, or by DCI format 0\_2 if the antenna ports field in the DCI format 0\_2 is 0 bit~~, or by DCI format 0\_3 if the antenna ports field in the DCI format 0\_3 is 0 bit~~; | |
|  |  |
|  |  |

**Editor proposal:**

I will update the draft CR as suggested above.

# Discussion – second round

An updated draft CR is uploaded here: <https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_112b-e/Inbox/drafts/9.18(Other)/%5B112bis-e-R18-38.211-NR_MC_enh%5D/R1-23xxxxx%20draft%20CR%2038.211%20NR_MC_enh-Core%20v2.docx>

Second checkpoint: April 25, UTC 17.00

|  |  |
| --- | --- |
| Company | Comments |
| Nokia/NSB | 7.3.1.6 – VRB mapping  Looking at the current situation on the RRC parameter discussions, there seems to be no different VRB interleaver configurable (but to reuse the one from 1\_3, as also captured in 212).  So maybe the following change could be done there:   |  | | --- | | 7.3.1.6 Mapping from virtual to physical resource blocks ... - for all other PDSCH transmissions, the set of resource blocks in bandwidth part  with starting position are divided into resource-block bundles in increasing order of the resource-block number and bundle number where  is the bundle size for bandwidth part  provided by the higher-layer parameter *vrb-ToPRB-Interleaver* for DCI formats 1\_0, ~~and~~ 1\_1 and 1\_3 in a UE-specific search space, or *vrb-ToPRB-InterleaverDCI-1-2* for DCI format 1\_2, ~~or~~ *~~vrb-ToPRB-InterleaverDCI-1-3~~* ~~for DCI format 1\_3~~ and | |
| Xiaomi | Sec.6.4.1.1.1.2  The main bullet has illustrated the transmission scheduled by DCI 0\_3 corresponding to the and =1 case. Hence, the DCI 0\_3 under second sub-bullet for should be removed.   |  | | --- | | 6.4.1.1.1.2 Sequence generation when transform precoding is enabled  ……  - if the higher-layer parameter *dmrs-UplinkTransformPrecoding* is configured, π/2-BPSK modulation is used for PUSCH, and the PUSCH transmission is not a msg3 transmission, and the transmission is not scheduled using DCI format 0\_0 in a common search space, is given by clause 5.2.3 with given by  where unless given by the DCI according to clause 7.3.1.1.2 in [4, TS38.212] for a transmission scheduled by DCI format 0\_1, or given by the DCI according to clause 7.3.1.1.3 in [4, TS38.212] for a transmission scheduled by DCI format 0\_2 if the antenna ports field in the DCI format 0\_2 is not 0 bit, or given by the DCI according to clause 7.3.1.1.4 in [4, TS38.212] for a transmission scheduled by DCI format 0\_3, or given by the higher-layer parameter *antennaPort* for a PUSCH transmission scheduled by a type-1 configured grant; and  - are given by the higher-layer parameters *pi2BPSK-ScramblingID0* and *pi2BPSK-ScramblingID1*, respectively, in the *DMRS-UplinkConfig* IE if provided and the PUSCH is scheduled by DCI format 0\_1, or by DCI format 0\_2 if the antenna ports field in the DCI format 0\_2 is not 0 bit, or by DCI format 0\_3, or by a PUSCH transmission with a configured grant;  - is given by the higher-layer parameter *pi2BPSK-ScramblingID0* in the *DMRS-UplinkConfig* IE if provided and the PUSCH is scheduled by DCI format 0\_0 with the CRC scrambled by C-RNTI, MCS-C-RNTI, or CS-RNTI, or by DCI format 0\_2 if the antenna ports field in the DCI format 0\_2 is 0 bit~~, or by DCI format 0\_3~~; | |