3GPP TS 36.304 V15.7.0 (2020-09)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Evolved Universal Terrestrial Radio Access (E-UTRA);   
User Equipment (UE) procedures in idle mode

(Release 15)

 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganisational Partners and shall not be implemented.

This Specification is provided for future development work within 3GPPonly. The Organisational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organisational Partners' Publications Offices.

Keywords

LTE, E-UTRAN, radio, terminal

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 5

1 Scope 6

2 References 6

3 Definitions and abbreviations 8

3.1 Definitions 8

3.2 Symbols 9

3.3 Abbreviations 10

4 General description of Idle mode 11

4.1 Overview 11

4.2 Functional division between AS and NAS in Idle mode 12

4.3 Service types in Idle Mode 14

4.4 NB-IoT functionality in Idle Mode 16

5 Process and procedure descriptions 16

5.1 PLMN selection 16

5.1.1 Void 17

5.1.2 Support for PLMN selection 17

5.1.2.1 General 17

5.1.2.2 E-UTRA and NB-IoT case 17

5.1.2.3 UTRA case 17

5.1.2.4 GSM case 17

5.1.2.5 CDMA2000 case 17

5.1.2.6 NR case 17

5.2 Cell selection and reselection 18

5.2.1 Introduction 18

5.2.2 States and state transitions in Idle Mode 19

5.2.3 Cell Selection process 20

5.2.3.1 Description 20

5.2.3.2 Cell Selection Criterion 21

5.2.3.2a Cell Selection Criterion for NB-IoT 22

5.2.3.3 CSG cells and Hybrid cells in Cell Selection 22

5.2.3.4 GSM case in Cell Selection 23

5.2.3.5 UTRAN case in Cell Selection 23

5.2.3.6 NR case in Cell Selection 23

5.2.4 Cell Reselection evaluation process 23

5.2.4.1 Reselection priorities handling 23

5.2.4.2 Measurement rules for cell re-selection 25

5.2.4.2a Measurement rules for cell re-selection for NB-IoT 25

5.2.4.3 Mobility states of a UE 25

5.2.4.3.1 Scaling rules 26

5.2.4.4 Cells with cell reservations, access restrictions or unsuitable for normal camping 27

5.2.4.5 E-UTRAN Inter-frequency and inter-RAT Cell Reselection criteria 27

5.2.4.6 Intra-frequency and equal priority inter-frequency Cell Reselection criteria 28

5.2.4.6a Reselection for enhanced coverage 30

5.2.4.7 Cell reselection parameters in system information broadcasts 30

5.2.4.7.1 Speed dependant reselection parameters 32

5.2.4.8 Cell reselection with CSG cells 33

5.2.4.8.1 Cell reselection from a non-CSG cell to a CSG cell 33

5.2.4.8.2 Cell reselection from a CSG cell 33

5.2.4.9 Cell reselection with Hybrid cells 33

5.2.4.10 E-UTRAN Inter-frequency Redistribution procedure 34

5.2.4.10.1 Redistribution target selection 34

5.2.4.11 Cell reselection or CN type change when storing UE AS context 35

5.2.4.12 Relaxed monitoring 35

5.2.4.12.0 Relaxed monitoring measurement rules 35

5.2.4.12.1 Relaxed monitoring criterion 35

5.2.4.13 Cell reselection or CN type change in RRC\_INACTIVE state 35

5.2.5 Void 35

5.2.6 Camped Normally state 35

5.2.7 Cell Selection at transition to RRC\_IDLE or RRC\_INACTIVE state 36

5.2.7a Cell Selection at transition to RRC\_IDLE state for NB-IoT 36

5.2.8 Any Cell Selection state 36

5.2.8a Any Cell Selection state for NB-IoT 36

5.2.9 Camped on Any Cell state 37

5.3 Cell Reservations and Access Restrictions 37

5.3.1 Cell status and cell reservations 37

5.3.2 Access control 39

5.3.3 Emergency call 39

5.4 Tracking Area registration 40

5.5 Support for manual CSG selection 40

5.5.1 E-UTRA case 40

5.5.2 UTRA case 40

5.6 RAN-assisted WLAN interworking 40

5.6.1 RAN assistance parameter handling in RRC\_IDLE 40

5.6.2 Access network selection and traffic steering rules 40

5.6.3 RAN assistance parameters definition 41

6 Reception of broadcast information 42

6.1 Reception of system information 42

6.2 Reception of MBMS 42

7 Paging 43

7.1 Discontinuous Reception for paging 43

7.2 Subframe Patterns 44

7.3 Paging in extended DRX 45

7.4 Paging with Wake Up Signal 46

8 Logged measurements 47

9 Accessibility measurements 47

10 Mobility History Information 47

11 Sidelink operation 47

11.1 Sidelink communication and V2X sidelink communication 47

11.2 Sidelink discovery 48

11.3 Sidelink synchronisation 48

11.4 Cell selection and reselection for sidelink 48

11.4.1 Parameters used for cell selection and reselection triggered for sidelink 48

12. General description of UE camping on E-UTRA connected to 5GC 49

Annex A (informative): Void 50

Annex B (informative): Example of Hashed ID Calculation using 32-bit FCS 51

Annex C (informative): Change history 52

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document specifies the Access Stratum (AS) part of the Idle Mode procedures applicable to a UE. The non-access stratum (NAS) part of Idle mode procedures and processes is specified in TS 23.122 [5].

The present document specifies the model for the functional division between the NAS and AS in a UE.

The present document applies to all UEs that support at least E-UTRA, including multi-RAT UEs as described in 3GPP specifications, in the following cases:

- When the UE is camped on an E-UTRA cell;

- When the UE is searching for a cell to camp on;

NOTE: When the UE is camped on or searching for a cell to camp on belonging to other RATs, the UE behaviour is described in the specifications of the other RAT.

The Idle Mode procedures defined in this specification are also applicable for a UE in RRC\_INACTIVE state unless specified otherwise.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non-specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 25.990: "Vocabulary for UTRAN".

[2] 3GPP TS 36.300: "E-UTRA and E-UTRAN Overall Description; Stage 2".

[3] 3GPP TS 36.331: "E-UTRA; Radio Resource Control (RRC) - Protocol Specification".

[4] 3GPP TS 22.011: "Service accessibility".

[5] 3GPP TS 23.122: "NAS functions related to Mobile Station (MS) in idle mode".

[6] 3GPP TS 36.213: "E-UTRA; Physical layer procedures".

[7] 3GPP TS 36.214: "E-UTRA; Physical layer; Measurements".

[8] 3GPP TS 25.304: "User Equipment (UE) procedures in idle mode and procedures for cell reselection in connected mode"

[9] 3GPP TS 43.022: "Functions related to Mobile Station in idle mode and group receive mode".

[10] 3GPP TS 36.133: "Requirements for Support of Radio Resource Management".

[11] void

[12] void

[13] void

[14] void

[15] void

[16] 3GPP TS 24.301: "Non-Access-Stratum (NAS) protocol for Evolved Packet System (EPS); Stage 3"

[17] 3GPP2 C.S0024-C v2.0: "cdma2000 High Rate Packet Data Air Interface Specification".

[18] 3GPP2 C.S0005-F v1.0: "Upper Layer (Layer 3) Signalling Standard for cdma2000 Spread Spectrum Systems".

[19] 3GPP TS 25.304: "User Equipment (UE) procedures in idle mode and procedures for cell reselection in connected mode".

[20] 3GPP TS 24.008: "Mobile Radio Interface Layer 3 specification; Core Network Protocols; Stage 3"

[21] 3GPP TS 37.320: "Universal Terrestrial Radio Access (UTRA) and Evolved Universal Terrestrial Radio Access (E-UTRA); Radio measurement collection for Minimization of Drive Tests (MDT); Overall description; Stage 2".

[22] 3GPP TS 26.346: "Multimedia Broadcast/Multicast Service (MBMS); Protocols and codecs".

[23] 3GPP TS 23.401: "Evolved Universal Terrestrial Radio Access Network (E-UTRAN) access".

[24] 3GPP TS 23.682: "Architecture enhancements to facilitate communications with packet data networks and applications".

[25] 3GPP TS 23.402: "Architecture enhancements for non-3GPP accesses".

[26] IEEE 802.11, Part 11: "Wireless LAN Medium Access Control (MAC) and Physical Layer (PHY) specifications, IEEE Std.".

[27] Wi-Fi Alliance Technical Committee, Hotspot 2.0 Technical Task Group: "Hotspot 2.0 (Release 2) Technical Specification".

[28] 3GPP TS 24.302: "Access to the 3GPP Evolved Packet Core (EPC) via non-3GPP access networks".

[29] 3GPP TS 23.303: "Proximity-based services (ProSe); Stage 2".

[30] 3GPP TS 36.321: "E-UTRA; Medium Access Control (MAC) protocol specification".

[31] 3GPP TS 24.105: "Application specific Congestion control for Data Communication (ACDC) Management Object (MO)".

[32] 3GPP TS 31.102: "Characteristics of the Universal Subscriber Identity Module (USIM) application".

[33] 3GPP TS 36.101: "Evolved Universal Terrestrial Radio Access (E-UTRA); User Equipment (UE) radio transmission and reception".

[34] Void

[35] 3GPP TS 23.003: "Numbering, addressing and identification".

[36] 3GPP TS 23.285: "Technical Specification Group Services and System Aspects; Architecture enhancements for V2X services".

[37] 3GPP TS 38.331: "NR; Radio Resource Control (RRC); Protocol specification".

[38] 3GPP TS 38.304: "New Generation Radio Access Network; User Equipment (UE) procedures in Idle mode and RRC Inactive state".

[39] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the following terms and definitions apply:

**Acceptable Cell:** A cell that satisfies certain conditions as specified in 4.3. A UE can always attempt emergency calls on an acceptable cell, but restriction as in 5.3.3 apply.

**CSG Whitelist**: A list provided by NAS containing all the CSG identities and their associated PLMN IDs of the CSGs to which the subscriber belongs.

NOTE: This list is known as Allowed CSG List in Rel-8 Access Stratum specifications.

**Available PLMN(s):** One or more PLMN(s) for which the UE has found at least one cell and read its PLMN identity(ies).

**Barred Cell**: A cell a UE is not allowed to camp on.

**Camped on a cell:** UE has completed the cell selection/reselection process and has chosen a cell. The UE monitors system information and (in most cases) paging information.

**Camped on any cell**: UE is in idle mode and has completed the cell selection/reselection process and has chosen a cell irrespective of PLMN identity.

**Closed Subscriber Group (CSG):** A Closed Subscriber Group identifies subscribers of an operator who are permitted to access one or more cells of the PLMN but which have restricted access (CSG cells).

**CN type:** The type of core network connectivity supported by an E-UTRA cell, either EPC or 5GC.

**Commercial Mobile Alert System:** Public Warning System that delivers *Warning Notifications* provided by *Warning Notification Providers* to CMAS capable UEs.

**CSG cell:** A cell broadcasting a CSG indication that is set to TRUE and a specific CSG identity.

**CSG identity:** An identifier broadcast by a CSG or hybrid cell/cells and used by the UE to facilitate access for authorised members of the associated Closed Subscriber Group.

**CSG member cell:** a cell broadcasting the identity of the selected PLMN, registered PLMN or equivalent PLMN and for which the CSG whitelist of the UE includes an entry comprising cell's CSG ID and the respective PLMN identity.

**DRX cycle:** Individual time interval between monitoring Paging Occasion for a specific UE.

**eDRX cycle:** Time interval between the first Paging Occasions occurring after successive extended DRX periods.

**eCall Only Mode:** A UE configuration option that allows the UE to attach at EPS and register in IMS to perform only eCall Over IMS, and a non-emergencyIMS call for test and/or terminal reconfiguration services.

**EHPLMN:** Any of the PLMN entries contained in the Equivalent HPLMN list TS 23.122 [5].

**Equivalent PLMN list:** List of PLMNs considered as equivalent by the UE for cell selection, cell reselection, and handover according to the information provided by the NAS.

**EU-Alert:** Public Warning System that delivers Warning Notifications provided by Warning Notification Providers using the same AS mechanisms as defined for CMAS.

**Home PLMN:** A PLMN where the Mobile Country Code (MCC) and Mobile Network Code (MNC) of the PLMN identity are the same as the MCC and MNC of the IMSI.

**HNB Name**: The Home eNodeB Name is a broadcast string in free text format that provides a human readable name for the Home eNodeB CSG identity and any broadcasted PLMN identity.

**HSDN cell**: A cell that has higher priority than other cells for cell reselection for HSDN capable UE in a High-mobility state.

**Hybrid cell:** A cell broadcasting a CSG Indicator that is set to FALSE and a specific CSG identity.

**Hyper SFN:** Index broadcast in System Information that increments at every SFN wrap around (i.e every 10.24s).

**Korean Public Alert System (KPAS):** Public Warning System that delivers Warning Notifications provided by Warning Notification Providers using the same AS mechanisms as defined for CMAS.

**Location Registration (LR):** UE registers its presence in a registration area, for instance regularly or when entering a new tracking area.

**MBMS-dedicated cell**: cell dedicated to MBMS transmission.

**MBMS/****Unicast-mixed cell**: cell supporting both unicast and MBMS transmissions.

**FeMBMS/Unicast-mixed cell**: cell supporting MBMS transmission and unicast transmission as SCell.

**NB-IoT:** NB-IoT allows access to network services via E-UTRA with a channel bandwidth limited to 200 kHz.

**Paging Time Window:** The period configured for a UE in extended DRX, during which the UE monitors Paging Occasions following DRX cycle.

**Power saving mode**: Mode allowing the UE to reduce its power consumption, as defined in TS 24.301 [16], TS 23.401 [23], TS 23.682 [24].

**Process:** A local action in the UE invoked by a RRC procedure or an Idle Mode or RRC\_INACTIVE state procedure.

**Radio Access Technology:** Type of technology used for radio access, for instance E-UTRA, UTRA, GSM, CDMA2000 1xEV-DO (HRPD) or CDMA2000 1x (1xRTT).

**Registered PLMN:** This is the PLMN on which certain Location Registration outcomes have occurred TS 23.122 [5].

**Registration Area**: (NAS) registration area is an area in which the UE may roam without a need to perform location registration, which is a NAS procedure.

**Reserved Cell**: A cell on which camping is not allowed, except for particular UEs, if so indicated in the system information.

**Restricted Cell**: A cell on which camping is allowed, but access attempts are disallowed for UEs whose access classes are indicated as barred.

**Selected PLMN:** This is the PLMN that has been selected by the NAS, either manually or automatically.

**Serving cell:** The cell on which the UE is camped.

**Sidelink**: UE to UE interface for sidelink communication, V2X sidelink communication and sidelink discovery. The Sidelink corresponds to the PC5 interface as defined in TS 23.303 [29].

**Sidelink communication**: AS functionality enabling ProSe Direct Communication as defined in TS 23.303 [29], between two or more nearby UEs, using E-UTRA technology but not traversing any network node. The terminology "sidelink communication" without "V2X" prefix only concerns PS unless specifically stated otherwise.

**Sidelink discovery**: AS functionality enabling ProSe Direct Discovery as defined in TS 23.303 [29], using E-UTRA technology but not traversing any network node.

**Strongest cell:** The cell on a particular carrier that is considered strongest according to the layer 1 cell search procedure TS 36.213 [6], TS 36.214 [7].

**Suitable Cell:** This is a cell on which an UE may camp. For a E-UTRA cell, the criteria are defined in clause 4.3, for a UTRA cell in TS 25.304 [8], for a GSM cell in TS 43.022 [9], and for a NR cell in TS 38.304 [38].

**V2X sidelink communication:** AS functionality enabling V2X Communication as defined in TS 23.285 [36], between nearby UEs, using E-UTRA technology but not traversing any network node.

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

<symbol> <Explanation>

## 3.3 Abbreviations

For the purposes of the present document, the following abbreviations apply:

1xRTT CDMA2000 1x Radio Transmission Technology

AS Access Stratum

AC Access Class (of the USIM)

ACDC Application specific Congestion control for Data Communication

BCCH Broadcast Control Channel

BL Bandwidth reduced Low complexity

BR-BCCH Bandwidth Reduced Broadcast Control Channel

BSS Basic Service Set

CMAS Commercial Mobile Altert System

CSG Closed Subscriber Group

DRX Discontinuous Reception

DL-SCH Downlink Shared Channel

EHPLMN Equivalent Home PLMN

EPC Evolved Packet Core

EPS Evolved Packet System

ETWS Earthquake and Tsunami Warning System

E-UTRA Evolved UMTS Terrestrial Radio Access

E-UTRAN Evolved UMTS Terrestrial Radio Access Network

FDD Frequency Division Duplex

GERAN GSM/EDGE Radio Access Network

HPLMN Home PLMN

HSDN High Speed Dedicated Network

H-SFN Hyper System Frame Number

HRPD High Rate Packet Data

IMSI International Mobile Subscriber Identity

MBMS Multimedia Broadcast-Multicast Service

MBSFN Multimedia Broadcast multicast service Single Frequency Network

MCC Mobile Country Code

MCCH Multicast Control Channel

MDT Minimization of Drive Tests

MM Mobility Management

MNC Mobile Network Code

MPDCCH MTC Physical Downlink Control Channel

MTCH Multicast Traffic Channel

NAS Non-Access Stratum

NB-IoT NarrowBand Internet of Things

NR NR Radio Access

PLMN Public Land Mobile Network

ProSe Proximity-based Services

PSM Power Saving Mode

PTW Paging Time Window

PWS Public Warning System

RAT Radio Access Technology

RNA RAN-based Notification Area

RNAU RAN-based Notification Area Update

RRC Radio Resource Control

SAP Service Access Point

SIBX SystemInformationBlockTypeX

TDD Time Division Duplex

UAC Unified Access Control

UE User Equipment

UMTS Universal Mobile Telecommunications System

USIM Universal Subscriber Identity Module

UTRA UMTS Terrestrial Radio Access

UTRAN UMTS Terrestrial Radio Access Network

V2X Vehicle-to-Everything

WUS Wake Up Signal

# 4 General description of Idle mode

## 4.1 Overview

The idle mode tasks can be subdivided into four processes:

- PLMN selection;

- Cell selection and reselection;

- Location registration;

- Support for manual CSG selection.

The relationship between these processes is illustrated in Figure 4.1-1.

**

Figure 4.1-1: Overall Idle Mode process

When a UE is switched on, a public land mobile network (PLMN) is selected by NAS. For the selected PLMN, associated RAT(s) may be set TS 23.122 [5]. The NAS shall provide a list of equivalent PLMNs, if available, that the AS shall use for cell selection and cell reselection.

With the cell selection, the UE searches for a suitable cell of the selected PLMN and chooses that cell to provide available services, further the UE shall tune to its control channel. This choosing is known as "camping on the cell".

For E-UTRA a cell may be associated with more than one CN type (EPC and/or 5GC) and hence the selected cell can be suitable for more than one CN type. The CN type(s) for which the selected cell is suitable are reported to NAS which selects a CN type to be used for camping and for the NAS registration procedure (see below). Note that CN type selection is only applicabe for UE supporting E-UTRA connected to 5GC.

The UE shall, if necessary, then register its presence, by means of a NAS registration procedure, in the tracking area of the chosen cell and as outcome of a successful Location Registration the selected PLMN becomes the registered PLMN TS 23.122 [5].

If the UE finds a more suitable cell, according to the cell reselection criteria, it reselects onto that cell and camps on it. Similar to cell selection procedure, if the reselected cell is an E-UTRA cell and the UE supports E-UTRA connected to 5GC, the CN type(s) for which the cell is suitable are reported to NAS which selects one of them. If the new cell does not belong to at least one tracking area to which the UE is registered, location registration is performed. In RRC\_INACTIVE state, if the new cell does not belong to the configured RNA, a RNA update procedure is performed.

If necessary, the UE shall search for higher priority PLMNs at regular time intervals as described in TS 22.011 [4] and search for a suitable cell if another PLMN has been selected by NAS.

Search of available CSGs may be triggered by NAS to support manual CSG selection.

If the UE loses coverage of the registered PLMN, either a new PLMN is selected automatically (automatic mode), or an indication of which PLMNs are available is given to the user, so that a manual selection can be made (manual mode).

Registration is not performed by UEs only capable of services that need no registration.

The UE may perform sidelink communication or V2X sidelink communication or sidelink discovery while in-coverage or out-of-coverage for sidelink, as specified in clause 11.

The purpose of camping on a cell in idle mode is fivefold:

a) It enables the UE to receive system information from the PLMN.

b) When registered and if the UE wishes to establish an RRC connection, it can do this by initially accessing the network on the control channel of the cell on which it is camped.

c) If the PLMN receives a call for the registered UE, it knows (in most cases) the set of tracking areas (in RRC\_IDLE state) or RNAs (in RRC\_INACTIVE state) in which the UE is camped. It can then send a "paging" message for the UE on the control channels of all the cells in this set of tracking areas. The UE will then receive the paging message because it is tuned to the control channel of a cell in one of the registered tracking areas and the UE can respond on that control channel.

d) It enables the UE to receive ETWS and CMAS notifications.

e) It enables the UE to receive MBMS services.

If the UE is unable to find a suitable cell to camp on or if the location registration failed (except for LR rejected with cause #12, cause #14, cause #15 or cause #25, see TS 23.122 [5] and TS 24.301 [16]), it attempts to camp on a cell irrespective of the PLMN identity, and enters a "limited service" state.

When NAS indicates that PSM starts, the AS configuration (e.g. priorities provided by dedicated signalling and logged measurements) is kept, all running timers continue to run but the UE need not perform any idle mode tasks. If a timer expires while the UE is in PSM it is up to UE implementation whether it performs the corresponding action immediately or the latest when PSM ends. When NAS indicates that PSM ends, the UE shall perform all idle mode tasks.

## 4.2 Functional division between AS and NAS in Idle mode

Table 1 presents the functional division between UE non-access stratum (NAS) and UE access stratum (AS) in idle mode. The NAS part is specified in TS 23.122 [5] and the AS part in the present document.

| Idle Mode Process | UE Non-Access Stratum | UE Access Stratum |
| --- | --- | --- |
| PLMN Selection | Maintain a list of PLMNs in priority order according to TS 23.122 [5]. Select a PLMN using automatic or manual mode as specified in TS 23.122 [5] and request AS to select a cell belonging to this PLMN. For each PLMN, associated RAT(s) may be set.  Evaluate reports of available PLMNs and, for E-UTRA if the UEs supports E-UTRA connected to 5GC, CN type(s) from AS for PLMN selection.  Maintain a list of equivalent PLMN identities. | Search for available PLMNs.  If associated RAT(s) is (are) set for the PLMN, search in this (these) RAT(s) and other RAT(s) for that PLMN as specified in TS 23.122 [5].  Perform measurements to support PLMN selection.  Synchronise to a broadcast channel to identify found PLMNs (and CN type(s).  Report available PLMNs with associated RAT(s) and, for E-UTRA if the UE supports E-UTRA connected to 5GC, CN type(s) to NAS on request from NAS or autonomously. |
| Cell  Selection | Control cell selection for example by indicating RAT(s) associated with the selected PLMN to be used initially in the search of a cell in the cell selection. NAS is also maintaining lists of forbidden registration areas and a list of CSG IDs and their associated PLMN ID on which the UE is allowed (CSG whitelist) and provide these lists to AS.  NAS may indicate whether the use of coverage enhancements is not authorized for the selected PLMN.  NAS may indicate whether the CE mode B is restricted for the UE supporting CE mode B.  For E-UTRA if the UE supports E-UTRA connected to 5GC, NAS indicates the CN type to be used for the selected cell. | Perform measurements needed to support cell selection.  Detect and synchronise to a broadcast channel. Receive and handle broadcast information. Forward NAS system information to NAS.  Search for a suitable cell. The cells broadcast one or more 'PLMN identity' in the system information. Respond to NAS whether such cell is found or not.  If associated RATs is (are) set for the PLMN, perform the search in this (these) RAT(s) and other RATs for that PLMN as specified in TS 23.122 [5].  If such a cell is found, the cell is selected to camp on.  For E-UTRA if the UE supports E-UTRA connected to 5GC, AS reports the CN type(s) for which the selected cell is suitable to NAS. |
| Cell  Reselection | Control cell reselection by for example, maintaining lists of forbidden registration areas.  Maintain a list of equivalent PLMN identities and provide the list to AS.  Maintain a list of forbidden registration areas and provide the list to AS.  Maintain a list of CSG IDs and their associated PLMN ID on which the UE is allowed (CSG whitelist) to camp and provide the list to AS.  For E-UTRA if the UE supports E-UTRA connected to 5GC, NAS indicates the CN type to be used for the selected cell. | Perform measurements needed to support cell reselection.  Detect and synchronise to a broadcast channel. Receive and handle broadcast information. Forward NAS system information to NAS.  Change cell if a more suitable cell is found.  For E-UTRA if the UE supports E-UTRA connected to 5GC, the UE reports the CN type(s) for which the selected cell is suitable to NAS. |
| Location registration | Register the UE as active after power on.  Register the UE's presence in a registration area, for instance regularly or when entering a new tracking area.  Maintain lists of forbidden registration areas.  Deregister UE when shutting down.  Control and restrict location registration for a UE in eCall only mode. | Report registration area information to NAS. |
| Support for manual CSG selection | Provide request to search for available CSGs.  Evaluate reports of available CSGs from AS for CSG selection.  Select a CSG and request AS to select a cell belonging to this CSG. | Search for cells with a CSG ID.  Read the HNB name from BCCH on SIB9 if a cell with a CSG ID is found.  Report CSG ID of the found cell broadcasting a CSG ID together with the HNB name and PLMN(s) to NAS.  On selection of a CSG by NAS, select any cell belonging to the selected CSG fulfilling the cell selection criteria and not barred or reserved for operator use for UEs not belonging to AC 11 or 15 and give an indication to NAS that access is possible (for the registration procedure). |
| RAN Notification Area Update | Not applicable | Register the UE's presence in a RAN-based notification area, periodically or when entering a new RAN-based notification area. |

Table 4.2-1: Functional division between AS and NAS in idle mode

## 4.3 Service types in Idle Mode

This clause defines the level of service that may be provided by the network to a UE in Idle mode.

The action of camping on a cell is necessary to get access to some services. Three levels of services are defined for UE:

- Limited service (emergency calls, ETWS and CMAS on an acceptable cell). It is not applicable to RRC\_INACTIVE state.

- Normal service (for public use on a suitable cell)

- Operator service (for operators only on a reserved cell)

Furthermore, the cells are categorised according to which services they offer:

**acceptable cell:**

An "acceptable cell" is a cell on which the UE may camp to obtain limited service (originate emergency calls and receive ETWS and CMAS notifications), and it is not applicable to RRC\_INACTIVE state. Such a cell shall fulfil the following requirements, which is the minimum set of requirements to initiate an emergency call and to receive ETWS and CMAS notification in a E-UTRAN network:

- The cell is not barred, see clause 5.3.1;

- The cell selection criteria are fulfilled, see clause 5.2.3.2;

**suitable cell:**

A "suitable cell" is a cell on which the UE may camp on to obtain normal service. The UE shall have a valid USIM and such a cell shall fulfil all the following requirements.

- The cell is part of either:

- the selected PLMN, or:

- the registered PLMN, or:

- a PLMN of the Equivalent PLMN list

- For a CSG cell, the cell is a CSG member cell for the UE;

According to the latest information provided by NAS:

- The cell is not barred, see clause 5.3.1;

- The cell is part of at least one TA that is not part of the list of "forbidden tracking areas for roaming" TS 22.011 [4], which belongs to a PLMN that fulfils the first bullet above;

- The cell selection criteria are fulfilled, see clause 5.2.3.2;

- Except for NB-IoT, if the UE supports authorization of coverage enhancements and upper layers indicated that use of coverage enhancements is not authorized for the selected PLMN:

- the cell selection criterion S in normal coverage shall be fulfilled;

- If the UE supports CE mode B and upper layers indicated that CE mode B is restricted:

- the cell selection criterion S in normal coverage based on values Qrxlevmin and Qqualmin or in enhanced coverage based on values Qrxlevmin\_CE and Qqualmin\_CE shall be fulfilled.

If more than one PLMN identity is broadcast in the cell, the cell is considered to be part of all TAs with TAIs constructed from the PLMN identities and the TAC broadcast in the cell.

**barred cell:**

A cell is barred if it is so indicated in the system information TS 36.331 [3].

**reserved cell:**

A cell is reserved if it is so indicated in system information TS 36.331 [3].

Following exceptions to these definitions are applicable for UEs:

- camped on a cell that belongs to a registration area that is forbidden for regional provision of service; a cell that belongs to a registration area that is forbidden for regional provision service (TS 23.122 [5], TS 24.301 [16]) is suitable but provides only limited service.

- as an outcome of the manual CSG selection procedure the UE is allowed to access an acceptable cell which fulfils the cell selection criteria and is not barred or reserved for operator use for UEs not belonging to AC 11 or 15 and inform NAS that access is possible (for location registration procedure).

NOTE: UE is not required to support manual search and selection of PLMN or CSGs while in RRC CONNECTED state. The UE may use local release of RRC connection to perform manual search if it is not possible to perform the search while RRC connected.

- if a UE has an ongoing emergency call, all acceptable cells of that PLMN are treated as suitable for the duration of the emergency call.

- if the UE in RRC\_IDLE fulfils the conditions to support sidelink communication or PS related sidelink discovery in limited service state as specified in TS 23.303 [29, 4.5.6], the UE may perform sidelink communication or PS-related sidelink discovery.

- if the UE in RRC\_IDLE fulfils the conditions to support V2X sidelink communication in limited service state as specified in TS23.285 [36, 4.4.8], the UE may perform V2X sidelink communication.

For E-UTRA the cell categorization defined above is per CN type. In this specification, when the term suitable/acceptable cell is used without specifying the CN type, it means the cell is suitable/acceptable for any of the CN type(s) supported by the UE.

NOTE: The selected CN Type is not considered during cell selection and reselection procedure.

## 4.4 NB-IoT functionality in Idle Mode

This specification is applicable to NB-IoT, except for the following functionality which is not applicable to NB-IoT:

- Acceptable cell

- Accessibility measurements

- Access Control based on ACDC categories

- Camped on Any cell state

- Camping on E-UTRA connected to 5GC

- CSG, including support for manual CSG selection and CSG or Hybrid cell related functionality in PLMN selection, or HNB name (SIB9), Cell selection and Cell reselection.

- Emergency call

- E-UTRAN Inter-frequency Redistribution procedure

- Inter-RAT Cell Selection and Reselection including measurements in other RATs

- Logged measurements

- Mobility History Information

- Mobility states of a UE

- Priority based reselection

- Public warning system including CMAS, ETWS, PWS.

- RAN-assisted WLAN interworking

- RRC\_INACTIVE state

- Sidelink operation

# 5 Process and procedure descriptions

## 5.1 PLMN selection

In the UE, the AS shall report available PLMNs to the NAS on request from the NAS or autonomously. For E-UTRA, if UE supports E-UTRA connected to 5GC, the AS shall also report CN type associated with the PLMN to NAS.

During PLMN selection, based on the list of PLMN identities in priority order, the particular PLMN may be selected either automatically or manually. Each PLMN in the list of PLMN identities is identified by a 'PLMN identity'. In the system information on the broadcast channel, the UE can receive one or multiple 'PLMN identity' (and, for E-UTRA, the CN type associated with the PLMN) in a given cell. The result of the PLMN selection performed by NAS (see TS 23.122 [5]) is an identifier of the selected PLMN.

### 5.1.1 Void

### 5.1.2 Support for PLMN selection

#### 5.1.2.1 General

On request of the NAS the AS shall perform a search for available PLMNs and report them to NAS.

#### 5.1.2.2 E-UTRA and NB-IoT case

The UE shall scan all RF channels in the E-UTRA bands according to its capabilities to find available PLMNs. On each carrier, the UE shall search for the strongest cell and read its system information, in order to find out which PLMN(s) the cell belongs to. If the UE can read one or several PLMN identities in the strongest cell, each found PLMN (see the PLMN reading in TS 36.331 [3]) shall be reported to the NAS as a high quality PLMN (but without the RSRP value), provided that the following high quality criterion is fulfilled:

1. For an E-UTRAN and NB-IoT cell, the measured RSRP value shall be greater than or equal to -110 dBm.

Found PLMNs that do not satisfy the high quality criterion, but for which the UE has been able to read the PLMN identities are reported to the NAS together with the RSRP value. The quality measure reported by the UE to NAS shall be the same for each PLMN found in one cell.

For each found PLMN, if the UE supports E-UTRA connected to 5GC, the associated CN type(s) shall also be reported to the NAS.

If the cell is barred for connectivity to EPC (as indicated by the *cellBarred*/cellBarred-CRS flag being set to the value barred, see clause 5.3.1) a UE supporting E-UTRA connected to 5GC shall only report the available 5GC PLMNs to NAS.

The search for PLMNs may be stopped on request of the NAS. The UE may optimise PLMN search by using stored information e.g. carrier frequencies and optionally also information on cell parameters from previously received measurement control information elements.

Once the UE has selected a PLMN, the cell selection procedure shall be performed in order to select a suitable cell of that PLMN to camp on.

If a CSG ID is provided by NAS as part of PLMN selection, the UE shall search for an acceptable or suitable cell belonging to the provided CSG ID to camp on. When the UE is no longer camped on a cell with the provided CSG ID, AS shall inform NAS.

#### 5.1.2.3 UTRA case

Support for PLMN selection in UTRA is described in TS 25.304 [8].

#### 5.1.2.4 GSM case

Support for PLMN selection in GERAN is described in TS 43.022 [9].

#### 5.1.2.5 CDMA2000 case

For CDMA2000 the network determination for HRPD and 1xRTT is described in [17] and [18] respectively.

#### 5.1.2.6 NR case

Support for PLMN selection in NR is described in TS 38.304 [38].

## 5.2 Cell selection and reselection

### 5.2.1 Introduction

UE shall perform measurements for cell selection and reselection purposes as specified in TS 36.133 [10].

The NAS can control the RAT(s) in which the cell selection should be performed, for instance by indicating RAT(s) associated with the selected PLMN, and by maintaining a list of forbidden registration area(s) and a list of equivalent PLMNs. The UE shall select a suitable cell based on idle mode measurements and cell selection criteria.

In order to speed up the cell selection process, stored information for several RATs may be available in the UE.

When camped on a cell, the UE shall regularly search for a better cell according to the cell reselection criteria. If a better cell is found, that cell is selected. The change of cell may imply a change of RAT, or if the current and selected cell are both E-UTRA cells, a change of the CN type. Details on performance requirements for cell reselection can be found in TS 36.133 [10].

The NAS is informed if the cell selection and reselection results in changes in the received system information relevant for NAS.

For normal service, the UE shall camp on a suitable cell, tune to that cell's control channel(s) so that the UE can:

- Receive system information from the PLMN; and

- receive registration area information from the PLMN, e.g., tracking area information; and

- receive other AS and NAS Information; and

- if registered:

- receive paging and notification messages from the PLMN; and

- initiate transfer to connected mode.

### 5.2.2 States and state transitions in Idle Mode

Except for NB-IoT, figure 5.2.2-1 shows the states and state transitions and procedures in RRC\_IDLE. Whenever a new PLMN selection is performed, it causes an exit to number 1.

**

Figure 5.2.2-1: RRC\_IDLE Cell Selection and Reselection

For NB-IoT, figure 5.2.2-2 shows the states and state transitions and procedures in RRC\_IDLE. Whenever a new PLMN selection is performed, it causes an exit to number 1.

**

Figure 5.2.2-2: RRC\_IDLE Cell Selection and Reselection for NB-IoT

### 5.2.3 Cell Selection process

#### 5.2.3.1 Description

The UE shall use one of the following two cell selection procedures:

a) Initial Cell Selection

This procedure requires no prior knowledge of which RF channels are E-UTRA or NB-IoT carriers. The UE shall scan all RF channels in the E-UTRA bands according to its capabilities to find a suitable cell. On each carrier frequency, the UE need only search for the strongest cell. Once a suitable cell is found this cell shall be selected.

b) Stored Information Cell Selection

This procedure requires stored information of carrier frequencies and optionally also information on cell parameters, from previously received measurement control information elements or from previously detected cells. Once the UE has found a suitable cell the UE shall select it. If no suitable cell is found the Initial Cell Selection procedure shall be started.

NOTE 1: Priorities between different frequencies or RATs provided to the UE by system information or dedicated signalling are not used in the cell selection process.

NOTE 2: If BL UE, UE in enhanced coverage or NB-IoT UE has been provisioned with EARFCN, the UE may use this information during Initial Cell Selection and Stored Information Cell Selection to find a suitable cell.

#### 5.2.3.2 Cell Selection Criterion

For NB-IoT the cell selection criterion is defined in clause 5.2.3.2a.

The cell selection criterion S in normal coverage is fulfilled when:

|  |
| --- |
| Srxlev > 0 AND Squal > 0 |

where:

|  |
| --- |
| Srxlev = Qrxlevmeas – (Qrxlevmin + Qrxlevminoffset) – Pcompensation - Qoffsettemp  Squal = Qqualmeas – (Qqualmin + Qqualminoffset) - Qoffsettemp |

where:

|  |  |
| --- | --- |
| Srxlev | Cell selection RX level value (dB) |
| Squal | Cell selection quality value (dB) |
| Qoffsettemp | Offset temporarily applied to a cell as specified in TS 36.331 [3] (dB) |
| Qrxlevmeas | Measured cell RX level value (RSRP) |
| Qqualmeas | Measured cell quality value (RSRQ) |
| Qrxlevmin | Minimum required RX level in the cell (dBm) . Qrxlevmin is obtained from *q-RxLevMin* in SIB1, SIB3, SIB5, or NR SIB5.  When the UE who is camped on a NR cell is evaluating an E-UTRA cell, if Qrxlevminoffsetcell is signalled in NR SIB5 in TS 38.331 [37] for the E-UTRA cell, this cell specific offset is added to *q-RxLevMin* to achieve the required minimum RX level in the E-UTRA cell. |
| Qqualmin | Minimum required quality level in the cell (dB)  When the UE who is camped on a NR cell is evaluating an E-UTRA cell, if Qqualminoffsetcell is signalled in NR SIB5 in TS 38.331 [37] for the E-UTRA cell, this cell specific offset is added to achieve the required minimum quality level in the E-UTRA cell. |
| Qrxlevminoffset | Offset to the signalled Qrxlevmin taken into account in the Srxlev evaluation as a result of a periodic search for a higher priority PLMN while camped normally in a VPLMN TS 23.122 [5] |
| Qqualminoffset | Offset to the signalled Qqualmin taken into account in the Squal evaluation as a result of a periodic search for a higher priority PLMN while camped normally in a VPLMN TS 23.122 [5] |
| Pcompensation | If the UE supports the *additionalPmax* in the *NS-PmaxList*, if present, in SIB1, SIB3 and SIB5:  max(PEMAX1 –PPowerClass, 0) – (min(PEMAX2, PPowerClass) – min(PEMAX1, PPowerClass)) (dB);  else:  if PPowerClass is 14 dBm:  max(PEMAX1 –(PPowerClass – Poffset), 0) (dB);  else:  max(PEMAX1 –PPowerClass, 0) (dB) |
| PEMAX1, PEMAX2 | Maximum TX power level an UE may use when transmitting on the uplink in the cell (dBm) defined as PEMAX in TS 36.101 [33]. PEMAX1 and PEMAX2 are obtained from the *p-Max* and the *NS-PmaxList* respectively in SIB1, SIB3 and SIB5 as specified in TS 36.331 [3]. |
| PPowerClass | Maximum RF output power of the UE (dBm) according to the UE power class as defined in TS 36.101 [33] |

The signalled values Qrxlevminoffset and Qqualminoffset are only applied when a cell is evaluated for cell selection as a result of a periodic search for a higher priority PLMN while camped normally in a VPLMN TS 23.122 [5]. During this periodic search for higher priority PLMN the UE may check the S criteria of a cell using parameter values stored from a different cell of this higher priority PLMN.

If cell selection criterion S in normal coverage is not fulfilled for a cell, UE shall consider itself to be in enhanced coverage if the cell selection criterion S for enhanced coverage is fulfilled, where:

|  |  |
| --- | --- |
| Qrxlevmin | UE applies coverage specific value Qrxlevmin\_CE (dBm) |
| Qqualmin | UE applies coverage specific value Qqualmin\_CE (dB) |

If cell selection criterion S in normal coverage is not fulfilled for a cell and UE does not consider itself in enhanced coverage based on coverage specific values Qrxlevmin\_CE and Qqualmin\_CE, UE shall consider itself to be in enhanced coverage if UE supports CE Mode B and CE mode B is not restricted by upper layers and the cell selection criterion S for enhanced coverage is fulfilled, where:

|  |  |
| --- | --- |
| Qrxlevmin | UE applies coverage specific value Qrxlevmin\_CE1 (dBm) |
| Qqualmin | UE applies coverage specific value Qqualmin\_CE1 (dB) |

For the UE in enhanced coverage, coverage specific values Qrxlevmin\_CE and Qqualmin\_CE (orQrxlevmin\_CE1 and Qqualmin\_CE1)are only applied for the suitability check in enhanced coverage (i.e. not used for measurement and reselection thresholds).

#### 5.2.3.2a Cell Selection Criterion for NB-IoT

The cell selection criterion S is fulfilled when:

|  |
| --- |
| Srxlev > 0 AND Squal > 0 |

where:

|  |
| --- |
| Srxlev = Qrxlevmeas – Qrxlevmin – Pcompensation - Qoffsettemp  Squal = Qqualmeas – Qqualmin - Qoffsettemp |

where:

|  |  |
| --- | --- |
| Srxlev | Cell selection RX level value (dB) |
| Squal | Cell selection quality value (dB) |
| Qoffsettemp | Offset temporarily applied to a cell as specified in TS 36.331 [3] (dB) |
| Qrxlevmeas | Measured cell RX level value (RSRP) |
| Qqualmeas | Measured cell quality value (RSRQ) |
| Qrxlevmin | Minimum required RX level in the cell (dBm)  If UE is not authorized for enhanced coverage and Qoffsetauthorization is valid then Qrxlevmin = Qrxlevmin + Qoffsetauthorization. |
| Qqualmin | Minimum required quality level in the cell (dB) |
| Pcompensation | If the UE supports the *additionalPmax* in the *NS-PmaxList-NB*, if present, in SIB1-NB, SIB3-NB and SIB5-NB:  max(PEMAX1 –PPowerClass, 0) – (min(PEMAX2, PPowerClass) – min(PEMAX1, PPowerClass)) (dB);  else:  if PPowerClass is 14 dBm:  max(PEMAX1 –(PPowerClass – Poffset), 0) (dB);  else:  max(PEMAX1 –PPowerClass, 0) (dB) |
| PEMAX1, PEMAX2 | Maximum TX power level an UE may use when transmitting on the uplink in the cell (dBm) defined as PEMAX in TS 36.101 [33]. PEMAX1 and PEMAX2 are obtained from the *p-Max* and the *NS-PmaxList-NB* respectively in SIB1-NB, SIB3-NB and SIB5-NB as specified in TS 36.331 [3]. |
| PPowerClass | Maximum RF output power of the UE (dBm) according to the UE power class as defined in TS 36.101 [33] |

#### 5.2.3.3 CSG cells and Hybrid cells in Cell Selection

In addition to normal cell selection rules a manual selection of CSGs shall be supported by the UE upon request from higher layers as defined in clause 5.5.

#### 5.2.3.4 GSM case in Cell Selection

The cell selection criteria and procedures in GSM are specified in TS 43.022 [9].

#### 5.2.3.5 UTRAN case in Cell Selection

The cell selection criteria and procedures in UTRAN are specified in TS 25.304 [8].

#### 5.2.3.6 NR case in Cell Selection

The cell selection criteria and procedures in NR are specified in TS 38.304 [38].

### 5.2.4 Cell Reselection evaluation process

#### 5.2.4.1 Reselection priorities handling

Absolute priorities of different E-UTRAN frequencies or inter-RAT frequencies may be provided to the UE in the system information, in the *RRCConnectionRelease* or *RRCEarlyDataComplete* message, or by inheriting from another RAT at inter-RAT cell (re)selection. In the case of system information, an E-UTRAN frequency or inter-RAT frequency may be listed without providing a priority (i.e. the field *cellReselectionPriority* is absent for that frequency). If priorities are provided in dedicated signalling, the UE shall ignore all the priorities provided in system information. If UE is in *camped on any cell* state, UE shall only apply the priorities provided by system information from current cell, and the UE preserves priorities provided by dedicated signalling and *deprioritisationReq* received in *RRCConnectionReject* unless specified otherwise. When the UE in *camped normally* state, has only dedicated priorities other than for the current frequency, the UE shall consider the current frequency to be the lowest priority frequency (i.e. lower than any of the network configured values). While the UE is camped on a suitable CSG cell in normal coverage, the UE shall always consider the current frequency to be the highest priority frequency (i.e. higher than any of the network configured values), irrespective of any other priority value allocated to this frequency. When the HSDN capable UE is in High-mobility state, the UE shall always consider the HSDN cells to be the highest priority (i.e. higher than any other network configured priorities). When the HSDN capable UE is not in High-mobility state, the UE shall always consider HSDN cells to be the lowest priority (i.e. lower than network configured priorities). If the UE capable of sidelink communication is configured to perform sidelink communication and can only perform the sidelink communication while camping on a frequency, the UE may consider that frequency to be the highest priority. If the UE capable of V2X sidelink communication is configured to perform V2X sidelink communication and can only perform the V2X sidelink communication while camping on a frequency, the UE may consider that frequency to be the highest priority. If the UE capable of V2X sidelink communication is configured to perform V2X sidelink communication and can only use pre-configuration while not camping on a frequency, the UE may consider the frequency providing inter-carrier V2X sidelink configuration to be the highest priority. If the UE capable of sidelink discovery is configured to perform Public Safety related sidelink discovery and can only perform the Public Safety related sidelink discovery while camping on a frequency, the UE may consider that frequency to be the highest priority.

NOTE 1: The prioritization among the frequencies which UE considers to be the highest priority frequency is left to UE implementation.

If the UE is capable either of MBMS Service Continuity or of SC-PTM reception and is receiving or interested to receive an MBMS service and can only receive this MBMS service while camping on a frequency on which it is provided, the UE may consider that frequency to be the highest priority during the MBMS session TS 36.300 [2] as long as the two following conditions are fulfilled:

1) Either:

- the UE is capable of MBMS service continuity and the reselected cell is broadcasting SIB13; or

- the UE is capable of SC-PTM reception and the reselected cell is broadcasting SIB20;

2) Either:

- SIB15 of the serving cell indicates for that frequency one or more MBMS SAIs included and associated with that frequency in the MBMS User Service Description (USD) TS 26.346 [22] of this service; or

- SIB15 is not broadcast in the serving cell and that frequency is included in the USD of this service.

If the UE is capable either of MBMS Service Continuity or of SC-PTM reception and is receiving or interested to receive an MBMS service provided on a downlink only MBMS frequency, on a frequency used by dedicated MBMS cells, on a frequency used by FeMBMS/Unicast-mixed cells as defined in TS 36.300 [2], or on a frequency belonging to PLMN different from its registered PLMN, the UE may consider cell reselection candidate frequencies at which it can not receive the MBMS service to be of the lowest priority during the MBMS session TS 36.300 [2], as long as the above mentioned condition 1) is fulfilled for the cell on the MBMS frequency which the UE monitors or this cell broadcasts SIB1-MBMS and as long as the above mentioned condition 2) is fulfilled for the serving cell.

NOTE 2: Example scenarios in which the previous down-prioritisation may be needed concerns the cases where camping is not possible, while the UE can only receive this MBMS frequency when camping on a subset of cell reselection candidate frequencies, e.g. the MBMS frequency is a downlink only carrier, the MBMS frequency is used by dedicated MBMS cells, the MBMS frequency is used by FeMBMS/Unicast-mixed cells TS 36.300 [2], or the MBMS frequency belongs to a PLMN different from UE's registered PLMN.

If the UE is not capable of MBMS Service Continuity but has knowledge on which frequency an MBMS service of interest is provided, it may consider that frequency to be the highest priority during the MBMS session TS 36.300 [2] as long as the reselected cell is broadcasting SIB13.

If the UE is not capable of MBMS Service Continuity but has knowledge on which downlink only frequency, on which frequency used by dedicated MBMS cells, on which frequency used by FeMBMS/Unicast-mixed cells as defined in TS 36.300 [2] or on which frequency belonging to PLMN different from its registered PLMN an MBMS service of interest is provided, it may consider cell reselection candidate frequencies at which it can not receive the MBMS service to be of the lowest priority during the MBMS session TS 36.300 [2] as long as the cell on the MBMS frequency which the UE monitors is broadcasting SIB13 or SIB1-MBMS.

NOTE 3: The UE considers that the MBMS session is ongoing using the session start and end times as provided by upper layers in the USD i.e. the UE does not verify if the session is indicated on MCCH.

In case UE receives *RRCConnectionReject* with *deprioritisationReq*, UE shall consider current carrier frequency and stored frequencies due to the previously received *RRCConnectionReject* with *deprioritisationReq* or all the frequencies of EUTRA to be the lowest priority frequency (i.e. lower than any of the network configured values) while T325 is running irrespective of camped RAT. The UE shall delete the stored deprioritisation request(s) when a PLMN selection is performed on request by NAS TS 23.122 [5].

NOTE 4: Connecting to CDMA2000 does not imply PLMN selection.

NOTE 5: UE should search for a higher priority layer for cell reselection as soon as possible after the change of priority. The minimum related performance requirements specified in TS 36.133 [10] are still applicable.

The UE shall delete priorities provided by dedicated signalling when:

- the UE enters a different RRC state; or

- the optional validity time of dedicated priorities (T320) expires; or

- a PLMN selection is performed on request by NAS TS 23.122 [5].

NOTE 6: Equal priorities between RATs are not supported.

The UE shall only perform cell reselection evaluation for E-UTRAN frequencies and inter-RAT frequencies that are given in system information and for which the UE has a priority provided.

The UE shall not consider any black listed cells as candidate for cell reselection.

The UE shall inherit the priorities provided by dedicated signalling and the remaining validity time (i.e., T320 in E-UTRA and NR, T322 in UTRA and T3230 in GERAN), if configured, at inter-RAT cell (re)selection.

NOTE 7: The network may assign dedicated cell reselection priorities for frequencies not configured by system information.

While T360 is running, redistribution target is considered to be the highest priority (i.e. higher than any of the network configured values). UE shall continue to consider the serving frequency as the highest priority until completion of E-UTRAN Inter-frequency Redistribution procedure specified in 5.2.4.10 if triggered on T360 expiry/ stop.

#### 5.2.4.2 Measurement rules for cell re-selection

For NB-IoT measurement rules for cell re-selection is defined in clause 5.2.4.2.a.

When evaluating Srxlev and Squal of non-serving cells for reselection purposes, the UE shall use parameters provided by the serving cell.

Following rules are used by the UE to limit needed measurements:

- If the serving cell fulfils Srxlev> SIntraSearchP and Squal > SIntraSearchQ, the UE may choose not to perform intra-frequency measurements.

- Otherwise, the UE shall perform intra-frequency measurements.

- The UE shall apply the following rules for E-UTRAN inter-frequencies and inter-RAT frequencies which are indicated in system information and for which the UE has priority provided as defined in 5.2.4.1:

- For an E-UTRAN inter-frequency or inter-RAT frequency with a reselection priority higher than the reselection priority of the current E-UTRA frequency the UE shall perform measurements of higher priority E-UTRAN inter-frequency or inter-RAT frequencies according to TS 36.133 [10].

- For an E-UTRAN inter-frequency with an equal or lower reselection priority than the reselection priority of the current E-UTRA frequency and for inter-RAT frequency with lower reselection priority than the reselection priority of the current E-UTRAN frequency:

- If the serving cell fulfils Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ, the UE may choose not to perform measurements of E-UTRAN inter-frequencies or inter-RAT frequency cells of equal or lower priority unless the UE is triggered to measure an E-UTRAN inter-frequency which is configured with *redistributionInterFreqInfo*.

- Otherwise,the UE shall perform measurements of E-UTRAN inter-frequencies or inter-RAT frequency cells of equal or lower priority according to TS 36.133 [10].

- If the UE supports relaxed monitoring and *s-SearchDeltaP* is present in *SystemInformationBlockType3*, the UE may further limit the needed measurements, as specified in clause 5.2.4.12.

#### 5.2.4.2a Measurement rules for cell re-selection for NB-IoT

When evaluating Srxlev and Squal of non-serving cells for reselection purposes, the UE shall use parameters provided by the serving cell.

Following rules are used by the UE to limit needed measurements:

- If the serving cell fulfils Srxlev> SIntraSearchP, the UE may choose not to perform intra-frequency measurements.

- Otherwise, the UE shall perform intra-frequency measurements.

- The UE shall apply the following rules for NB-IoT inter-frequencies which are indicated in system information:

- If the serving cell fulfils Srxlev > SnonIntraSearchP, the UE may choose not to perform inter-frequency measurements.

- Otherwise,the UE shall perform inter-frequency measurements.

- If the UE supports relaxed monitoring and *s-SearchDeltaP* is present in *SystemInformationBlockType3-NB*, the UE may further limit the needed measurements, as specified in clause 5.2.4.12.

#### 5.2.4.3 Mobility states of a UE

Besides Normal-mobility state a High-mobility and a Medium-mobility state are applicable if the parameters (TCRmax, NCR\_H, NCR\_M, TCRmaxHyst and *cellEquivalentSize*) are sent in the system information broadcast of the serving cell.

**State detection criteria:**

Medium-mobility state criteria:

- If number of cell reselections during time period TCRmax exceeds NCR\_M and not exceeds NCR\_H

High-mobility state criteria:

- If number of cell reselections during time period TCRmax exceeds NCR\_H

The UE shall not count consecutive reselections between same two cells into mobility state detection criteria if same cell is reselected just after one other reselection. If the UE is capable of HSDN and the *cellEquivalentSize* is configured, the UE counts the number of cell reselections for this cell as *cellEquivalentSize* configured for this cell.

**State transitions:**

The UE shall:

- if the criteria for High-mobility state is detected:

- enter High-mobility state.

- else if the criteria for Medium-mobility state is detected:

- enter Medium-mobility state.

- else if criteria for either Medium- or High-mobility state is not detected during time period TCRmaxHys**t**:

- enter Normal-mobility state.

If the UE is in High- or Medium-mobility state, the UE shall apply the speed dependent scaling rules as defined in clause 5.2.4.3.1.

##### 5.2.4.3.1 Scaling rules

UE shall apply the following scaling rules:

- If neither Medium- nor Highmobility state is detected:

- no scaling is applied.

- If High-mobility state is detected:

- Add the *sf-High* of "Speed dependent ScalingFactor for Qhyst" to Qhyst if sent on system information

- For E-UTRAN cells multiply TreselectionEUTRA by the *sf-High* of "Speed dependent ScalingFactor for TreselectionEUTRA" if sent on system information

- For UTRAN cells multiply TreselectionUTRA by the *sf-High* of "Speed dependent ScalingFactor for TreselectionUTRA" if sent on system information

- For GERAN cells multiply TreselectionGERA by the *sf-High* of "Speed dependent ScalingFactor for TreselectionGERA state" if sent on system information

- For CDMA2000 HRPD cells Multiply TreselectionCDMA\_HRPD by the *sf-High* of "Speed dependent ScalingFactor for TreselectionCDMA\_HRPD" if sent on system information

- For CDMA2000 1xRTT cells Multiply TreselectionCDMA\_1xRTT by the *sf-High* of "Speed dependent ScalingFactor for TreselectionCDMA\_1xRTT" if sent on system information

- For NR cells multiply TreselectionNR by the *sf-High* of "Speed dependent ScalingFactor for TreselectionNR" if sent on system information

- If Medium-mobility state is detected:

- Add the *sf-Medium* of "Speed dependent ScalingFactor for Qhyst" to Qhyst if sent on system information

- For E-UTRAN cells multiply TreselectionEUTRA by the *sf-Medium* of "Speed dependent ScalingFactor for TreselectionEUTRA" if sent on system information

- For UTRAN cells multiply TreselectionUTRA by the *sf-Medium* of "Speed dependent ScalingFactor for TreselectionUTRA" if sent on system information

- For GERAN cells multiply TreselectionGERA by the *sf-Medium* of "Speed dependent ScalingFactor for TreselectionGERA" if sent on system information

- For CDMA2000 HRPD cells Multiply TreselectionCDMA\_HRPD by the *sf-Medium* of "Speed dependent ScalingFactor for TreselectionCDMA\_HRPD" if sent on system information

- For CDMA2000 1xRTT cells Multiply TreselectionCDMA\_1xRTT by the *sf-Medium* of "Speed dependent ScalingFactor for TreselectionCDMA\_1xRTT" if sent on system information

- For NR cells multiply TreselectionNR by the *sf-Medium* of "Speed dependent ScalingFactor for TreselectionNR" if sent on system information

In case scaling is applied to any TreselectionRAT parameter the UE shall round up the result after all scalings to the nearest second.

#### 5.2.4.4 Cells with cell reservations, access restrictions or unsuitable for normal camping

For the highest ranked cell (including serving cell) according to cell reselection criteria specified in clause 5.2.4.6, for the best cell according to absolute priority reselection criteria specified in clause 5.2.4.5, the UE shall check if the access is restricted according to the rules in clause 5.3.1.

If that cell and other cells have to be excluded from the candidate list, as stated in clause 5.3.1, the UE shall not consider these as candidates for cell reselection. This limitation shall be removed when the highest ranked cell changes.

If the highest ranked cell or best cell according to absolute priority reselection rules is an intra-frequency or inter-frequency cell which is not suitable for a CN type due to being part of the "list of forbidden TAs for roaming" or belonging to a PLMN which is not indicated as being equivalent to the registered PLMN, the UE shall not consider this cell and other cells on the same frequency, as candidates for reselection for the CN type for a maximum of 300s. If the UE enters into state *any cell selection*, any limitation shall be removed. If the UE is redirected under E-UTRAN control to a frequency for which the timer is running, any limitation on that frequency shall be removed.

If the highest ranked cell or best cell according to absolute priority reselection rules is an inter-RAT cell which is not suitable due to being part of the "list of forbidden TAs for roaming" or belonging to a PLMN which is not indicated as being equivalent to the registered PLMN, the UE shall not consider this cell and other cells on the same frequency as candidates for reselection for a maximum of 300s. In case of UTRA further requirements are defined in the TS 25.304 [8]. In case of NR further requirements are defined in the TS 38.304 [38]. If the UE enters into state *any cell selection*, any limitation shall be removed. If the UE is redirected under E-UTRAN control to a frequency for which the timer is running, any limitation on that frequency shall be removed.

If the highest ranked cell or best cell according to absolute priority reselection rules is a CSG cell which is not suitable due to not being a CSG member cell, the UE shall not consider this cell as candidate for cell reselection but shall continue considering other cells on the same frequency for cell reselection.

#### 5.2.4.5 E-UTRAN Inter-frequency and inter-RAT Cell Reselection criteria

For NB-IoT inter-frequency cell reselection shall be based on ranking as defined in clause 5.2.4.6.

If *threshServingLowQ* is provided in *SystemInformationBlockType3* and more than 1 second has elapsed since the UE camped on the current serving cell, cell reselection to a cell on a higher priority E-UTRAN frequency or inter-RAT frequency than the serving frequency shall be performed if:

- A cell of a higher priority EUTRAN, NR or UTRAN FDD RAT/ frequency fulfils Squal > ThreshX, HighQ during a time interval TreselectionRAT; or

- A cell of a higher priority UTRAN TDD, GERAN or CDMA2000 RAT/ frequency fulfils Srxlev > ThreshX, HighP during a time interval TreselectionRAT.

Otherwise, cell reselection to a cell on a higher priority E-UTRAN frequency or inter-RAT frequency than the serving frequency shall be performed if:

- A cell of a higher priority RAT/ frequency fulfils Srxlev > ThreshX, HighP during a time interval TreselectionRAT; and

- More than 1 second has elapsed since the UE camped on the current serving cell.

Cell reselection to a cell on an equal priority E-UTRAN frequency shall be based on ranking for Intra-frequency cell reselection as defined in clause 5.2.4.6.

If *threshServingLowQ* is provided in *SystemInformationBlockType3* and more than 1 second has elapsed since the UE camped on the current serving cell, cell reselection to a cell on a lower priority E-UTRAN frequency or inter-RAT frequency than the serving frequency shall be performed if:

- The serving cell fulfils Squal < ThreshServing, LowQ and a cell of a lower priority EUTRAN, NR or UTRAN FDD RAT/ frequency fulfils Squal > ThreshX, LowQ during a time interval TreselectionRAT; or

- The serving cell fulfils Squal < ThreshServing, LowQ and a cell of a lower priority UTRAN TDD, GERAN or CDMA2000 RAT/ frequency fulfils Srxlev > ThreshX, LowP during a time interval TreselectionRAT.

Otherwise, cell reselection to a cell on a lower priority E-UTRAN frequency or inter-RAT frequency than the serving frequency shall be performed if:

- The serving cell fulfils Srxlev < ThreshServing, LowP and a cell of a lower priority RAT/ frequency fulfils Srxlev > ThreshX, LowP during a time interval TreselectionRAT; and

- More than 1 second has elapsed since the UE camped on the current serving cell.

Cell reselection to a higher priority RAT/ frequency shall take precedence over a lower priority RAT/ frequency, if multiple cells of different priorities fulfil the cell reselection criteria.

The UE shall not perform cell reselection to NR or UTRAN FDD cells for which the cell selection criterion S is not fulfilled.

For cdma2000 RATs, Srxlev is equal to -FLOOR(-2 x 10 x log10 Ec/Io) in units of 0.5 dB, as defined in [18], with Ec/Io referring to the value measured from the evaluated cell.

For cdma2000 RATs, ThreshX, HighP and ThreshX, LowP are equal to -1 times the values signalled for the corresponding parameters in the system information.

In all the above criteria the value of TreselectionRAT is scaled when the UE is in the medium or high mobility state as defined in clause 5.2.4.3.1. If more than one cell meets the above criteria, the UE shall reselect a cell as follows:

- If the highest-priority frequency is an E-UTRAN frequency, a cell ranked as the best cell among the cells on the highest priority frequency(ies) meeting the criteria according to clause 5.2.4.6;

- If the highest-priority frequency is from another RAT, a cell ranked as the best cell among the cells on the highest priority frequency(ies) meeting the criteria of that RAT.

Cell reselection to another RAT, for which Squal based cell reselection parameters are broadcast in system information, shall be performed based on the Squal criteria if the UE supports Squal (RSRQ) based cell reselection to E-UTRAN from all the other RATs provided by system information which UE supports. Otherwise, cell reselection to another RAT shall be performed based on Srxlev criteria.

Cell reselection to NR, for which a cell reselection parameter, *q-RxLevMinSUL* is broadcast in system information and the UE supports SUL, shall be performed based on Srxlev criteria taking the parameter into account.

#### 5.2.4.6 Intra-frequency and equal priority inter-frequency Cell Reselection criteria

The cell-ranking criterion Rs for serving cell and Rn for neighbouring cells is defined by:



where:

|  |  |
| --- | --- |
| Qmeas | RSRP measurement quantity used in cell reselections. |
| Qoffset | For intra-frequency: Equals to Qoffsets,n, if Qoffsets,n is valid, otherwise this equals to zero.  For inter-frequency:  Except for NB-IoT, equals to Qoffsets,n plus Qoffsetfrequency, if Qoffsets,n is valid, otherwise this equals to Qoffsetfrequency.  For NB-IoT equals to QoffsetDedicatedfrequency for any frequency other than the frequency of the dedicated frequency offset, if QoffsetDedicatedfrequency is valid, otherwise this equals to Qoffsetfrequency (if QoffsetDedicatedfrequency is valid Qoffsetfrequency is not used). |
| Qoffsettemp | Offset temporarily applied to a cell as specified in TS 36.331 [3] |
| QoffsetSCPTM | Offset temporarily applied to an SC-PTM frequency as specified below. The offset is applied to all cells on the SC-PTM frequency. If QoffsetSCPTM is valid, Qoffset for inter-frequency neighbour cells is not used. |

If the NB-IoT UE or UE in enhanced coverage is capable of SC-PTM reception and is receiving or interested to receive an MBMS service and can only receive this MBMS service while camping on a frequency on which it is provided (SC-PTM frequency), the UE considers QoffsetSCPTM to be valid during the MBMS session TS 36.300 [2] as long as the following condition is fulfilled:

Either:

- SIB15 (or SIB15-NB) of the serving cell indicates for that frequency one or more MBMS SAIs included in the MBMS User Service Description (USD) TS 26.346 [22] of this service; or

- SIB15 (or SIB15-NB) is not broadcast in the serving cell and that frequency is included in the USD of this service.

NOTE: UE should search for a higher ranked cell on another frequency for cell reselection as soon as possible after the UE stops using QoffsetSCPTM.

The UE shall perform ranking of all cells that fulfil the cell selection criterion S, which is defined in 5.2.3.2 (5.2.3.2a for NB-IoT), but may exclude all CSG cells that are known by the UE not to be CSG member cells.

The cells shall be ranked according to the R criteria specified above, deriving Qmeas,n and Qmeas,s and calculating the R values using averaged RSRP results.

If a cell is ranked as the best cell the UE shall perform cell reselection to that cell. If this cell is found to be not-suitable, the UE shall behave according to clause 5.2.4.4.

In all cases, the UE shall reselect the new cell, only if the following conditions are met:

- the new cell is better ranked than the serving cell during a time interval TreselectionRAT;

- more than 1 second has elapsed since the UE camped on the current serving cell.

When the UE uses infinite dBs for QoffsetSCPTM, the UE shall use QoffsetSCPTM zero and rank the cells on the SC-PTM frequency(ies) only first. If the UE cannot find a suitable cell on an SC-PTM frequency, the UE shall rank the cells on all frequencies.

#### 5.2.4.6a Reselection for enhanced coverage

Ranking as defined in clause 5.2.4.6 is applied for intra-frequency and inter-frequency cell reselection (irrespective of configured frequency priorities, if any) while the UE is in enhanced coverage.

#### 5.2.4.7 Cell reselection parameters in system information broadcasts

Cell reselection parameters are broadcast in system information and are read from the serving cell as follows:

**cellReselectionPriority**

This specifies the absolute priority for E-UTRAN frequency or NR frequency or UTRAN frequency or group of GERAN frequencies or band class of CDMA2000 HRPD or band class of CDMA2000 1xRTT.

**cellReselectionSubPriority**

This specifies the fractional priority value added to cellReselectionPriority for E-UTRAN frequency or NR frequency.

**Poffset**

This specifies the offset for 14 dBm power class for BL or NB-IoT UE.

**Qoffsetauthorization**

This specifies the offset for enhanced coverage authorization for NB-IoT.

**Qoffsets,n**

This specifies the offsetbetween the two cells.

**Qoffsetfrequency**

Frequency specific offset for equal priority E-UTRAN frequencies.

**Qoffsetscptm**

This specifies the offset to be used for cell re-selection for SC-PTM service reception for BL UE, UE in enhanced coverage and NB-IoT UE. The same offset is applicable to all frequencies providing MBMS services via SC-PTM.

**Qoffsettemp**

This specifies the additional offset to be used for cell selection and re-selection. It is temporarily used in case the T300 expires consecutively on the cell as specified in TS 36.331 [3].

**Qhyst**

This specifies the hysteresis value for ranking criteria.

**Qqualmin**

This specifies the minimum required quality level in the cell in dB.

**Qqualmin\_CE, Qqualmin\_CE1**

This specifies the coverage specific minimum required quality level in the cell in dB.

**Qrxlevmin**

This specifies the minimum required Rx level in the cell in dBm.

**Qrxlevmin\_CE, Qrxlevmin\_CE1**

This specifies the coverage specific minimum required Rx level in the cell in dBm.

**RedistributionFactorFreq**

This specifies the redistribution factor for a neighbour E-UTRAN frequency.

**RedistributionFactorCell**

This specifies the redistribution factor for a neighbour E-UTRAN cell.

**RedistributionFactorServing**

This specifies the redistribution factor for serving cell or serving frequency.

**TreselectionRAT**

This specifies the cell reselection timer value. For each target E-UTRA frequency and for each RAT (other than E-UTRA) a specific value for the cell reselection timer is defined, which is applicable when evaluating reselection within E-UTRAN or towards other RAT (i.e. TreselectionRAT for E-UTRAN is TreselectionEUTRA, for NR TreselectionNR, for UTRAN TreselectionUTRA for GERAN TreselectionGERA, for TreselectionCDMA\_HRPD, and for TreselectionCDMA\_1xRTT). For NB-IoT intra-frequency and inter-frequency specific values for the cell reselection timer are defined, which are applicable when evaluating reselection within NB-IoT.

NOTE: TreselectionRAT is not sent on system information, but used in reselection rules by the UE for each RAT.

**TreselectionEUTRA\_ CE**

This specifies the cell reselection timer value TreselectionRAT for E-UTRAN when a neighbour cell is evaluated for camping in enhanced coverage. The parameter can be set per E-UTRAN frequency.

**TreselectionEUTRA**

This specifies the cell reselection timer value TreselectionRAT for E-UTRAN. The parameter can be set per E-UTRAN frequency TS 36.331 [3].

**TreselectionNR**

This specifies the cell reselection timer value TreselectionRAT for NR.

**TreselectionNB-IoT\_Intra**

This specifies the intra-frequency cell reselection timer value TreselectionRAT for NB-IoT.**TreselectionNB-IoT\_Inter**

This specifies the inter-frequency cell reselection timer value TreselectionRAT for NB-IoT.

**TreselectionUTRA**

This specifies the cell reselection timer value TreselectionRAT for UTRAN.

**TreselectionGERA**

This specifies the cell reselection timer value TreselectionRAT for GERAN.

**TreselectionCDMA\_HRPD**

This specifies the cell reselection timer value TreselectionRAT for CDMA HRPD.

**TreselectionCDMA\_1xRTT**

This specifies the cell reselection timer value TreselectionRAT for CDMA 1xRTT.

**ThreshX, HighP**

This specifies the Srxlev threshold (in dB) used by the UE when reselecting towards a higher priority RAT/ frequency than the current serving frequency. Each frequency of E-UTRAN, NR and UTRAN, each group of GERAN frequencies, each band class of CDMA2000 HRPD and CDMA2000 1xRTT might have a specific threshold.

**ThreshX, HighQ**

This specifies the Squal threshold (in dB) used by the UE when reselecting towards a higher priority RAT/ frequency than the current serving frequency. Each frequency of E-UTRAN, NR and UTRAN FDD might have a specific threshold.

**ThreshX, LowP**

This specifies the Srxlev threshold (in dB) used by the UE when reselecting towards a lower priority RAT/ frequency than the current serving frequency. Each frequency of E-UTRAN, NR and UTRAN, each group of GERAN frequencies, each band class of CDMA2000 HRPD and CDMA2000 1xRTT might have a specific threshold.

**ThreshX, LowQ**

This specifies the Squal threshold (in dB) used by the UE when reselecting towards a lower priority RAT/ frequency than the current serving frequency. Each frequency of E-UTRAN, NR and UTRAN FDD might have a specific threshold.

**ThreshServing, LowP**

This specifies the Srxlev threshold (in dB) used by the UE on the serving cell when reselecting towards a lower priority RAT/ frequency.

**ThreshServing, LowQ**

This specifies the Squal threshold (in dB) used by the UE on the serving cell when reselecting towards a lower priority RAT/ frequency.

**SIntraSearchP**

This specifies the Srxlev threshold (in dB) for intra-frequency measurements.

**SIntraSearchQ**

This specifies the Squal threshold (in dB) for intra-frequency measurements.

**SnonIntraSearchP**

This specifies the Srxlev threshold (in dB) for E-UTRAN inter-frequency and inter-RAT measurements.

**SnonIntraSearchQ**

This specifies the Squal threshold (in dB) for E-UTRAN inter-frequency and inter-RAT measurements.

SSearchDeltaP

This specifies the Srxlev delta threshold (in dB) during relaxed monitoring.

##### 5.2.4.7.1 Speed dependant reselection parameters

**TCRmax**

This specifies the duration for evaluating allowed amount of cell reselection(s).

**NCR\_M**

This specifies the maximum number of cell reselections to enter Medium-mobility state.

**NCR\_H**

This specifies the maximum number of cell reselections to enter High-mobility state.

**TCRmaxHyst**

This specifies the additional time period before the UE can enter Normal-mobility state.

**Speed dependent ScalingFactor for Qhyst**

This specifies scaling factor for Qhyst in *sf-High* for High-mobility state and *sf-Medium* for Medium-mobility state

**Speed dependent ScalingFactor for TreselectionNR**

This specifies scaling factor for TreselectionNR in *sf-High* for High-mobility state and *sf-Medium* for Medium-mobility state

**Speed dependent ScalingFactor for TreselectionEUTRA**

This specifies scaling factor for TreselectionEUTRA in *sf-High* for High-mobility state and *sf-Medium* for Medium-mobility state

**Speed dependent ScalingFactor for TreselectionUTRA**

This specifies scaling factor for TreselectionUTRA in *sf-High* for High-mobility state and *sf-Medium* for Medium-mobility state

**Speed dependent ScalingFactor for TreselectionGERA**

This specifies scaling factor for TreselectionGERAin H *sf-High* for High-mobility state and *sf-Medium* for Medium-mobility state

**Speed dependent ScalingFactor for TreselectionCDMA\_HRPD**

This specifies scaling factor for TreselectionCDMA\_HRPDin *sf-High* for High mobility state and *sf-Medium* for Medium-mobility state

**Speed dependent ScalingFactor for TreselectionCDMA\_1xRTT**

This specifies scaling factor for TreselectionCDMA\_1xRTTin *sf-High* for High mobility state and *sf-Medium* for Medium-mobility state

#### 5.2.4.8 Cell reselection with CSG cells

##### 5.2.4.8.1 Cell reselection from a non-CSG cell to a CSG cell

In addition to normal cell reselection, the UE shall use an autonomous search function to detect at least previously visited CSG member cells on non-serving frequencies, including inter-RAT frequencies, according to the performance requirements specified in TS 36.133 [10], when at least one CSG ID with associated PLMN identity is included in the UE's CSG whitelist. The UE may also use autonomous search on the serving frequency. The UE shall disable the autonomous search function for CSG cells if the UE's CSG whitelist is empty.

NOTE: The UE autonomous search function, per UE implementation, determines when and/or where to search for CSG member cells.

If the UE detects one or more suitable CSG cells on different frequencies, then the UE shall reselect to one of the detected cells irrespective of the frequency priority of the cell the UE is currently camped on, if the concerned CSG cell is the highest ranked cell on that frequency.

If the UE detects a suitable CSG cell on the same frequency, it shall reselect to this cell as per normal reselection rules (5.2.4.6.).

If the UE detects one or more suitable CSG cells on another RAT, the UE shall reselect to one of them according to TS 25.304 [19].

##### 5.2.4.8.2 Cell reselection from a CSG cell

While camped on a suitable CSG cell, the UE shall apply the normal cell reselection rules as defined in clause 5.2.4.

To search for suitable CSG cells on non-serving frequencies, the UE may use an autonomous search function. If the UE detects a CSG cell on a non-serving frequency, the UE may reselect to the detected CSG cell if it is the highest ranked cell on its frequency.

If the UE detects one or more suitable CSG cells on another RAT, the UE may reselect to one of them if allowed according to TS 25.304 [19].

#### 5.2.4.9 Cell reselection with Hybrid cells

In addition to normal cell reselection rules, the UE shall use an autonomous search function to detect at least previously visited hybrid cells whose CSG ID and associated PLMN identity is in the UE's CSG whitelist according to the performance requirements specified in TS 36.133 [10]. The UE shall treat detected hybrid cells as CSG cells if the CSG ID and associated PLMN identity of the hybrid cell is in the UE's CSG whitelist and as normal cells otherwise.

#### 5.2.4.10 E-UTRAN Inter-frequency Redistribution procedure

If a UE is redistribution capable and *redistributionServingInfo* is included in *SystemInformationBlockType3* and *redistributionInterFreqInfo* is included in *SystemInformationBlockType5* and the UE is not configured with dedicated priorities and

- if T360 is not running and if *redistrOnPagingOnly* is not present in *SystemInformationBlockType3*; or

- if T360 expires and if *redistrOnPagingOnly* is not present in *SystemInformationBlockType3*; or

- if *Paging* message is received and the *redistributionIndication* is included:

- Perform inter-frequency measurement as specified in 5.2.4.2;

- Once measurement results are available perform redistribution target selection as specified in 5.2.4.10.1;

- Start T360.

The UE shall stop T360 and cease to consider a frequency or cell to be redistribution target when:

- the UE enters RRC\_CONNECTED state; or

- T360 expires; or

- if *Paging* message is received and the *redistributionIndication* is included while T360 is running; or

- the UE reselects a cell not belonging to redistribution target.

##### 5.2.4.10.1 Redistribution target selection

The UE shall compile a sorted list of one or more candidate redistribution targets, and for each candidate entry [j] a valid *redistrFactor[j]*,in which entries are added in increasing index order starting with index 0 as follows:

- for the serving frequency (*redistributionFactorServing* is included in *SystemInformationBlockType3* whenever redistribution is configured*)*:

- the serving cell if *redistributionFactorCell* is included;

- otherwise the serving frequency;

- In both cases, *redistrFactor*[0] is set to *redistributionFactorServing*;

- for each entry in *InterFreqCarrierFreqList* and subsequent for each entry in *InterFreqCarrierFreqListExt:*

- the cell ranked as the best cell on this frequency according to clause 5.2.4.6 if *redistributionNeighCellList* is configured and includes this cell;

- otherwise, the concerned frequency if *redistributionFactorFreq* is configured and if at least one cell on the frequency fullfills the cell selection criterion S defined in 5.2.3.2;

- If the cell is included, *redistrFactor*[j] is set to the corresponding *redistributionFactorCell*; If the frequency is included, *redistrFactor*[j] is set to the corresponding *redistributionFactorFreq*;

The UE shall choose a redistribution target as follows:

- If [0], the UE shall choose the frequency or the cell corresponding to redistrFactor[0] as its redistribution target or;

- If , then the UE shall choose the frequency or cell corresponding to *redistrFactor*[i] as its redistribution target;

- ;

If there are no redistribution candidates apart from the serving frequency or cell, the redistrRange[0] = 1.

Otherwise, the redistrRange[i] of E-UTRAN frequency or cell is defined by:



Where: maxCandidates is the total number of frequencies/cells with valid redistrFactor[j].

#### 5.2.4.11 Cell reselection or CN type change when storing UE AS context

For UEs storing UE AS context and *resumeIdentity* as specified in TS 36.331 [3], upon cell reselection to another RAT or upon reselecting to another CN type, the UE shall discard the stored UE AS context and *resumeIdentity*.

#### 5.2.4.12 Relaxed monitoring

##### 5.2.4.12.0 Relaxed monitoring measurement rules

When the UE is required to perform intra-frequency or inter-frequency measurement according to the measurement rules in clause 5.2.4.2 or 5.2.4.2a, the UE may choose not to perform intra-frequency or inter-frequency measurements when:

- The relaxed monitoring criterion in clause 5.2.4.12.1 is fulfilled for a period of TSearchDeltaP, and

- Less than 24 hours have passed since measurements for cell reselection were last performed, and

- The UE has performed intra-frequency or inter-frequency measurements for at least TSearchDeltaP after selecting or reselecting a new cell.

##### 5.2.4.12.1 Relaxed monitoring criterion

The relaxed monitoring criterion is fulfilled when:

- (SrxlevRef – Srxlev) < SSearchDeltaP

Where:

- Srxlev = current Srxlev value of the serving cell (dB).

- SrxlevRef = reference Srxlev value of the serving cell (dB), set as follows:

- After selecting or reselecting a new cell, or

- If (Srxlev - SrxlevRef) > 0, or

- If the relaxed monitoring criterion has not been met for TSearchDeltaP:

- the UE shall set the value of SrxlevRef to the current Srxlev value of the serving cell;

- TSearchDeltaP = 5 minutes, or the eDRX cycle length if eDRX is configured and the eDRX cycle length is longer than 5 minutes.

#### 5.2.4.13 Cell reselection or CN type change in RRC\_INACTIVE state

For UE in the RRC\_INACTIVE state, upon cell reselection to another RAT or CN type change, UE transitions from RRC\_INACTIVE to RRC\_IDLE and performs actions as specified in TS 36.331 [3].

### 5.2.5 Void

### 5.2.6 Camped Normally state

This state is applicable for RRC\_IDLE and RRC\_INACTIVE state.

When camped normally, the UE shall perform the following tasks:

- monitor the paging channel of the cell as specified in clause 7 according to information sent in system information;

- monitor relevant System Information as specified in TS 36.331 [3];

- perform necessary measurements for the cell reselection evaluation procedure;

- execute the cell reselection evaluation process on the following occasions/triggers:

1) UE internal triggers, so as to meet performance as specified in TS 36.133 [10];

2) When information on the BCCH or BR-BCCH used for the cell reselection evaluation procedure has been modified.

### 5.2.7 Cell Selection at transition to RRC\_IDLE or RRC\_INACTIVE state

For NB-IoT cell selection at transition to RRC\_IDLE state is defined in clause 5.2.7a.

At reception of *RRCConnectionRelease* message or *RRCEarlyDataComplete* message to move the UE into RRC\_IDLE or RRC\_INACTIVE, UE shall attempt to camp on a suitable cell according to *redirectedCarrierInfo*, if included in the *RRCConnectionRelease* or *RRCEarlyDataComplete* message. If the UE cannot find a suitable cell, the UE is allowed to camp on any suitable cell of the indicated RAT. If the *RRCConnectionRelease* message or *RRCEarlyDataComplete* message does not contain the *redirectedCarrierInfo* UE shall attempt to select a suitable cell on an EUTRA carrier. If no suitable cell is found according to the above, the UE shall perform a cell selection starting with Stored Information Cell Selection procedure in order to find a suitable cell to camp on.

When returning to RRC\_IDLE or RRC\_INACTIVE state after UE moved to RRC\_CONNECTED state from *camped on any cell* state, UE shall attempt to camp on an acceptable cell according to *redirectedCarrierInfo*, if included in the *RRCConnectionRelease* message. If the UE cannot find an acceptable cell, the UE is allowed to camp on any acceptable cell of the indicated RAT. If the *RRCConnectionRelease* message does not contain *redirectedCarrierInfo* UE shall attempt to select an acceptable cell on an EUTRA carrier. If no acceptable cell is found according to the above, the UE shall continue to search for an acceptable cell of any PLMN in state *any cell selection*.

### 5.2.7a Cell Selection at transition to RRC\_IDLE state for NB-IoT

At reception of *RRCConnectionRelease-NB* message or *RRCEarlyDataComplete-NB* message to move the UE into RRC\_IDLE, UE shall attempt to camp on a suitable cell according to *redirectedCarrierInfo*, if included in the *RRCConnectionRelease-NB* message or *RRCEarlyDataComplete-NB* message. If the UE cannot find a suitable cell, the UE is allowed to camp on a suitable cell of any NB-IoT carrier. If the *RRCConnectionRelease-NB* message or *RRCEarlyDataComplete-NB* message does not contain the *redirectedCarrierInfo* UE shall attempt to select a suitable cell on a NB-IoT carrier.

### 5.2.8 Any Cell Selection state

For NB-IoT Any Cell Selection state is defined in clause 5.2.8a.

This state is applicable for RRC\_IDLE and RRC\_INACTIVE state. In this state, the UE shall perform cell selection process to find a suitable cell. If the cell selection process fails to find a suitable cell after a complete scan of all RATs and all frequency bands supported by the UE, the UE shall attempt to find an acceptable cell of any PLMN to camp on, trying all RATs that are supported by the UE and searching first for a high quality cell, as defined in clause 5.1.2.2.

The UE, which is not camped on any cell, shall stay in this state.

### 5.2.8a Any Cell Selection state for NB-IoT

In this state, the UE shall attempt to find a suitable cell of any PLMN to camp on and searching first for a high quality cell, as defined in clause 5.1.2.2.

The UE, which is not camped on any cell, shall stay in this state until a suitable cell is found.

### 5.2.9 Camped on Any Cell state

In this state, the UE shall perform the following tasks:

- monitor the paging channel of the cell as specified in clause 7 according to information sent in system information;

- monitor relevant System Information as specified in TS 36.331 [3];

- perform necessary measurements for the cell reselection evaluation procedure;

- execute the cell reselection evaluation process on the following occasions/triggers:

1) UE internal triggers, so as to meet performance as specified in TS 36.133 [10];

2) When information on the BCCH or BR-BCCH used for the cell reselection evaluation procedure has been modified;

- regularly attempt to find a suitable cell trying all frequencies of all RATs that are supported by the UE. If a suitable cell is found, UE shall move to *camped normally* state;

- if the UE supports voice services and the current cell does not support emergency call as indicated in System information specified in TS 36.331 [3], the UE should perform cell selection/ reselection to an acceptable cell of any supported RAT regardless of priorities provided in system information from current cell, if no suitable cell is found.

NOTE: The UE is allowed to not perform reselection to an inter-frequency E-UTRAN cell in order to prevent camping on a cell on which it cannot initiate an IMS emergency call.

## 5.3 Cell Reservations and Access Restrictions

There are two mechanisms which allow an operator to impose cell reservations or access restrictions. The first mechanism uses indication of cell status and special reservations for control of cell selection and reselection procedures. The second mechanism, referred to as Access Control, shall allow preventing selected classes of users or ACDC categories from sending initial access messages for load control reasons. For Access Control based on Access Classes, at subscription, one or more Access Classes are allocated to the subscriber and stored in the USIM TS 22.011 [4]. For Access Control based on ACDC categories, at subscription at least four ACDC categories are allocated to the subscriber and stored in the ACDC MO TS 24.105 [31] or USIM TS 31.102 [32].

### 5.3.1 Cell status and cell reservations

Cell status and cell reservations are indicated in the *SystemInformationBlockType1* message (or *SystemInformationBlockType1-BR* message or *SystemInformationBlockType1-NB* message) TS 36.331 [3] by means of the following fields:

- *cellBarred* (IE type: "barred" or "not barred")   
This field indicates if the cell is barred for connectivity to EPC.  
This field is ignored by the UEs supporting *crs-IntfMitig* while *crs-IntfMitigEnabled* is included in SIB1.   
This field is ignored by the BL UEs or UEs in CE supporting *ce-CRS-IntfMitig* while *crs-IntfMigitNumPRBs* is included in SIB1-BR.  
In case of multiple EPC PLMNs indicated in SIB1/SIB1-BR, this field is common for all EPC PLMNs

- *cellBarred-5GC* (IE type: "barred" or "not barred")  
This field indicates if the cell is barred for connectivity to 5GC.  
This field is ignored if the UE does not support E-UTRA connected to 5GC or if the UE supports network-based CRS interference mitigation and *nw-BasedCRS-InterferenceMitigation* is included in *SystemInformationBlockType1*.  
In case of multiple 5GC PLMNs indicated in SIB1, this field is common for all 5GC PLMNs.

- *cellReservedForOperatorUse* (IE type: "reserved" or "not reserved")  
This field indicates if the cell is reserved for operator use.  
This field is ignored by the UEs supporting *crs-IntfMitig* while *crs-IntfMitigEnabled* is included in SIB1.   
This field is ignored by the BL UEs or UEs in CE supporting *ce-CRS-IntfMitig* while *crs-IntfMigitNumPRBs* is included in SIB1-BR.   
In case of multiple EPC or 5GC PLMNs indicated in SIB1/SIB1-BR, this field is specified per EPC or 5GC PLMN.

- *cellBarred-CRS* (IE type: "barred" or "not barred")  
This field indicates if the cell is barred for connectivity to EPC for UEs supporting network-based CRS interference mitigation.  
*barred* means the cell is barred for UEs supporting *crs-IntfMitig* while *crs-IntfMitigEnabled* is included in SIB1. For BL UEs or UEs in CE capable of *ce-CRS-IntfMitig*, *barred* means the cell is barred while *crs-IntfMitigNumPRBs* is included in SIB1-BR.  
This field is ignored by the UE if the UE does not support CRS interference mitigation or while *crs-IntfMitigConfig* is not included in SIB1 (SIB1-BR for BL UEs or UEs in CE).  
In case of multiple PLMNs indicated in SIB1/SIB1-BR, this field is common for all PLMNs.

- *cellBarred-5GC-CRS* (IE type: "barred" or "not barred")  
This field indicates if the cell is barred for connectivity to 5GC for UEs supporting network-based CRS interference mitigation.  
This field is ignored if the UE does not support E-UTRA connected to 5GC or network-based CRS interference mitigation.  
In case of multiple 5GC PLMNs indicated in SIB1, this field is common for all 5GC PLMNs.

- *cellReservedForOperatorUse-CRS* (IE type: "reserved" or "not reserved")  
This field indicates if the cell is reserved for operator use for UEs supporting network-based CRS interference mitigation.  
*reserved* means the cell is "reserved" for operator use for UEs supporting *crs-IntfMitig* while *crs-IntfMitigEnabled* is included in SIB1.   
For BL UEs or UEs in CE capable of *ce-CRS-IntfMitig*, *reserved* means the cell is "reserved" for operator use while *crs-IntfMitigNumPRBs* is included in SIB1-BR.  
This field is ignored if the UE does not support CRS interference mitigation or while *crs-IntfMitigConfig* is not included in SIB1 (SIB1-BR for BL UEs or UEs in CE).  
In case of multiple PLMNs indicated in SIB1/SIB1-BR, this field is specified per PLMN.

The following description for handling of barred and reserved cells is per CN type. If the UE supports more than one CN type, the UE shall only exclude a cell as candidate for selection/reselection if it is excluded for both CN types.

NOTE: Fields *cellBarred-CRS* and *cellReservedForOperatorUse-CRS* are not indicated in *SystemInformationBlockType1-NB*

When cell status is indicated as "not barred" and "not reserved" for operator use,

- All UEs shall treat this cell as candidate during the cell selection and cell reselection procedures.

When cell status is indicated as "not barred" and "reserved" for operator use for any PLMN,

- UEs assigned to Access Class 11 or 15 operating in their HPLMN/EHPLMN shall treat this cell as candidate during the cell selection and reselection procedures if the field *cellReservedForOperatorUse* for that PLMN set to "reserved".

- UEs assigned to an Access Class in the range of 0 to 9, 12 to 14 shall behave as if the cell status is "barred" in case the cell is "reserved for operator use" for the registered PLMN or the selected PLMN.

NOTE: ACs 11, 15 are only valid for use in the HPLMN/ EHPLMN; ACs 12, 13, 14 are only valid for use in the home country TS 22.011 [4].

When cell status "barred" is indicated or to be treated as if the cell status is "barred",

- The UE is not permitted to select/reselect this cell, not even for emergency calls.

- The UE shall consider other cells for cell selection/reselection according to the following rule:

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *MasterInformationBlock (*or *MasterInformationBlock-NB),* the *SystemInformationBlockType1 (*or *SystemInformationBlockType1-BR* message or *SystemInformationBlockType1-NB),* or the *SystemInformationBlockType2 (*or *SystemInformationBlockType2-NB)*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds.

- the UE may select another cell on the same frequency if the selection criteria are fulfilled.

- the UE may select the same cell in normal coverage if the UE was barred in the cell due to being unable to acquire *MasterInformationBlock*, *SystemInformationBlockType1-BR*, or *SystemInformationBlockType2* in enhanced coverage, but was able to acquire *MasterInformationBlock*, *SystemInformationBlockType1*, and *SystemInformationBlockType2* in normal coverage, if the selection criteria are fulfilled.

- else

- If the cell is a CSG cell:

- the UE may select another cell on the same frequency if the selection/reselection criteria are fulfilled.

- else

- If the field *intraFreqReselection* in field *cellAccessRelatedInfo* in *SystemInformationBlockType1 (*or *SystemInformationBlockType1-BR* message or *SystemInformationBlockType1-NB)* message is set to "allowed", the UE may select another cell on the same frequency if re-selection criteria are fulfilled.

- The UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

- If the field *intraFreqReselection* in field *cellAccessRelatedInfo* in *SystemInformationBlockType1* (or *SystemInformationBlockType1-BR* message or *SystemInformationBlockType1-NB*) message is set to "not allowed" the UE shall not re-select a cell on the same frequency as the barred cell;

- The UE shall exclude the barred cell and the cells on the same frequency as a candidate for cell selection/reselection for 300 seconds.

The cell selection of another cell may also include a change of RAT or, if the previous and selected cell are both E-UTRA cells, a change of the CN type.

### 5.3.2 Access control

For UE camping on E-UTRA connected to EPC, information on cell access restrictions associated with the Access Classes or ACDC categories is broadcast as system information, TS 36.331 [3]. For UE camping on E-UTRA connected to 5GC, information on cell access restrictions associated with Access Categories and Identities is broadcast as system information, TS 36.331 [3].

For UE camping on E-UTRA connected to EPC, the UE shall ignore Access Class or ACDC category related cell access restrictions when selecting a cell to camp on, i.e. it shall not reject a cell for camping on because access on that cell is not allowed for any of the Access Classes or ACDC categories of the UE. A change of the indicated access restriction shall not trigger cell reselection by the UE. For UE camping on E-UTRA connected to 5GC, the UE shall ignore Access Category and Identity related cell access restrictions for cell reselection. A change of the indicated access restriction shall not trigger cell reselection by the UE.

For UE camping on E-UTRA connected to EPC, access Class or ACDC category related cell access restrictions shall be checked by the UE when starting RRC connection establishment procedure as specified in TS 36.331 [3]. For UE camping on E-UTRA connected to 5GC, Access Category and Identity related cell access restrictions shall be checked by the UE for NAS initiated access attempts and RNAU as specified in TS 36.331 [3].

### 5.3.3 Emergency call

A restriction on emergency calls, if needed, is indicated by the field *ac-BarringForEmergency* TS 36.331 [3]. If access class 10 is indicated as barred in a cell, UEs with access class 0 to 9 or without an IMSI are not allowed to initiate emergency calls in this cell. For UEs with access classes 11 to 15, emergency calls are not allowed if both access class 10 and the relevant access class (11 to 15) are barred. Otherwise, emergency calls are allowed for those UEs.

Full details of operation under "Access class barred list" are described in TS 22.011 [4].

For E-UTRA connected to 5GC, the restriction on emergency calls is indicated by access control information of access category 2 under unified access control TS 36.331 [3].

## 5.4 Tracking Area registration

In the UE, the AS shall report tracking area information to the NAS.

If the UE reads more than one PLMN identity in the current cell, the UE shall report the found PLMN identities that make the cell suitable in the tracking area information to NAS.

The NAS part of the location registration process is specified in TS 23.122 [5].

Actions for the UE AS upon reception of Location Registration reject are specified in TS 22.011 [4] and TS 24.301 [16].

## 5.5 Support for manual CSG selection

### 5.5.1 E-UTRA case

In the UE on request of NAS, the AS shall scan all RF channels in the E-UTRA bands according to its capabilities to find available CSGs. On each carrier, the UE shall at least search for the strongest cell, read its system information and report available CSG ID(s) together with their "HNB name" (if broadcast) and PLMN(s) to the NAS. The search for available CSGs may be stopped on request of the NAS.

If NAS has selected a CSG and provided this selection to AS, the UE shall search for an acceptable or suitable cell belonging to the selected CSG to camp on.

### 5.5.2 UTRA case

Support for manual CSG selection in UTRA is described in TS 25.304 [8].

## 5.6 RAN-assisted WLAN interworking

The purpose of this procedure is to facilitate RAN-assisted WLAN interworking.

### 5.6.1 RAN assistance parameter handling in RRC\_IDLE

RAN assistance parameters may be provided to the UE in *SystemInformationBlockType17* or in the *RRCConnectionReconfiguration* message. RAN assistance parameters are used only if the UE is camped normally.

### 5.6.2 Access network selection and traffic steering rules

The rules in this clause are only applicable for WLANs for which identifiers has been signaled to the UE by E-UTRAN and the UE is capable of RAN-assisted WLAN interworking based on access network selection and traffic steering rules. Coexistence with ANDSF based WLAN selection and traffic steering methods on the UE is based on mechanism described in TS 23.402 [25]. The rules refer to the following quantities:

|  |  |
| --- | --- |
| ChannelUtilizationWLAN | WLAN channel utilization as defined in clause 8.4.2.30 in [26]. |
| BackhaulRateDlWLAN | WLAN DLBandwidth as defined in clause 9.1.2 in [27]. |
| BackhaulRateUlWLAN | WLAN ULBandwidth as defined in clause 9.1.2 in [27]. |
| WLANRSSI | WLAN RSSI as defined in TS 36.214 [7]. |
| RSRPmeas | Qrxlevmeas in RRC\_IDLE, and PCell RSRP in RRC\_CONNECTED as defined in TS 36.331 TS 36.331 [3]. |
| RSRQmeas | Qqualmeas in RRC\_IDLE, and PCell RSRQ in RRC\_CONNECTED as defined in TS 36.331 TS 36.331 [3]. |

The upper layers in the UE shall be notified (see TS 24.302 [28]) when and for which WLAN(s), that matches all the provided identifiers (in clause 5.6.3) for a specific entry in the list, the following conditions 1 and 2 for steering traffic from E-UTRAN to WLAN are satisfied for a time interval TsteeringWLAN:

1. In the E-UTRAN serving cell:

- RSRPmeas < ThreshServingOffloadWLAN, LowP; or

- RSRQmeas < ThreshServingOffloadWLAN, LowQ;

2. In the target WLAN:

- ChannelUtilizationWLAN < ThreshChUtilWLAN, Low; and

- BackhaulRateDlWLAN > ThreshBackhRateDLWLAN, High; and

- BackhaulRateUlWLAN > ThreshBackhRateULWLAN, High; and

- WLANRSSI > ThreshWLANRSSI, High;

The UE shall not consider the metrics for which a threshold has not been provided. The UE shall evaluate the E-UTRAN conditions on PCell only. If not all metrics related to the provided thresholds can be acquired for a WLAN BSS, the UE shall exclude that WLAN BSS from the evaluation of the above rule.

The upper layers in the UE shall be notified (see TS 24.302 [28]) when the following conditions 3 or 4 for steering traffic from WLAN to E-UTRAN are satisfied for a time interval TsteeringWLAN:

1. In the source WLAN:

- ChannelUtilizationWLAN > ThreshChUtilWLAN, High; or

- BackhaulRateDlWLAN < ThreshBackhRateDLWLAN, Low; or

- BackhaulRateUlWLAN < ThreshBackhRateULWLAN, Low; or

- WLANRSSI < ThreshWLANRSSI, Low;

2. In the target E-UTRAN cell:

- RSRPmeas > ThreshServingOffloadWLAN, HighP; and

- RSRQmeas > ThreshServingOffloadWLAN, HighQ;

The UE shall not consider the metrics for which a threshold has not been provided. The UE shall evaluate the E-UTRAN conditions on PCell only.

### 5.6.3 RAN assistance parameters definition

The following RAN assistance parameters for RAN-assisted WLAN interworking may be provided:

**ThreshServingOffloadWLAN, LowP**

This specifies the RSRP threshold (in dBm) used by the UE for traffic steering to from E-UTRAN to WLAN.

**ThreshServingOffloadWLAN, HighP**

This specifies the RSRP threshold (in dBm) used by the UE for traffic steering from WLAN to E-UTRAN.

**ThreshServingOffloadWLAN, LowQ**

This specifies the RSRQ threshold (in dB) used by the UE for traffic steering from E-UTRAN to WLAN.

**ThreshServingOffloadWLAN, HighQ**

This specifies the RSRQ threshold (in dB) used by the UE for traffic steering from WLAN to E-UTRAN.

**ThreshChUtilWLAN, Low**

This specifies the WLAN channel utilization (BSS load) threshold used by the UE for traffic steering from E-UTRAN to WLAN.

**ThreshChUtilWLAN, High**

This specifies the WLAN channel utilization (BSS load) threshold used by the UE for traffic steering from WLAN to E-UTRAN.

**ThreshBackhRateDLWLAN, Low**

This specifies the backhaul available downlink bandwidth threshold used by the UE for traffic steering from WLAN to E-UTRAN.

**ThreshBackhRateDLWLAN, High**

This specifies the backhaul available downlink bandwidth threshold used by the UE for traffic steering from E-UTRAN to WLAN.

**ThreshBackhRateULWLAN, Low**

This specifies the backhaul available uplink bandwidth threshold used by the UE for traffic steering from WLAN to E-UTRAN.

**ThreshBackhRateULWLAN, High**

This specifies the backhaul available uplink bandwidth threshold used by the UE for traffic steering from E-UTRAN to WLAN.

**ThreshWLANRSSI, Low**

This specifies the WLAN RSSI threshold used by the UE for traffic steering from WLAN to E-UTRAN.

**ThreshWLANRSSI, High**

This specifies the Beacon RSSI threshold used by the UE for traffic steering from E-UTRAN to WLAN.

**TsteeringWLAN**

This specifies the timer value TsteeringWLAN during which the rules should be fulfilled before starting traffic steering between E-UTRAN and WLAN.

**WLAN identifiers**

Only the SSIDs, BSSIDs and HESSIDs which are provided in this parameter shall be considered for traffic steering between E-UTRAN and WLAN based on the rules in this clause.

# 6 Reception of broadcast information

## 6.1 Reception of system information

The NAS is informed if the cell selection and reselection results in changes in the received NAS system information.

The UE shall monitor the Paging Occasions (POs) as described in chapter 7.1 to receive System Information change notifications in RRC\_IDLE. Changes in the system information are indicated by the network using a *Paging* message or Direct Indication information on MPDCCH and NPDCCH respectively. When the *Paging* message or Direct Indication information indicates system information changes then the UE shall re-acquire the concerned system information, as specified in TS 36.331 [3].

## 6.2 Reception of MBMS

A UE, except for BL UE or UE in enhanced coverage or NB-IoT UE, interested to receive MBMS services provided using MBSFN transmission shall apply the MCCH information acquision procedure as specified in TS 36.331 [3] to receive the MCCH information upon entering the corresponding MBSFN area and upon receiving a notification that the MCCH information has changed. A UE interested to receive MBMS services provided using MBSFN transmission identifies if a service that it is interested to receive is started or ongoing by receiving the MCCH information, and then receives a MTCH corresponding to the identified service.

A UE interested to receive MBMS services provided using SC-PTM transmission shall apply the SC-MCCH information acquisition procedure as specified in TS 36.331 [3] to receive the SC-MCCH information upon entering a new cell and upon receiving a notification that the SC-MCCH information has changed. A UE interested to receive MBMS services provided using SC-PTM transmission identifies if a service that it is interested to receive is started or ongoing by receiving the SC-MCCH information, and then receives a SC-MTCH configured using the SC-MRB establishment procedure in TS 36.331 [3] and using the DL-SCH reception and SC-PTM DRX procedure as specified in TS 36.321 [30].

For BL UE or UE in enhanced coverage or NB-IoT UE interested to receive MBMS services provided using SC-PTM transmission, in case of conflict, reception of paging or establishment of a RRC connection for Mobile Terminated Call and Mobile Originated Signalling takes precedence over SC-PTM reception.

# 7 Paging

## 7.1 Discontinuous Reception for paging

The UE may use Discontinuous Reception (DRX) in idle mode in order to reduce power consumption. One Paging Occasion (PO) is a subframe where there may be P-RNTI transmitted on PDCCH or MPDCCH or, for NB-IoT on NPDCCH addressing the paging message. In P-RNTI transmitted on MPDCCH case, PO refers to the starting subframe of MPDCCH repetitions. In case of P-RNTI transmitted on NPDCCH, PO refers to the starting subframe of NPDCCH repetitions unless subframe determined by PO is not a valid NB-IoT downlink subframe then the first valid NB-IoT downlink subframe after PO is the starting subframe of the NPDCCH repetitions. The paging message is same for both RAN initiated paging and CN initiated paging.

The UE initiates RRC Connection Resume procedure upon receiving RAN paging. If the UE receives a CN initiated paging in RRC\_INACTIVE state, the UE moves to RRC\_IDLE and informs NAS.

One Paging Frame (PF) is one Radio Frame, which may contain one or multiple Paging Occasion(s). When DRX is used the UE needs only to monitor one PO per DRX cycle.

One Paging Narrowband (PNB) is one narrowband, on which the UE performs the paging message reception.

PF, PO, and PNB are determined by following formulae using the DRX parameters provided in System Information:

PF is given by following equation:

SFN mod T= (T div N)\*(UE\_ID mod N)

Index i\_s pointing to PO from subframe pattern defined in 7.2 will be derived from following calculation:

i\_s = floor(UE\_ID/N) mod Ns

If P-RNTI is monitored on MPDCCH, the PNB is determined by the following equation:

PNB = floor(UE\_ID/(N\*Ns)) mod Nn

If P-RNTI is monitored on NPDCCH and the UE supports paging on a non-anchor carrier, and if paging configuration for non-anchor carrier is provided in system information, then the paging carrier is determined by the paging carrier with smallest index n (0 ≤ n ≤ Nn-1) fulfilling the following equation:

floor(UE\_ID/(N\*Ns)) mod W < W(0) + W(1) + … + W(n)

System Information DRX parameters stored in the UE shall be updated locally in the UE whenever the DRX parameter values are changed in SI. If the UE has no IMSI, for instance when making an emergency call without USIM, the UE shall use as default identity UE\_ID = 0 in the PF, i\_s, and PNB formulas above. If the UE has no 5G-S-TMSI, for instance when the UE has not yet registered onto the network, the UE shall use as default identity UE\_ID = 0 in the PF and i\_s formulas above.

The following Parameters are used for the calculation of the PF, i\_s, PNB, and the NB-IoT paging carrier:

- T: DRX cycle of the UE. Except for NB-IoT, if a UE specific extended DRX value of 512 radio frames is configured by upper layers according to 7.3, T =512. Otherwise, T is determined by the shortest of the UE specific DRX value, if allocated by upper layers, and a default DRX value broadcast in system information. If UE specific DRX is not configured by upper layers, the default value is applied. UE specific DRX is not applicable for NB-IoT. In RRC\_INACTIVE state, T is determined by the shortest of the RAN paging cycle, the UE specific paging cycle, and the default paging cycle, if allocated by upper layers.

- nB: 4T, 2T, T, T/2, T/4, T/8, T/16, T/32, T/64, T/128, and T/256, and for NB-IoT also T/512, and T/1024.

- N: min(T,nB)

- Ns: max(1,nB/T)

- Nn : number of paging narrowbands (for P-RNTI monitored on MPDCCH) or paging carriers (for P-RNTI monitored on NPDCCH) provided in system information

- UE\_ID:

If the UE supports E-UTRA connected to 5GC and NAS indicated to use 5GC for the selected cell:

5G-S-TMSI mod 1024, if P-RNTI is monitored on PDCCH.

else

IMSI mod 1024, if P-RNTI is monitored on PDCCH.

IMSI mod 4096, if P-RNTI is monitored on NPDCCH.

IMSI mod 16384, if P-RNTI is monitored on MPDCCH or if P-RNTI is monitored on NPDCCH and the UE supports paging on a non-anchor carrier, and if paging configuration for non-anchor carrier is provided in system information.

- W(i): Weight for NB-IoT paging carrier i.

- W: Total weight of all NB-IoT paging carriers, i.e. W = W(0) + W(1) + … + W(Nn-1).

IMSI is given as sequence of digits of type Integer (0..9), IMSI shall in the formulae above be interpreted as a decimal integer number, where the first digit given in the sequence represents the highest order digit.

For example:

IMSI = 12 (digit1=1, digit2=2)

In the calculations, this shall be interpreted as the decimal integer "12", not "1x16+2 = 18".

5G-S-TMSI is a 48 bit long bit string as defined in TS 23.501 [39]. 5G-S-TMSI shall in the PF and i\_s formulae above be interpreted as a binary number where the left most bit represents the most significant bit.

## 7.2 Subframe Patterns

FDD:

- If P-RNTI is transmitted on PDCCH or NPDCCH, or if P-RNTI is transmitted on MPDCCH with system bandwidth > 3MHz:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Ns | PO when i\_s=0 | PO when i\_s=1 | PO when i\_s=2 | PO when i\_s=3 |
| 1 | 9 | N/A | N/A | N/A |
| 2 | 4 | 9 | N/A | N/A |
| 4 | 0 | 4 | 5 | 9 |

- If P-RNTI is transmitted on MPDCCH with system bandwidth of 1.4MHz and 3MHz:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Ns | PO when i\_s=0 | PO when i\_s=1 | PO when i\_s=2 | PO when i\_s=3 |
| 1 | 5 | N/A | N/A | N/A |
| 2 | 5 | 5 | N/A | N/A |
| 4 | 5 | 5 | 5 | 5 |

TDD (all UL/DL configurations):

- If P-RNTI is transmitted on PDCCH or NPDCCH, or if P-RNTI is transmitted on MPDCCH with system bandwidth > 3MHz:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Ns | PO when i\_s=0 | PO when i\_s=1 | PO when i\_s=2 | PO when i\_s=3 |
| 1 | 0 | N/A | N/A | N/A |
| 2 | 0 | 5 | N/A | N/A |
| 4 | 0 | 1 | 5 | 6 |

- If P-RNTI is transmitted on MPDCCH with system bandwidth of 1.4MHz and 3MHz:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Ns | PO when i\_s=0 | PO when i\_s=1 | PO when i\_s=2 | PO when i\_s=3 |
| 1 | 1 | N/A | N/A | N/A |
| 2 | 1 | 6 | N/A | N/A |
| 4 | 1 | 1 | 6 | 6 |

## 7.3 Paging in extended DRX

The UE may be configured by upper layers with an extended DRX (eDRX) cycle TeDRX. Except for NB-IoT, the UE may operate in extended DRX only if the UE is configured by upper layers and the cell indicates support for eDRX in System Information. For NB-IoT, the UE may operate in extended DRX only if the UE is configured by upper layers. If the UE is configured with a TeDRX cycle of 512 radio frames, it monitors POs as defined in 7.1 with parameter T = 512. Otherwise, a UE configured with eDRX monitors POs as defined in 7.1 (i.e, based on the upper layer configured DRX value and a default DRX value determined in 7.1), during a periodic Paging Time Window (PTW) configured for the UE or until a paging message including the UE's NAS identity is received for the UE during the PTW, whichever is earlier. The PTW is UE-specific and is determined by a Paging Hyperframe (PH), a starting position within the PH (PTW\_start) and an ending position (PTW\_end). PH, PTW\_start and PTW\_end are given by the following formulae:

The PH is the H-SFN satisfying the following equation:

H-SFN mod TeDRX,H= (UE\_ID\_H mod TeDRX,H), where

- UE\_ID\_H:

- 10 most significant bits of the Hashed ID, if P-RNTI is monitored on PDCCH or MPDCCH

- 12 most significant bits of the Hashed ID, if P-RNTI is monitored on NPDCCH

- T eDRX,H : eDRX cycle of the UE in Hyper-frames, (TeDRX,H =1, 2, …, 256 Hyper-frames) (for NB-IoT, TeDRX,H =2, …, 1024 Hyper-frames) and configured by upper layers.

PTW\_start denotes the first radio frame of the PH that is part of the PTW and has SFN satisfying the following equation:

SFN = 256\* ieDRX, where

- ieDRX = floor(UE\_ID\_H /TeDRX,H) mod 4

PTW\_end is the last radio frame of the PTW and has SFN satisfying the following equation:

SFN = (PTW\_start + L\*100 - 1) mod 1024, where

- L = Paging Time Window length (in seconds) configured by upper layers

Hashed ID is defined as follows:

Hashed\_ID is Frame Check Sequence (FCS) for the bits b31, b30…, b0 of S-TMSI

S-TMSI = <b39, b38, …, b0> as defined in TS 23.003 [35]

The 32-bit FCS shall be the ones complement of the sum (modulo 2) of Y1 and Y2, where

- Y1 is the remainder of xk (x31 + x30 + x29 + x28 + x27 + x26 + x25 + x24 + x23 + x22 + x21 + x20 + x19 + x18 + x17 + x16 + x15 + x14 + x13 + x12 + x11 + x10 + x9 + x8 + x7 + x6 + x5 + x4 + x3 + x2 + x1 + 1) divided (modulo 2) by the generator polynomial x32 + x26 + x23 + x22 + x16 + x12 + x11 + x10 + x8 + x7 + x5 + x4 + x2 + x + 1, where k is 32; and

- Y2 is the remainder of Y3 divided (modulo 2) by the generator polynomial x32 + x26 + x23 + x22 + x16 + x12 + x11 + x10 + x8 + x7 + x5 + x4 + x2 + x + 1, where Y3 is the product of x32 by "b31, b30…, b0 of S-TMSI", i.e., Y3 is the generator polynomial x32 (b31\*x31 + b30\*x30 + … + b0\*1).

NOTE: The Y1 is 0xC704DD7B for any S-TMSI value. An example of hashed ID calculation is in Annex B.

## 7.4 Paging with Wake Up Signal

Paging with Wake Up Signal is only used in the cell in which the UE most recently entered RRC\_IDLE triggered by:

- reception of *RRCEarlyDataComplete*; or

- reception of *RRCConnectionRelease* not including *noLastCellUpdate*; or

- reception of *RRCConnectionRelease* including *noLastCellUpdate* and the UE was using WUS in this cell prior to this RRC connection attempt.

When the UE supports WUS and WUS configuration is provided in system information, the UE shall monitor WUS using the WUS parameters provided in System Information. When DRX is used and the UE detects WUS the UE shall monitor the following PO. When extended DRX is used and the UE detects WUS the UE shall monitor the following *numPOs* POs or until a paging message including the UE's NAS identity is received, whichever is earlier. If the UE does not detect WUS the UE is not required to monitor the following PO(s). If the UE missed a WUS occasion (e.g. due to cell reselection), it monitors every PO until the start of next WUS or until the PTW ends, whichever is earlier.

- *numPOs* = Number of consecutive Paging Occasions (PO) mapped to one WUS provided in system information where (*numPOs*≥1).

The WUS configuration, provided in system information, includes time-offset between end of WUS and start of the first PO of the *numPOs* POs UE is required to monitor. The timeoffset in subframes, used to calculate the start of a subframe *g*0 (see TS 36.213 [6]), is defined as follows:

- for UE using DRX, it is the signalled *timeoffsetDRX*;

- for UE using eDRX, it is the signalled *timeoffset-eDRX-Short* if *timeoffset-eDRX-Long* is not broadcasted;

- for UE using eDRX, it is the value determined according to Table 7.4-1 if *timeoffset-eDRX-Long* is broadcasted

Table 7.4-1: Determination of GAP between end of WUS and associated PO

|  |  |  |  |
| --- | --- | --- | --- |
|  | | *timeoffset-eDRX-Long* | |
| *1000ms* | *2000ms* |
| *UE Reported wakeUpSignalMinGap-eDRX* | ***40ms or not reported*** | *timeoffset-eDRX-Short* | *timeoffset-eDRX-Short* |
| ***240ms*** | *timeoffset-eDRX-Short* | *timeoffset-eDRX-Short* |
| ***1000ms*** | *timeoffset-eDRX-Long* | *timeoffset-eDRX-Long* |
| ***2000ms*** | *timeoffset-eDRX-Short* | *timeoffset-eDRX-Long* |

The timeoffset is used to determine the actual subframe *g*0 as follows (taking into consideration resultant SFN and/or H-SFN wrap-around of this computation):

*g*0 = PO – timeoffset, where PO is the Paging Occasion subframe as defined in clause 7.1

For UE using eDRX, the same timeoffset applies between the end of WUS and associated first PO of the *numPOs* POs for all the WUS occurrences for a PTW.

The timeoffset, *g*0, is used to calculate the start of the WUS as defined in TS 36.213 [6].

# 8 Logged measurements

The UE may be configured to perform logging of measurement results in RRC\_IDLE mode with the *LoggedMeasurementConfiguration* message as specified in TS 36.331 [3]*.* This configuration is valid while the logging duration timer is running.

If the configuration of logged measurements is valid, the UE shall perform logging of measurement results if all of the following conditions are met:

- The UE is in *camped normally* state in RRC\_IDLE mode;

- The RPLMN of the UE is the same as the RPLMN at the point of time of *LoggedMeasurementConfiguration* message reception, or is present in the *plmn-IdentityList* (see TS 36.331 [3]) if configured;

*-* The UE iscamped on a cell belonging to the *areaConfiguration* (see TS 36.331 [3]), if configured;

- The UE is camped on the RAT where the logged measurement configuration was received;

- The UE receives MBMS service from MBSFN area(s) belonging to *targetMBSFN-AreaList*, if included in the logged measurement configuration;

- The IDC capable UE does not detect the presence of in-device coexistence interference.

If the configuration of logged measurements is valid, but the UE is in *any cell* selection state in RRC\_IDLE mode, the UE perform logging of available information (i.e. at least indicator on *any cell selection* state and time stamp).

If the configuration of logged MBSFN measurements is valid, the UE shall perform logging of measurement results in RRC\_CONNECTED in addition to RRC\_IDLE, as described in TS 36.331 [3].

Otherwise, the logging of measurement results shall be suspended.

NOTE: Even if logging of measurement results is suspended, the logging duration timer and time stamp will continue, and the logged measurement configuration and corresponding log are kept.

# 9 Accessibility measurements

The UE logs failure information when the RRC connection establishment procedure fails as specified in TS 36.331 [3].

# 10 Mobility History Information

The UE stores the history of serving cells as specified in TS 36.331[3].

# 11 Sidelink operation

## 11.1 Sidelink communication and V2X sidelink communication

The UE may transmit or receive sidelink communication if it fulfils the condition(s) defined in TS 36.331 [3, 5.10.1a]. The UE may transmit or receive V2X sidelink communication if it fulfils the condition(s) defined in TS 36.331 [3, 5.10.1d]. When UE is in-coverage for sidelink operation as defined in clause 11.4, the UE may perform the sidelink communication according to *SystemInformationBlockType18* or perform the V2X sidelink communication according to *SystemInformationBlockType21* or *SystemInformationBlockType26,* and when out-of-coverage for sidelink, the UE may perform the sidelink communication according to *SL-Preconfiguration* or perform V2X sidelink communication according to *SL-V2X-Preconfiguration* or according to *SystemInformationBlockType21* or *SystemInformationBlockType26* of the cell on the frequency which provides inter-carrier V2X sidelink configuration, as specified in TS 36.331 [3]. The UE shall not perform V2X sidelink communication according to *SL-V2X-Preconfiguration* if the UE detects a cell providing V2X sidelink configuration or inter-carrier V2X sidelink configuration for the frequency UE is interested to perform V2X sidelink communication on.

## 11.2 Sidelink discovery

The UE may transmit sidelink discovery if it fulfils the condition(s) defined in TS 36.331 [3, 5.10.1b and 5.10.1c]. When UE is in-coverage for sidelink as defined in clause 11.4, the UE may perform the sidelink discovery according to *SystemInformationBlockType19*, and when out-of-coverage for sidelink as defined in clause 11.4, the UE may perform the sidelink discovery according to *SL-Preconfiguration*, as specified in TS 36.331 [3].

NOTE: Sidelink discovery reception in idle mode is up to UE implementation.

## 11.3 Sidelink synchronisation

The UE may perform sidelink synchronisation according to *SystemInformationBlockType18* for sidelink communication, *SystemInformationBlockType19* for sidelink discovery or *SystemInformationBlockType21* for V2X sidelink communication, as specified in TS 36.331 [3].

## 11.4 Cell selection and reselection for sidelink

The requirements defined in this clause for sidelink operation apply for UEs in RRC\_IDLE and in RRC\_CONNECTED.

When UE is interested to perform sidelink communication or sidelink discovery announcement on non-serving frequency, it shall perform measurements on that frequency for cell selection and intra-frequency reselection purpose in accordance with TS 36.133 [10]. When UE is interested to perform V2X sidelink communication on non-serving frequency, it may perform measurements on that frequency or the frequencies which can provide inter-carrier V2X sidelink configuration for that frequency for cell selection and intra-frequency reselection purpose in accordance with TS 36.133 [10].

If the UE detects at least one cell on the frequency which UE is configured to perform sidelink operation on fulfilling the S criterion in accordance with clause 11.4.1, it shall consider itself to be in-coverage for sidelink operation on that frequency. If the UE cannot detect any cell on that frequency meeting the S criterion, it shall consider itself to be out-of-coverage for sidelink operation on that frequency.

If the UE has selected a cell on a non-serving frequency for sidelink communication or V2X sidelink communication or sidelink discovery announcement, it shall perform additional intra-frequency reselection process to select a better cell for sidelink operation on that frequency in accordance with clause 11.4.1.

NOTE 1: The UE may consider the carrier pre-configured for sidelink communication or V2X sidelink communication, or the frequencies pre-configured for providing inter-carrier V2X sidelink configuration to have the highest cell reselection priority in accordance with clause 5.2.4.1.

NOTE 2: If the frequency the UE is configured to perform sidelink communication on is a serving frequency, the UE uses the serving cell on that frequency for the sidelink operation.

### 11.4.1 Parameters used for cell selection and reselection triggered for sidelink

When evaluating S criterion or R criterion (ranking), as defined in clause 5.2.3.2 and clause 5.2.4.6 respectively, for cell selection/reselection triggered for sidelink communication or V2X sidelink communication or sidelink discovery announcement on a non-serving frequency, UE shall perform the evaluation as follows:

- if the UE intends to perform sidelink discovery announcement and it is configured with *discCellSelectionInfo* applicable for that frequency as specified in TS 36.331 [3], the UE shall use cell selection/reselection parameters included in the *discCellSelectionInfo* for the evaluation, and for a parameter used in the evaluation but not included in the *discCellSelectionInfo* applicable for thatfrequency, UE shall apply zero value.

- else, the UE shall use cell selection/reselection parameters broadcast by the concerned cell (i.e. selected cell for the sidelink operation) for the evaluation.

# 12. General description of UE camping on E-UTRA connected to 5GC

The functions listed below are applicable to UE camping on E-UTRA connected to 5GC:

- RAN paging (only applicable to RRC\_INACTIVE state)

- Unified Access Control

The functions listed below are not applicable to UE camping on E-UTRA connected to 5GC:

- 5.5 Support for manual CSG selection

- 5.6 RAN-assisted WLAN interworking

- 6.2 Reception of MBMS

- 7.3 Paging in extended DRX

- 8 Logged measurements

- 9 Accessibility measurements

- 11 Sidelink operation

Annex A (informative):  
Void

Annex B (informative):  
Example of Hashed ID Calculation using 32-bit FCS

**Inputs:**

- Least significant bits of S-TMSI: 0x12341234

- Generator polynomial: 0x104C11DB7 (1 0000 0100 1100 0001 0001 1101 1011 0111)

**Procedure to Calculate Hashed ID:**

step a)

- k = 32

- numerator: 0xFFFF FFFF 0000 0000

- denominator: 0x1 04C1 1DB7

- remainder Y1 = 0xC704DD7B

step b)

- numerator: 0x1234 1234 0000 0000

- denominator: 0x1 04C1 1DB7

- remainder Y2 = 0x1D66F1A6

**Hashed\_ID** = FCS = ones complement of (remainder Y1 XOR remainder Y2)

= ones complement of (0xC704DD7B XOR 0x1D66F1A6)

= negation of (0xDA622CDD)

**= 0x259DD322**

Annex C (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| Date | TSG # | TSG Doc. | CR | Rev | Cat | Subject/Comment | New version |
| 2007-06 |  |  |  |  |  | Agreed text proposals from TSG RAN2#58bis meeting | 0.0.1 |
| 2007-09 | RP-37 | RP-070687 |  |  |  | Presented for information at TSG RAN-37 | 1.0.0 |
| 2007-11 | RP-38 | RP-070915 |  |  |  | Presented for approval at TSG RAN-38 | 2.0.0 |
|  | RP-38 | - |  |  |  | Approved at TSG RAN-38 and placed under change control | 8.0.0 |
| 2008-03 | RP-39 | RP-080193 | 0001 | 1 |  | CR to 36.304 on Miscellaneous corrections | 8.1.0 |
| 2008-05 | RP-40 | RP-080408 | 0002 | - |  | Add RAT specific Treselection parameters for CDMA HRPD and 1xRTT | 8.2.0 |
|  | RP-40 | RP-080408 | 0003 | 1 |  | Paging Subframe Patterns for FDD and TDD and paging parameters clarification | 8.2.0 |
|  | RP-40 | RP-080408 | 0004 | 1 |  | Editorial corrections to 36.304 | 8.2.0 |
|  | RP-40 | RP-080408 | 0005 | - |  | PLMN selection ping-pong control | 8.2.0 |
| 2008-09 | RP-41 | RP-080689 | 0006 | 1 |  | CR on Considerations on various open items in 36.304 | 8.3.0 |
|  | RP-41 | RP-080689 | 0007 | 1 |  | CSG related correction to 36.304 | 8.3.0 |
|  | RP-41 | RP-080689 | 0008 | 1 |  | Clarification of the medium mobility state criteria | 8.3.0 |
|  | RP-41 | RP-080689 | 0009 | - |  | Support for Manual CSG ID Selection | 8.3.0 |
|  | RP-41 | RP-080689 | 0010 | - |  | USIM less paging occasion calculation | 8.3.0 |
|  | RP-41 | RP-080689 | 0013 | 1 |  | Definition of Qoffset in cell reselection criteria | 8.3.0 |
|  | RP-41 | RP-080689 | 0017 | - |  | Correction to Discontinuous Reception for paging | 8.3.0 |
|  | RP-41 | RP-080689 | 0018 | - |  | Lifetime of dedicated cell reselection priorities | 8.3.0 |
|  | RP-41 | RP-080689 | 0019 | - |  | Clarification on cell reselection parameters | 8.3.0 |
| 2008-12 | RP-42 | RP-081017 | 0020 | 1 |  | Correcting the UE behaviour when Sintrasearch and Snonintrasearch are not provided | 8.4.0 |
|  | RP-42 | RP-081017 | 0021 | - |  | Proposed CR to 36.304 [Rel-8] on Definition of | 8.4.0 |
|  | RP-42 | RP-081017 | 0022 | 1 |  | Proposed CR to 36.304 [Rel-8] on Intra-frequency reselection allowed/not-allowed concept | 8.4.0 |
|  | RP-42 | RP-081017 | 0023 | - |  | Proposed CR to 36.304 [Rel-8] on Introduction of Pcompensation | 8.4.0 |
|  | RP-42 | RP-081017 | 0024 | - |  | Proposed CR to 36.304 [Rel-8] on Support of UE autonomous search for E-UTRAN CSG cells when camped on other RAT than E-UTRAN | 8.4.0 |
|  | RP-42 | RP-081017 | 0025 | - |  | Correction to range of nB in TS 36.304 | 8.4.0 |
|  | RP-42 | RP-081017 | 0026 | 2 |  | Miscellaneous corrections to 36.304 | 8.4.0 |
|  | RP-42 | RP-081017 | 0027 | 1 |  | Proposed CR to 36.304 [Rel-8] on Support of registration procedures as outcome of a manual CSG ID selection | 8.4.0 |
|  | RP-42 | RP-081017 | 0029 | 2 |  | Implicit priority for CSG cells | 8.4.0 |
|  | RP-42 | RP-081017 | 0032 | - |  | Correction of the reselection formula for offset used for PLMN selection | 8.4.0 |
|  | RP-42 | RP-081017 | 0036 | - |  | Clarification of definition of SnonServingCell,x for cdma2000 RATs in TS 36.304 | 8.4.0 |
|  | RP-42 | RP-081017 | 0038 | 1 |  | Support of emergency calls in LTE Rel-8 | 8.4.0 |
|  | RP-42 | RP-081017 | 0042 | - |  | CR to 36.304 on Removal of cellReservationExtension | 8.4.0 |
|  | RP-42 | RP-081017 | 0044 | 1 |  | Idle mode agreements related to 36.304 | 8.4.0 |
| 2009-03 | RP-43 | RP-090125 | 0045 | - |  | CR to 36.304 on correction of definition of Pmax | 8.5.0 |
|  | RP-43 | RP-090125 | 0046 | 1 |  | Emergency call in camped on any cell state in LTE Rel8 | 8.5.0 |
|  | RP-43 | RP-090125 | 0047 | - |  | Handling of Priority of Camping Frequency | 8.5.0 |
|  | RP-43 | RP-090125 | 0048 | 2 |  | Correction to implementation of CR0009 to 36.304 | 8.5.0 |
|  | RP-43 | RP-090125 | 0049 | - |  | UE Behaviour on Registration Failure to CSG | 8.5.0 |
|  | RP-43 | RP-090125 | 0050 | 2 |  | CR to 36.304 to capture several editorial corrections | 8.5.0 |
|  | RP-43 | RP-090125 | 0051 | 1 |  | CR to 36.304 on Update of Figure 4.1-1 Overall Idle Mode Process | 8.5.0 |
|  | RP-43 | RP-090125 | 0053 | 2 |  | Correction to priority based reselection handling | 8.5.0 |
|  | RP-43 | RP-090125 | 0057 | 3 |  | CR on UE behaviour in absence of reselection priorities in system information | 8.5.0 |
|  | RP-43 | RP-090125 | 0058 | 3 |  | Cell reselection for CSG | 8.5.0 |
|  | RP-43 | RP-090125 | 0060 | - |  | Corrections to Inter-RAT Cell Reselection Criteria | 8.5.0 |
|  | RP-43 | RP-090125 | 0062 | - |  | Manual selection | 8.5.0 |
|  | RP-43 | RP-090145 | 0063 | 1 |  | Reception of ETWS notification without verifying digital signature | 8.5.0 |
|  | RP-43 | RP-090125 | 0066 | - |  | Draft CR to 36.304 on Inheriting of dedicated priorities at inter-RAT reselection | 8.5.0 |
|  | RP-43 | RP-090125 | 0067 | - |  | Proposed CR to 36.304 Clarification on applying DRX value | 8.5.0 |
|  | RP-43 | RP-090125 | 0070 | - |  | Draft CR to 36.304 on Correction to UE behaviour if dedicated cell reselection priority is assigned but frequency is not configured by system information | 8.5.0 |
|  | RP-43 | RP-090125 | 0071 | - |  | Clarification to the best non-allowed CSG cell | 8.5.0 |
| 2009-06 | RP-44 | RP-090510 | 0072 | 2 |  | CR on correction of sign in SnonServingCell,x for CDMA2000 RATs | 8.6.0 |
|  | RP-44 | RP-090510 | 0073 | - |  | Correction to UE behaviour while 300s frequency barring timer is running | 8.6.0 |
|  | RP-44 | RP-090510 | 0074 | 1 |  | Correction to any cell selection procedure | 8.6.0 |
|  | RP-44 | RP-090510 | 0075 | 1 |  | Correction to reselection in case IFRI is not allowed | 8.6.0 |
|  | RP-44 | RP-090510 | 0076 | 1 |  | Clarification when no candidate cells on serving frequency | 8.6.0 |
|  | RP-44 | RP-090510 | 0077 | 1 |  | Clarification of the Priority Handling in CSG Cell | 8.6.0 |
|  | RP-44 | RP-090510 | 0079 | - |  | Correction to cell selection when leaving RRC connected mode | 8.6.0 |
|  | RP-44 | RP-090510 | 0080 | - |  | CR for Removing FFS for T3230 | 8.6.0 |
|  | RP-44 | RP-090510 | 0082 | - |  | Correction on the Lower Priority Cell Reselection Rule | 8.6.0 |
|  | RP-44 | RP-090510 | 0084 | - |  | Clarification on disabling E-UTRA capabilities with a USIM | 8.6.0 |
| 2009-09 | RP-45 | RP-090906 | 0085 | - |  | Clarification on cell status and cell reservations | 8.7.0 |
|  | RP-45 | RP-090906 | 0089 | - |  | Correction on Cell reserved for operators use | 8.7.0 |
|  | RP-45 | RP-090906 | 0094 | - |  | clarifications for manual CSG ID selection | 8.7.0 |
| 2009-09 | RP-45 | RP-090934 | 0086 | 1 |  | Some clarifications on TS 36.304 | 9.0.0 |
|  | RP-45 | RP-090926 | 0091 | 1 |  | IMS emergency call when UE camps on acceptable cell | 9.0.0 |
|  | RP-45 | RP-090933 | 0096 | - |  | Reception of CMAS notifications in limited service state | 9.0.0 |
| 2009-12 | RP-46 | RP-091314 | 0098 | - |  | Clarification on Parameters for Cell Selection | 9.1.0 |
|  | RP-46 | RP-091346 | 0099 | - |  | Clarifications on autonomous search function for CSG | 9.1.0 |
|  | RP-46 | RP-091346 | 0100 | 1 |  | Correction of Treselection inconsistency regarding frequency groups | 9.1.0 |
|  | RP-46 | RP-091346 | 0102 | - |  | CR to 36.304 - Handling of barring in case of priority based reselection | 9.1.0 |
|  | RP-46 | RP-091346 | 0103 | - |  | Functions supported for the UE "limited service state" | 9.1.0 |
|  | RP-46 | RP-091334 | 0104 | 3 |  | UE's behaviour when camping on cell supporting emergency call | 9.1.0 |
|  | RP-46 | RP-091343 | 0106 | 2 |  | Stage3 CR for LTE hybrid cell Idle Mode Mobility | 9.1.0 |
|  | RP-46 | RP-091314 | 0109 | - |  | Correction related to Location Registration in manual CSG ID selection procedure. | 9.1.0 |
|  | RP-46 | RP-091343 | 0114 | - |  | Access Stratum support for manual CSG selection across PLMN (CR 36.304 Rel-9) | 9.1.0 |
|  | RP-46 | RP-091343 | 0117 | - |  | Renaming Allowed CSG List (36.304 Rel-9) | 9.1.0 |
|  | RP-46 | RP-091341 | 0119 | - |  | Proposed CR to 36.304 on Introduction of MBMS | 9.1.0 |
| 2010-03 | RP-47 | RP-100296 | 0122 | - |  | Clarification on RRC connection re-establishment for emergency calls | 9.2.0 |
|  | RP-47 | RP-100308 | 0123 | 1 |  | Correction on reselection from non-CSG cell to CSG inter-RAT cell | 9.2.0 |
|  | RP-47 | RP-100308 | 0124 | 1 |  | Miscellaneous correction on 36.304 | 9.2.0 |
|  | RP-47 | RP-100305 | 0125 | - |  | Proposed CR to 36.304 on Addition of missing abbreviations related with MBMS | 9.2.0 |
|  | RP-47 | RP-100308 | 0129 | - |  | Cell reselection enhancements CR for 36.304 | 9.2.0 |
| 2010-06 | RP-48 | RP-100556 | 0133 | - |  | Correction to CSG autonomous search function | 9.3.0 |
| 2010-09 | RP-49 | RP-100855 | 0134 | - |  | Clarification on CSG autonomous search | 9.4.0 |
|  | RP-49 | RP-100851 | 0136 | 1 |  | Clarifications Regarding Redirection from LTE | 9.4.0 |
|  | RP-49 | RP-100845 | 0138 | - |  | Correct the PEMAX\_H to PEMAX | 9.4.0 |
|  | RP-49 | RP-100851 | 0139 | 1 |  | Clarification on the use of RSRQ for cell reselection towards GERAN or CDMA | 9.4.0 |
| 2010-12 | RP-50 | RP-101210 | 0142 | - |  | Cell selection in case of redirection based CSFB procedure | 9.5.0 |
| 2010-12 | RP-50 | RP-101221 | 0140 | 2 |  | 36.304 CR on MDT | 10.0.0 |
| 2011-03 | RP-51 | RP-110271 | 0151 | - |  | 36.304 correction on manual CSG selection | 10.1.0 |
| 2011-06 | RP-52 | RP-110835 | 0154 | - |  | CR to align NAS and AS for handling of CSG cells | 10.2.0 |
|  | RP-52 | RP-110843 | 0155 | 1 |  | Clean up of MDT section | 10.2.0 |
| 2011-09 | RP-53 | RP-111281 | 0160 | - |  | Correction of inter-frequency or inter-RAT cell reselection criteria for UTRA TDD case | 10.3.0 |
| 2011-12 | RP-54 | RP-111710 | 0167 | 1 |  | Clarification of inter-RAT cell reselection enhancements | 10.4.0 |
| 2012-03 | RP-55 | RP-120325 | 0175 | - |  | MBMS Multibands Cell Selection and Reselection | 10.5.0 |
| 2012-06 | RP-56 | RP-120813 | 0183 | 1 |  | Korean Public Alert System (KPAS) in relation to CMAS | 10.6.0 |
|  | RP-56 | RP-120807 | 0187 | 1 |  | Avoiding unexpected UE prioritization for MBMS where MBMS is not deployed | 10.6.0 |
|  | RP-56 | RP-120813 | 0188 | 1 |  | EU-Alert in relation to CMAS | 11.0.0 |
| 2012-09 | RP-57 | RP-121370 | 0192 | 1 |  | Introduction of MDT multi-PLMN | 11.1.0 |
|  | RP-57 | RP-121375 | 0195 | - |  | Introducing MBMS enhancements | 11.1.0 |
| 2012-12 | RP-58 | RP-121940 | 0196 | - |  | Clarification of MBMS Prioritisation | 11.2.0 |
|  | RP-58 | RP-121957 | 0197 | - |  | Correction to absolute priority cell reselection | 11.2.0 |
|  | RP-58 | RP-121946 | 0198 | - |  | Introduction of MDT accessibility measurements | 11.2.0 |
|  | RP-58 | RP-121958 | 0199 | 1 |  | RAN overload handling using RRC Reject | 11.2.0 |
| 2013-03 | RP-59 | RP-130241 | 0209 | - |  | Clarification on MBMS Service Continuity | 11.3.0 |
|  | RP-59 | RP-130248 | 0210 | - |  | Clarification of De-prioritization in idle mode | 11.3.0 |
|  | RP-59 | RP-130247 | 0213 | - |  | Corrections on mobility to CSG and hybrid cells in idle mode | 11.3.0 |
|  | RP-59 | RP-130248 | 0214 | 1 |  | Clarification on handling of deprioritsation information upon PLMN selection | 11.3.0 |
| 2013-06 | RP-60 | RP-130808 | 0221 | - |  | Correction of MBMS prioritisation | 11.4.0 |
|  | RP-60 | RP-130809 | 0222 | - |  | Updating 3GPP2 specification references | 11.4.0 |
| 2013-09 | RP-61 | RP-131311 | 0223 | 1 |  | Cell reselection criteria with threshServingLowQ provided | 11.5.0 |
| 2013-12 | RP-62 | RP-131987 | 0227 | 1 |  | Correction of MBMS prioritisation for DL only carrier | 11.6.0 |
| 2014-03 | RP-63 | RP-140359 | 0233 | - |  | Introduction of UE mobility history reporting (option 2) | 12.0.0 |
| 2014-06 | RP-64 | RP-140881 | 0235 | - |  | Introduction of support for UE power saving mode | 12.1.0 |
|  | RP-64 | RP-140892 | 0238 | 1 |  | Introduction of RRC Connection Establishment failure temporary Qoffset handling | 12.1.0 |
| 2014-09 | RP-65 | RP-141507 | 0244 | - |  | Introduction of MBSFN MDT | 12.2.0 |
|  | RP-65 | RP-141504 | 0243 | 1 |  | Procedures of WLAN/3GPP Radio Interworking for LTE | 12.2.0 |
| 2014-12 | RP-66 | RP-142122 | 0251 | - |  | Clarification on handling of dedicated parameters upon cell selection | 12.3.0 |
|  | RP-66 | RP-142122 | 0253 | - |  | UE behavior when the cell temporarily becomes unsuitable. | 12.3.0 |
| 2015-03 | RP-67 | RP-150373 | 0260 | - |  | UE capability signaling for WLAN/3GPP radio interworking | 12.4.0 |
|  | RP-67 | RP-150373 | 0265 | 1 |  | Cleanup on RAN-assisted WLAN interworking | 12.4.0 |
|  | RP-67 | RP-150373 | 0266 | - |  | Correction on WLAN identifiers | 12.4.0 |
|  | RP-67 | RP-150374 | 0264 | 1 |  | Introduction of ProSe | 12.4.0 |
| 2015-06 | RP-68 | RP-150921 | 0267 | - |  | Correction on limited service state conditions | 12.5.0 |
|  | RP-68 | RP-150923 | 0272 | 1 |  | Correction to SI acquisition failure | 12.5.0 |
| 2015-09 | RP-69 | RP-151441 | 0273 | 1 |  | Sidelink terminology alignment in TS 36.304 | 12.6.0 |
| 2015-12 | RP-70 | RP-152048 | 0277 | 2 |  | Enabling multiple NS and P-Max per cell | 12.7.0 |
| 2015-12 | RP-70 | RP-152082 | 0285 | 1 |  | Introduction of IDC Impact to Logged Measurements | 13.0.0 |
|  | RP-70 | RP-152075 | 0280 | 1 |  | Extension of Frequency Priorities | 13.0.0 |
|  | RP-70 | RP-152066 | 0286 | - |  | Introduction of ACDC in TS 36.304 | 13.0.0 |
|  | RP-70 | RP-152080 | 0278 | 2 |  | Introduction of SC-PTM | 13.0.0 |
|  | RP-70 | RP-152075 | 0281 | 3 |  | Introduction of load redistribution in RRC\_IDLE | 13.0.0 |
|  | RP-70 | RP-152072 | 0287 | - |  | Introducing eSL | 13.0.0 |
|  | RP-70 | RP-152076 | 0288 | - |  | Introducing extended DRX | 13.0.0 |
| 2016-03 | RP-71 | RP-160456 | 0289 | 1 |  | Correction on PO monitoring during paing window in eDRX | 13.1.0 |
|  | RP-71 | RP-160470 | 0290 | 1 |  | Clarification of idle mode load distribution | 13.1.0 |
|  | RP-71 | RP-160454 | 0291 | 1 |  | Miscellaneous corrections | 13.1.0 |
|  | RP-71 | RP-160456 | 0293 | 1 |  | PTW terminology alignment | 13.1.0 |
|  | RP-71 | RP-160470 | 0295 | 1 |  | Correction to E-UTRAN Inter-frequency Redistribution procedure\_alt2 | 13.1.0 |
|  | RP-71 | RP-160453 | 0299 | 3 |  | The introduction of the Idle procedure for eMTC UE | 13.1.0 |
|  | RP-71 | RP-160457 | 0300 | - |  | Introduction of WLAN RSSI measurements | 13.1.0 |
| 2016-06 | RP-72 | RP-161080 | 0302 | - |  | Correction for conditions of sidelink operation | 13.2.0 |
|  | RP-72 | RP-161080 | 0313 | - |  | Corrections on nB extension | 13.2.0 |
|  | RP-72 | RP-161080 | 0315 | - |  | Correction to eMTC message classes and logical channels | 13.2.0 |
|  | RP-72 | RP-161080 | 0312 | - |  | Renaming UE\_ID used for MCLD purposes | 13.2.0 |
|  | RP-72 | RP-161080 | 0304 | 1 |  | Corrections on carrier frequency prioritization for PS sidelink discovery | 13.2.0 |
|  | RP-72 | RP-161080 | 0305 | 1 |  | Correction to System Information change notifications in RRC\_IDLE for MTCe | 13.2.0 |
|  | RP-72 | RP-161080 | 0314 | 1 |  | Corrections on TS 36.304 for eMTC | 13.2.0 |
|  | RP-72 | RP-161080 | 0307 | 1 |  | Clarification of UE behaviour immediately after T360 expiry | 13.2.0 |
|  | RP-72 | RP-161195 | 0311 | 2 |  | Introduction of NB-IoT in 36.304 | 13.2.0 |
| 2016-09 | RP-73 | RP-161762 | 0321 | - |  | The field name is not highlighted with italic | 13.3.0 |
|  | RP-73 | RP-161759 | 0322 | 2 |  | Idle mode UE behaviour on user plane CIoT EPS optimisation | 13.3.0 |
|  | RP-73 | RP-161758 | 0325 | 1 |  | Corrections to NB-IoT | 13.3.0 |
|  | RP-73 | RP-161762 | 0328 | - |  | Clarification of UE redistribution target selection | 13.3.0 |
|  | RP-73 | RP-161762 | 0329 | - |  | PH and PTW\_Start calculation for eDRX paging | 13.3.0 |
| 2016-09 | RP-73 | RP-161746 | 0324 | 1 |  | Introduction of PC5 V2V for 36.304 | 14.0.0 |
| 2016-12 | RP-74 | RP-162314 | 0331 | 1 |  | Editorial corrections to TS 36.304 | 14.1.0 |
|  | RP-74 | RP-162328 | 0332 | 1 |  | Corrections on V2V description in TS 36.304 | 14.1.0 |
|  | RP-74 | RP-162313 | 0340 | - |  | Clarification on TreselectionEUTRA\_CE | 14.1.0 |
|  | RP-74 | RP-162327 | 0341 | - |  | Support of eCall Only Mode for Network and Cell Selection | 14.1.0 |
| 2017-03 | RP-75 | RP-170655 | 0344 | - | A | Correction on channel bandwidth definition for NB-IoT | 14.2.0 |
|  | RP-75 | RP-170636 | 0347 | 1 | B | Introduction of authorization of coverage enhancements | 14.2.0 |
|  | RP-75 | RP-170643 | 0349 | 1 | F | Correction on V2X sidelink communication in limited service state in in TS 36.304 | 14.2.0 |
|  | RP-75 | RP-170636 | 0350 | 1 | B | Introduction of SC-PTM for FeMTC and NB-IoT | 14.2.0 |
|  | RP-75 | RP-170633 | 0351 | 1 | B | Introduction of FeMBMS to 36.304 | 14.2.0 |
|  | RP-75 | RP-170637 | 0352 | 1 | B | Introduction of Rel-14 NB-IoT enhancements into idle mode | 14.2.0 |
|  | RP-75 | RP-170651 | 0357 | - | A | Clarification for Hashed\_ID | 14.2.0 |
|  | RP-75 | RP-170653 | 0358 | - | A | Clarifications on reselection for eMTC | 14.2.0 |
|  | RP-75 | RP-170653 | 0360 | - | A | New S-criteria for enhanced coverage in idle mode | 14.2.0 |
|  | RP-75 | RP-170635 | 0361 | - | B | Introduction of PC5 V2X for 36.304 | 14.2.0 |
| 2017-06 | RP-76 | RP-171224 | 0363 | 2 | F | Correction to paging carrier selection formula in Rel-14 NB-IoT | 14.3.0 |
|  | RP-76 | RP-171243 | 0370 | 2 | A | Correction for eDRX Hashed ID | 14.3.0 |
|  | RP-76 | RP-171223 | 0376 | 2 | F | Correction to usage of SC-PTM offset in NB-IoT and FeMTC | 14.3.0 |
|  | RP-76 | RP-171221 | 0380 | 1 | F | Correction to Reselection priorities handling for FeMBMS | 14.3.0 |
| 2017-09 | RP-77 | RP-171920 | 0386 | 1 | A | Adding reference to SystemInformationBlockType1-BR to the section on cell status and cell reservations | 14.4.0 |
| 2017-12 | RP-78 | RP-172617 | 0392 | 2 | C | Introduction of relaxed monitoring in NB-IoT | 14.5.0 |
|  | RP-78 | RP-172624 | 0397 | 2 | A | Correction to cell barring for coverage enhancement | 14.5.0 |
|  | RP-78 | RP-172623 | 0399 | 1 | A | Clarification on eDRX in NB-IoT | 14.5.0 |
| 2018-03 | RP-79 | RP-180445 | 0402 | 4 | F | Correction to relaxed monitoring reference RSRP reset (Alternative 1) | 14.6.0 |
|  | RP-79 | RP-180443 | 0405 | 1 | C | Introduction of support of relaxed monitoring for BL and CE UE | 14.6.0 |
|  | RP-79 | RP-180443 | 0407 | 2 | F | Support of CE mode B restriction for Rel-14 eMTC | 14.6.0 |
| 2018-06 | RP-80 | RP-181228 | 0410 | - | B | TS 36.304 running CR for HSDN | 15.0.0 |
|  | RP-80 | RP-181224 | 0411 | r | B | EARFCN provisioning for UE in enhanced coverage | 15.0.0 |
|  | RP-80 | RP-181252 | 0416 | 2 | B | Introduction of further NB-IoT enhancements in 36.304 | 15.0.0 |
|  | RP-80 | RP-181224 | 0417 | 1 | B | Introduction of further eMTC enhancements in 36.304 | 15.0.0 |
|  | RP-80 | RP-181223 | 0419 | 1 | B | Introduction of E-UTRA connected to 5GCN | 15.0.0 |
|  | RP-80 | RP-181228 | 0420 | 1 | B | Support for Logging of 'Any cell selection' state | 15.0.0 |
|  | RP-80 | RP-181225 | 0729 | 1 | B | Implementing network-based CRS interference mitigation | 15.0.0 |
| 2018-09 | RP-81 | RP-181940 | 0412 | 4 | B | Introduction of LTE to NR reselection in 36.304 | 15.1.0 |
|  | RP-81 | RP-181950 | 0731 | 1 | F | CR to 36.304 on CN selection for LTE connected to 5GC | 15.1.0 |
|  | RP-81 | RP-181963 | 0736 | 1 | A | Correction to entering condition for relaxed monitoring | 15.1.0 |
|  | RP-81 | RP-181944 | 0737 | 3 | F | Define relation between WUS occasion and PO | 15.1.0 |
|  | RP-81 | RP-181944 | 0740 | 2 | F | Corrections for CRS muting in TS 36.304 | 15.1.0 |
|  | RP-81 | RP-181950 | 0742 | - | F | Correction on RRC\_INACTIVE and camping on E-UTRA connected to 5GC in NB-IoT | 15.1.0 |
|  | RP-81 | RP-181940 | 0747 | - | F | Paging Monitoring in Camped Normally state and Camped on Any Cell state | 15.1.0 |
|  | RP-81 | RP-181960 | 0748 | - | F | Corrections to 36.304 speed dependent mobility and inter-RAT cells with cell reservations, access restrictions, or unsuitable for normal camping | 15.1.0 |
| 2018-12 | RP-82 | RP-182671 | 0741 | 3 | F | Small correction to paging with wake up signal | 15.2.0 |
|  | RP-82 | RP-182676 | 0744 | 5 | F | Corrections to TS 36.304 for E-UTRA connected to 5GC | 15.2.0 |
|  | RP-82 | RP-182652 | 0750 | 1 | F | Correction on paging for LTE connected to 5GC | 15.2.0 |
|  | RP-82 | RP-182676 | 0752 | 2 | F | Clarification of Qoffsettemp for eLTE in 36.304 | 15.2.0 |
|  | RP-82 | RP-182681 | 0757 | 1 | F | Correction to gap determination for the wake-up signal | 15.2.0 |
|  | RP-82 | RP-182675 | 0758 | - | F | TS36.304 CR on [103bis#43][LTEeLTE] Capture NR agreements | 15.2.0 |
|  | RP-82 | RP-182676 | 0762 | - | F | TS36.304 CR on [104#23][LTE/5GC] Capture NR agreements | 15.2.0 |
| 2019-03 | RP-83 | RP-190540 | 0763 | 1 | F | Suitable cell criteria for reselection to NR cell | 15.3.0 |
|  | RP-83 | RP-190551 | 0764 | - | F | CR on missing descprition of transmission pool sharing | 15.3.0 |
| 2019-06 | RP-84 | RP-191380 | 0765 | 2 | F | Correction to mobility state handling in case of LTE to NR reselection | 15.4.0 |
| 2019-12 | RP-86 | RP-192941 | 0775 | 1 | F | Correction on handling of stored AS context for UP optimization and RRC\_INACTIVE state | 15.5.0 |
| 2020-07 | RP-88 | RP-201168 | 0793 | 1 | F | Clarification for CP EDT | 15.6.0 |
| 2020-09 | RP-89 | RP-201936 | 0795 | 3 | F | System support for Wake Up Signal | 15.7.0 |
|  | RP-89 | RP-201938 | 0806 | 1 | F | Correction on Srxlev Calculation for IRAT Cell Reselection | 15.7.0 |