3GPP TSG-RAN WG2 Meeting #110 electronic R2-200xxxx

Online, June 1 – June 12 2020

Agenda Item: 6.1.7

Source: Huawei, HiSilicon

**Title:** Summary of offline discussion [AT110e][049][IAB] Other

Document for: Discussion and Decision

# Introduction

This paper aims at capturing the summary of the following offline discussion:

* [AT110e][049][IAB] Other (Huawei)

Scope: Treat papers under 6.1.7, identify agreeable items, make agreements as far as possible.

Part 1: Agreements

Part 2: Agreed CRs 304, 322, (RRC impacts should be captured in the main IAB RRC CR).

Deadline: EOM

# Discussion

**Issue 1: NPN related issue**

As discussed in R2-2004876 and R2-2005406, followings are observed:

|  |
| --- |
| Observation 1: A NPN capable IAB MT, which ignores *cellReservedForOtherUse*, will incorrectly use the first PLMN ID which is invalid for SIB validity check when camping on NPN-only cell.Observation 2: A NPN capable IAB MT, which ignores *cellReservedForOtherUse*, will incorrectly calculate the index of the “selectedPLMN-Identity” including in RRCSetupComplete/RRCResumeComplete message when camping on NPN-only cell. |

With the above issues identified, the NPN capable IAB-MT should use *cellReservedForOtherUse* to determine the NPN-only cell, rather than totally ignore it.

It is straight forward to have the following proposal, if R2 will agree the CRs to support NPN in IAB.

**Potential Proposal 1: *cellReservedForOtherUse* is ignored by IAB-MT, except for determination of an NPN-only cell for the NPN capable IAB-MT.**

**Question 1: Do you agree with the above proposal and its impact to 38.331 and 38.304?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Agree or not?** | **Comments** |
| Ericsson | Agree | IEs should be ignored for the determination of the cell status and cell reservations i.e. for the determination of a cell considered barred. It should not be ignored for the determination of an NPN cell. |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 2: Is there any other spec impact for IAB-MT supporting NPN, other than above proposal and endorsed changes in R2-2004280/R2-2004281?**

|  |  |
| --- | --- |
| **Companies** | **Comments** |
|  |  |
|  |  |
|  |  |
|  |  |

**Issue 2: cell barring related issues**

**2.1 Ignore *cellReservedForFutureUse***

As proposed in R2-2004876 and R2-2004783, it seems straight forward for IAB-MT to ignore *cellReservedForFutureUse*, and just check its specific *iab-Spport* for cell barring.

**Potential Proposal 2: IAB-MTs ignore the *cellReservedForFutureUse***

**Question 3: Do you agree with the above proposal?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Agree or not?** | **Comments** |
| Ericsson | Agree |  |
|  |  |  |
|  |  |  |
|  |  |  |

**2.2 intraFreqReselection for IAB-MT**

We have agreed in last meeting that “IAB-MT ignores *intraFreqReselection*” and also in the endorsed CR as “IAB-MT ignores *intraFreqReselection* (i.e. treats *intraFreqReselection* as if it was set to *allowed*)”. In this meeting, new option is proposed in R2-2004783 as option 2.

**Option 1: Keep the current agreement and running CR: IAB-MT ignores *intraFreqReselection* as if it was set to *allowed.***

**Option 2: Introduce new IE *intraFreqReselection*-IAB for IAB-MT specific network control of *intraFreqReselection*.**

**Question 4: Which option do you prefer on *intraFreqReselection* for IAB-MT?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Option 1 or 2?** | **Comments** |
| Ericsson | Option 1 |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Issue 3: RLC spec correction on supporting BAP**

[R2-2005523](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2005523.zip) Correction on RLC spec to support the BAP as upper layer

As proposed in the above paper, in the current TS 38.322, the RLC PDU carries the Data field. In R15, only PDCP is the upper layer of the RLC, so “The maximum Data field size is the maximum size of a PDCP PDU”, which was true for access RLC. Since we have introduced BAP also as the upper layer of BH RLC in IAB, the RLC SDU could either be PDCP PDU or BAP PDU.

For now, we don’t have the limitation (or not define) the maximum size of BAP PDU. This should be clarified in the RLC spec that the current description “The maximum Data field size is the maximum size of a PDCP PDU” only applies to the case of access RLC, rather than to the BH RLC for BAP layer.

**--------------------Text Proposal for TS 38.322------------------------**

|  |
| --- |
| 6.2.3.2 Data fieldData field elements are mapped to the Data field in the order which they arrive to the RLC entity at the transmitter.For TMD PDU, UMD PDU and AMD PDU:- The granularity of the Data field size is one byte;- The maximum Data field size is the maximum size of a PDCP PDU in case the upper layer is PDCP.For TMD PDU:- Only one RLC SDU can be mapped to the Data field of one TMD PDU.For UMD PDU, and AMD PDU:- Either of the following can be mapped to the Data field of one UMD PDU, or AMD PDU:- One RLC SDU;- One RLC SDU segment. |

**Question 5: Do you agree with the above proposed change?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Agree or not?** | **Comments** |
| Ericsson | Disagree | While we understand the rapporteur intention, this section applies to TMD PDUs and that is, for example, SRB0. SRB0 is not associated to a PDCP entity. Thus, the highlighted sentence is already inaccurate. Adding the new text will make it worse. In any case, the BAP entity is just below the PDU in the IAB-donor, so the one BAP SDUs will be equal to a PDCP PDU. The IAB donor will deliver BAP PDUs with the size equal to a PDCP PDU plus the BAP headers, and BAP PDUs/SDUs will not increase within the intermediate IAB nodes.If something related to the specifics of IAB is to be added, we suggest it is captured explicitly without really touching anything which could affect the legacy text. Nevertheless, we do not see at this moment anything specific. |
|  |  |  |
|  |  |  |
|  |  |  |

**Issue 4: Others**

Following two papers are resubmission from last meeting, which were marked as “not treated” by chair, since they are kind of clarifications and further enhancements.

[R2-2004780](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2004780.zip) Better cell selection for IAB Nodes Apple discussion Rel-16 38.304 NR\_IAB

[R2-2005142](file:///D%3A%5CDocuments%5C3GPP%5Ctsg_ran%5CWG2%5CTSGR2_110-e%5CDocs%5CR2-2005142.zip) PWS information handling in IAB Sony discussion Rel-16 NR\_IAB-Core R2-2002664

|  |
| --- |
| Clarifications and further enhancements – not treatedR2-2002664 PWS information handling in IAB Sony discussion Rel-16 NR\_IAB-Core R2-2000824R2-2002814 Better cell selection for IAB Nodes Apple discussion NR\_IAB-Core |

Therefore, rapporteur assumes we will discuss those only if we have sufficient supporters, given that this is the very last meeting.

|  |  |
| --- | --- |
| R2-2004780 | Proposal 1: Introduce a new set of Qrxlevmin, Qrxlevminoffset and PMax along with Qqualmin and Qqualminoffset for IAB Nodes for cell selection criteria. This is different from the ones which regular UEs use. Proposal 2: Introduce a priority information among IAB parents in order for service classification and reduced latency. Proposal 3: Allow IAB Nodes to select the best parent in terms of not only the best signal strength but also based on the best performance. Proposal 4: Use # of hops as a metric along with signal strength as a cell selection criterion for IAB nodes. |
| R2-2005142 | Proposal: PWS System information is broadcasted once it is received from IAB-CU only. IAB node does not broadcast the information received in system information broadcasted from upstream/parent IAB-node. |

**Question 6: Companies are asked to provide your comments to the above proposals, if you support any of those. If you are fine to not discuss those for now, you can skip this question.**

|  |  |
| --- | --- |
| **Companies** | **Comments** |
| Ericsson | About R2-2004780: These proposals can be brought up during Rel-17. It is too late to discuss new functionality when ASN.1 should be frozen in this meeting.About R2-2005142: IAB nodes do not re-broadcast the system information which the parent node was broadcasting. Given so, we do not think there is anything to clarify. |
|  |  |
|  |  |

# Conclusion and proposals

Based on the above summary, following proposals are given.

**TBD**

# Reference

1. R2-2005406 [C502] Corrections to IAB behavior in Determining the NPN-only Cell CATT
2. R2-2004780 Better cell selection for IAB Nodes Apple
3. R2-2004783 Remaining issue on idle mode procedure for IAB-MT Kyocera
4. R2-2004784 Corrections to 38.331 for supporting IAB in NPN Huawei, HiSilicon, Kyocera
5. R2-2004785 Corrections to 38.304 for supporting IAB in NPN Huawei, HiSilicon, Kyocera
6. R2-2004876 Remaining issues of IAB in NPN CATT
7. R2-2005142 PWS information handling in IAB Sony
8. R2-2005516 Miscellaneous corrections to 38.304 for IAB Huawei, HiSilicon
9. R2-2005517 Miscellaneous corrections to 36.304 for IAB Huawei, HiSilicon
10. R2-2005523 Correction on RLC spec to support the BAP as upper layer Huawei, HiSilicon