3GPP TSG-RAN WG2 #113 electronic R2-20xxxxx

e-Meeting, 25 January – 05 February 2021

Agenda Item: 5.4.3

Source: ZTE, Sanechips

Title: Summary of offline [AT113-e][010][NR15] UE Capabilities II (ZTE)

Document for: Discussion, Decision

# 1 Introduction

This contribution summarizes the following discussion:

* [AT113-e][010][NR15] UE Capabilities II (ZTE)

Scope: Treat R2-2101559, R2-2101560, R2-2100064, R2-2101561, R2-2101913, R2-2101914, R2-2100961, R2-2100962,

Phase 1, determine agreeable parts, Phase 2, for agreeable parts Work on CRs.

Intended outcome: Report and Agreed CRs.

Deadline: Schedule A

|  |
| --- |
| **Deadline:** Email discussions with Deadline ***Schedule A***:  A first round with **Deadline for comments Thursday Feb 28 1200 UTC** to settle scope what is agreeable etc  A Final round with **Final deadline Thursday Feb 4 1200 UTC.** to settle details / agree CRs etc. Additional check points etc if needed are defined by the Rapporteur. In case some parts of an email discussion need more time, doesn’t converge, need on-line treatment etc Rapporteur please contact chair. |

**Contact from companies**

|  |  |
| --- | --- |
| Company | Email |
| Qualcomm Incorporated | mkitazoe@qti.qualcomm.com |
| Ericsson | lian.araujo@ericssom.com |
|  |  |
|  |  |
|  |  |
|  |  |

# Discussion

## 2.1 Part 1: Intended to determine agreeable parts

Part 1 discussion is focusing on reaching conclusion whether the proposals/CRs can be agreed in principle, and Part 2 discussion would then focus on detailed changes for those agreeable contributions.

### Bandwidth

In the current spec, for the *supportedBandwidthDL/supportedBandwidthUL/channelBWs-DL/channelBWs-UL*, it was noted that when determine the channel bandwidth the network shall also validate the *supportedBandwidthCombinationSet.* Meanwhile the s*upportedBandwidthCombinationSetIntraENDC* has been added for intra-band (NG)EN-DC/NE-DC with additional inter-band CA to limit the bandwidth of the intra-band component.

In the below 2 CRs, the s*upportedBandwidthCombinationSetIntraENDC* was added to the Note part of the *supportedBandwidthDL/supportedBandwidthUL/channelBWs-DL/channelBWs-UL.*

[R2-2101559](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101559.zip) CR on the SupportedBandwidth/channelBWs-R15 ZTE Corporation, Sanechips CR Rel-15 38.306 15.12.0 0515 - F NR\_newRAT-Core

[R2-2101560](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101560.zip) CR on the SupportedBandwidth/channelBWs-R16 ZTE Corporation, Sanechips CR Rel-16 38.306 16.3.0 0516 - A NR\_newRAT-Core

You may notice that the s*upportedBandwidthCombinationSetIntraENDC* was also discussed in another offline discussion [AT113-e][009][NR15], however it will not affect the general principle of this CR, it will only affect the wording highlighted in red as below*.*

*“ supportedBandwidthCombinationSetIntraENDC* (for intra-band (NG)EN-DC/NE-DC with additional inter-band CA component(s) of LTE and/or NR)”

Note: In this CR, the wording “(for intra-band (NG)EN-DC/NE-DC with additional inter-band CA component(s) of LTE and/or NR)” was added based on the current field description of *supportedBandwidthCombinationSetIntraENDC,* which can be further revised based on the offline discussion result [AT113-e][009][NR15] if necessary.

**Q1: Do companies generally agree with the intention and modification of the CRs above?** (Maybe with some correction for the wording of “for intra-band (NG)EN-DC/NE-DC with additional inter-band CA component(s) of LTE and/or NR” based on another offline discussion result [AT113-e][009][NR15])

|  |  |  |  |
| --- | --- | --- | --- |
| **Company** | **Agree Intention**  **(Yes or No)** | **Agree Modifications**  **(Yes or No)** | **Comments** |
| Qualcomm Incorporated | Yes | Yes |  |
| Huawei, HiSilicon | Yes | No | We understand the intention, but we’d like to first confirm the usage of BCS in [009] before changing more parts relevant to this.  [ZTE] As explained above, the [009] may have some impact on the field description of *supportedBandwidthCombinationSetIntraENDC”.*  *However, the supportedBandwidthCombinationSetIntraENDC itself should be taken into the consideration when determine the bandwidth.*  *To make progress, we think the CR can be generally agreed in phase 1, then determine whether some revision was needed based on [009] in the phase 2.* |
| ZTE | Yes | *Yes (maybe with some correction based on [009])* | *As explained above, we think the CR can be generally agreed in phase 1, then determine whether some revision was needed based on result of [009] in phase 2.*  *Another solution is that don’t add any clarification to the supportedBandwidthCombinationSetIntraENDC in this CR if companies have concern on it.*  *“ supportedBandwidthCombinationSetIntraENDC* |
| Ericsson | Yes | No | The intention is ok. But the note just needs to clarify what fields are used to validate the UE supported BW. In which particular context they are used is already clarified in each corresponding field description. Hence, it is sufficient to say:  NOTE: To determine whether the UE supports a channel bandwidth of 90 MHz the network may ignore this capability for and validate instead the *channelBW-90mhz* and the *supportedBandwidthCombiantionSet*. For serving cells with other channel bandwidths the network validates the *channelBWs-UL*, the *supportedBandwidthUL*, and any of the fields *supportedBandwidthCombinationSet*, *supportedBandwidthCombinationSetIntraENDC* or *asymmetricBandwidthCombinationSet* ~~and~~ *~~supportedBandwidthUL~~*. |
|  |  |  |  |
|  |  |  |  |

### 2.1.2 SUO for intra-band EN-DC

On this topic, we would like to discuss some detail issues first then collect companies’ views on which CRs can be taken as baseline.

[R2-2100064](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100064.zip) LS on single UL operation (RP-202932; contact: Huawei) RAN LS in Rel-15 NR\_newRAT-Core To:RAN2, RAN4

[R2-2101561](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101561.zip) Clarification on the SingleUL-Transmission ZTE Corporation, Sanechips discussion Rel-15 NR\_newRAT-Core

[R2-2101913](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101913.zip) Clarfication on single uplink operation capability report (LS Contact) Huawei, HiSilicon CR Rel-15 38.306 15.12.0 0524 - F NR\_newRAT-Core

[R2-2101914](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101914.zip) Clarfication on single uplink operation capability report (LS Contact) Huawei, HiSilicon CR Rel-16 38.306 16.3.0 0525 - A NR\_newRAT-Core

[R2-2100961](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100961.zip) Handling of single UL for intra-band EN-DC band combinations Nokia, Nokia Shanghai Bell CR Rel-15 38.306 15.12.0 0497 - F NR\_newRAT-Core

[R2-2100962](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100962.zip) Handling of single UL for intra-band EN-DC band combinations Nokia, Nokia Shanghai Bell CR Rel-16 38.306 16.3.0 0498 - A NR\_newRAT-Core

According to above papers, as clarified in [R2-2101913](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101913.zip)/[R2-2101914](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101914.zip)/[R2-2100961](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100961.zip)/[R2-2100962](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100962.zip),it is mandatory to report this field for BCs where only single switched UL transmission is allowed as defined in TS 38.101-3 [4]. (In [R2-2100961](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100961.zip)/[R2-2100962](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100962.zip), it said the UE shall include this field for band combinations for which only single UL transmission is specified in TS 38.101-3 [4] if the UE supports UL on the carriers where only single UL is specified.)

**Q2: Do companies generally agree that “it is mandatory to report *singleUL-Transmission***

**field for BCs where only single switched UL transmission is allowed as defined in TS 38.101-3 [4]”**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree?**  **(Yes or No)** | **Comments** |
| Qualcomm Incorporated | Yes |  |
| Huawei, HiSilicon | Yes | Proponent |
| ZTE | Yes |  |
| Ericsson | No | Actually singleUL-Transmission is an incapability bit. So we prefer to not mandate an incapability. Our understanding is that RAN4 is also working on some clarification in their specifications, we think this may be sufficient. |
|  |  |  |
|  |  |  |

Furthermore, as noted/discussed in the [R2-2101913](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101913.zip)/[R2-2101914](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101914.zip)/[R2-2101561](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101561.zip), for the legacy problematic UE (the UE that only supports single UL transmission for a BC, but doesn’t report *singleUL-Transmission* for that BC), the network ignore the BC or ignore the single UL transmission requirement in the BC.

**Q3: Do companies generally agree that “**For UE with earlier version, if *singleUL-Transmission* field is not included in a BC where only single switched UL transmission is allowed, the network may ignore the BC”?

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree?**  **(Yes or No)** | **Comments** |
| Qualcomm Incorporated |  | (Not sure how we can respond by Yes or No to the question above.)  It looks unsafe to just ignore the single UL transmission limitation that the UE may have. Safest approach would be to consider such band combination is invalid.  [Rapporteur] We had a littler modification to the question, hope that can avoid the confusion. |
| Huawei, HiSilicon |  | We understand Q3 is a bit confusing. The original change was to ignore the BC, or the part of the BC which requires the single UL transmission. We did not propose to ignore the single UL requirement. So basically we have same understanding as QC.  [Rapporteur] We had a littler modification to the question, hope that can avoid the confusion. |
| ZTE | Yes | Note: With rapporteur hat on, we also had a little modification to the question itself to avoid the confusion that mentioned by Qulcomm and Huawei.. |
| Ericsson |  | We think we do not need to spend much time on this case, which would be more an error case, but either of the option in Q3 could happen, i.e. “ignore the BC or consider that this UE supports dual UL, since it did not report the incapability bit”. Especially the latter option is basically how any other UE capability parameter would work i.e. the network can know what the UE supports based on what the UE reported. |
|  |  |  |
|  |  |  |

**Q3-a: If say yes to the Q2, do companies generally agree to add a related note (e.g. Note in the** [R2-2101913](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101913.zip)/[R2-2101914](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101914.zip)) **to the field description of *singleUL-Transmission?***

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree?**  **(Yes or No)** | **Comments** |
| Qualcomm Incorporated | Yes |  |
| Huawei, HiSilicon | Yes | Proponent |
| ZTE | Yes |  |
| Ericsson | No | See comments in Q3, we think this is not essential to clarify. |
|  |  |  |
|  |  |  |

The third question is for the field description of *tdm-Pattern*, as clarified in the [R2-2100961](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100961.zip)/[R2-2100962](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100962.zip), *“When RAN2 discussed the Rel-15 SUO, the support of TDM pattern was coupled to the SUO capability since it was necessary for UE to support such operation. However, there was still the option for network to not use the TDM pattern but rely on scheduling to resolve the single UL operation. Therefore, for these new cases where single UL is required, it seems not necessary to require UE to always support the TDM pattern”*, some modification was also added for the *tdm-Pattern in* [R2-2100961](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100961.zip)/[R2-2100962](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100962.zip)*.*

**Q3: Do companies generally agree with the modification for the *tdm-Pattern* in the** [R2-2100961](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100961.zip)/[R2-2100962](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100962.zip) **?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree?**  **(Yes or No)** | **Comments** |
| Qualcomm Incorporated | No | Change to singleUL-Transmission is sufficient because the inclusion of tdm-Pattern is already conditioned on singleUL-Transmission. Also, UE “allowing” something via UE capability signalling is also a bit strange. |
| Huawei, HiSilicon | No | We agree that tdm-Pattern is not the capability which directly associates with the RAN4 defined band combinations where single UL is required.  The tdm-Pattern is conditionally mandatory when the UEs do not support dynamic power sharing, or support single UL transmission. So no further discussion is needed here, the conditions when mandating the tdm-Pattern is already captured well in the current field description. |
| ZTE | FFS | We understand the intention, but the main modification is for the “other case”, we don’t think it’s necessary to add this clarification. Anyway we can follow the majorities’ view on it. |
| Ericsson |  | As we do not see a need for a modification in the *singleUL-Transmission* field description, there would also be no need for a change in *tdm-Pattern*. |
|  |  |  |
|  |  |  |

The forth question is about the BC reporting, as clarified in the [R2-2101561](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101561.zip), the BCs that have different *singleUL-Transmission* capabilities shall be reported in different BCs.

|  |
| --- |
| **Observation 1: The BCs that with different UL band component shall not be reported in a super BC if the corresponding super BC are not defined in RAN4.**  **Proposal 1: The BCs that have different *singleUL-Transmission* capabilities shall be reported in different BCs.** |

**Q4: Do companies generally agree that “the BCs that have different *singleUL-Transmission* capabilities shall be reported in different BCs”?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree?**  **(Yes or No)** | **Comments** |
| Qualcomm Incorporated | Yes | We understand this is for band combinations where single UL and simultaneous transmissions are supported. |
| Huawei, HiSilicon | Yes | We understand existing mechanism already supports so and no specification change is required? |
| ZTE | Yes | It’s just a clarification, no spec change is needed. |
| Ericsson |  | We agree the UE may report a fallback band combination for which it supports additional functionality compared to its corresponding superset band combination. But this is more a generic statement and there seems to be nothing to clarify particularly for *singleUL-Transmission*. |
|  |  |  |
|  |  |  |

Based on the above questions, we want to collect companies’ views on which CRs can be chosen as the baseline CR.

Option 1: [R2-2100961](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100961.zip)/[R2-2100962](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100962.zip)

Option 2: [R2-2101913](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101913.zip)/[R2-2101914](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101914.zip)

**Q5: Which CRs can be chosen as the baseline CR?**

**Option 1:** [**R2-2100961**](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100961.zip)**/**[**R2-2100962**](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100962.zip)

**Option 2:** [**R2-2101913**](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101913.zip)**/**[**R2-2101914**](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101914.zip)

|  |  |  |
| --- | --- | --- |
| **Company** | **Option?**  **(1or 2)** | **Comments** |
| Qualcomm Incorporated | 2 |  |
| Huawei, HiSilicon | 2 | As the LS contact we are volunteer to continue updating the potential agreeable CRs. Of course the further updates are dependent on the above feedback from companies. |
| ZTE | 2 |  |
| Ericsson |  | See comments to Q2 and Q3, we actually do not see a need to capture anything in RAN2 specifications. |
|  |  |  |
|  |  |  |

## 2.2 Part 2: Intended to progress discussion on agreeable parts

- To be updated after discussion on part 1 -

# 3 Conclusion

- To be updated after discussion on part 1 -

# 4 References

1. [R2-2101559](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101559.zip) CR on the SupportedBandwidth/channelBWs-R15 ZTE Corporation, Sanechips CR Rel-15 38.306 15.12.0 0515 - F NR\_newRAT-Core
2. [R2-2101560](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101560.zip) CR on the SupportedBandwidth/channelBWs-R16 ZTE Corporation, Sanechips CR Rel-16 38.306 16.3.0 0516 - A NR\_newRAT-Core
3. [R2-2100064](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100064.zip) LS on single UL operation (RP-202932; contact: Huawei) RAN LS in Rel-15 NR\_newRAT-Core To:RAN2, RAN4
4. [R2-2101561](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101561.zip) Clarification on the SingleUL-Transmission ZTE Corporation, Sanechips discussion Rel-15 NR\_newRAT-Core
5. [R2-2101913](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101913.zip) Clarfication on single uplink operation capability report (LS Contact) Huawei, HiSilicon CR Rel-15 38.306 15.12.0 0524 - F NR\_newRAT-Core
6. [R2-2101914](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2101914.zip) Clarfication on single uplink operation capability report (LS Contact) Huawei, HiSilicon CR Rel-16 38.306 16.3.0 0525 - A NR\_newRAT-Core
7. [R2-2100961](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100961.zip) Handling of single UL for intra-band EN-DC band combinations Nokia, Nokia Shanghai Bell CR Rel-15 38.306 15.12.0 0497 - F NR\_newRAT-Core
8. [R2-2100962](file:///D:/Documents/3GPP/tsg_ran/WG2/RAN2/2101_R2_113e/Docs/R2-2100962.zip) Handling of single UL for intra-band EN-DC band combinations Nokia, Nokia Shanghai Bell CR Rel-16 38.306 16.3.0 0498 - A NR\_newRAT-Core