3GPP TSG-RAN WG2 Meeting #116bis-e R2-22XXXX

Electronic Meeting, 17 – 25 January 2022

**Agenda item: 8.24.1**

**Source: CMCC**

**Title: [AT116bis-e][039][NR17] RRM enh for HST (CMCC)**

**WID/SID: NR\_HST\_FR1\_enh**

**Document for: Discussion and Decision**

# Introduction

This document aims at address the remaining details for slice groups

 **[AT116bis-e][039][NR17] RRM enh for HST (CMCC)**

 Scope: Treat R2-2200123, R2-2201334, R2-2201335, R2-2201336, R2-2200864, R2-2200865. 1 Determine what RAN2 need to do / agreeable parts 2 endorse Draft CRs.

 Intended outcome: Report, endorsed Draft CRs.

 Deadline: EOM (assume no online CB)

**Contact List**

|  |  |  |
| --- | --- | --- |
| Company | Name | Email |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Discussion

## RRC CR

In Rel-16, some enhancement on RRM measurement was introduced for HST with an IE highSpeedMeasFlag-r16 signalled per serving cell basis in both ServingCellConfigCommonSIB and ServingCellConfigCommon. However the Rel-16 HST only considers single carrier scenario. Therefore, some clarification that this parameter only applies to SpCell is essential. [2-6]

**Q1: Do you agree to clarify that *highSpeedMeasFlag-r16* is not applicable to SCell.**

|  |  |  |
| --- | --- | --- |
| Company | Agree with Q1? | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

When we come to the Rel-17 signalling design for HST, RAN4 had agreed the following networking indication.

•For CA enhancement: RAN4 agreed that network needs to inform UE whether to apply the enhanced RRM requirements for CA specified in TS38.133.

•For inter-frequency measurement enhancement: for idle mode, RAN4 agrees to introduce network signalling to inform UE whether the enhanced inter-frequency HST measurement requirements are applied per each inter-frequency carrier

Based on the above requirement, for CA enhancement, considering we already have the Rel-16 per serving cell indication to indicate the UE to apply the enhanced RRM requirement, it is quite straightforward to reuse this parameter in Rel-17 for SpCell, some clarification for the field description is enough. [2-6]

**Q2: Do you agree to reuse *highSpeedMeasFlag-r16* to apply CA measurement enhancement for SpCell, and a new IE *highSpeedMeasCA-Scell-r17* is introduced in *HighSpeedConfig* to apply CA measurement for SCell.**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not? | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

In [2], Huawei proposed that, for SCells within the same serving cell group, the RRM enhancement should be enabled or disabled simultaneously, i.e., it is not allowed to enable some SCells while disable the others within the same cell group. Therefore the network should set the same value of highSpeedMeasFlag-r16 for the SCells contained in the same serving cell group.

**Q3: Do you agree that Network should set the values of *highSpeedMeasFlag-r16* to the same value for the SCells contained in the same serving cell group?**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not? | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

The following RRC CR is taken as baseline, please share comments if there is any further issue.

R2-2200864 Introduction of RRM enhancements for Rel-17 NR FR1 HST CMCC, Ericsson draftCR Rel-17 38.331 16.7.0 B NR\_HST\_FR1\_enh

**Q4: Do you agree with above draft CR** R2-2200864**?**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not? | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Capability CR

According to RAN4 LS, capabilities for CA and inter-frequency measurement enhancement are needed.

* For CA enhancement
* RAN4 notices that the IE *highSpeedMeasFlag-r16* is signalled per serving cell basis in both *ServingCellConfigCommonSIB* and *ServingCellConfigCommon*, however the Rel-16 HST WI only considers single carrier scenario. The enhancement of CA requirements is under discussion in Rel-17 NR FR1 HST, and RAN4 agreed that network needs to inform UE whether to apply the enhanced RRM requirements for CA specified in TS38.133. The signalling design is up to RAN2
* RAN4 agrees to introduce a per-UE capability to indicate whether the UE is capable of supporting the enhanced RRM requirements for CA in Rel-17
* For inter-frequency measurement enhancement
* RAN4 agrees to introduce a per-UE capability to indicate whether the UE is capable of supporting the enhanced RRM requirements for inter-frequency measurement for connected mode. RAN4 also agrees that the support of HST idle mode inter-frequency measurement enhancements is an optional UE feature without capability signalling.
* For idle mode, RAN4 agrees to introduce network signalling to inform UE whether the enhanced inter-frequency HST measurement requirements are applied per each inter-frequency carrier. The signalling design is up to RAN2
* For connected mode, the discussion for the network signalling is on-going in RAN4. RAN4 will provide further updates if the conclusions are reached.

The following 38.306 CR is taken as baseline.

R2-2200865 Introduction of RRM enhancements for Rel-17 NR FR1 HST CMCC, Ericsson draftCR Rel-17 38.306 16.7.0 B NR\_HST\_FR1\_enh

***Capability with RRC signalling***

| **Definitions for parameters** | **Per** | **M** | **FDD-TDD****DIFF** | **FR1-FR2****DIFF** |
| --- | --- | --- | --- | --- |
| ***measurementEnhancementCA-Scell-r17***Indicates whether the UE supports the enhanced RRM requirements to SCell for carrier aggregation to support high speed up to 500 km/h as specified in TS 38.133 [5]. This field does not apply when Dual Connectivity is configured. This field is applied to SCell only. | UE | No | No | FR1 only |
| ***measurementEnhancementInterFreq-r17***Indicates whether the UE supports the enhanced RRM requirements for inter-frequency measurements in connected mode to support high speed up to 500 km/h as specified in TS 38.133 [5]. | UE | No | No | FR1 only |

**Q5: Do you agree to introduce the above capability with RRC signalling reporting?**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not? | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

***Capability without RRC signalling***

| **Definitions for feature** |
| --- |
| **High speed inter-frequency IDLE/INACTIVE measurements**It is optional for UE to support high speed inter-frequency measurements in RRC\_IDLE/RRC\_INACTIVE as specified in TS 38.133 [5]. |

**Q6: Do you agree to introduce the above optional capability without RRC signalling reporting?**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not? | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q7: Any other issue for 38.306 CR R2-2200865 ?**

|  |  |
| --- | --- |
| Company |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Summary

# References

1. R2-2200123 LS on signalling for RRM enhancements for Rel-17 NR FR1 HST (R4-2120286; contact: CMCC) RAN4 LS in Rel-17 NR\_HST\_FR1\_enh To:RAN2
2. R2-2201334 Discussion on the signaling for RRM enhancement for Rel-17 HST Huawei, HiSilicon discussion
3. R2-2201335 On the signaling for RRM enhancements for Rel-17 HST Huawei, HiSilicon draftCR Rel-17 38.331 16.7.0 B NR\_HST\_FR1\_enh
4. R2-2201336 On the UE capabilities for RRM enhancements for Rel-17 HST Huawei, HiSilicon draftCR Rel-17 38.306 16.7.0 B NR\_HST\_FR1\_enh
5. R2-2200864 Introduction of RRM enhancements for Rel-17 NR FR1 HST CMCC, Ericsson draftCR Rel-17 38.331 16.7.0 B NR\_HST\_FR1\_enh
6. R2-2200865 Introduction of RRM enhancements for Rel-17 NR FR1 HST CMCC, Ericsson draftCR Rel-17 38.306 16.7.0 B NR\_HST\_FR1\_enh