**3GPP TSG RAN WG2#116-bis-e draft R2-2201744**

**Online meeting, January 17-25th, 2022**

Title: [draft] LS on UE location during initial access in NTN

Response to: -

Release: Release 17

Source: Thales [to be RAN2]

To: SA2, RAN3

Cc: CT1, SA3

**Contact Person:**

Name: Nicolas Chuberre

E-mail Address: nicolas.chuberre@thalesaleniaspace.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

Attachments: None

**1. Overall Description:**

RAN2 had decided (see R2-2109216) that the UE may report to the NG-RAN *its coarse GNSS coordinates during initial access (before AS security is activated).*The reporting would be under network control (i.e. it could be disabled if/when needed).

Following liaisons from SA2, SA3 and RAN3 (see R2-2200145/S2-2109337, R2-2200149/S3-214360, R2-2202542/S3i200056) on this, RAN2 is discussing an alternative option and requires the views of SA2 and RAN3 to take its decision.

Due to possible security issues, RAN2 may decide that UE does not report to the NG-RAN its coarse GNSS coordinates during initial access (before AS security is activated). RAN2 assumes UE location information can be reported after AS security is activate, and 5G-AN can reselect an AMF serving a PLMN corresponding to the UE's current location (acquired after AS security is activated) if needed.

Does SA2/RAN3 foresee any issue with RAN2’s possible decision (e.g. when NTN beam covers several countries and un-cooperating PLMN) ?

**2. Actions:**

**To** **SA2, RAN3**

**ACTION:** RAN2 kindly asks SA2, RAN3 to answer the questions above.

**3. Date of Next RAN2 Meetings:**

TSG-RAN WG2#117- e February 21st – March 3rd, 2022 Online meeting