**3GPP TSG-RAN WG2 Meeting #118-e R2-220xxxx**

**Online, May 9th – May 20th, 2022**

**Agenda item:** **6.1.3.1**

**Source: CATT**

**Title: Report of [AT118-e][030][MBS] CP other**

**WI code: NR\_MBS-Core**

**Document for:** **Discussion and Decision**

# Introduction

This document aims at gathering and summarizing companies’ views for the following offline discussion:

* [AT118-e][030][MBS] CP other (CATT)

 Scope: Treat R2-2204669, R2-2204827, R2-2205749, R2-2204670, R2-2204828, R2-2205249, R2-2205632, R2-2206123, R2-2205626, R2-2206124, R2-2204830, R2-2205627, R2-2204668, R2-2205745

 Collect one round of comments, pave the way for on-line agreement (identify agreeable points, discussion points),

 Intended outcome: Report

 Deadline: For online CB W1 Thursday

# Contact details

|  |  |
| --- | --- |
| **Company** | **Contact details (name, e-mail)** |
| CATT | Rui Zhou(zhourui@catt.cn) |
|  |  |
|  |  |

# Discussion

## Group paging Handling

### [C006] Correction to UE Behavior on Group Paging Handling

In R2-2204669, it is proposed to specify that when UE receiving group paging that does not contain CN paging, UE should not forward TMGI to upper layers.

In this case, RRC inactive UE directly triggers RRC resume procedure, and thus from this point of view RRC does not expect any trigger from NAS. In this case if TMGI is forwarded to NAS, unexpected procedure (e.g. NAS requests the lower layer to establish an RRC connection) may be triggered by NAS. It is unnecessary and may conflict with ongoing RRC resume procedure.

|  |  |
| --- | --- |
| TDoc | Proposals |
| CATTR2-2204669 | 5.3.2.3 Reception of the *Paging* *message* by the UE……1> if in RRC\_IDLE, for each *TMGI* included in *pagingGroupList*, if any, included in the *Paging* message:2> if the UE has joined an MBS session indicated by the *TMGI* included in the *pagingGroupList*:3> forward the *TMGI* to the upper layers;1> if in RRC\_INACTIVE and the UE has joined one or more MBS session(s) indicated by the *TMGI* included in the *pagingGroupList:*2> if none of the *ue-Identity* included in any of the *PagingRecord*, if included in the *Paging* message, matches the UE identity allocated by upper layers:3> initiate the RRC connection resumption procedure according to 5.3.13 with *resumeCause* set as below:4> if the UE is configured by upper layers with Access Identity 1:5> *resumeCause* is set to *mps-PriorityAccess*;4> else if the UE is configured by upper layers with Access Identity 2:5> *resumeCause* is set to *mcs-PriorityAccess*;4> else if the UE is configured by upper layers with one or more Access Identities equal to 11-15:5> *resumeCause* is set to *highPriorityAccess*;4> else:5> *resumeCause* is set to *mt-Access*.2> else: 3> forward the *TMGI* to the upper layers;3> perform the actions upon going to RRC\_IDLE as specified in 5.3.11; |

Companies are then requested to answer the following question.

**Question 1: Do you agree the change proposed in R2-2204669?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | Yes | According to the spec, RRC inactive UE directly triggers RRC resume procedure if there is only TMGIs in paging message, and thus from this point of view RRC does not expect any trigger from NAS. To avoid unexpected procedure (e.g. NAS requests the lower layer to establish an RRC connection) triggered by NAS, this change makes sense. |
|  |  |  |
|  |  |  |

### [V500] Clarification on Group Paging for INACTIVE UE

In R2-2204827, it is proposed to clarify that UE in RRC\_INACTIVE only monitor RAN paging using TMGI as CN paging using TMGI is only used to page CM-IDLE UEs.

|  |  |
| --- | --- |
| TDoc | Proposals |
| VIVOR2-2204827 | **Proposal 1: Update the description in TS 38.331 clause 4.2.8 that “If configured by upper layers for MBS multicast reception, monitors Paging channel for paging using TMGI” to “If configured by upper layers for MBS multicast reception, monitors Paging channel for RAN paging using TMGI”.**Annex: Proposed TP to TS 38.3314.2.1 UE states and state transitions including inter RATA UE is either in RRC\_CONNECTED state or in RRC\_INACTIVE state when an RRC connection has been established. If this is not the case, i.e. no RRC connection is established, the UE is in RRC\_IDLE state. The RRC states can further be characterised as follows:……**- RRC\_INACTIVE**:- A UE specific DRX may be configured by upper layers or by RRC layer;- UE controlled mobility based on network configuration;- The UE stores the UE Inactive AS context;- A RAN-based notification area is configured by RRC layer;- Transfer of unicast data and/or signalling to/from UE over radio bearers configured for SDT;The UE:- Monitors Short Messages transmitted with P-RNTI over DCI (see clause 6.5);- During SDT procedure, monitors control channels associated with the shared data channel to determine if data is scheduled for it;- While SDT procedure is not ongoing, monitors a Paging channel for CN paging using 5G-S-TMSI and RAN paging using fullI-RNTI;- If configured by upper layers for MBS multicast reception, monitors Paging channel for RAN paging using TMGI; |

Companies are then requested to answer the following question.

**Question 2: Do you agree the change proposed in R2-2204827?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | No | For inactive UE, it is still possible to receive a CN paging using TMGI. |
|  |  |  |
|  |  |  |

### Multicast session start and Paging

In R2-2205749, it is proposed to change the Need code for pagingGroupList and add field description for serviceID, and it is also proposed that UE should report TMGI to upper layers when the when the multicast MRB is established.

|  |  |
| --- | --- |
| TDoc | Proposals |
| Ericsson R2-2205749 | **Proposal 1**: Need code N is used for *pagingGroupList***Proposal 2**: The following field description is used for the *serviceID* (similar as in LTE): ***serviceId***Uniquely identifies the identity of an MBS service within a PLMN. The field contains octet 3- 5 of the IE Temporary Mobile Group Identity (TMGI) as defined in TS 24.008 [49]. The first octet contains the third octet of the TMGI, the second octet contains the fourth octet of the TMGI and so on.**Proposal 3**: When the multicast MRB is established the TMGI is reported to the upper layers.  |

Companies are then requested to answer the following question.

**Question 3: Do you agree the P1 in R2-2205749?**

***Proposal 1****: Need code N is used for pagingGroupList*

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | Yes |  |
|  |  |  |
|  |  |  |

**Question 4: Do you agree the P2 in R2-2205749?**

*Proposal 2: The following field description is used for the serviceID (similar as in LTE):*

***serviceId***

*Uniquely identifies the identity of an MBS service within a PLMN. The field contains octet 3- 5 of the IE Temporary Mobile Group Identity (TMGI) as defined in TS 24.008 [49]. The first octet contains the third octet of the TMGI, the second octet contains the fourth octet of the TMGI and so on.*

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | Yes |  |
|  |  |  |
|  |  |  |

**Question 5: Do you agree the P3 in R2-2205749?**

*Proposal 3: When the multicast MRB is established the TMGI is reported to the upper layers.*

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | No | Not necessary. There is no such requirement” for display purposes” from CT1/SA2. |
|  |  |  |
|  |  |  |

## Multicast MRB ID change handling

In RAN2#117e meeting, the following agreement is made,

* **MRB ID can be changed without releasing/adding MRB (delta config)**

The agreement is captured in the 38.331 CR as below. However, it seems that the current procedure does not reflect the agreement correctly.

|  |
| --- |
| 5.3.5.6.7 Multicast MRB addition/modificationThe UE shall:1> for each *mrb-Identity* value included in the *mrb-ToAddModList* for which *mrb-IdentityNew* is included (multicast MRB ID change):2> update the *mrb-Identity* to the value *mrb-IdentityNew*;1> for each *mrb-Identity* value included in the *mrb-ToAddModList* that is not part of the current UE configuration (multicast MRB establishment including the case when full configuration option is used):2> establish a PDCP entity and configure it in accordance with the received *pdcp-Config*;……<omitted>1> for each *mrb-Identity* value included in the *mrb-ToAddModList* that is part of the current UE configuration (prior treating this *mrb-ToAddModList)*:2> if the *reestablishPDCP* is set:3> if *drb-ContinueROHC* is included in *pdcp-Config*:4> indicate to lower layer that *drb-ContinueROHC* is configured;3> if *drb-ContinueEHC-DL* is included in *pdcp-Config*:4> indicate to lower layer that *drb-ContinueEHC-DL* is configured;3> re-establish the PDCP entity of this multicast MRB as specified in TS 38.323 [5], clause 5.1.2;2> else, if the *recoverPDCP* is set:3> trigger the PDCP entity of this MRB to perform data recovery as specified in TS 38.323 [5];2> if the *pdcp-Config* is included:3> reconfigure the PDCP entity in accordance with the received *pdcp-Config*. |

During R17 asn.1 review, [C001] [V503][V504][V508] [H002] are raised on this issue. The below papers are also submitted by companies to address this issue.

|  |  |
| --- | --- |
| TDoc | Proposals/TP |
| CATTR2-2204670 | 5.3.5.6.7 Multicast MRB addition/modificationThe UE shall:1> for each *mrb-Identity* value included in the *mrb-ToAddModList* that is not part of the current UE configuration (multicast MRB establishment including the case when full configuration option is used):2> establish a PDCP entity and configure it in accordance with the received *pdcp-Config*;……<omitted>1> for each *mrb-Identity* value included in the *mrb-ToAddModList* that is part of the current UE configuration (prior treating this *mrb-ToAddModList)*:2> if the *mrb-IdentityNew* is included (multicast MRB ID change):3> update the MRB Identity in current UE configurationto the value *mrb-IdentityNew*;2> if the *reestablishPDCP* is set:3> if *drb-ContinueROHC* is included in *pdcp-Config*:4> indicate to lower layer that *drb-ContinueROHC* is configured;3> if *drb-ContinueEHC-DL* is included in *pdcp-Config*:4> indicate to lower layer that *drb-ContinueEHC-DL* is configured;3> re-establish the PDCP entity of this multicast MRB as specified in TS 38.323 [5], clause 5.1.2;2> else, if the *recoverPDCP* is set:3> trigger the PDCP entity of this MRB to perform data recovery as specified in TS 38.323 [5];2> if the *pdcp-Config* is included:3> reconfigure the PDCP entity in accordance with the received *pdcp-Config*. |
| VIVOR2-2204828 | **Proposal 1: Remove the first bullet 1 in TS 38.331 clause 5.3.5.6.7, and add the operation of updating the mrb-Identity to the value *mrb-IdentityNew* in the loop of “for each *mrb-Identity* value included in the *mrb-ToAddModList* that is part of the current UE configuration”.****Proposal 2: Add a note in TS 38.331 clause 5.3.5.6.7 that “UE is not expected to receive the *mrb-ToAddModList* in which an entry carrying *mrb-IdentityNew* is put behind an entry carrying only *mrb-Identity*”.**5.3.5.6.7 Multicast MRB addition/modificationThe UE shall:1> for each *mrb-Identity* value included in the *mrb-ToAddModList* that is part of the current UE configuration (prior treating this *mrb-ToAddModList)*:2> update the *mrb-Identity* to the value *mrb-IdentityNew* if included;2> if the *reestablishPDCP* is set:3> if *drb-ContinueROHC* is included in *pdcp-Config*:4> indicate to lower layer that *drb-ContinueROHC* is configured;3> if *drb-ContinueEHC-DL* is included in *pdcp-Config*:4> indicate to lower layer that *drb-ContinueEHC-DL* is configured;3> re-establish the PDCP entity of this multicast MRB as specified in TS 38.323 [5], clause 5.1.2;2> else, if the *recoverPDCP* is set:3> trigger the PDCP entity of this MRB to perform data recovery as specified in TS 38.323 [5];2> if the *pdcp-Config* is included:3> reconfigure the PDCP entity in accordance with the received *pdcp-Config*.1> for each *mrb-Identity* value included in the *mrb-ToAddModList* that is not part of the current UE configuration (multicast MRB establishment including the case when full configuration option is used):2> establish a PDCP entity and configure it in accordance with the received pdcp-Config;2> if an SDAP entity with the received tmgi does not exist:3> establish an SDAP entity as specified in TS 37.324 [24] clause 5.1.1;3> if an SDAP entity with the received *tmgi* did not exist prior to receiving this reconfiguration:4> indicate the establishment of the user plane resources for the *tmgi* to upper layers;NOTE 1: When setting the *reestablishPDCP* flag for a radio bearer, the network ensures that the RLC receiver entities do not deliver old PDCP PDUs to the re-established PDCP entity. It does that e.g. by triggering a reconfiguration with sync of the cell group hosting the old RLC entity or by releasing the old RLC entity.NOTE 2: In this specification, UE configuration refers to the parameters configured by NR RRC unless otherwise stated.NOTE 3: In this specification, UE is not expected to receive the *mrb-ToAddModList* in which an entry carrying *mrb-IdentityNew* is put behind an entry carrying only *mrb-Identity*. |
| Nokia,HuaweiR2-2205249 | Annex A: TP of modified procedural text for handling each element of mrb add mod list separately5.3.5.6.7 Multicast MRB addition/modificationThe UE shall for each element in the order of entry in the list the *mrb-ToAddModList*:1> if *mrb-Identity* value included in the *mrb-ToAddModList* that is part of the UE configuration:2> if *mrb-Identity* value included in the *mrb-ToAddModList* for which *mrb-IdentityNew* is included (multicast MRB ID change):3> update the *mrb-Identity* to the value *mrb-IdentityNew*;2> if the *reestablishPDCP* is set:3> if *drb-ContinueROHC* is included in *pdcp-Config*:4> indicate to lower layer that *drb-ContinueROHC* is configured;3> if *drb-ContinueEHC-DL* is included in *pdcp-Config*:4> indicate to lower layer that *drb-ContinueEHC-DL* is configured;3> re-establish the PDCP entity of this multicast MRB as specified in TS 38.323 [5], clause 5.1.2;2> else, if the *recoverPDCP* is set:3> trigger the PDCP entity of this MRB to perform data recovery as specified in TS 38.323 [5];2> if the *pdcp-Config* is included:3> reconfigure the PDCP entity in accordance with the received *pdcp-Config*.1> else if *mrb-Identity* value included in the *mrb-ToAddModList* that is not part of the UE configuration (multicast MRB establishment including the case when full configuration option is used):2> establish a PDCP entity and configure it in accordance with the received *pdcp-Config*;2> if the multicast MRB was configured with the same *tmgi* prior to receiving this reconfiguration message:3> associate the established multicast MRB with the corresponding *tmgi*;2> else:3> indicate the establishment of the multicast MRB(s) and the *tmgi* of the established multicast MRB(s) to upper layers;2> if an SDAP entity with the received *tmgi* does not exist:3> establish an SDAP entity as specified in TS 37.324 [24] clause 5.1.1;NOTE 1: When setting the *reestablishPDCP* flag for a radio bearer, the network ensures that the RLC receiver entities do not deliver old PDCP PDUs to the re-established PDCP entity. It does that e.g. by triggering a reconfiguration with sync of the cell group hosting the old RLC entity or by releasing the old RLC entity.NOTE 2: In this specification, UE configuration refers to the parameters configured by NR RRC unless otherwise stated.Annex B: TP for retaining existing style with required modifications5.3.5.6.7 Multicast MRB addition/modificationThe UE shall:1> for each *mrb-Identity* value included in the *mrb-ToAddModList* for which *mrb-IdentityNew* is included (multicast MRB ID change):2> update the *mrb-Identity* in the current UE configurationandthe *mrb-Identity* in the *mrb-ToAddModList* to the value *mrb-IdentityNew*;1> for each *mrb-Identity* value included in the *mrb-ToAddModList* that is part of the current UE configuration:2> if the *reestablishPDCP* is set:3> if *drb-ContinueROHC* is included in *pdcp-Config*:4> indicate to lower layer that *drb-ContinueROHC* is configured;3> if *drb-ContinueEHC-DL* is included in *pdcp-Config*:4> indicate to lower layer that *drb-ContinueEHC-DL* is configured;3> re-establish the PDCP entity of this multicast MRB as specified in TS 38.323 [5], clause 5.1.2;2> else, if the *recoverPDCP* is set:3> trigger the PDCP entity of this MRB to perform data recovery as specified in TS 38.323 [5];2> if the *pdcp-Config* is included:3> reconfigure the PDCP entity in accordance with the received *pdcp-Config*.NOTE 1: When setting the *reestablishPDCP* flag for a radio bearer, the network ensures that the RLC receiver entities do not deliver old PDCP PDUs to the re-established PDCP entity. It does that e.g. by triggering a reconfiguration with sync of the cell group hosting the old RLC entity or by releasing the old RLC entity.NOTE 2: In this specification, UE configuration refers to the parameters configured by NR RRC unless otherwise stated. |
| ZTER2-2205632 | 1. **For the deployment scenarios of PDCP SN sync based on SN on NG-U, the MRB ID and PDCP SN length are synced by means of network implementation.**
2. **MRB ID is of the same length of DRB, i.e., no need to extend MRB ID length.**
3. **One multicast MRB is uniquely identified by MRD ID and the MBS session ID (i.e., TMGI).**
4. Do not support the MRB ID modification on the fly, i.e., MRB ID modification without release/add MRB explicitly.
 |

Companies (CATT,VIVO,Nokia/Huawei) propose different solutions to correctly capture the agreement in the 38.331 spec. On the other hand, it seems that ZTE proposes to override the RAN2 agreement (i.e. MRB ID can be changed without releasing/adding MRB (delta config)).

Therefore, there are following options to address the MRB ID change issue,

Option 1: TP from CATT (as in R2-2204670)

Option 2: TP from VIVO (as in R2-2204828)

Option 3: TP (Annex A) from Noika, Huawei(as in R2-2205249)

Option 4: TP (Annex B) from Noika, Huawei(as in R2-2205249)

Option 5: Do not support the MRB ID modification on the fly (as in R2-2205632),which means to override the previous agreement(i.e. MRB ID can be changed without releasing/adding MRB (delta config)), i.e.

Companies are then requested to answer the following question,

**Question 6: Which option do you prefer to address the MRB ID change issue?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Preferred option****(option1,2,3,4,5)** | **Comments / justification** |
| CATT | Option 1 | Option 1 is simplest and can address the MRB ID change issue well. |
|  |  |  |
|  |  |  |

In R2-2204828, it is also proposed that only when UE establishes an SDAP for a TMGI, UE informs the establishment of user plane resources for the TMGI.

|  |  |
| --- | --- |
| TDoc | Proposals/TP |
| VIVOR2-2204828 | **Proposal 3: Only when UE establishes an SDAP for a TMGI, UE informs the establishment of user plane resources for the TMGI.**Annex: Proposed TP to TS 38.331……5.9.3.3 Broadcast MRB establishmentUpon a broadcast MRB establishment, the UE shall:1> establish a PDCP entity and an RLC entity in accordance with *MRB-InfoBroadcast* for this broadcast MRB included in the *MBSBroadcastConfiguration* message and the configuration specified in 9.1.1.7;1> receive DL-SCH on the cell where the *MBSBroadcastConfiguration* message was received for the MBS broadcast service for which the broadcast MRB is established and using *g-RNTI* and *mtch-SchedulingInfo* (if included) in this message for this MBS broadcast service;1> configure the physical layer in accordance with the *mbs-SessionInfoList*, *searchSpaceMTCH,* *pdsch-ConfigMTCH*, applicable for the broadcast MRB, as included in the *MBSBroadcastConfiguration* message;1> if an SDAP entity with the received *tmgi* does not exist:2> establish an SDAP entity as specified in TS 37.324 [24] clause 5.1.1.2> if an SDAP entity with the received *tmgi* did not exist prior to receiving this reconfiguration:3> indicate the establishment of the user plane resources for the *tmgi* to upper layers; |

Companies are then requested to answer the following question,

**Question 7: Do you agree P3 and corresponding TP in R2-2204828?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | Yes |  |
|  |  |  |
|  |  |  |

## Other topics

### [H091]Corrections for GroupConfig structure

Currently in the *Group-Config* type specified for MBS within *MAC-CellGroupConfig* IE, two different types of identifiers are used to denote the identity of the particular group config. The type of identifier that is used depends on whether G-RNTI or G-CS-RNTI is configured within Group-Config IE (which in turn depends on whether the Group-Config is within *g-RNTI-ConfigToAddModList-r17* or within *g-CS-RNTI-ConfigToAddModList-r17*).

In R2-2206123, company thinks that this results in using a CHOICE structure for choosing the identifier which is then used for managing the lists of G-RNTI and G-CS-RNTI configurations. This is rather an unusual practice and it also is not required to have two different identifiers for these two listst as a single identifier will equally serve the purpose.so it is proposed that:

1. The Group-Config structure is modified so that it relies on a single identifier for list management.
2. Group-Config type is renamed as MBS-RNTI-SpecificConfig to better express its purpose.

The text proposals are as below,

|  |  |
| --- | --- |
| TDoc | Proposals |
| Huawei R2-2206123 | -MAC-CellGroupConfigThe IE *MAC-CellGroupConfig* is used to configure MAC parameters for a cell group, including DRX.*MAC-CellGroupConfig* information element-- ASN1START-- TAG-MAC-CELLGROUPCONFIG-STARTMAC-CellGroupConfig ::= SEQUENCE { drx-Config SetupRelease { DRX-Config } OPTIONAL, -- Need M schedulingRequestConfig SchedulingRequestConfig OPTIONAL, -- Need M bsr-Config BSR-Config OPTIONAL, -- Need M tag-Config TAG-Config OPTIONAL, -- Need M phr-Config SetupRelease { PHR-Config } OPTIONAL, -- Need M skipUplinkTxDynamic BOOLEAN, ..., [[ csi-Mask BOOLEAN OPTIONAL, -- Need M dataInactivityTimer SetupRelease { DataInactivityTimer } OPTIONAL -- Cond MCG-Only ]], [[ usePreBSR-r16 ENUMERATED {true} OPTIONAL, -- Need R schedulingRequestID-LBT-SCell-r16 SchedulingRequestId OPTIONAL, -- Need R lch-BasedPrioritization-r16 ENUMERATED {enabled} OPTIONAL, -- Need R schedulingRequestID-BFR-SCell-r16 SchedulingRequestId OPTIONAL, -- Need R drx-ConfigSecondaryGroup-r16 SetupRelease { DRX-ConfigSecondaryGroup } OPTIONAL -- Need M ]], [[ enhancedSkipUplinkTxDynamic-r16 ENUMERATED {true} OPTIONAL, -- Need R enhancedSkipUplinkTxConfigured-r16 ENUMERATED {true} OPTIONAL -- Need R ]], [[ intraCG-Prioritization-r17 ENUMERATED {enabled} OPTIONAL, -- Cond LCH-PrioWithReTxTimer drx-ConfigSL-r17 SetupRelease { DRX-ConfigSL } OPTIONAL, -- Cond Mode1AndDRX-Only drx-ConfigExt-v1700 SetupRelease { DRX-ConfigExt-v1700 } OPTIONAL, -- Cond DRX schedulingRequestID-BFR-r17 SchedulingRequestId OPTIONAL, -- Need R schedulingRequestID-BFR2-r17 SchedulingRequestId OPTIONAL, -- Need R schedulingRequestConfig-v1700 SchedulingRequestConfig-v1700 OPTIONAL, -- Need M --Editor’s note: extension done according to A4.3.5  offsetThresholdTA ENUMERATED{ms05, ms1, ms2, ms3, ms4, ms5, ms6 ,ms7, ms8, ms9, ms10, ms11, ms12, ms13, ms14, ms15} OPTIONAL, -- Need R --Editor’s note: may need to add here parameter TimingAdvanceSR g-RNTI-ConfigToAddModList-r17 SEQUENCE (SIZE (1..maxG-RNTI-r17)) OF MBS-RNTI-SpecificConfig-r17 OPTIONAL, -- Need N g-RNTI-ConfigToReleaseList-r17 SEQUENCE (SIZE (1..maxG-RNTI-r17)) OF MBS-GroupConfigId-r17 OPTIONAL, -- Need N g-CS-RNTI-ConfigToAddModList-r17 SEQUENCE (SIZE (1..maxG-CS-RNTI-r17)) OF MBS-RNTI-SpecificConfig-r17 OPTIONAL, -- Need N g-CS-RNTI-ConfigToReleaseList-r17 SEQUENCE (SIZE (1..maxG-CS-RNTI-r17)) OF MBS-GroupConfigId-r17 OPTIONAL, -- Need N allowCSI-SRS-Tx-MulticastDRX-Active-r17 BOOLEAN ]]}DataInactivityTimer ::= ENUMERATED {s1, s2, s3, s5, s7, s10, s15, s20, s40, s50, s60, s80, s100, s120, s150, s180}MBS-RNTI-SpecificConfig-r17 ::= SEQUENCE { mbs-RNTI-SpecificConfigId-r17 MBS-RNTI-SpecificConfigId-r17; groupCommon-RNTI CHOICE { g-RNTI RNTI-Value, g-CS-RNTI RNTI-Value }, drx-ConfigPTM-r17 SetupRelease { DRX-ConfigPTM-r17 } OPTIONAL, -- Need M harq-FeedbackEnablerMulticast-r17 ENUMERATED {dci-enabler, enabled} OPTIONAL, -- Need S harq-FeedbackOptionMulticast-r17 ENUMERATED {ack-nack, nack-only} OPTIONAL, -- CondHARQFeedback pdsch-AggregationFactorMulticast-r17 ENUMERATED {n2, n4, n8} OPTIONAL -- Cond G-RNTI}MBS-RNTI-SpecificConfigId ::= INTEGER (0..maxG-RNTI-1-r17)-- TAG-MAC-CELLGROUPCONFIG-STOP-- ASN1STOP***mbs-RNTI-SpecificConfigId***An identifier of the RNTI specific configuration for MBS multicast.  |

Companies are then requested to answer the following question,

**Question 8: Do you agree the change proposed in R2-2206123?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | Yes |  |
|  |  |  |
|  |  |  |

### [H001, H005, Z608, C005] Discussion on multicast MRB and DRB in RRC

In R2-2205626, several proposals are proposed on how to treat multicast MRB in

- connection management

- priority of multicast MRB in MII.

|  |  |
| --- | --- |
| TDoc | Proposals |
| ZTER2-2205626 | **Observation 1 Based on the resource model defined by SA2, there will always be a DRB if there is MRB configured by network.****Proposal 1 The *conditionalReconfiguration* for CHO or CPA is configured regardless of the existence of multicast MRB.****Proposal 2 RRC Connection suspension can be issued regardless of the existence of multicast MRB.****Proposal 3 The prioritization over unicast bearer applies to multicast MRB too, that is, if indicated by UE, the reception of broadcast services is prioritized compared to unicast bearer and also multicast MRB.** |

For P1 in R2-2205626, regarding the co-existence of CHO and MRB it has been agreed in RAN2#116bis meeting as following,

* RAN2 will not do additional work to support CHO for UEs for which MRB is configured in R17.

In rapporteur’s understanding, whether there are spec impacts is not clear if P1 is agreed.

Companies are then requested to answer the following question,

**Question 9: Do you agree P1 in R2-2205626?**

*Proposal 1 The conditionalReconfiguration for CHO or CPA is configured regardless of the existence of multicast MRB.*

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | No | RAN2 has agreed that RAN2 will no specify anything to support CHO for UEs for which MRB is configured in R17 |
|  |  |  |
|  |  |  |

**Question 10: Do you agree P2 in R2-2205626?**

*Proposal 2 RRC Connection suspension can be issued regardless of the existence of multicast MRB.*

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | Yes |  |
|  |  |  |
|  |  |  |

In MBS interest indication message, priority between the reception of all listed MBMS frequencies and the reception of any unicast bearer can be included,according to the RAN2 agreement,

* The UE reports the following MBS interest information (as LTE SC-PTM):

MBS frequency list (20/24)

priority between the reception of all listed MBMS frequencies and the reception of any unicast bearer (23/24)

TMGI list (24/24)

For P3 in R2-2205626,it is proposed to extend the priority to cover multicast MRB too.

**Question 11: Do you agree P3 in R2-2205626?**

*Proposal 3 The prioritization over unicast bearer applies to multicast MRB too, that is, if indicated by UE, the reception of broadcast services is prioritized compared to unicast bearer and also multicast MRB.*

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | No | UE preference on the priority of multicast reception may be different from unicast, we think it is not suitable to treat multicast reception same as unicast reception. |
|  |  |  |
|  |  |  |

### LS to CT1 on AS-NAS layer interactions for MBS

In R2-2206124, it is proposed to send LS to CT1 to confirm whether the AS to NAS layer indications as mentioned below are needed and/or whether there are any other events concerning MBS at AS layer which the NAS layer should be informed about.

|  |  |
| --- | --- |
| TDoc | Proposals |
| Huawei R2-2206124 | RAN2 is currently reviewing the procedures in RAN2 specifications related to MBS and one of the doubts that arose during the process was related to whether some of the information should be passed to NAS layers or not. Currently, according to RAN2 specifications, AS layer will indicate the following events related to MBS session:1. When the UE receives a Paging message including a TMGI for a multicast MBS sessions which the UE has previously joined, the UE will forward the TMGI to upper layers (for both UE in RRC\_IDLE and RRC\_INACTIVE states).
2. When MRB(s) is/are established for either MBS broadcast or MBS multicast, the UE will notify upper layers about this (and include TMGI to identify the session the notification concerns).
3. When MRB(s) is/are released for either MBS broadcast or MBS multicast, the UE will notify upper layers about this (and include TMGI to identify the session the notification concerns).

RAN2 respectfully asks CT1 to confirm whether the AS to NAS layer indications as mentioned above are needed and/or whether there are any other events concerning MBS at AS layer which the NAS layer should be informed about. |

Companies are then requested to answer the following questions,

**Question 12: Do you agree to send LS to CT1 to confirm the AS-NAS layer interactions for MBS?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | Yes | It is beneficial to confirm with CT1 |
|  |  |  |
|  |  |  |

###  [V533] Correction on Logical Channel Setup for PTM Transmission

In R2-2204830, company thinks that logicalChannelIdentityExt is only applied to PTM according to RAN2 agreement. So it is proposed to update the field description of logicalChannelIdentityExt as below,

|  |  |
| --- | --- |
| TDoc | Proposals |
| vivo R2-2204830 | **Proposal 1: Update the field description of *logicalChannelIdentityExt* to “Extended logical channel ID used commonly for the MAC logical channel and for the RLC bearer for PTM reception. If this field is configured, the UE shall ignore *logicalChannelIdentity*”.****Proposal 2: If proposal 1 is agreed, RAN2 adopts the TP in the Annex.** |

Companies are then requested to answer the following question,

**Question 13: Do you agree the change proposed in R2-2204830?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | Yes |  |
|  |  |  |
|  |  |  |

### Miscellaneous correction to TS 38331

In R2-2205627, miscellaneous corrections to TS 38331 are proposed,

|  |  |
| --- | --- |
| TDoc | Proposals |
| ZTER2-2205627 | Change 1: In 5.3.5.2, and 5.3.8.1, the initiation of RRC reconfiguration and release can be done regardless of configured multicast MRB.Change 2: In 5.3.5.6.7, 5.9.3.3, 5.9.3.4 SDAP related procedure was deleted.Change 3: In 5.9.4, the priority between broadcast and unicast/multicast was clarified. The prioritization is applied to both unicast and multicast.change 4: In 6.3.2, to achieve better power efficiency and scheduling flexibility, put the parameter allowCSI-SRS-Tx-MulticastDRX-Active in Group-Config instead of per UE config.change 5: in the MRB-Identity, the length of MRB ID is changed to 5bits, in the RadioBearerConfig, TMGI is indicated in the the MRB release; in the RLC-BearerConfig, TMGI is added in the served MRB. |

Companies are then requested to answer the following questions,

**Question 14: Do you agree the corrections proposed in R2-2205627?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | Chang 1:NoChang 2:NoChang 3:NoChang 4:NoChang 5:No | Change 1: Disagree. We think the current text is correct.Change 2: Disagree. SDAP entity is needed to handle MBS data according to 37.324Change 3: Disagree, same comments as Q11.change 4: Disagree, we think it is not motivated to make parameter allowCSI-SRS-Tx-MulticastDRX-Active on a per multicast DRX basis.change 5: Disagree.it overrides the RAN2 agreement(“Extend MRB ID space beyond current 32 limit and up to 512.”) |
|  |  |  |
|  |  |  |

## 38.304 corrections

### Scenario on setting frequencies to be of the lowest priority

In RAN2#115e meeting, the following agreement was reached,

* The UE may consider cell reselection candidate frequencies at which it cannot receive the MBS service to be of the lowest priority during the MBS session, as LTE SC-PTM. (25/25)

And the agreement is captured in 38.304 CR as below,

|  |
| --- |
| 5.2.4 Cell Reselection evaluation process5.2.4.1 Reselection priorities handling……<omitted>If the MBS broadcast capable UE is receiving or interested to receive an MBS broadcast service(s), the UE may consider cell reselection candidate frequencies at which it can not receive the MBS broadcast service to be of the lowest priority during the MBS broadcast session as specified in TS 38.300 [2], as long as the SIB20 is provided by the cell on the MBS frequency which the UE monitors and as long as the condition 2) above is fulfilled for the serving cell. |

During previous CR update discussions, some companies mentioned that it is still not clear on what scenarios UE should consider frequencies to be of the lowest priority during the MBS session.

Since this function mainly reuses the LTE mechanism, so we can take the corresponding text in 36.304 as a reference,

|  |
| --- |
| //TS 36.3045.2.4 Cell Reselection evaluation process5.2.4.1 Reselection priorities handling……If the UE is capable either of MBMS Service Continuity or of SC-PTM reception and is receiving or interested to receive an MBMS service provided on a downlink only MBMS frequency, on a frequency used by dedicated MBMS cells, on a frequency used by FeMBMS/Unicast-mixed cells as defined in TS 36.300 [2], or on a frequency belonging to PLMN different from its registered PLMN, the UE may consider cell reselection candidate frequencies at which it can not receive the MBMS service to be of the lowest priority during the MBMS session TS 36.300 [2], as long as the above mentioned condition 1) is fulfilled for the cell on the MBMS frequency which the UE monitors or this cell broadcasts SIB1-MBMS and as long as the above mentioned condition 2) is fulfilled for the serving cell.NOTE 2: Example scenarios in which the previous down-prioritisation may be needed concerns the cases where camping is not possible, while the UE can only receive this MBMS frequency when camping on a subset of cell reselection candidate frequencies, e.g. the MBMS frequency is a downlink only carrier, the MBMS frequency is used by dedicated MBMS cells, the MBMS frequency is used by FeMBMS/Unicast-mixed cells TS 36.300 [2], or the MBMS frequency belongs to a PLMN different from UE's registered PLMN. |

It seems also necessary to add similar clarification in 38.304. Therefore, in R2-2204668, it is proposed to add NOTE to clarify the scenarios on setting frequencies to be of the lowest priority during the MBS session,

|  |  |
| --- | --- |
| TDoc | Proposals |
| CATT,CBN R2-2204668 | 5.2.4 Cell Reselection evaluation process5.2.4.1 Reselection priorities handling……If the MBS broadcast capable UE is receiving or interested to receive an MBS broadcast service(s), the UE may consider cell reselection candidate frequencies at which it can not receive the MBS broadcast service to be of the lowest priority during the MBS broadcast session as specified in TS 38.300 [2], as long as the SIB20 is provided by the cell on the MBS frequency which the UE monitors and as long as the condition 2) above is fulfilled for the serving cell.NOTE: Example scenarios in which the previous down-prioritisation may be needed concerns the cases where camping is not possible, while the UE can only receive the MBS broadcast service when camping on a subset of the cell reselection candidate frequencies, e.g. the MBS broadcast frequency is a downlink only carrier, or the MBS broadcast frequency belongs to a PLMN different from UE's registered PLMN. |

Companies are then requested to answer the following question,

**Question 15: Do you agree the change proposed in R2-2204668?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | Yes | We think it is essential to clarify it, or for the intended scenario on setting frequencies to be of the lowest priority during the MBS session, it may not implemented correctly at UE side. |
|  |  |  |
|  |  |  |

### Correction to frequency prioritization

|  |  |
| --- | --- |
| TDoc | Proposals |
| Ericsson R2-2205745 | **Proposal 1**: Clarify (e.g. in a NOTE) that the UE no longer considers the frequency of the highest priority when the MCCH does not include the MBS broadcast service the UE is interested in.**Proposal 2**: Clarify in NOTE 7 what is up to UE implementation concerning frequency prioritization. **Observation 1**: Stop prioritizing the MBS frequency does not resolve the possible congregation on the MBS frequency.**Proposal 3**: Clarify in a NOTE that when the UE stops prioritizing the MBS frequency, the UE triggers inter-frequency measurements for cell reselection to another frequency.  |

For P1 and P3 in R2-2205745, they are enhancements on stopping frequency prioritization. The rapporteur understands that spec impact on stopping frequency prioritization has been extensively discussed during the WI phase, and there is no additional spec impact identified according to below agreements,

* When the conditions for frequency prioritization are no longer met, the UE should stop prioritizing the frequency of this cell (e.g. when the cell reselected by the UE due to frequency prioritization for MBS stops providing SIBx etc.). FFS whether there is additional TS impact.
* There is no additional TS impact on stopping frequency prioritization.

Companies are then requested to answer the following question,

**Question 16: Do you agree that P1 in R2-2205745?**

*Proposal 1: Clarify (e.g. in a NOTE) that the UE no longer considers the frequency of the highest priority when the MCCH does not include the MBS broadcast service the UE is interested in.*

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | No | We think there is no additional spec impact on stopping frequency prioritization according to previous discussions and RAN2 agreements |
|  |  |  |
|  |  |  |

**Question 17: Do you agree that P3 in R2-2205745?**

*Proposal 3: Clarify in a NOTE that when the UE stops prioritizing the MBS frequency, the UE triggers inter-frequency measurements for cell reselection to another frequency.*

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | No | Same comments as Q16 |
|  |  |  |
|  |  |  |

For P2 in R2-2205745, it is proposed to clarify the NOTE 7 in 38.304 further,

|  |
| --- |
| 5.2.4 Cell Reselection evaluation process5.2.4.1 Reselection priorities handling……If the MBS broadcast capable UE is receiving or interested to receive an MBS broadcast service(s) and can only receive this MBS broadcast service(s) by camping on a frequency on which it is provided, the UE may consider that frequency to be the highest priority during the MBS broadcast session as specified in TS 38.300 [2] as long as the two following conditions are fulfilled:1) The cell reselected by the UE due to frequency prioritization for MBS is providing SIB20;2) Either:- One or more MBS FSAI(s) of that frequency is indicated in SIB21 of the serving cell and the same MBS FSAI(s) is also indicated for this MBS broadcast service in MBS User Service Description (USD) as specified in TS 26.346 [20], or- SIB21 is not provided in the serving cell and that frequency is included in the USD of this service, or- SIB21 is provided in the serving cell but does not provide the frequency mapping for the concerned service, and that frequency is included in the USD of this service.NOTE 7: It is up to UE implementation how to use information in USD to determine whether/how to do the frequency prioritization for specific frequency/frequencies included in USD. |

NOTE 7 was added according to the RAN2#116bis-e agreement as below,

* UE can prioritize the frequency indicated in USD when SIBy is provided in the cell but does not provide the frequency mapping for the concerned service.
* It is up to UE implementation how to use information in USD (e.g. with other explicit knowledge) to determine whether to (or how to) do the frequency prioritization for specific frequency/frequencies in USD.

The rapporteur understands that NOTE 7 is aligned well with the agreement already.

Companies are then requested to answer the following question,

**Question 18: Do you agree to clarify NOTE 7 further, as proposed in P2 of R2-2205745?**

*Proposal 2: Clarify in NOTE 7 what is up to UE implementation concerning frequency prioritization.*

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments / justification** |
| CATT | No strong view | We are not sure if there is something to clarify further, but we follow the majority view. |
|  |  |  |
|  |  |  |

## Other issues

**Question 19: Any other CP open issues?**

|  |  |
| --- | --- |
| **Company** | **Comments / justification** |
|  |  |
|  |  |
|  |  |

# Summary

Based on the discussion above, we propose:

# Reference

 [1] R2-2204669 [C006] Correction to UE Behavior on Group Paging Handling CATT CR Rel-17 38.331 17.0.0 2991 - F NR\_MBS-Core

[2] R2-2204827 [V500] Clarification on Group Paging for INACTIVE UE vivo discussion Rel-17 NR\_MBS-Core

[3] R2-2205749 Multicast session start and Paging Ericsson discussion Rel-17 NR\_MBS-Core

 [4] R2-2204670 [C001] Modificaitons towards the MRB ID Change Procedure CATT CR Rel-17 38.331 17.0.0 2992 - F NR\_MBS-Core

[5] R2-2204828 [V503][V504][V508] Correction on MRB Handling vivo discussion Rel-17 NR\_MBS-Core

[6] R2-2205249 [V503][H002] MRB identity change procedural text issue Nokia, Nokia Shanghai Bell discussion Rel-17 NR\_MBS-Core Late

[7] R2-2205632 [C001, H002, v503, Z609] MRB ID scope and its modification on the fly ZTE, Sanechips discussion Rel-17 NR\_MBS-Core

 [8] R2-2206123 Corrections for GroupConfig structure (RIL: H091) Huawei, HiSilicon draftCR Rel-17 38.331 17.0.0 F NR\_MBS-Core

[9] R2-2205626 [H001, H005, Z608, C005] Discussion on multicast MRB and DRB in RRC ZTE, Sanechips discussion Rel-17 NR\_MBS-Core

 [10] R2-2206124 Draft LS on AS-NAS layer interactions for MBS Huawei, HiSilicon LS out Rel-17 NR\_MBS-Core

[11] R2-2204830 [V533] Correction on Logical Channel Setup for PTM Transmission vivo discussion Rel-17 NR\_MBS-Core

[12] R2-2205627 Miscellaneous correction to TS 38331 ZTE, Sanechips CR Rel-17 38.331 17.0.0 3106 - F NR\_MBS-Core

 [13] R2-2204668 Correction to 38.304 for MBS CATT, CBN CR Rel-17 38.304 17.0.0 0237 - F NR\_MBS-Core

[14] R2-2205745 Frequency prioritization Ericsson discussion Rel-17 NR\_MBS-Core