**3GPP TSG-RAN WG2 Meeting #118-e R2-22xxxxx**

**E-meeting, May 9 - 20, 2022**

**Agenda item:** 6.4.1.3

**Source:** Qualcomm Incorporated (Rapporteur)

**Title:** [AT118-e][067][eIAB] 38300 - Discussion

**Document for:** Discussion

# Introduction

This document captures:

* [AT118-e][067][eIAB] 38300 (Qualcomm)

 Scope: 1. Address the remaining TS issues from tdocs submitted under AI 6.4 (and below), except those issues addressed in specific discussion. Review collect comments identify agreement points, points for online CB etc. 2. Progress the CR, merge all TS impacts into a single CR.

 Intended outcome: Report, CR

 Deadline: 1 for CB W2 Wed (CB only if needed, attempt offline agreement), 2 CR agreement is expected in Post meeting discussion

**This discussion has two phases:**

**Phase 1 deadline: Tue May 17, 10:00 UTC (to have time for preparation to Wed CB if necessary)**

**Phase 2 deadline: TBD**

**This discussion document only includes proposals, which may be controversial. Other proposals, which are of editorial nature or potentially less controversial, have been captured in R2-22xxxxx draft CR to 38300 minor changes.**

# Phase 1: Discussion

## On section: 4.7.4.5 OTA timing synchronization

Proposals by R2-2205147 on OTA timing synchronization:

|  |
| --- |
| 4.7.4.5 OTA timing synchronizationAn IAB-DU is subject to the same downlink timing alignment of a gNB. The IAB-DU may use the received downlink signal from a parent as a reference to control its downlink timing using TA in conjunction with an additional Tdelta parameter received by the collocated IAB-MT from the parent via MAC-CE. |

**Q1: Do you agree on this addition by R2-2205147 to section 4.7.4.5 on OTA timing synchronization?**

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## On section: 5.3.5.3          Uplink timing control

Proposal by R2-2204994:

|  |
| --- |
| The gNB (/IAB-DU or IAB-donor-DU) determines the desired Timing Advance setting and provides that to the UE (/ IAB-MT). The UE/IAB-MT uses the provided TA to determine its uplink transmit timing relative to the UE's/IAB-MTs observed downlink receive timing. |

**The Rapporteur agrees that IAB-DU or IAB-donor-DU should be added. The brackets are fine, too. However, we may want to state a little more, such as “gNB (including IAB-DU and IAB-donor-DU)”. This ends up being:**

|  |
| --- |
| The gNB (including IAB-DU and IAB-donor-DU) determines the desired Timing Advance setting and provides that to the UE (or IAB-MT). The UE/IAB-MT uses the provided TA to determine its uplink transmit timing relative to the UE's/IAB-MTs observed downlink receive timing. |

**Q2: Do you agree on the Rapporteur’s proposed rewording of the rewording proposed by R2-2204994?**

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## On section: 6.11.1 Services and Functions

Proposals by R2-2204898 and R2-2205256:

**Both contributions propose to include BAP header rewriting to the BAP services and functions.**

|  |
| --- |
| 6.11.1 Services and FunctionsThe main service and functions of the BAP sublayer include:- Transfer of data;- Routing of packets to next hop;- Determination of BAP destination and BAP path for packets from upper layers;- Determination of egress BH RLC channels for packets routed to next hop;- Differentiating traffic to be delivered to upper layers from traffic to be delivered to egress link;- Flow control feedback and polling signalling;- BH RLF detection indication, BH RLF recovery indication, and BH RLF indication.- BAP header rewriting |

**Q3: Do you agree that BAP header rewriting is added under the BAP services and functions?**

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## On section: 6.11.3 Routing, BAP Header Rewriting and BH-RLC-channel Mapping on BAP sublayer

Proposal by R2-2204794 on adding Rel-17 re-routing enhancements to Rel-16 re-routing section:

|  |
| --- |
| …The IAB-node can receive multiple routing configurations with the same destination BAP address but different BAP path IDs. These routing configurations may resolve to the same or different egress BH links.In case the BH link resolved from the routing entry is considered *unavailable* for this packet, the IAB-node may perform local rerouting as defined in TS38.340 [31], i.e., select another BH link by considering only the packet's BAP address and by disregarding the BAP path ID for intra-donor DU re-routing, or select another BH link by disregarding both the packet’s BAP address and BAP path ID for inter-donor DU re-routing. In this manner, the packet can be delivered via an alternative path as defined in TS 38.340 [31].…The IAB-node may rewrite the BAP routing ID in the packet’s BAP header under the following circumstances:A packet is routed between two IAB topologies via a boundary IAB-node as defined in TS 38.401[31]. In this case, the BAP routing ID carried by the received BAP PDU is allocated by the IAB-donor-CU of the ingress IAB topology, while the BAP routing ID carried by the BAP PDU after header rewriting is allocated by the IAB-donor-CU of the egress IAB topology. An upstream packet is locally re-routed to a different IAB-donor-DU than indicated by the BAP address in the BAP header of the received packet. The rewritten BAP header carries the BAP address of the alternative IAB-donor-DU and the BAP path ID for a path to this alternative IAB-donor-DU. BAP header rewriting for upstream inter-IAB-donor-DU local rerouting is only applied if neither routing nor local re-routing without header rewriting resolve to an available BH link. … |

**The Rapporteur believes that this addition is incorrect. This section introduces the concept of local re-routing introduced in Rel-16, which is also supported in Rel-17. This should not be mixed up with Rel-17 inter-donor-DU re-routing using header-rewriting, which is a special case of local re-routing, and which is already captured here.**

**Q4a: Do you agree with the Rapporteur’s view?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Proposal by R2-2204898 on link unavailability due to IAB-node migration:

|  |
| --- |
| A BH link may be considered *unavailable* in case the BH link has RLF. A parent link may be considered *unavailable* after a BH RLF detection indication has been received on this parent link and before a subsequent BH RLF recovery indication has been received on the same parent link. For DL traffic, a BH link may be considered *unavailable* due to congestion derived from flow-control feedback information, as defined in TS 38.340 [31]. For UL traffic, after inter-donor-DU migration of an IAB-node, the egress BH link corresponding to the BAP Routing ID of a received BAP PDU with the BAP address of the original IAB-donor-DU, may be considered unavailable.  |

**The Rapporteur has the following problems with this CR:**

* **There is no inter-donor-DU migration. There is only intra-CU and inter-CU IAB-node migration.**
* **During IAB-node migration, the source parent link always becomes unavailable, not only if the IAB-donor-DU has changed.**
* **The lengthy term “the egress BH link corresponding to the BAP Routing ID of a received BAP PDU with the BAP address of the original IAB-donor-DU” can be better captured as “the source parent link”.**

**The Rapporteur therefore proposes the following rewording of R2-2204898:**

|  |
| --- |
| For UL traffic, after IAB-node migration, the BH link to the source parent node may be considered unavailable. |

**Q4b: Should the source parent-node BH link after IAB-node migration be included under “unavailable” BH links? If yes, do you agree on the above rewording proposed by the Rapporteur of the addition proposed by R2-2204898?**

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

Proposals by R2-2205256 on link unavailability:

|  |
| --- |
| A BH link may be considered *unavailable* for local rerouting in case the BH link has RLF. A parent link may be considered *unavailable* after a BH RLF detection indication has been received on this parent link and before a subsequent BH RLF recovery indication has been received on the same parent link. For DL traffic, a BH link may be considered *unavailable* for some routing ID for local rerouting due to congestion derived from flow-control feedback information, as defined in TS 38.340 [31]. |

**The Rapporteur believes that the addition of “for local rerouting” should NOT be included since the BH link is considered unavailable for ROUTING in general, not only for LOCAL RErouting.**

**The Rapporteur also proposes to change “some routing ID” to “a BAP routing ID”.**

**This would end up being:**

|  |
| --- |
| A BH link may be considered *unavailable* in case the BH link has RLF. A parent link may be considered *unavailable* after a BH RLF detection indication has been received on this parent link and before a subsequent BH RLF recovery indication has been received on the same parent link. For DL traffic, a BH link may be considered *unavailable* for a BAP routing ID due to congestion derived from flow-control feedback information, as defined in TS 38.340 [31]. |

**Q4c: Do you agree with the Rapporteur’s rewording of the rewording proposed by R2-2205256?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## On section: 9.2.3.4 Conditional Handover

Proposal by R2-2205902

**The following text is proposed to be removed by R2-2205902.**

|  |
| --- |
| CHO is also supported for the IAB-MT . |

**Q5: Do you agree with removal of the above text?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## On section: 9.2.7 Radio Link Failure

Proposals by R2-2204977 and R2-2205902:

|  |
| --- |
| The IAB-DU can transmit a BH RLF detection indication to its child nodes in the following cases:- The collocated IAB-MT initiates RRC re-establishment;- The collocated IAB-MT is dual-connected, e.g., configured with CP-UP split/NR-DC/EN-DC, detects BH RLF(s) on all the link(s)providing F1 interface over BAP; - The collocated IAB-MT has received a BH RLF detection indication from a parent node, and cannot perform UL re-routing for any traffic. |

**Q6: Do you agree with Change 1 and/or Change 2 to the RLF section?**

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## On section: 10.4 Measurements to Support Scheduler Operation

Proposals by R2-2205041 and R2-2205147:

**Both contributions propose to include the new BSRs into Section 10.4 on Basic Scheduler Operation. The contributions propose different wordings:**

**Proposal by R2-2205041:**

|  |
| --- |
| Uplink buffer status reports (BSR) are needed to provide support for QoS-aware packet scheduling. In NR, uplink buffer status reports refer to the data that is buffered in for a group of logical channels (LCG) in the UE. Four formats are used for reporting in uplink:- A short format to report only one BSR (of one LCG);- A flexible long format to report several BSRs (up to all eight LCGs).- An extended short format to report one BSR (of one LCG).- An extended long format to report several BSRs (up to all 256 LCGs).NOTE: The Extended versions of the BSR formats can only be used by IAB nodes. |

**Proposal by R2-2205147:**

|  |
| --- |
| Uplink buffer status reports (BSR) are needed to provide support for QoS-aware packet scheduling. In NR, uplink buffer status reports refer to the data that is buffered in for a group of logical channels (LCG) in the UE. Eight LCGs and two formats are used for reporting in uplink, except for IAB-MT where up to 256 LCGs are supported:- A short format to report only one BSR (of one LCG);- A flexible long format to report several BSRs (up to all eight LCGs/up to all 256 LCGs for an IAB-MT). |

**Q7: Should the new BSRs be included? If so, do you prefer the rewording by R2-2205041 or R2-2205147? Do you prefer a different rewording?**

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## On section: 10.9 IAB Resource Configuration

Proposals by R2-2204898

**R2-2204898 proposes multiple rewordings and additions for the purpose of clarification.**

|  |
| --- |
| If, the IAB-DU and the IAB-MT of an IAB-node are subject to a half-duplex constraint, as correct transmission/reception by one cannot be guaranteed during transmission/reception by the other and vice versa, e.g., when collocated and operating in the same frequency. If an IAB-node supports enhanced frequency or spatial multiplexing capabilities, additional multiplexing modes can be supported, i.e., simultaneous operation of IAB-MT Rx / IAB-DU Rx, IAB-MT Tx / IAB-DU Tx, IAB-MT Rx / IAB-DU Tx, IAB-MT Tx / IAB-DU Rx. An IAB-node can report its duplexing constraints between the IAB-MT and the IAB-DU via F1AP. An IAB-node can indicate via F1AP whether or not FDM is required for an enhanced multiplexing operation.…To facilitate transitioning from IAB-MT to IAB-DU operation and vice versa, guard symbols can be used at the beginning and/or the end of slots where the IAB-node switches operation from its IAB-DU to its IAB-MT function and operation from its IAB-MT to its IAB-DU function, to overcome potentially misaligned symbol boundaries between the IAB-MT domain and the IAB-DU domain (e.g., IAB-MT Rx boundaries are not aligned with the IAB-DU Tx boundaries). Specifically, an IAB-node can indicate to a parent node a number of desired guard symbols, while the parent node can indicate to the IAB-node the number of actually provided guard symbols for specific transitions (MT Rx to DU Tx, MT Rx to DU Rx, MT Tx to DU Tx, MT Tx to DU Rx, DU Rx to MT Tx, DU Rx to MT Rx, DU Tx to MT Tx, and DU Tx to MT Rx). An IAB-node supporting enhanced multiplexing capabilities, i.e., IAB-MT Rx / IAB-DU Rx, IAB-MT Tx / IAB-DU Tx, IAB-MT Rx / IAB-DU Tx, IAB-MT Tx / IAB-DU Rx, can provide via MAC-CE to a parent node information to facilitate scheduling for enhanced multiplexing operation by the IAB-node, specifically:* recommended IAB-MT’s Tx/Rx beams,
* desired IAB-MT Tx PSD range,
* desired parent node’s IAB-DU Tx power adjustment,
* required IAB-MT’s uplink transmission timing mode (for setting the IAB-MT transmission time to the transmission time of the IAB-DU).
 |

**Q8: Do you agree with Change 1, Change 2, Change 3 and Change 4 proposed?**

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## On further changes captured in draft CR

**Various minor changes proposed by various contributions have been captured in** **R2-22xxxxx draft CR to 38300 minor changes.**

**Q9: Do you agree with the changes proposed in this draft? Did you add comments into this draft?**

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 Conclusion

…

# 4 References

[1] R2-2204794, Miscellaneous IAB Corrections in 38.300, ZTE, Sanechips

[2] R2-2204898, Corrections to 38300, vivo

[3] R2-2204977, Correction on BH RLF detection indication, Lenovo (Beijing) Ltd

[4] R2-2205041, Clarification on extended BSR of eIAB for TS 38.300, NEC

[5] R2-2205147, Miscellaneous eIAB corrections to 38.300, Samsung R&D Institute UK

[6] R2-2205256, Corrections on rerouting in TS 38.300 for eIAB, Huawei, HiSilicon

[7] R2-2205902, Miscellaneous corrections to IAB stage-2 specification, Ericsson