**3GPP TSG-RAN WG3 Meeting #118-e *R2-22nnnn***

**E-meeting, 09 May – 19 May 2022**

**Title:** **[Draft] Reply LS on Flexible Global RAN Node ID**

**Response to: LS on Flexible Global RAN Node ID (R2-2206492/R3-223883)**

**Release: Rel-17**

**Work Item: TEI17**

**Source: RAN2**

**To: RAN3**

**Cc: -**

**Contact person: Ali Parichehreh**

**Ali.Parichehreh@Ericsson.com**

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

# Overall description

In response to RAN3 LS (R2-2206492/R3-223883), RAN2 would like to inform that RAN2 discussed the flexible gNB ID length issue and the gNB ID broadcast solution has been agreed with the following agreements.

* Include gNB ID length in PLMN-IdentityInfoList IE in SIB1.
* As an optional UE feature, the network can configure the UE to include the gNB ID length in reportCGI measurement report.

Hence RAN3 can consider that RAN2 supports the broadcast and reporting of gNB ID length in the relevant RAN2 specifications in Rel 17.

# 2 Actions

**To RAN3:**

**ACTION:** RAN2 asks RAN3 to take the above in to account.

# 3 Dates of next RAN2 meetings

The upcoming RAN2 meetings can be found in the [RAN2 Meetings calendar](https://portal.3gpp.org/Home.aspx?tbid=380&SubTB=380#/)